(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 42)
    (no_connects 0)
    (area 58.979999 113.589999 103.580001 140.410001)
    (thickness 1.6)
    (drawings 5)
    (tracks 151)
    (zones 0)
    (modules 23)
    (nets 34)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.006)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.027)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 "Net-(IC1-Pad1)")
  (net 2 "Net-(IC1-Pad11)")
  (net 3 "Net-(IC1-Pad12)")
  (net 4 "Net-(IC1-Pad13)")
  (net 5 "Net-(IC1-Pad14)")
  (net 6 "Net-(IC1-Pad15)")
  (net 7 "Net-(IC1-Pad16)")
  (net 8 "Net-(IC1-Pad17)")
  (net 9 "Net-(IC1-Pad19)")
  (net 10 "Net-(IC1-Pad20)")
  (net 11 "Net-(IC1-Pad22)")
  (net 12 "Net-(IC1-Pad23)")
  (net 13 "Net-(IC1-Pad25)")
  (net 14 "Net-(IC1-Pad26)")
  (net 15 "Net-(IC1-Pad27)")
  (net 16 "Net-(IC1-Pad28)")
  (net 17 "Net-(IC1-Pad29)")
  (net 18 "Net-(IC1-Pad30)")
  (net 19 "Net-(IC1-Pad31)")
  (net 20 GND)
  (net 21 +5V)
  (net 22 "Net-(C2-Pad1)")
  (net 23 "Net-(C2-Pad2)")
  (net 24 "Net-(C3-Pad2)")
  (net 25 "Net-(C4-Pad2)")
  (net 26 /DATA)
  (net 27 /TOUCH)
  (net 28 /SNS)
  (net 29 /DATA2)
  (net 30 "Net-(D1-Pad2)")
  (net 31 "Net-(D1-Pad1)")
  (net 32 "Net-(PJ1-Pad3)")
  (net 33 "Net-(IC1-Pad32)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /DATA)
    (add_net /DATA2)
    (add_net /SNS)
    (add_net /TOUCH)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad15)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad17)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad29)")
    (add_net "Net-(IC1-Pad30)")
    (add_net "Net-(IC1-Pad31)")
    (add_net "Net-(IC1-Pad32)")
    (add_net "Net-(PJ1-Pad3)")
  )
  (module Crystals:Crystal_HC49-SD_SMD (layer F.Cu) (tedit 570C52CF)
    (at 93.218 129.9845 90)
    (descr "Crystal Quarz HC49-SD SMD")
    (tags "Crystal Quarz HC49-SD SMD")
    (attr smd)
    (fp_text reference Y1 (at -6.9596 2.3876 90) (layer F.SilkS))
    (fp_text value 16MHZ (at -0.2032 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.84886 0 90) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 4.84886 0 90) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C4-Pad2)"))
    (model Crystals.3dshapes/Q_49U3HMS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ConnorFootprint:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 5718D70E)
    (at 81.3435 130.1115 180)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at -5.1816 -4.8895 180) (layer F.SilkS))
    (fp_text value ATMEGA328P-A (at 0 6.05 180) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -4.25 -2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 4 smd rect (at -4.25 -0.4 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 5 smd rect (at -4.25 0.4 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 6 smd rect (at -4.25 1.2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 7 smd rect (at -4.25 2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C3-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C4-Pad2)"))
    (pad 9 smd rect (at -2.8 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 /DATA))
    (pad 10 smd rect (at -2 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 /DATA2))
    (pad 11 smd rect (at -1.2 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at 1.2 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad14)"))
    (pad 15 smd rect (at 2 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad15)"))
    (pad 16 smd rect (at 2.8 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad16)"))
    (pad 17 smd rect (at 4.25 2.8 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad17)"))
    (pad 18 smd rect (at 4.25 2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 19 smd rect (at 4.25 1.2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 22 smd rect (at 4.25 -1.2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 27 /TOUCH))
    (pad 25 smd rect (at 2.8 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad25)"))
    (pad 26 smd rect (at 2 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad27)"))
    (pad 28 smd rect (at 0.4 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad28)"))
    (pad 29 smd rect (at -0.4 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad29)"))
    (pad 30 smd rect (at -1.2 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(IC1-Pad30)"))
    (pad 31 smd rect (at -2 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(IC1-Pad31)"))
    (pad 32 smd rect (at -2.8 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad32)"))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_8x10 (layer F.Cu) (tedit 57E84D03)
    (at 68.1355 134.1755)
    (descr "SMT capacitor, aluminium electrolytic, 8x10")
    (attr smd)
    (fp_text reference C5 (at -6.5405 3.6195) (layer F.SilkS))
    (fp_text value 4700uF (at 0 5.08) (layer F.Fab))
    (pad 1 smd rect (at 3.2512 0) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at -3.2512 0) (size 3.50012 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (model Capacitors_SMD.3dshapes/c_elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 57D6B205)
    (at 85.725 118.8085 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -3.175 -0.0635 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.1016 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 57D6B209)
    (at 88.8365 122.428 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -1.905 270) (layer F.SilkS))
    (fp_text value 10nF (at 0.1016 0.2032 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 570C5818)
    (at 97.155 132.2705 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 3.6068 -0.1524 270) (layer F.SilkS))
    (fp_text value 18pF (at -0.3048 0.1016 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 57D6B09C)
    (at 97.155 127.635 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 3.2639 -0.0127 90) (layer F.SilkS))
    (fp_text value 18pF (at 0 -0.1524 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ConnorFootprint:Solder_Pad (layer F.Cu) (tedit 570ECE24)
    (at 100.3935 118.3005 90)
    (fp_text reference SNS (at 1.9304 0.0508 180) (layer F.SilkS))
    (fp_text value SNS (at 0.0508 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 28 /SNS))
  )
  (module ConnorFootprint:Solder_Pad (layer F.Cu) (tedit 570ECDFA)
    (at 100.4316 126.2507 90)
    (fp_text reference DATA (at 1.8542 0.1524 180) (layer F.SilkS))
    (fp_text value DATA (at 0.1016 -0.1016 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 26 /DATA))
  )
  (module ConnorFootprint:Solder_Pad (layer F.Cu) (tedit 57D7662D)
    (at 100.457 137.287 90)
    (fp_text reference +5V (at 1.905 -0.127 180) (layer F.SilkS))
    (fp_text value 5V (at -0.127 -0.254 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
  )
  (module ConnorFootprint:Solder_Pad (layer F.Cu) (tedit 57D76635)
    (at 100.457 131.8895 90)
    (fp_text reference GND (at -1.905 0.127 180) (layer F.SilkS))
    (fp_text value GND (at 0.1016 -0.1016 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 57D6B20D)
    (at 82.677 122.2375 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.905 90) (layer F.SilkS))
    (fp_text value 10k (at -0.1524 0.0508 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 /TOUCH))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 570C5547)
    (at 95.758 118.237 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 10k (at 0.0508 -0.0508 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 /SNS))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ConnorFootprint:SOT-23-6 (layer F.Cu) (tedit 57D6B189)
    (at 85.8393 122.3391 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference PS1 (at -2.6289 0.0762 180) (layer F.SilkS))
    (fp_text value AT42QT1010 (at 0.6096 -2.2098 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 /TOUCH))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C2-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C2-Pad1)"))
    (pad 6 smd rect (at 1.1 -0.95 90) (size 1.06 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 5 smd rect (at 1.1 0 90) (size 1.06 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ConnorFootprint:Solder_Pad (layer F.Cu) (tedit 570ECDBE)
    (at 100.457 122.3645 90)
    (fp_text reference DATA2 (at 2.032 0 180) (layer F.SilkS))
    (fp_text value DATA2 (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 29 /DATA2))
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57D6B244)
    (at 85.5345 136.8425)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at -0.0635 1.651) (layer F.SilkS))
    (fp_text value Blink (at -0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 57D6B246)
    (at 80.8355 136.8425)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 1.9685) (layer F.SilkS))
    (fp_text value 270 (at -0.0635 0.127) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57D7672D)
    (at 74.803 129.3495 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 3.937 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57D6B1FD)
    (at 88.773 128.9685)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -0.0635 -1.651) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57D6B200)
    (at 88.773 131.318)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -0.127 1.651) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ConnorFootprint:LOGO (layer F.Cu) (tedit 0)
    (at 77.9145 120.65)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module C-Power:2.1x5.5_Barrel_Receptacle (layer F.Cu) (tedit 57E82F4F)
    (at 68.072 122.1105 270)
    (fp_text reference PJ1 (at 3.937 2.794 270) (layer F.SilkS))
    (fp_text value PJ-002AH-SMT (at -0.381 -2.54 270) (layer F.Fab))
    (pad 1 smd rect (at -3.128 -5.5 270) (size 2.4 2.8) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 1 smd rect (at 2.972 -5.5 270) (size 2.4 2.8) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at -3.128 5.5 270) (size 2.4 2.8) (layers F.Cu F.Paste F.Mask)
      (net 20 GND))
    (pad 3 smd rect (at 2.972 5.5 270) (size 2.4 2.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(PJ1-Pad3)"))
    (pad 0 thru_hole circle (at -3.128 0 270) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at 1.372 0 270) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask F.SilkS))
    (model "../../../../../../Users/Connor/Google Drive/Home Projects/DIY PCB/KiCad/Connor Library/3D/Barrel_Jack_SMD.wrl"
      (at (xyz -0.325 -0.22 0))
      (scale (xyz 0.035 0.035 0.04))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57E84D2C)
    (at 75.565 136.906)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.8415) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad29)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 59.055 140.335) (end 59.055 113.665) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.505 140.335) (end 59.055 140.335) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.505 113.665) (end 103.505 140.335) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.055 113.665) (end 103.505 113.665) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Neopixel Ctrl V1.6\nDDC Ltd." (at 80.01 116.84) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.0745 124.1679) (xy 88.1253 124.1679) (xy 88.1253 124.2187) (xy 88.0745 124.1679)
      )
    )
  )
  (zone (net 20) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69.85 127) (xy 67.31 127) (xy 67.31 139.7) (xy 59.69 139.7) (xy 59.69 114.3)
        (xy 69.85 114.3) (xy 69.85 127)
      )
    )
  )
  (zone (net 20) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.87 139.7) (xy 59.69 139.7) (xy 59.69 114.3) (xy 102.87 114.3) (xy 102.87 139.7)
      )
    )
  )
  (zone (net 21) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.87 127) (xy 102.87 127) (xy 102.87 133.35) (xy 102.87 133.35) (xy 102.87 139.7)
        (xy 68.58 139.7) (xy 68.58 128.27) (xy 71.12 128.27) (xy 71.12 114.3) (xy 102.87 114.3)
        (xy 102.87 127)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.455 133.35) (xy 78.105 133.35) (xy 78.105 127) (xy 84.455 127) (xy 84.455 133.35)
      )
    )
  )
)
