(kicad_pcb (version 4) (host pcbnew 4.0.4+dfsg1-stable)
  (general
    (links 99)
    (no_connects 0)
    (area 25.153 28.818 86.60696 77.677333)
    (thickness 1.6)
    (drawings 8)
    (tracks 549)
    (zones 0)
    (modules 37)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /+3.3v)
  (net 2 /GND)
  (net 3 "Net-(C6-Pad1)")
  (net 4 "Net-(C7-Pad1)")
  (net 5 "Net-(C8-Pad2)")
  (net 6 "Net-(C9-Pad2)")
  (net 7 "Net-(C10-Pad2)")
  (net 8 /MISO)
  (net 9 /MOSI)
  (net 10 /SCK)
  (net 11 /CS)
  (net 12 /RST)
  (net 13 "Net-(IC1-Pad14)")
  (net 14 /LEDB)
  (net 15 /LEDA)
  (net 16 "Net-(J1-PadYK)")
  (net 17 "Net-(J1-PadGK)")
  (net 18 /VIN)
  (net 19 /SW1)
  (net 20 /SW2)
  (net 21 /TEMP)
  (net 22 /TX)
  (net 23 /RX)
  (net 24 /PA0)
  (net 25 /PA1)
  (net 26 /PA2)
  (net 27 /PA3)
  (net 28 /P2)
  (net 29 /P3)
  (net 30 /P8)
  (net 31 /P10)
  (net 32 "Net-(P7-Pad9)")
  (net 33 /CLKOUT)
  (net 34 /Int)
  (net 35 /WOL)
  (net 36 /TPIN-)
  (net 37 /TPIN+)
  (net 38 /TPOUT-)
  (net 39 /TPOUT+)
  (net 40 /P9)
  (net 41 /P6)
  (net 42 "Net-(P6-Pad10)")
  (net 43 "Net-(P7-Pad10)")
  (net 44 "Net-(P7-Pad12)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+3.3v)
    (add_net /CLKOUT)
    (add_net /CS)
    (add_net /GND)
    (add_net /Int)
    (add_net /LEDA)
    (add_net /LEDB)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /P10)
    (add_net /P2)
    (add_net /P3)
    (add_net /P6)
    (add_net /P8)
    (add_net /P9)
    (add_net /PA0)
    (add_net /PA1)
    (add_net /PA2)
    (add_net /PA3)
    (add_net /RST)
    (add_net /RX)
    (add_net /SCK)
    (add_net /SW1)
    (add_net /SW2)
    (add_net /TEMP)
    (add_net /TPIN+)
    (add_net /TPIN-)
    (add_net /TPOUT+)
    (add_net /TPOUT-)
    (add_net /TX)
    (add_net /VIN)
    (add_net /WOL)
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(J1-PadGK)")
    (add_net "Net-(J1-PadYK)")
    (add_net "Net-(P6-Pad10)")
    (add_net "Net-(P7-Pad10)")
    (add_net "Net-(P7-Pad12)")
    (add_net "Net-(P7-Pad9)")
  )
  (module Magjack:MagJack-SI-52008-F (layer F.Cu) (tedit 58CF1376)
    (at 31.75 74.803)
    (fp_text reference J1 (at 5.588 -1.524) (layer F.SilkS))
    (fp_text value RJ45-SI52008-F (at 5.842 -3.556) (layer F.Fab))
    (pad YA thru_hole circle (at 8.636 -21.336) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 14 /LEDB))
    (pad YK thru_hole circle (at 11.176 -21.336) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-PadYK)"))
    (pad GK thru_hole circle (at 2.794 -21.336) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-PadGK)"))
    (pad GA thru_hole circle (at 0.254 -21.336) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 15 /LEDA))
    (pad 11 thru_hole circle (at 1.27 -19.05) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 8 thru_hole circle (at 2.54 -16.51) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 18 /VIN))
    (pad 9 thru_hole circle (at 1.27 -13.97) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 10 thru_hole circle (at 0 -16.51) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 18 /VIN))
    (pad 5 thru_hole circle (at 6.35 -13.97) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 36 /TPIN-))
    (pad 4 thru_hole circle (at 7.62 -16.51) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 37 /TPIN+))
    (pad 3 thru_hole circle (at 8.89 -13.97) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 38 /TPOUT-))
    (pad 2 thru_hole circle (at 10.16 -16.51) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 "Net-(C10-Pad2)"))
    (pad 13 thru_hole circle (at -2.032 -10.668) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad "" np_thru_hole circle (at 11.43 -7.62) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -7.62) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 13.462 -10.668) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 /GND))
    (pad 1 thru_hole circle (at 11.43 -13.97) (size 1.27 1.27) (drill 0.889) (layers *.Cu *.Mask)
      (net 39 /TPOUT+))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58CF1EAC)
    (at 66.675 53.848)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.429 0) (layer F.SilkS))
    (fp_text value C_Small (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58CF1EAE)
    (at 66.675 59.309)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.556 0.127) (layer F.SilkS))
    (fp_text value C_Small (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58CF1EB0)
    (at 66.675 61.468)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.556 0.127) (layer F.SilkS))
    (fp_text value C_Small (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58CF1EB2)
    (at 66.675 63.627)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 3.556 0) (layer F.SilkS))
    (fp_text value C_Small (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58D0F6D3)
    (at 78.867 59.69)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -0.127 -1.651) (layer F.SilkS))
    (fp_text value C_Small (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58D0F6CD)
    (at 78.867 63.246)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.651) (layer F.SilkS))
    (fp_text value C_Small (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58D0F6DB)
    (at 78.867 56.261)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -0.127 -1.778) (layer F.SilkS))
    (fp_text value C_Small (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58CF233F)
    (at 49.657 55.499)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -3.429 -0.127) (layer F.SilkS))
    (fp_text value C_Small (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58CF1FF2)
    (at 60.325 66.294 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -3.556 0 270) (layer B.SilkS))
    (fp_text value C_Small (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58CF1FDB)
    (at 58.166 66.294 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -3.937 0 270) (layer B.SilkS))
    (fp_text value C_Small (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C10-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 58.166 58.42)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference IC1 (at 0 -6.25) (layer F.SilkS))
    (fp_text value ENC28J60-C/SS (at 0 6.25) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -4.225) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C8-Pad2)"))
    (pad 2 smd rect (at -3.6 -3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 3 smd rect (at -3.6 -2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 /CLKOUT))
    (pad 4 smd rect (at -3.6 -2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 /Int))
    (pad 5 smd rect (at -3.6 -1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 /WOL))
    (pad 6 smd rect (at -3.6 -0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 /MISO))
    (pad 7 smd rect (at -3.6 -0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 /MOSI))
    (pad 8 smd rect (at -3.6 0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCK))
    (pad 9 smd rect (at -3.6 0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 /CS))
    (pad 10 smd rect (at -3.6 1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 /RST))
    (pad 11 smd rect (at -3.6 2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 12 smd rect (at -3.6 2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 /TPIN-))
    (pad 13 smd rect (at -3.6 3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 /TPIN+))
    (pad 14 smd rect (at -3.6 4.225) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad14)"))
    (pad 15 smd rect (at 3.6 4.225) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (pad 16 smd rect (at 3.6 3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 38 /TPOUT-))
    (pad 17 smd rect (at 3.6 2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 /TPOUT+))
    (pad 18 smd rect (at 3.6 2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 19 smd rect (at 3.6 1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (pad 20 smd rect (at 3.6 0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (pad 21 smd rect (at 3.6 0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 22 smd rect (at 3.6 -0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (pad 23 smd rect (at 3.6 -0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C6-Pad1)"))
    (pad 24 smd rect (at 3.6 -1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad1)"))
    (pad 25 smd rect (at 3.6 -2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 26 smd rect (at 3.6 -2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 14 /LEDB))
    (pad 27 smd rect (at 3.6 -3.575) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 /LEDA))
    (pad 28 smd rect (at 3.6 -4.225) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (model Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_Mini-Universal:MiniUniversalMate-N-LokSocket_2PinHorizontal (layer F.Cu) (tedit 58D2D4AA)
    (at 67.691 36.195 90)
    (descr "Mini Universal Mate-N-Lok Socket, 2 Pin, Horizontal,")
    (tags "Mini Universal Mate-N-Lok Socket, 2 Pin, Horizontal,")
    (fp_text reference P1 (at 1.27 -23.368 180) (layer F.SilkS))
    (fp_text value Door1 (at -0.16002 17.84096 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.0701 0 180) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 1 /+3.3v))
    (pad "" np_thru_hole circle (at 0 7.3406 90) (size 4.0005 4.0005) (drill 4.0005) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.0701 0.01016 180) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 19 /SW1))
  )
  (module Sockets_Mini-Universal:MiniUniversalMate-N-LokSocket_2PinHorizontal (layer F.Cu) (tedit 58D2D4A5)
    (at 67.691 47.244 90)
    (descr "Mini Universal Mate-N-Lok Socket, 2 Pin, Horizontal,")
    (tags "Mini Universal Mate-N-Lok Socket, 2 Pin, Horizontal,")
    (fp_text reference P2 (at 1.143 -23.241 180) (layer F.SilkS))
    (fp_text value Door2 (at -0.16002 17.84096 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.0701 0 180) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 1 /+3.3v))
    (pad "" np_thru_hole circle (at 0 7.3406 90) (size 4.0005 4.0005) (drill 4.0005) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.0701 0.01016 180) (size 2.49936 2.49936) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 20 /SW2))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58D0F70D)
    (at 30.353 32.893)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 7.239) (layer F.SilkS))
    (fp_text value Temp (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /TEMP))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /+3.3v))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 58CF2325)
    (at 47.498 72.644 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05 (layer F.Cu) (tedit 58D0F6AB)
    (at 76.708 70.358 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -2.54 10.922 360) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /+3.3v))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /TX))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /RX))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /P2))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /P3))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /PA0))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /PA1))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /PA2))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /PA3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12 (layer F.Cu) (tedit 0)
    (at 35.433 32.893 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value TOP (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /P9))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /P8))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /TEMP))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /P6))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /SW2))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /SW1))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /P3))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /P2))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P6-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /RX))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /TX))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12 (layer F.Cu) (tedit 0)
    (at 35.433 48.133 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value Bottom (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /P10))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /MOSI))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /MISO))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SCK))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /PA0))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /PA1))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /PA2))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /PA3))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(P7-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P7-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(P7-Pad12)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 58D0F6FD)
    (at 30.353 48.133 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 0 4.572 180) (layer F.SilkS))
    (fp_text value ArduinoPower (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(P7-Pad9)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /+3.3v))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D0F72E)
    (at 62.738 38.989 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.429 0 180) (layer F.SilkS))
    (fp_text value R_Small (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /SW1))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D0F735)
    (at 62.738 41.275 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.429 0 180) (layer F.SilkS))
    (fp_text value R_Small (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /SW2))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D0F711)
    (at 33.147 37.084 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -2.1 360) (layer F.SilkS))
    (fp_text value R_Small (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /TEMP))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58CF2338)
    (at 49.657 59.944 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.429 0 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /RST))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58CF233B)
    (at 49.657 57.658 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 3.429 0 180) (layer F.SilkS))
    (fp_text value R (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /CS))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3v))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58CF2333)
    (at 49.657 62.103)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -3.429 0.127) (layer F.SilkS))
    (fp_text value R (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad14)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58D0F7BA)
    (at 53.848 66.294 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.302 -0.127 90) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 /+3.3v))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58CF1FEA)
    (at 49.53 66.294 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -3.429 -0.127 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 37 /TPIN+))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58CF1FEE)
    (at 47.371 66.294 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -3.429 -0.127 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 36 /TPIN-))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58D0F7B2)
    (at 51.689 66.294 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 3.81 0 90) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 38 /TPOUT-))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D0F717)
    (at 38.735 39.116)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 3.81 0) (layer F.SilkS))
    (fp_text value 0 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /P8))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /CS))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D0F71F)
    (at 38.735 41.275)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 3.81 0) (layer F.SilkS))
    (fp_text value 0 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /P10))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /CS))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58D0F7C4)
    (at 56.007 66.294 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 3.81 0 90) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C10-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 39 /TPOUT+))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D0F7D7)
    (at 33.147 51.562)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 3.8735 -0.0635) (layer F.SilkS))
    (fp_text value R (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-PadGK)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58D0F7CF)
    (at 41.529 51.562)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 3.8735 0.0635) (layer F.SilkS))
    (fp_text value R (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-PadYK)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-SD_SMD (layer F.Cu) (tedit 58D80153)
    (at 73.787 60.706 90)
    (descr "Crystal Quarz HC49-SD SMD")
    (tags "Crystal Quarz HC49-SD SMD")
    (attr smd)
    (fp_text reference Y1 (at 6.985 2.413 180) (layer F.SilkS))
    (fp_text value Crystal_Small (at 2.54 5.08 90) (layer F.Fab))
    (pad 1 smd rect (at -4.84886 0 90) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 4.84886 0 90) (size 5.6007 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad1)"))
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 58D0F6A1)
    (at 57.785 71.374 180)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference U1 (at 4.445 2.794 180) (layer F.SilkS))
    (fp_text value LM1117-3.3 (at 0 3.81 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 /+3.3v))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 /GND))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 18 /VIN))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "A2 A3\n\n\nA0 A1\n\n\n 2  3\n\n\nTX RX\n\n\n V  G" (at 71.374 66.7385 90) (layer B.SilkS))
  (gr_text Door2 (at 75.692 50.7365) (layer F.SilkS))
  (gr_text Door1 (at 75.565 39.878) (layer F.SilkS))
  (gr_text "Arduino Pro Mini" (at 46.4185 43.815) (layer F.SilkS))
  (gr_line (start 82.1055 74.676) (end 27.813 74.676) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82.1055 30.988) (end 82.1055 74.676) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 27.813 30.988) (end 82.1055 30.988) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 27.813 74.676) (end 27.813 30.988) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.8515 31.242) (xy 81.8515 74.422) (xy 28.067 74.422) (xy 28.067 31.242)
      )
    )
  )
  (zone (net 2) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.8515 31.242) (xy 81.8515 74.422) (xy 28.067 74.422) (xy 28.067 31.242)
      )
    )
  )
)
