<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="71.11740625" y2="0.01143125" width="0" layer="20"/>
<wire x1="71.11740625" y1="0.01143125" x2="71.11740625" y2="60.96" width="0" layer="20"/>
<wire x1="71.11740625" y1="60.96" x2="0" y2="60.96" width="0" layer="20"/>
<wire x1="0" y1="60.96" x2="0" y2="0" width="0" layer="20"/>
<text>RV-Project.Com 4 Channel Receiver
A2D2 Combo</text>
<text>Ver2.0</text>
<text>For BX-3308BMB</text>
<text>Motor</text>
<text>Motor</text>
<text>GND</text>
<text>Mo Switch</text>
<text>Mo Switch</text>
<text>12V Constant</text>
<text>Switched
 12VDC</text>
<text>GND</text>
<text>3/4/2019</text>
<text>Max 8.5A w/o Trace Solder</text>
<text>2A</text>
<hole x="11.3284" y="6.2484" drill="2.794"/>
<text>5V    GND   ANT</text>
<text>GND DATA        5V</text>
<text>USB</text>
<text>Ch3 GND</text>
<text>Ch4 GND</text>
<text>and 2 Oz Copper.</text>
<hole x="59.7916" y="6.2484" drill="2.54"/>
<text>Receive</text>
<text>Channel</text>
<text>RX6B</text>
<text>SDA</text>
<text>SCL</text>
<text>5V</text>
<text>GND</text>
<text>Specify 2 Oz Copper</text>
<text>Monitor</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="RADIAL_ELECTROLYTIC_100MIL(5MM)">
<description>Generic Electrolytic Capacitor 0.100 spacing 0.200 diameter.</description>
</package>
<package name="1206-CAP">
</package>
<package name="KF7.62CONNECTOR2">
</package>
<package name="ARDUINO_NANO">
</package>
<package name="TO-220-REGULATOR">
</package>
<package name="SOD-123(LARGE)">
<description>100V/150mA 1N4148 - Super Cheap</description>
</package>
<package name="KEYSTONE_3553">
</package>
<package name="CREATIVECOMMONS_SMALL">
</package>
<package name="ART_CHEROKEE_LARGE">
</package>
<package name="RX6B_ASK_RECEIVER">
</package>
<package name="ANT_CONN_V">
</package>
<package name="ACJ21XX_RELAY">
</package>
<package name="ACJ51XX_RELAY">
</package>
<package name="TO-92-AMMO">
</package>
<package name="SMA-DIODE_ALT">
</package>
<package name="G5V">
</package>
<package name="1206-RES">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="KF7.62CONNECTOR3">
</package>
<package name="WAFER4PINVERTICAL">
</package>
</packages>
</library>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="ICSP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="a-lib" package="RADIAL_ELECTROLYTIC_100MIL(5MM)" value="10UF">
<attribute name="MARKING" value="106"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value="25v"/>
</element>
<element name="C2" library="a-lib" package="1206-CAP" value="0.33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="a-lib" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="a-lib" package="ARDUINO_NANO" value="ARDUINO_NANO">
<attribute name="NAME"/>
</element>
<element name="U1" library="a-lib" package="TO-220-REGULATOR" value="78XX">
<attribute name="VALUE" value="78XX"/>
</element>
<element name="C4" library="a-lib" package="1206-CAP" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="a-lib" package="SOD-123(LARGE)" value="TVS-SEASY_SOD-123">
<attribute name="NAME"/>
</element>
<element name="F1" library="a-lib" package="KEYSTONE_3553" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="a-lib" package="CREATIVECOMMONS_SMALL" value=""/>
<element name="U$1" library="a-lib" package="ART_CHEROKEE_LARGE" value=""/>
<element name="RX1" library="a-lib" package="RX6B_ASK_RECEIVER" value="RXB6_ASK_RECEIVER"/>
<element name="J5" library="a-lib" package="ANT_CONN_V" value="SMT_ANT_CONNVERTICAL"/>
<element name="K2" library="a-lib" package="ACJ21XX_RELAY" value="TWINCOILMOTORRELAYACJ21XX">
<attribute name="NAME"/>
</element>
<element name="K1" library="a-lib" package="ACJ51XX_RELAY" value="TWINCOILSPDTRELAYACJ51XX_10PIN">
<attribute name="NAME"/>
</element>
<element name="Q4" library="a-lib" package="TO-92-AMMO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="a-lib" package="TO-92-AMMO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="a-lib" package="SMA-DIODE_ALT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="a-lib" package="SMA-DIODE_ALT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="a-lib" package="KF7.62CONNECTOR2" value="KF762-2CONNECTOR"/>
<element name="RY1" library="a-lib" package="G5V" value="G5V5V">
<attribute name="ALTPARTNO" value="G5V-1-1"/>
<attribute name="COIL" value="30mA"/>
<attribute name="CONTACT" value="1Amp"/>
<attribute name="INPUT" value="5V"/>
<attribute name="NAME"/>
<attribute name="PARTNO" value="G5V-1-2"/>
</element>
<element name="RY2" library="a-lib" package="G5V" value="G5V5V">
<attribute name="ALTPARTNO" value="G5V-1-1"/>
<attribute name="COIL" value="30mA"/>
<attribute name="CONTACT" value="1Amp"/>
<attribute name="INPUT" value="5V"/>
<attribute name="NAME"/>
<attribute name="PARTNO" value="G5V-1-2"/>
</element>
<element name="R6" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R4" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="R2" library="a-lib" package="1206-RES" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE" value="10k"/>
</element>
<element name="Q2" library="a-lib" package="TO-92-AMMO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="a-lib" package="TO-92-AMMO" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="a-lib" package="SMA-DIODE_ALT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="a-lib" package="SMA-DIODE_ALT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="a-lib" package="KF7.62CONNECTOR3" value="KF762-3CONNECTOR"/>
<element name="J3" library="a-lib" package="KF7.62CONNECTOR3" value="KF762-3CONNECTOR"/>
<element name="J1" library="a-lib" package="WAFER4PINVERTICAL" value="WAFER4PVERTICAL"/>
<element name="LED3" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R7" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="a-lib_Connectors" package="ICSP" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="GND"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="GND"/>
<contactref element="C4" pad="2"/>
<contactref element="U2" pad="GND1"/>
<contactref element="D3" pad="A"/>
<contactref element="J5" pad="G1"/>
<contactref element="J5" pad="G2"/>
<contactref element="J5" pad="G3"/>
<contactref element="J5" pad="G4"/>
<contactref element="RX1" pad="GND1"/>
<contactref element="RX1" pad="GND2"/>
<contactref element="RX1" pad="GND"/>
<contactref element="K2" pad="NC"/>
<contactref element="Q3" pad="1"/>
<contactref element="Q4" pad="1"/>
<contactref element="K1" pad="L2A"/>
<contactref element="K1" pad="L1A"/>
<contactref element="Q2" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="LED2" pad="K"/>
<contactref element="J3" pad="2"/>
<contactref element="J2" pad="3"/>
<contactref element="J1" pad="P$1"/>
<contactref element="J1" pad="P$3"/>
<contactref element="LED3" pad="K"/>
<contactref element="J6" pad="GND"/>
<contactref element="J6" pad="RST"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="OUT"/>
<contactref element="C3" pad="1"/>
<contactref element="RX1" pad="5V"/>
<contactref element="RX1" pad="5V1"/>
<contactref element="D2" pad="C"/>
<contactref element="RY2" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="RY1" pad="2"/>
<contactref element="U2" pad="VIN"/>
<contactref element="C4" pad="1"/>
<contactref element="J6" pad="VCC"/>
<contactref element="J6" pad="MOSI"/>
</signal>
<signal name="N$24">
<contactref element="R4" pad="2"/>
<contactref element="U2" pad="A1"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="D2"/>
<contactref element="RX1" pad="DATA"/>
</signal>
<signal name="N$2">
<contactref element="RX1" pad="ANT"/>
<contactref element="J5" pad="A1"/>
</signal>
<signal name="N$3">
<contactref element="K1" pad="2NC"/>
<contactref element="K2" pad="C1"/>
</signal>
<signal name="N$5">
<contactref element="K1" pad="1NC"/>
<contactref element="K2" pad="C2"/>
</signal>
<signal name="N$8">
<contactref element="Q3" pad="3"/>
<contactref element="K2" pad="L2B"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="Q4" pad="3"/>
<contactref element="K2" pad="L1B"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="IN"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="F1" pad="P$2"/>
</signal>
<signal name="12V">
<contactref element="K2" pad="L2A"/>
<contactref element="K2" pad="L1A"/>
<contactref element="D5" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="K2" pad="NO"/>
<contactref element="K1" pad="2NO"/>
<contactref element="RY2" pad="COM1"/>
<contactref element="RY2" pad="COM2"/>
<contactref element="RY1" pad="COM1"/>
<contactref element="RY1" pad="COM2"/>
<contactref element="K1" pad="1NO"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="K1" pad="L1B"/>
<contactref element="J4" pad="2A"/>
</signal>
<signal name="N$15">
<contactref element="R4" pad="1"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="A2"/>
</signal>
<signal name="N$25">
<contactref element="R1" pad="2"/>
<contactref element="U2" pad="A3"/>
</signal>
<signal name="N$26">
<contactref element="Q2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="Q1" pad="3"/>
<contactref element="RY1" pad="9"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$29">
<contactref element="Q2" pad="3"/>
<contactref element="RY2" pad="9"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$30">
<contactref element="RY2" pad="NO"/>
<contactref element="J1" pad="P$2"/>
</signal>
<signal name="N$31">
<contactref element="RY1" pad="NO"/>
<contactref element="J1" pad="P$4"/>
</signal>
<signal name="N$32">
<contactref element="LED2" pad="A"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="U2" pad="A0"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R6" pad="1"/>
<contactref element="Q4" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="F1" pad="P$1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="K1" pad="2C"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="J4" pad="1"/>
<contactref element="K1" pad="1C"/>
</signal>
<signal name="N$13">
<contactref element="K1" pad="L2B"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R5" pad="2"/>
<contactref element="U2" pad="D4"/>
</signal>
<signal name="N$10">
<contactref element="LED3" pad="A"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="U2" pad="D5"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="U2" pad="A4"/>
<contactref element="J6" pad="MISO"/>
</signal>
<signal name="N$33">
<contactref element="U2" pad="A5"/>
<contactref element="J6" pad="SCK"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
