<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="9.3472" y2="0" width="0" layer="20"/>
<wire x1="9.3472" y1="0" x2="9.3472" y2="75.1586" width="0" layer="20"/>
<wire x1="9.3472" y1="75.1586" x2="0" y2="75.1586" width="0" layer="20"/>
<wire x1="0" y1="75.1586" x2="0" y2="0" width="0" layer="20"/>
<text>VCC</text>
<text>GND</text>
<text>Mike Neiderhauser</text>
<text>Rev: 0.1  -  May 21, 2014</text>
<text>WS2812B Chain Stick</text>
<text>VCC</text>
<text>GND</text>
<text>DOUT</text>
<text>DOUT</text>
<text>DIN</text>
<text>LED 0
Cap 0</text>
<text>LED 1
Cap 1</text>
<text>LED 2
Cap 2</text>
<text>LED 3
Cap 3</text>
<text>LED 4
Cap 4</text>
<text>LED 5
Cap 5</text>
<text>LED 6
Cap 6</text>
<text>LED 7
Cap 7</text>
<text>CAPS: 0805</text>
<text>&lt;-</text>
<text>DIN</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="WS2812B">
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="L1" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L2" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L3" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L4" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L5" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L6" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L7" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L8" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="C1" library="adafruit" package="C0805" value="">
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0805" value="">
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0805" value="">
<attribute name="VALUE"/>
</element>
<element name="C4" library="adafruit" package="C0805" value="">
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="C0805" value="">
<attribute name="VALUE"/>
</element>
<element name="C6" library="adafruit" package="C0805" value="">
<attribute name="VALUE"/>
</element>
<element name="C7" library="adafruit" package="C0805" value="">
<attribute name="VALUE"/>
</element>
<element name="C8" library="adafruit" package="C0805" value="">
<attribute name="VALUE"/>
</element>
<element name="TP1_VCC" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP2_DIN" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP3_GND" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP4_VCC" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP5_DOUT" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP6_GND" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TPE_VCC" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TPE_GND" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP_DIN2" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP_DOUT2" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
</elements>
<signals>
<signal name="L_1_2">
<contactref element="L1" pad="2-DOUT"/>
<contactref element="L2" pad="4-DIN"/>
</signal>
<signal name="L_2_3">
<contactref element="L2" pad="2-DOUT"/>
<contactref element="L3" pad="4-DIN"/>
</signal>
<signal name="L_3_4">
<contactref element="L3" pad="2-DOUT"/>
<contactref element="L4" pad="4-DIN"/>
</signal>
<signal name="L_4_5">
<contactref element="L4" pad="2-DOUT"/>
<contactref element="L5" pad="4-DIN"/>
</signal>
<signal name="L_5_6">
<contactref element="L5" pad="2-DOUT"/>
<contactref element="L6" pad="4-DIN"/>
</signal>
<signal name="L_6_7">
<contactref element="L6" pad="2-DOUT"/>
<contactref element="L7" pad="4-DIN"/>
</signal>
<signal name="L_7_8">
<contactref element="L7" pad="2-DOUT"/>
<contactref element="L8" pad="4-DIN"/>
</signal>
<signal name="GND">
<contactref element="L1" pad="3-GND"/>
<contactref element="L2" pad="3-GND"/>
<contactref element="L3" pad="3-GND"/>
<contactref element="L4" pad="3-GND"/>
<contactref element="L5" pad="3-GND"/>
<contactref element="L6" pad="3-GND"/>
<contactref element="L7" pad="3-GND"/>
<contactref element="L8" pad="3-GND"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="TP6_GND" pad="TP"/>
<contactref element="TP3_GND" pad="TP"/>
<contactref element="TPE_GND" pad="TP"/>
</signal>
<signal name="VCC">
<contactref element="L1" pad="1-VDD"/>
<contactref element="C1" pad="1"/>
<contactref element="L2" pad="1-VDD"/>
<contactref element="C2" pad="1"/>
<contactref element="L3" pad="1-VDD"/>
<contactref element="C3" pad="1"/>
<contactref element="L4" pad="1-VDD"/>
<contactref element="C4" pad="1"/>
<contactref element="L5" pad="1-VDD"/>
<contactref element="C5" pad="1"/>
<contactref element="L6" pad="1-VDD"/>
<contactref element="C6" pad="1"/>
<contactref element="L7" pad="1-VDD"/>
<contactref element="C7" pad="1"/>
<contactref element="L8" pad="1-VDD"/>
<contactref element="C8" pad="1"/>
<contactref element="TP1_VCC" pad="TP"/>
<contactref element="TP4_VCC" pad="TP"/>
<contactref element="TPE_VCC" pad="TP"/>
</signal>
<signal name="DIN">
<contactref element="L1" pad="4-DIN"/>
<contactref element="TP2_DIN" pad="TP"/>
<contactref element="TP_DIN2" pad="TP"/>
</signal>
<signal name="DOUT">
<contactref element="L8" pad="2-DOUT"/>
<contactref element="TP5_DOUT" pad="TP"/>
<contactref element="TP_DOUT2" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
