(kicad_pcb (version 20171130) (host pcbnew 5.1.9)
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 32)
    (zones 0)
    (modules 16)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net 3 "Net-(J3-Pad1)")
  (net 4 "Net-(J4-Pad1)")
  (net 5 "Net-(J5-Pad1)")
  (net 6 "Net-(J6-Pad1)")
  (net 7 "Net-(J7-Pad1)")
  (net 8 "Net-(J8-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
  )
  (module cell-12-puck:wire_pad (layer F.Cu) (tedit 603FE6BB)
    (at 100.33 100.838)
    (fp_text reference 4 (at 1.143 -0.635) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.54) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J4-Pad1)"))
  )
  (module cell-12-puck:wire_pad (layer F.Cu) (tedit 603FE6BB)
    (at 97.663 105.029 90)
    (fp_text reference 8 (at -1.016 0.762 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.54 90) (layer F.Fab))
    (pad 1 smd oval (at 0 0 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J8-Pad1)"))
  )
  (module cell-12-puck:wire_pad (layer F.Cu) (tedit 603FE6BB)
    (at 99.441 105.156 135)
    (fp_text reference 7 (at -1.436841 0.179605 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.54 135) (layer F.Fab))
    (pad 1 smd oval (at 0 0 135) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J7-Pad1)"))
  )
  (module cell-12-puck:wire_pad (layer F.Cu) (tedit 603FE6BB)
    (at 100.457 104.14 135)
    (fp_text reference 6 (at -0.35921 0.898026 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.54 135) (layer F.Fab))
    (pad 1 smd oval (at 0 0 135) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J6-Pad1)"))
  )
  (module cell-12-puck:wire_pad (layer F.Cu) (tedit 603FE6BB)
    (at 100.33 102.362)
    (fp_text reference 5 (at 1.143 0.635) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.54) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J5-Pad1)"))
  )
  (module cell-12-puck:wire_pad (layer F.Cu) (tedit 603FE6BB)
    (at 100.457 99.06 45)
    (fp_text reference 3 (at 0.35921 0.898026) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.54 45) (layer F.Fab))
    (pad 1 smd oval (at 0 0 45) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J3-Pad1)"))
  )
  (module cell-12-puck:wire_pad (layer F.Cu) (tedit 603FE6BB)
    (at 99.441 98.044 45)
    (fp_text reference 2 (at 1.436841 0.179605 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.54 45) (layer F.Fab))
    (pad 1 smd oval (at 0 0 45) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad1)"))
  )
  (module cell-12-puck:wire_pad (layer F.Cu) (tedit 603FE6BB)
    (at 97.663 98.171 90)
    (fp_text reference 1 (at 1.016 0.762 180) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.54 90) (layer F.Fab))
    (pad 1 smd oval (at 0 0 90) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (module cell-12-puck:sample_pad (layer F.Cu) (tedit 603FCDC8)
    (at 105.537 105.537)
    (fp_text reference 8 (at -1.016 0.381) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J8-Pad1)"))
  )
  (module cell-12-puck:sample_pad (layer F.Cu) (tedit 603FCDC8)
    (at 102.362 105.537)
    (fp_text reference P7 (at 1.778 2.286) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J7-Pad1)"))
  )
  (module cell-12-puck:sample_pad (layer F.Cu) (tedit 603FCDC8)
    (at 105.537 102.362)
    (fp_text reference 6 (at -0.889 0.381) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J6-Pad1)"))
  )
  (module cell-12-puck:sample_pad (layer F.Cu) (tedit 603FCDC8)
    (at 102.362 102.362)
    (fp_text reference P5 (at 10.795 3.937) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J5-Pad1)"))
  )
  (module cell-12-puck:sample_pad (layer F.Cu) (tedit 603FCDC8)
    (at 102.362 100.838)
    (fp_text reference P4 (at 9.398 -2.413) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J4-Pad1)"))
  )
  (module cell-12-puck:sample_pad (layer F.Cu) (tedit 603FCDC8)
    (at 105.537 100.838)
    (fp_text reference 3 (at -0.889 -0.381) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J3-Pad1)"))
  )
  (module cell-12-puck:sample_pad (layer F.Cu) (tedit 603FCDC8)
    (at 102.362 97.663)
    (fp_text reference P2 (at 0.127 -1.397) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad1)"))
  )
  (module cell-12-puck:sample_pad (layer F.Cu) (tedit 603FCDC8)
    (at 105.537 97.663)
    (fp_text reference 1 (at -1.016 -0.381) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -2.54) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (gr_text "Cell-12 rotator\nsample board\nv1" (at 102.997 101.6 -90) (layer B.SilkS))
  (gr_line (start 99.06 102.616) (end 99.06 100.584) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.917 103.759) (end 99.06 102.616) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.409 103.759) (end 97.917 103.759) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.409 99.441) (end 97.917 99.441) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.917 99.441) (end 99.06 100.584) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 96.901 97.409) (end 96.901 98.933) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.409 96.901) (end 96.901 97.409) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.172 96.901) (end 97.409 96.901) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.299 97.028) (end 106.172 96.901) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.299 106.172) (end 106.299 97.028) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 106.172 106.299) (end 106.299 106.172) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.409 106.299) (end 106.172 106.299) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 96.901 105.791) (end 97.409 106.299) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 96.901 104.267) (end 96.901 105.791) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.409 99.441) (end 96.901 98.933) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.409 103.759) (end 96.901 104.267) (layer Edge.Cuts) (width 0.05))
)
