(kicad_pcb (version 4) (host pcbnew 4.0.4-1.fc25-product)
  (general
    (links 47)
    (no_connects 1)
    (area 89.326719 43.215559 178.510001 123.265001)
    (thickness 1.6)
    (drawings 33)
    (tracks 199)
    (zones 0)
    (modules 19)
    (nets 58)
  )
  (page USLetter)
  (title_block
    (title "Project Title")
  )
  (layers
    (0 F.Cu jumper)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.1524)
    (edge_width 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3556)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.1524)
    (pcb_text_size 1.016 1.016)
    (mod_edge_width 0.1524)
    (mod_text_size 1.016 1.016)
    (mod_text_width 0.1524)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (pad_to_paste_clearance -0.0762)
    (aux_axis_origin 196.5452 123.5456)
    (grid_origin -114.10188 32.77616)
    (visible_elements FFFCFF01)
    (pcbplotparams
      (layerselection 0x310fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad12)")
  (net 12 "Net-(J1-Pad18)")
  (net 13 "Net-(J1-Pad19)")
  (net 14 "Net-(J1-Pad20)")
  (net 15 "Net-(J1-Pad21)")
  (net 16 "Net-(J1-Pad22)")
  (net 17 "Net-(J1-Pad23)")
  (net 18 "Net-(C2-Pad1)")
  (net 19 "Net-(C2-Pad2)")
  (net 20 VGH)
  (net 21 PRVGL)
  (net 22 VGL)
  (net 23 VDD)
  (net 24 VSH)
  (net 25 VGH2)
  (net 26 VSL)
  (net 27 VCOM)
  (net 28 GDR)
  (net 29 RESE)
  (net 30 TSCL)
  (net 31 TSDA)
  (net 32 BUSY)
  (net 33 ^RES)
  (net 34 ^D/C)
  (net 35 ^CS)
  (net 36 SCK)
  (net 37 DOUT)
  (net 38 VPP)
  (net 39 VDDIO)
  (net 40 "Net-(J1-Pad0)")
  (net 41 "Net-(J1-PadPGM)")
  (net 42 "Net-(J1-PadDAC)")
  (net 43 "Net-(J1-Pad3V2)")
  (net 44 "Net-(J1-PadVIN)")
  (net 45 "Net-(J1-PadVBAT)")
  (net 46 GND)
  (net 47 "Net-(J2-Pad2)")
  (net 48 "Net-(J2-Pad1)")
  (net 49 "Net-(J2-Pad3)")
  (net 50 "Net-(J2-Pad4)")
  (net 51 "Net-(J2-Pad5)")
  (net 52 "Net-(J2-Pad29)")
  (net 53 "Net-(J2-Pad30)")
  (net 54 "Net-(J2-Pad31)")
  (net 55 "Net-(J2-Pad32)")
  (net 56 "Net-(J2-Pad33)")
  (net 57 "Net-(J2-Pad34)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3556)
    (uvia_drill 0.254)
    (add_net BUSY)
    (add_net DOUT)
    (add_net GDR)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad3V2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J1-PadDAC)")
    (add_net "Net-(J1-PadPGM)")
    (add_net "Net-(J1-PadVBAT)")
    (add_net "Net-(J1-PadVIN)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad29)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad30)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad34)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net PRVGL)
    (add_net RESE)
    (add_net SCK)
    (add_net TSCL)
    (add_net TSDA)
    (add_net VCOM)
    (add_net VDD)
    (add_net VDDIO)
    (add_net VGH)
    (add_net VGH2)
    (add_net VGL)
    (add_net VPP)
    (add_net VSH)
    (add_net VSL)
    (add_net ^CS)
    (add_net ^D/C)
    (add_net ^RES)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 105.02392 63.28156)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 2.1) (layer B.SilkS))
    (fp_text value CAP-CER-1UF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 39 VDDIO))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 97.4979 80.52562 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value CAP-CER-1UF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 135.63092 58.02376 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value CAP-CER-1UF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 20 VGH))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 135.74522 74.40676 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value CAP-CER-1UF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 21 PRVGL))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 135.58012 53.95976 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value CAP-CER-1UF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 22 VGL))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 105.02646 65.82918)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 2.1) (layer B.SilkS))
    (fp_text value CAP-CER-1UF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 23 VDD))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 135.52932 61.93536 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value CAP-CER-1UF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 24 VSH))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 135.43788 65.93332 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value CAP-CER-1UF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 25 VGH2))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 135.74522 78.14056 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value CAP-CER-1UF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 27 VCOM))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 135.47852 70.13956 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value CAP-CER-1UF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 26 VSL))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 5530FCB9)
    (at 102.09276 80.13192 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 2 270) (layer B.SilkS))
    (fp_text value DIODE (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C2-Pad1)"))
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 5530FCB9)
    (at 104.6226 53.4924 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 2 180) (layer B.SilkS))
    (fp_text value DIODE (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.635 0 180) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 20 VGH))
    (pad 2 smd rect (at 1.635 0 180) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C2-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 5530FCB9)
    (at 106.7308 80.13192 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 0 2 90) (layer B.SilkS))
    (fp_text value DIODE (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.635 0 90) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.635 0 90) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 21 PRVGL))
  )
  (module Wickerlib:TEENSY-3.2-SILK (layer F.Cu) (tedit 583B5CF0)
    (at 155.2194 70.4977 180)
    (fp_text reference J1 (at -2 0 180) (layer F.Fab))
    (fp_text value TEENSY3.2-72MHz (at -2.54 20.32 180) (layer F.Fab) hide)
    (fp_text user VIN (at 8.382095 -10.16 180) (layer F.SilkS))
    (fp_text user %R (at 5.08 -12.7 180) (layer F.SilkS))
    (fp_text user AGND (at 9.144 -7.62 180) (layer F.SilkS))
    (fp_text user 3.3V (at 8.810666 -5.08 180) (layer F.SilkS))
    (fp_text user 23 (at 8.144 -2.54 180) (layer F.SilkS))
    (fp_text user 22 (at 8.144 0 180) (layer F.SilkS))
    (fp_text user 21 (at 8.144 2.54 180) (layer F.SilkS))
    (fp_text user 20 (at 8.144 5.08 180) (layer F.SilkS))
    (fp_text user 19 (at 8.144 7.62 180) (layer F.SilkS))
    (fp_text user 18 (at 8.144 10.16 180) (layer F.SilkS))
    (fp_text user 17 (at 8.144 12.7 180) (layer F.SilkS))
    (fp_text user 16 (at 8.144 15.24 180) (layer F.SilkS))
    (fp_text user 15 (at 8.144 17.78 180) (layer F.SilkS))
    (fp_text user 14 (at 8.144 20.32 180) (layer F.SilkS))
    (fp_text user 13 (at 8.144 22.86 180) (layer F.SilkS))
    (fp_text user 0 (at -12.668381 -7.62 180) (layer F.SilkS))
    (fp_text user GND (at -13.716 -10.16 180) (layer F.SilkS))
    (fp_text user VBAT (at -7.62 26.416 270) (layer F.SilkS))
    (fp_text user 3.3V (at -5.08 26.416 270) (layer F.SilkS))
    (fp_text user GND (at -2.54 26.416 270) (layer F.SilkS))
    (fp_text user PGM (at 0 26.416 270) (layer F.SilkS))
    (fp_text user DAC (at 2.54 26.416 270) (layer F.SilkS))
    (fp_text user 1 (at -12.668381 -5.08 180) (layer F.SilkS))
    (fp_text user 2 (at -12.668381 -2.54 180) (layer F.SilkS))
    (fp_text user 3 (at -12.668381 0 180) (layer F.SilkS))
    (fp_text user 4 (at -12.668381 2.54 180) (layer F.SilkS))
    (fp_text user 5 (at -12.668381 5.08 180) (layer F.SilkS))
    (fp_text user 6 (at -12.668381 7.62 180) (layer F.SilkS))
    (fp_text user 7 (at -12.668381 10.16 180) (layer F.SilkS))
    (fp_text user 8 (at -12.668381 12.7 180) (layer F.SilkS))
    (fp_text user 9 (at -12.668381 15.24 180) (layer F.SilkS))
    (fp_text user 10 (at -13.144571 17.78 180) (layer F.SilkS))
    (fp_text user 11 (at -13.144571 20.32 180) (layer F.SilkS))
    (fp_text user 12 (at -13.144571 22.86 180) (layer F.SilkS))
    (pad G1 thru_hole circle (at -10.16 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad 0 thru_hole circle (at -10.16 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(J1-Pad0)"))
    (pad 1 thru_hole circle (at -10.16 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -10.16 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -10.16 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -10.16 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -10.16 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at -10.16 17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -10.16 20.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 DOUT))
    (pad 12 thru_hole circle (at -10.16 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad12)"))
    (pad VBAT thru_hole circle (at -7.62 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(J1-PadVBAT)"))
    (pad 3V1 thru_hole circle (at -5.08 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 VDDIO))
    (pad G2 thru_hole circle (at -2.54 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad PGM thru_hole circle (at 0 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(J1-PadPGM)"))
    (pad DAC thru_hole circle (at 2.54 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(J1-PadDAC)"))
    (pad 13 thru_hole circle (at 5.08 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 SCK))
    (pad 16 thru_hole circle (at 5.08 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 ^D/C))
    (pad 3V2 thru_hole circle (at 5.08 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(J1-Pad3V2)"))
    (pad 18 thru_hole circle (at 5.08 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at 5.08 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 ^CS))
    (pad AG thru_hole circle (at 5.08 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 GND))
    (pad 22 thru_hole circle (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad22)"))
    (pad VIN thru_hole circle (at 5.08 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(J1-PadVIN)"))
    (pad 21 thru_hole circle (at 5.08 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 5.08 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad19)"))
    (pad 23 thru_hole circle (at 5.08 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad23)"))
    (pad 14 thru_hole circle (at 5.08 20.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 ^RES))
    (pad 15 thru_hole circle (at 5.08 17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 BUSY))
  )
  (module Wickerlib:CONN-HEADER-FH34SRJ-34S-0.5SH (layer F.Cu) (tedit 58425DB7)
    (at 112.36452 63.10376 90)
    (fp_text reference J2 (at -0.225 -0.325 270) (layer F.Fab))
    (fp_text value HEADER-FEMALE-34POS-FFC-SMT-1x34-P0.5MM (at 0 2.9 270) (layer F.Fab) hide)
    (fp_text user %R (at -10.425 -0.075 180) (layer F.SilkS))
    (pad 2 smd rect (at 9.175 -1.325 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -8.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -7.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at -7.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at -6.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at -6.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J2-Pad5)"))
    (pad 6 smd rect (at -5.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 VCOM))
    (pad 7 smd rect (at -5.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 PRVGL))
    (pad 8 smd rect (at -4.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 VSL))
    (pad 9 smd rect (at -4.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 VGH2))
    (pad 10 smd rect (at -3.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 VSH))
    (pad 11 smd rect (at -3.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 VPP))
    (pad 12 smd rect (at -2.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VDD))
    (pad 13 smd rect (at -2.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 GND))
    (pad 14 smd rect (at -1.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 VDDIO))
    (pad 15 smd rect (at -1.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 VDDIO))
    (pad 16 smd rect (at -0.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 DOUT))
    (pad 17 smd rect (at -0.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 SCK))
    (pad 18 smd rect (at 0.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 ^CS))
    (pad 19 smd rect (at 0.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 ^D/C))
    (pad 20 smd rect (at 1.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 ^RES))
    (pad 21 smd rect (at 1.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 BUSY))
    (pad 22 smd rect (at 2.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 GND))
    (pad 23 smd rect (at 2.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 TSDA))
    (pad 24 smd rect (at 3.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 TSCL))
    (pad 25 smd rect (at 3.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 VGH))
    (pad 26 smd rect (at 4.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 VGL))
    (pad 27 smd rect (at 4.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 RESE))
    (pad 28 smd rect (at 5.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 GDR))
    (pad 29 smd rect (at 5.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J2-Pad29)"))
    (pad 30 smd rect (at 6.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(J2-Pad30)"))
    (pad 31 smd rect (at 6.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J2-Pad31)"))
    (pad 32 smd rect (at 7.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J2-Pad32)"))
    (pad 33 smd rect (at 7.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J2-Pad33)"))
    (pad 34 smd rect (at 8.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J2-Pad34)"))
    (pad 2 smd rect (at -9.125 -1.325 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J2-Pad2)"))
  )
  (module Inductors:Inductor_1212 (layer B.Cu) (tedit 5652586A)
    (at 104.81564 58.33364 180)
    (attr smd)
    (fp_text reference L1 (at 0 -2.75 180) (layer B.SilkS))
    (fp_text value INDUCTOR (at 0 2.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.75 0 180) (size 2.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 39 VDDIO))
    (pad 2 smd rect (at 1.75 0 180) (size 2.5 2.5) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C2-Pad2)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 54E9291B)
    (at 95.4786 57.72404 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value Q_NMOS_GDS (at 0 -3.81 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.50114 270) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 28 GDR))
    (pad 2 smd rect (at 0.95 -1.50114 270) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 29 RESE))
    (pad 3 smd rect (at 0 1.50114 270) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(C2-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 54189DEE)
    (at 135.70712 50.06086)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 2.1) (layer B.SilkS))
    (fp_text value "2.2R 1%" (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 29 RESE))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 46 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 111.80572 74.02576 180)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference R2 (at 0.09 0.04 180) (layer F.Fab))
    (fp_text value RES-0.0-JUMPER-1/8W-0603 (at 0 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 2.4645 -0.3175 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J2-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J2-Pad2)"))
  )
  (gr_text JUMPER (at 111.75492 75.19416) (layer F.SilkS))
  (gr_text "pdp7/kicad-teensy-epaper\n2017-03-29\n" (at 103.22052 48.87976) (layer B.SilkS))
  (gr_line (start 166.77132 43.29176) (end 169.56532 46.08576) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 166.21252 43.29176) (end 166.77132 43.29176) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 154.22372 43.29176) (end 166.21252 43.29176) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 169.61612 82.61096) (end 169.61612 46.03496) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 166.82212 85.40496) (end 169.61612 82.61096) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 165.09492 85.40496) (end 166.82212 85.40496) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 94.53372 85.40496) (end 165.09492 85.40496) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 89.40292 80.27416) (end 94.53372 85.40496) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 89.40292 77.27696) (end 89.40292 80.27416) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 89.40292 46.59376) (end 89.40292 77.27696) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 90.57132 45.42536) (end 89.40292 46.59376) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 92.70492 43.29176) (end 90.57132 45.42536) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 154.32532 43.29176) (end 92.70492 43.29176) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_text "pdp7/kicad-teensy-epaper\n2017-03-29\n" (at 119.93372 79.81696) (layer F.SilkS))
  (zone (net 46) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.06052 44.25696) (xy 166.36492 44.30776) (xy 168.80332 46.39056) (xy 168.75252 82.15376) (xy 166.16172 84.74456)
        (xy 95.24492 84.84616) (xy 90.46972 80.07096) (xy 90.41892 46.64456) (xy 93.00972 44.25696)
      )
    )
  )
)
