(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 53)
    (no_connects 0)
    (area 66.924999 33.091666 136.325001 67.075)
    (thickness 1.6)
    (drawings 26)
    (tracks 225)
    (zones 0)
    (modules 19)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(P2-Pad2)")
  (net 6 "Net-(P3-Pad4)")
  (net 7 "Net-(P3-Pad5)")
  (net 8 "Net-(P4-Pad3)")
  (net 9 "Net-(P4-Pad4)")
  (net 10 "Net-(P4-Pad5)")
  (net 11 "Net-(P5-Pad1)")
  (net 12 "Net-(R1-Pad1)")
  (net 13 "Net-(R2-Pad1)")
  (net 14 "Net-(R3-Pad2)")
  (net 15 "Net-(R4-Pad2)")
  (net 16 "Net-(R5-Pad2)")
  (net 17 "Net-(U2-Pad5)")
  (net 18 "Net-(U2-Pad6)")
  (net 19 "Net-(U2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P4-Pad5)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
  )
  (net_class Power ""
    (clearance 0.5)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module ESP8266:ESP-07v2-smd (layer F.Cu) (tedit 5701C953)
    (at 85 41)
    (descr "Module, ESP-8266, ESP-07v2, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U2 (at -3.5 -1.5) (layer F.SilkS) hide)
    (fp_text value ESP-12 (at 7.25 2.25) (layer F.Fab))
    (fp_text user "No Copper" (at 6.892 -5.4) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd oval (at 0 2) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd oval (at 0 4) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R2-Pad1)"))
    (pad 4 smd oval (at 0 6) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R3-Pad2)"))
    (pad 5 smd oval (at 0 8) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad5)"))
    (pad 6 smd oval (at 0 10) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad6)"))
    (pad 7 smd oval (at 0 12) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad7)"))
    (pad 8 smd oval (at 0 14) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 9 smd oval (at 14 14) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd oval (at 14 12) (size 2.5 1.1) (drill (offset 0.6 0)) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R4-Pad2)"))
    (pad 11 smd oval (at 14 10) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd oval (at 14 8) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R5-Pad2)"))
    (pad 13 smd oval (at 14 6) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd oval (at 14 4) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd oval (at 14 2) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P3-Pad4)"))
    (pad 16 smd oval (at 14 0) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P3-Pad5)"))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-07v2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D12.5_L25_P5 (layer F.Cu) (tedit 57C06970)
    (at 116 47)
    (descr "Radial Electrolytic Capacitor Diameter 12.5mm x Length 25mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 0 -3) (layer F.SilkS))
    (fp_text value CP (at 2.5 7.6) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D12.5_L25_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 57C07927)
    (at 78.5 57.5)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -3.25 0) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57C06983)
    (at 78.5 54.5 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -1.75 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 57C06C5B)
    (at 131 57.5 90)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference POWER (at 2.75 -3.75 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 2.5 -6.6 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812:WS2812_Strip (layer F.Cu) (tedit 57C07E81)
    (at 71 50 270)
    (fp_text reference WS2812 (at 0 -4 270) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -4 270) (layer F.Fab))
    (fp_text user GND (at 2.5 1.5 270) (layer F.SilkS))
    (fp_text user D0 (at 0 1.5 270) (layer F.SilkS))
    (fp_text user +5V (at -2.5 1.5 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at 2.5 0 270) (size 1.7 3.7) (drill 0.762 (offset 0 -1)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 0 270) (size 1.7 3.7) (drill 0.762 (offset 0 -1)) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at -2.5 0 270) (size 1.7 3.7) (drill 0.762 (offset 0 -1)) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 57C069A8)
    (at 117 38.5 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference FTDI (at 0 -3 270) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 57C076D9)
    (at 93 61.5 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 2.75 3 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P4-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P4-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P4-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 57C069D3)
    (at 117 60)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference PWM (at 2.25 -3.75) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 2.5 -6.6) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P5-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 57C0695C)
    (at 112 58 90)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference Q2 (at 4.25 0 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0 3.81 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P5-Pad1)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P4-Pad5)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 57C06989)
    (at 78.5 47 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -3 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 57C06993)
    (at 78.5 49.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -3 -2.5 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 57C06990)
    (at 78.5 52)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 3 -2.5) (layer F.SilkS))
    (fp_text value 330 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 57C07B6A)
    (at 105 53.25 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.75 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 57C07B6E)
    (at 105 51 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.75 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 57C06932)
    (at 78.5 41 270)
    (fp_text reference RESET (at 0 4.75 270) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 1.016 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.81 2.54 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R1-Pad1)"))
    (pad 1 thru_hole circle (at -3.81 -2.54 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -3.81 2.54 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R1-Pad1)"))
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_SMALL (layer F.Cu) (tedit 57C06946)
    (at 106.5 45)
    (fp_text reference PGM (at 2.75 4.75) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 1.016) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.81 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.81 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(R5-Pad2)"))
    (pad 1 thru_hole circle (at -3.81 -2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -3.81 2.54) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(R5-Pad2)"))
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 0)
    (at 131 45.5 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -0.762 270) (layer F.SilkS))
    (fp_text value AP1117 (at 0 0.762 270) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302 270) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 3.302 270) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 2.286 3.302 270) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -2.286 3.302 270) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-14_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 57C076CE)
    (at 85.25 62.25)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 -0.5) (layer F.SilkS))
    (fp_text value SN54AHCT125 (at 0 3.55) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.95 -1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P3-Pad4)"))
    (pad 3 smd rect (at -2.95 -0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P2-Pad2)"))
    (pad 4 smd rect (at -2.95 0) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -2.95 0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad6)"))
    (pad 6 smd rect (at -2.95 1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P4-Pad3)"))
    (pad 7 smd rect (at -2.95 1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 2.95 1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P4-Pad4)"))
    (pad 9 smd rect (at 2.95 1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad7)"))
    (pad 10 smd rect (at 2.95 0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.95 0) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P4-Pad5)"))
    (pad 12 smd rect (at 2.95 -0.65) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad5)"))
    (pad 13 smd rect (at 2.95 -1.3) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 2.95 -1.95) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Housings_SSOP.3dshapes/TSSOP-14_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "LUKE CYCA • 2016-08-26 • rev 2" (at 102.5 53.5) (layer B.SilkS))
  (gr_text "light controller" (at 102.5 49.75) (layer B.SilkS))
  (gr_text "party cat" (at 103.75 44.5) (layer B.SilkS))
  (gr_text ESP8266 (at 92 47.25) (layer F.SilkS))
  (gr_text +5V (at 134.5 52.5 90) (layer B.SilkS))
  (gr_text GND (at 134.5 57.5 90) (layer B.SilkS))
  (gr_text "(-)" (at 117 65.25) (layer F.SilkS))
  (gr_text +5V (at 122 65.25) (layer F.SilkS))
  (gr_text GND (at 105.75 64.5 90) (layer F.SilkS))
  (gr_text D14 (at 103.25 64.5 90) (layer F.SilkS))
  (gr_text D13 (at 100.75 64.5 90) (layer F.SilkS))
  (gr_text D12 (at 98 64.5 90) (layer F.SilkS))
  (gr_text D3 (at 95.5 64.5 90) (layer F.SilkS))
  (gr_text +5V (at 93 64.5 90) (layer F.SilkS))
  (gr_circle (center 71 63) (end 72 62.5) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 71 39) (end 72 38.5) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 133 63) (end 133.5 64) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 133 39) (end 134 39.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72 36) (end 132 36) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68 62) (end 68 40) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132 66) (end 72 66) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136 40) (end 136 62) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 72 62) (end 72 66) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 72 40) (end 68 40) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 132 62) (end 136 62) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 132 40) (end 132 36) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.8) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100 39) (xy 84 39) (xy 84 36) (xy 100 36) (xy 100 39)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.8) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100 39) (xy 84 39) (xy 84 36) (xy 100 36) (xy 100 39)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.8) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136 66) (xy 68 66) (xy 68 36) (xy 136 36) (xy 136 66)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.8) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136 66) (xy 68 66) (xy 68 36) (xy 136 36) (xy 136 66)
      )
    )
  )
)
