(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 38)
    (no_connects 0)
    (area 165.036499 67.246499 180.403501 82.613501)
    (thickness 1.6002)
    (drawings 42)
    (tracks 153)
    (zones 0)
    (modules 10)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(J1-PadP$1)")
  (net 4 "Net-(J1-PadP$2)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(J1-PadP$1)")
    (add_net "Net-(J1-PadP$2)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B5524B3)
    (at 169.037 74.93 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:adafruit-LED3535 (layer F.Cu) (tedit 5B5524BD)
    (at 172.72 74.93)
    (attr smd)
    (fp_text reference LED1 (at 3.175 -0.254 90) (layer F.SilkS) hide)
    (fp_text value WS2812BSK6812MINI (at 0.127 2.54) (layer F.SilkS) hide)
    (pad 1-DO smd rect (at 1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-PadP$1)"))
    (pad 2-GN smd rect (at 1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 3-DI smd rect (at -1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-PadP$2)"))
    (pad 4-VD smd rect (at -1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module nixiemisc:nixiemisc-4PINDOUBLEBIG (layer F.Cu) (tedit 5B5523FF)
    (at 168.91 68.58 270)
    (attr smd)
    (fp_text reference J1 (at -2.794 -4.191 270) (layer Dwgs.User))
    (fp_text value 4PIN (at 0 0 270) (layer F.SilkS) hide)
    (pad P$1 smd rect (at 0 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-PadP$1)"))
    (pad P$2 smd rect (at 0 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-PadP$2)"))
    (pad P$3 smd rect (at 0 -5.08 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad P$4 smd rect (at 0 -7.62 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad P$5 smd rect (at 0 0 270) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 3 "Net-(J1-PadP$1)"))
    (pad P$6 smd rect (at 0 -2.54 270) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 4 "Net-(J1-PadP$2)"))
    (pad P$7 smd rect (at 0 -5.08 270) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad P$8 smd rect (at 0 -7.62 270) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad2)"))
  )
  (module nixiemisc:nixiemisc-4PINDOUBLEBIG (layer F.Cu) (tedit 5B5523F4)
    (at 179.07 78.74)
    (attr smd)
    (fp_text reference J2 (at 3.81 -3.81) (layer Dwgs.User))
    (fp_text value 4PIN (at 0 0) (layer F.SilkS) hide)
    (pad P$1 smd rect (at 0 0) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-PadP$1)"))
    (pad P$2 smd rect (at 0 -2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-PadP$2)"))
    (pad P$3 smd rect (at 0 -5.08) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad P$4 smd rect (at 0 -7.62) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad P$5 smd rect (at 0 0) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 3 "Net-(J1-PadP$1)"))
    (pad P$6 smd rect (at 0 -2.54) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 4 "Net-(J1-PadP$2)"))
    (pad P$7 smd rect (at 0 -5.08) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad P$8 smd rect (at 0 -7.62) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad2)"))
  )
  (module nixiemisc:nixiemisc-4PINDOUBLEBIG (layer F.Cu) (tedit 5B5523E6)
    (at 168.91 81.28 270)
    (attr smd)
    (fp_text reference J3 (at 2.54 -3.81 270) (layer Dwgs.User))
    (fp_text value 4PIN (at 0 0 270) (layer F.SilkS) hide)
    (pad P$1 smd rect (at 0 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-PadP$2)"))
    (pad P$2 smd rect (at 0 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-PadP$1)"))
    (pad P$3 smd rect (at 0 -5.08 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad P$4 smd rect (at 0 -7.62 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad P$5 smd rect (at 0 0 270) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 4 "Net-(J1-PadP$2)"))
    (pad P$6 smd rect (at 0 -2.54 270) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 3 "Net-(J1-PadP$1)"))
    (pad P$7 smd rect (at 0 -5.08 270) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad P$8 smd rect (at 0 -7.62 270) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad2)"))
  )
  (module nixiemisc:nixiemisc-4PINDOUBLEBIG (layer F.Cu) (tedit 5B552407)
    (at 166.37 78.74)
    (attr smd)
    (fp_text reference J4 (at -3.81 -3.81) (layer Dwgs.User))
    (fp_text value 4PIN (at 0 0) (layer F.SilkS) hide)
    (pad P$1 smd rect (at 0 0) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-PadP$2)"))
    (pad P$2 smd rect (at 0 -2.54) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-PadP$1)"))
    (pad P$3 smd rect (at 0 -5.08) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad P$4 smd rect (at 0 -7.62) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad P$5 smd rect (at 0 0) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 4 "Net-(J1-PadP$2)"))
    (pad P$6 smd rect (at 0 -2.54) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 3 "Net-(J1-PadP$1)"))
    (pad P$7 smd rect (at 0 -5.08) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad P$8 smd rect (at 0 -7.62) (size 2.54 1.27) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad2)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X01_NO_SILK (layer F.Cu) (tedit 5B5527B6)
    (at 166.37 81.28)
    (descr "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J5 (at -2.159 0) (layer Dwgs.User))
    (fp_text value VDD (at 1.397 0 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X01_NO_SILK (layer F.Cu) (tedit 5B5527C5)
    (at 179.07 81.28)
    (descr "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J6 (at 0 2.413) (layer Dwgs.User))
    (fp_text value GND (at 0 -1.397) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 1 "Net-(C1-Pad2)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X01_NO_SILK (layer F.Cu) (tedit 5B5527A8)
    (at 166.37 68.58)
    (descr "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J7 (at 0 -2.413) (layer Dwgs.User))
    (fp_text value DI (at 0 1.397) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(J1-PadP$2)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X01_NO_SILK (layer F.Cu) (tedit 5B5527D3)
    (at 179.07 68.58)
    (descr "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J8 (at 2.413 0) (layer Dwgs.User))
    (fp_text value DO (at -1.397 0 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(J1-PadP$1)"))
  )
  (gr_text GND (at 175.768 70.739 90) (layer B.SilkS))
  (gr_text VDD (at 173.99 70.739 90) (layer B.SilkS))
  (gr_text DI (at 171.45 70.485 90) (layer B.SilkS))
  (gr_text DO (at 168.91 70.485 90) (layer B.SilkS))
  (gr_text GND (at 168.783 71.501) (layer B.SilkS))
  (gr_text VDD (at 168.656 73.66) (layer B.SilkS))
  (gr_text DO (at 168.402 76.2) (layer B.SilkS))
  (gr_text DI (at 168.148 78.74) (layer B.SilkS))
  (gr_text DI (at 168.91 79.502 90) (layer B.SilkS))
  (gr_text DO (at 171.45 79.375 90) (layer B.SilkS))
  (gr_text VDD (at 173.99 78.994 90) (layer B.SilkS))
  (gr_text GND (at 176.022 78.994 90) (layer B.SilkS))
  (gr_text DO (at 177.165 78.74) (layer B.SilkS))
  (gr_text DI (at 177.165 76.2) (layer B.SilkS))
  (gr_text VDD (at 176.784 73.66) (layer F.SilkS))
  (gr_text VDD (at 167.767 81.28 90) (layer F.SilkS))
  (gr_text GND (at 179.07 79.883) (layer F.SilkS))
  (gr_text DO (at 177.673 68.58 90) (layer F.SilkS))
  (gr_text DI (at 166.37 69.977 360) (layer F.SilkS))
  (gr_text GND (at 176.784 71.755) (layer B.SilkS))
  (gr_text GND (at 175.768 70.739 90) (layer F.SilkS))
  (gr_text DI (at 168.91 79.502 90) (layer F.SilkS))
  (gr_text DO (at 168.91 70.485 90) (layer F.SilkS))
  (gr_text DO (at 171.45 79.375 90) (layer F.SilkS))
  (gr_text DO (at 177.165 78.74) (layer F.SilkS))
  (gr_text DO (at 168.402 76.2) (layer F.SilkS))
  (gr_text DI (at 177.165 76.2 360) (layer F.SilkS))
  (gr_text DI (at 171.45 70.485 90) (layer F.SilkS))
  (gr_text DI (at 168.148 78.74) (layer F.SilkS))
  (gr_text VDD (at 173.99 70.739 90) (layer F.SilkS))
  (gr_text VDD (at 173.99 78.994 90) (layer F.SilkS))
  (gr_text VDD (at 176.784 73.66) (layer B.SilkS))
  (gr_text VDD (at 168.656 73.66) (layer F.SilkS))
  (gr_text GND (at 176.022 78.994 90) (layer F.SilkS))
  (gr_text GND (at 168.783 71.501) (layer F.SilkS))
  (gr_text GND (at 176.784 71.755) (layer F.SilkS))
  (dimension 15.24 (width 0.127) (layer Dwgs.User)
    (gr_text "0.6000 in" (at 184.15 74.93 270) (layer Dwgs.User))
    (feature1 (pts (xy 184.15 82.55) (xy 184.15 82.55)))
    (feature2 (pts (xy 184.15 67.31) (xy 184.15 67.31)))
    (crossbar (pts (xy 184.15 67.31) (xy 184.15 82.55)))
    (arrow1a (pts (xy 184.15 82.55) (xy 183.563579 81.423496)))
    (arrow1b (pts (xy 184.15 82.55) (xy 184.736421 81.423496)))
    (arrow2a (pts (xy 184.15 67.31) (xy 183.563579 68.436504)))
    (arrow2b (pts (xy 184.15 67.31) (xy 184.736421 68.436504)))
  )
  (dimension 15.24 (width 0.127) (layer Dwgs.User)
    (gr_text "0.6000 in" (at 172.72 86.36) (layer Dwgs.User))
    (feature1 (pts (xy 180.34 86.36) (xy 180.34 86.36)))
    (feature2 (pts (xy 165.1 86.36) (xy 165.1 86.36)))
    (crossbar (pts (xy 165.1 86.36) (xy 180.34 86.36)))
    (arrow1a (pts (xy 180.34 86.36) (xy 179.213496 86.946421)))
    (arrow1b (pts (xy 180.34 86.36) (xy 179.213496 85.773579)))
    (arrow2a (pts (xy 165.1 86.36) (xy 166.226504 86.946421)))
    (arrow2b (pts (xy 165.1 86.36) (xy 166.226504 85.773579)))
  )
  (gr_line (start 165.1 82.55) (end 165.1 67.31) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 180.34 82.55) (end 165.1 82.55) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 180.34 67.31) (end 180.34 82.55) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 165.1 67.31) (end 180.34 67.31) (layer Edge.Cuts) (width 0.127))
)
