(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 25)
    (no_connects 0)
    (area 107.924999 106.924999 146.075001 136.575001)
    (thickness 1.6)
    (drawings 14)
    (tracks 70)
    (zones 0)
    (modules 8)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.50012 3.50012)
    (pad_drill 1.00076)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J1-Pad2)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J1-Pad4)")
  (net 7 "Net-(J1-Pad6)")
  (net 8 "Net-(J1-Pad7)")
  (net 9 "Net-(J1-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
  )
  (net_class 12v ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Connect:RJ45_8 (layer F.Cu) (tedit 5792AD93)
    (at 135.89 110.49 180)
    (tags RJ45)
    (fp_text reference J1 (at -6.35 -8.89 180) (layer F.SilkS))
    (fp_text value RJ45 (at 0.14224 -0.1016 180) (layer F.Fab))
    (pad Hole np_thru_hole circle (at 5.93852 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 -6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -3.175 -8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -1.905 -6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -0.635 -8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 0.635 -6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole circle (at 1.905 -8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at 3.175 -6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 4.445 -8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad8)"))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:RJ45_8 (layer F.Cu) (tedit 5792AD89)
    (at 118.11 110.49 180)
    (tags RJ45)
    (fp_text reference J2 (at 6.35 -8.89 180) (layer F.SilkS))
    (fp_text value RJ45 (at 0.14224 -0.1016 180) (layer F.Fab))
    (pad Hole np_thru_hole circle (at 5.93852 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 -6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -3.175 -8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -1.905 -6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -0.635 -8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 0.635 -6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole circle (at 1.905 -8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at 3.175 -6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 4.445 -8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad8)"))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 5792ADB0)
    (at 130.81 129.54 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 3.175 -4.445 270) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5792ADA4)
    (at 115.57 124.46 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 1.905 270) (layer F.SilkS))
    (fp_text value 0 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 118.11 124.46 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -2.3 270) (layer F.SilkS))
    (fp_text value 0 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad7)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 115.57 132.715 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Keyboard:BARREL_JACK (layer F.Cu) (tedit 5792B0BF)
    (at 140.843 129.413 180)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON1 (at 30.353 -0.127 270) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -5.99948 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 6.20014 0 180) (size 3.50012 3.50012) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 2 thru_hole rect (at 0.20066 0 180) (size 3.50012 3.50012) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at 3.2004 4.699 180) (size 3.50012 3.50012) (drill 3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer B.Cu) (tedit 5792B2B1)
    (at 114.75 123.25 180)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference "" (at 0.09906 4.38912 180) (layer B.SilkS))
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 -6.56082 180) (layer B.Fab))
  )
  (gr_text "nanoMoCo \nEthernet Breakout" (at 130.4 125.7) (layer B.SilkS))
  (gr_line (start 146 107) (end 108 107) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146 136.5) (end 146 107) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 108 136.5) (end 146 136.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 108 107) (end 108 136.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Designed by:\nAdam McCombs" (at 130.2 122.8) (layer B.SilkS))
  (gr_text GND (at 121.92 134.747) (layer F.SilkS))
  (gr_text 12V (at 119.126 134.747) (layer F.SilkS))
  (gr_text 12V (at 116.55 134.75) (layer F.SilkS))
  (gr_text COM3 (at 112.395 131.445 90) (layer F.SilkS))
  (gr_text COM2 (at 123.19 131.445 90) (layer F.SilkS))
  (gr_text COM1 (at 125.73 131.445 90) (layer F.SilkS))
  (gr_text 485-B (at 128.27 131.445 90) (layer F.SilkS))
  (gr_text 485-A (at 130.81 131.445 90) (layer F.SilkS))
  (zone (net 1) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.415 135.89) (xy 108.585 135.89) (xy 108.585 107.315) (xy 145.415 107.315) (xy 145.415 135.89)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.415 135.89) (xy 108.585 135.89) (xy 108.585 107.315) (xy 145.415 107.315) (xy 145.415 135.89)
      )
    )
  )
)
