<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="14.6324875" x2="0" y2="3.381634375" width="0" layer="20"/>
<wire x1="0" y1="3.381634375" x2="3.381634375" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.381634375" y1="0" x2="22.02971875" y2="0" width="0" layer="20"/>
<wire x1="22.02971875" y1="0" x2="24.943" y2="2.91328125" width="0" layer="20" curve="90"/>
<wire x1="24.943" y1="2.91328125" x2="24.943" y2="14.85016875" width="0" layer="20"/>
<wire x1="24.943" y1="14.85016875" x2="22.02316875" y2="17.77" width="0" layer="20" curve="90"/>
<wire x1="22.02316875" y1="17.77" x2="3.1375125" y2="17.77" width="0" layer="20"/>
<wire x1="3.1375125" y1="17.77" x2="0" y2="14.6324875" width="0" layer="20" curve="90"/>
<text>+</text>
<text>+</text>
<text>USB Lipo</text>
<text>Charger</text>
</plain>
<libraries>
<library name="max1811">
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFunEagle-6-6-07">
<packages>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="0603">
</package>
<package name="S2B-PH">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="MOLEX-1X2_LOCK">
</package>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
<package name="LED-0603">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="max1811" package="SO08" value="MAX1811"/>
<element name="C1" library="SparkFunEagle-6-6-07" package="EIA3216" value="10uF"/>
<element name="C2" library="SparkFunEagle-6-6-07" package="EIA3216" value="10uF"/>
<element name="R1" library="SparkFun" package="0603" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="MOLEX-1X2_LOCK" value=""/>
<element name="X2" library="SparkFun" package="USB-A-H" value="USB-A-H"/>
<element name="JP3" library="SparkFun" package="S2B-PH" value=""/>
<element name="CHARGING" library="SparkFun" package="LED-0603" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="3"/>
<contactref element="C2" pad="C"/>
<contactref element="C1" pad="C"/>
<contactref element="X2" pad="GND"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="CHARGING" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="8"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="BAT">
<contactref element="U$1" pad="5"/>
<contactref element="C2" pad="A"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="U$1" pad="7"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="2"/>
<contactref element="C1" pad="A"/>
<contactref element="X2" pad="VBUS"/>
<contactref element="CHARGING" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
