(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 0.8)
    (drawings 35)
    (tracks 472)
    (zones 0)
    (modules 87)
    (nets 60)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.2032)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.1524)
    (zone_clearance 0.6)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.635 0.381)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.1524)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.508 0.508)
    (pad_drill 0.254)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.101)
    (pad_to_paste_clearance -0.025)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +12V)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad2)")
  (net 5 "Net-(C5-Pad2)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C7-Pad1)")
  (net 8 "Net-(C8-Pad2)")
  (net 9 "Net-(C9-Pad2)")
  (net 10 "Net-(C9-Pad1)")
  (net 11 "Net-(C11-Pad1)")
  (net 12 "Net-(C12-Pad2)")
  (net 13 "Net-(C13-Pad2)")
  (net 14 "Net-(C13-Pad1)")
  (net 15 "Net-(C15-Pad1)")
  (net 16 "Net-(C16-Pad2)")
  (net 17 "Net-(C17-Pad2)")
  (net 18 "Net-(C17-Pad1)")
  (net 19 +3V3)
  (net 20 /NRST)
  (net 21 "Net-(D2-Pad2)")
  (net 22 "Net-(D5-Pad2)")
  (net 23 "Net-(D8-Pad2)")
  (net 24 "Net-(D11-Pad2)")
  (net 25 "Net-(D102-Pad1)")
  (net 26 "Net-(D104-Pad1)")
  (net 27 "Net-(D105-Pad1)")
  (net 28 "Net-(D107-Pad1)")
  (net 29 "Net-(D108-Pad1)")
  (net 30 "Net-(D109-Pad1)")
  (net 31 "Net-(J1-Pad3)")
  (net 32 /UV_CTRL)
  (net 33 /FAR_RED_CTRL)
  (net 34 /DEEP_BLUE_CTRL)
  (net 35 /DEEP_RED_CTRL)
  (net 36 "Net-(U1-Pad20)")
  (net 37 /SWCLK)
  (net 38 /SWDIO)
  (net 39 "Net-(U1-Pad3)")
  (net 40 /LSE_MEMS)
  (net 41 "Net-(U1-Pad1)")
  (net 42 "Net-(U2-Pad3)")
  (net 43 "Net-(U3-Pad4)")
  (net 44 "Net-(U3-Pad3)")
  (net 45 "Net-(U4-Pad3)")
  (net 46 "Net-(U5-Pad3)")
  (net 47 "Net-(U6-Pad3)")
  (net 48 "Net-(U7-Pad3)")
  (net 49 "Net-(C25-Pad1)")
  (net 50 "Net-(C26-Pad2)")
  (net 51 "Net-(C26-Pad1)")
  (net 52 /I2C2_SDA)
  (net 53 /I2C2_SCL)
  (net 54 /DISP_~RST)
  (net 55 "Net-(DBG1-Pad6)")
  (net 56 /UP_BUT)
  (net 57 /DOWN_BUT)
  (net 58 /LEFT_BUT)
  (net 59 /RIGHT_BUT)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net /DEEP_BLUE_CTRL)
    (add_net /DEEP_RED_CTRL)
    (add_net /DISP_~RST)
    (add_net /DOWN_BUT)
    (add_net /FAR_RED_CTRL)
    (add_net /I2C2_SCL)
    (add_net /I2C2_SDA)
    (add_net /LEFT_BUT)
    (add_net /LSE_MEMS)
    (add_net /NRST)
    (add_net /RIGHT_BUT)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /UP_BUT)
    (add_net /UV_CTRL)
    (add_net GND)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C26-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D102-Pad1)")
    (add_net "Net-(D104-Pad1)")
    (add_net "Net-(D105-Pad1)")
    (add_net "Net-(D107-Pad1)")
    (add_net "Net-(D108-Pad1)")
    (add_net "Net-(D109-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(DBG1-Pad6)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(U6-Pad3)")
    (add_net "Net-(U7-Pad3)")
  )
  (module Symbol:ESD-Logo_8.9x8mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 84 95.5)
    (descr "Electrostatic discharge Logo")
    (tags "Logo ESD")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value ESD-Logo_8.9x8mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Symbol:WEEE-Logo_8.4x12mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 112 94)
    (descr "Waste Electrical and Electronic Equipment Directive")
    (tags "Logo WEEE")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value WEEE-Logo_8.4x12mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Symbol:Symbol_Barrel_Polarity (layer B.Cu) (tedit 5765E9A7)
    (at 104.902 66.802 180)
    (descr "Barrel connector polarity indicator")
    (tags "barrel polarity")
    (attr virtual)
    (fp_text reference REF** (at -0.175 -0.075) (layer B.SilkS) hide)
    (fp_text value Symbol_Barrel_Polarity (at 0 -2) (layer B.Fab))
  )
  (module Symbol:KiCad-Logo2_8mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 131.572 105.156)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_8mm_SilkScreen (at 0 7.62) (layer F.Fab) hide)
  )
  (module 1_Custom_Footprints:PTS647 (layer B.Cu) (tedit 5DF0614B)
    (at 104.14 127.508 90)
    (fp_text reference SW5 (at 2.9 -1.6 90) (layer B.SilkS))
    (fp_text value PTS647 (at 2.7 1.5 90) (layer B.Fab))
    (pad 4 smd rect (at 5.25 -3.2 90) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 59 /RIGHT_BUT))
    (pad 3 smd rect (at 0 -3.2 90) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 59 /RIGHT_BUT))
    (pad 2 smd rect (at 5.25 0 90) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 90) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CKCOMPONENTS_PTS647SN50SMTR2LFS/PTS647SN50SMTR2LFS.stp"
      (offset (xyz 2.65 -1.6 -0.03))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 -90))
    )
  )
  (module 1_Custom_Footprints:PTS647 (layer B.Cu) (tedit 5DF0614B)
    (at 113.538 122.258 270)
    (fp_text reference SW4 (at 2.9 -1.6 90) (layer B.SilkS))
    (fp_text value PTS647 (at 2.7 1.5 90) (layer B.Fab))
    (pad 4 smd rect (at 5.25 -3.2 270) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 58 /LEFT_BUT))
    (pad 3 smd rect (at 0 -3.2 270) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 58 /LEFT_BUT))
    (pad 2 smd rect (at 5.25 0 270) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CKCOMPONENTS_PTS647SN50SMTR2LFS/PTS647SN50SMTR2LFS.stp"
      (offset (xyz 2.65 -1.6 -0.03))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 -90))
    )
  )
  (module 1_Custom_Footprints:PTS647 (layer B.Cu) (tedit 5DF0614B)
    (at 111.422 128.27 180)
    (fp_text reference SW3 (at 2.9 -1.6) (layer B.SilkS))
    (fp_text value PTS647 (at 2.7 1.5) (layer B.Fab))
    (pad 4 smd rect (at 5.25 -3.2 180) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 57 /DOWN_BUT))
    (pad 3 smd rect (at 0 -3.2 180) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 57 /DOWN_BUT))
    (pad 2 smd rect (at 5.25 0 180) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 180) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CKCOMPONENTS_PTS647SN50SMTR2LFS/PTS647SN50SMTR2LFS.stp"
      (offset (xyz 2.65 -1.6 -0.03))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 -90))
    )
  )
  (module 1_Custom_Footprints:PTS647 (layer B.Cu) (tedit 5DF0614B)
    (at 106.172 121.666)
    (fp_text reference SW2 (at 2.9 -1.6) (layer B.SilkS))
    (fp_text value PTS647 (at 2.7 1.5) (layer B.Fab))
    (pad 4 smd rect (at 5.25 -3.2) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 56 /UP_BUT))
    (pad 3 smd rect (at 0 -3.2) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 56 /UP_BUT))
    (pad 2 smd rect (at 5.25 0) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 1.55 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CKCOMPONENTS_PTS647SN50SMTR2LFS/PTS647SN50SMTR2LFS.stp"
      (offset (xyz 2.65 -1.6 -0.03))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 -90))
    )
  )
  (module 1_Custom_Footprints:PTS647 (layer F.Cu) (tedit 5DF0614B)
    (at 91.778 99.924)
    (fp_text reference SW1 (at 2.9 1.6) (layer F.SilkS))
    (fp_text value PTS647 (at 2.7 -1.5) (layer F.Fab))
    (pad 4 smd rect (at 5.25 3.2) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 20 /NRST))
    (pad 3 smd rect (at 0 3.2) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 20 /NRST))
    (pad 2 smd rect (at 5.25 0) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0) (size 1.55 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CKCOMPONENTS_PTS647SN50SMTR2LFS/PTS647SN50SMTR2LFS.stp"
      (offset (xyz 2.65 -1.6 -0.03))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 -90))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 102.593 124.46)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /RIGHT_BUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 110.744 120.419 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /LEFT_BUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 108.458 129.817 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C28 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /DOWN_BUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 108.458 120.119 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C27 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /UP_BUT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_Cree-XHP35 (layer F.Cu) (tedit 5DF03815)
    (at 134 76 180)
    (descr http://www.cree.com/~/media/Files/Cree/LED-Components-and-Modules/XLamp/Data-and-Binning/ds--XHP35.pdf)
    (tags "LED Cree XHP35")
    (attr smd)
    (fp_text reference D101 (at -2.67 0 270) (layer F.SilkS))
    (fp_text value "IN-C33CTN 390/400nm" (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.15 0 180) (size 8 3.3) (layers F.Cu)
      (net 4 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 5.15 0 180) (size 8 3.3) (layers F.Cu)
      (net 3 "Net-(C3-Pad1)"))
    (pad 1 smd rect (at -1.4 0 180) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 1.4 0 180) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad NC thru_hole circle (at 0 -0.5 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 0.5 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 -1.5 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 1.5 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1 -2.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 -2.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 -3.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2 -3.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2 -3.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -3 -2.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 3 -2.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -3.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -3.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -3 -4.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 -4.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1 -4.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 3 -4.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 2.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1 2.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 3 2.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -3 2.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 3.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2 3.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 3.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2 3.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 3.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 3 4.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1 4.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 4.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -3 4.5 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_Cree-XHP35.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CAD_GF_CSSPM1_24_20170509-fr/Gx_CSSPM1_20170509_geometry.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 1_Custom_Footprints:PJ-079AH (layer B.Cu) (tedit 5DEF188F)
    (at 116.586 65.088 270)
    (descr "DC barrel jack, 5A, 24V, 5.5mm outer, 2mm inner")
    (fp_text reference J1 (at 8.064 -2.286 180) (layer B.SilkS))
    (fp_text value Barrel_Jack_Switch (at 4.8 3.5 90) (layer B.Fab))
    (pad 3 thru_hole oval (at 10.3 0 270) (size 2.8 1.6) (drill oval 2 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 10.3 5.3 270) (size 2.8 1.6) (drill oval 2 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 3 -3.7 270) (size 3.1 1.6) (drill oval 2.3 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 4 0 270) (size 4 4) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 3 6.2 270) (size 3.1 1.6) (drill oval 2.3 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at 10.3 -3.3 270) (size 2.8 1.6) (drill oval 2 0.8) (layers *.Cu *.Mask)
      (net 2 +12V))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CUI_DEVICES_PJ-079AH/CUI_DEVICES_PJ-079AH.step"
      (offset (xyz -4.65 -2.75 5.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 1_Custom_Footprints:OSRAM_CSS (layer F.Cu) (tedit 5DEEFC1C)
    (at 134.066 120.114 270)
    (descr "OSRAM Opto 3030 SMD High-power LED")
    (attr smd)
    (fp_text reference D102 (at 0.5 -2.3 90) (layer F.SilkS))
    (fp_text value "GF CSSPM1.24 730nm" (at 0 -4.3 90) (layer F.Fab))
    (pad NC thru_hole circle (at 1 -0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 -0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -0.5 0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1.5 0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -0.7 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 0.7 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 2.1 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -2.1 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 2.1 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 0.7 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -0.7 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -2.1 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 -0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1.5 0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0.5 0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -1.4 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 1.4 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 1.4 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -1.4 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 2.75 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -2.75 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 0 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 2.75 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 0 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -2.75 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 smd rect (at 0 -1.65 270) (size 2.8 1.6) (layers F.Cu)
      (net 25 "Net-(D102-Pad1)") (solder_paste_margin -0.1))
    (pad 2 smd rect (at 0 1.65 270) (size 2.8 1.6) (layers F.Cu)
      (net 7 "Net-(C7-Pad1)") (solder_paste_margin -0.1))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CAD_GD_CSSRM2_14_20170907-db/Gx_CSSRM2_20170907_geometry.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module 1_Custom_Footprints:OSRAM_CSS (layer F.Cu) (tedit 5DEEFC1C)
    (at 134.066 129.766 90)
    (descr "OSRAM Opto 3030 SMD High-power LED")
    (attr smd)
    (fp_text reference D103 (at 0.5 -2.3 90) (layer F.SilkS))
    (fp_text value "GF CSSPM1.24 730nm" (at 0 -4.3 90) (layer F.Fab))
    (pad NC thru_hole circle (at 1 -0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 -0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -0.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 -0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 smd rect (at 0 -1.65 90) (size 2.8 1.6) (layers F.Cu)
      (net 8 "Net-(C8-Pad2)") (solder_paste_margin -0.1))
    (pad 2 smd rect (at 0 1.65 90) (size 2.8 1.6) (layers F.Cu)
      (net 25 "Net-(D102-Pad1)") (solder_paste_margin -0.1))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CAD_GD_CSSRM2_14_20170907-db/Gx_CSSRM2_20170907_geometry.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module 1_Custom_Footprints:OSRAM_CSS (layer F.Cu) (tedit 5DEEFC1C)
    (at 83.85 130 90)
    (descr "OSRAM Opto 3030 SMD High-power LED")
    (attr smd)
    (fp_text reference D105 (at 0.5 -2.3 90) (layer F.SilkS))
    (fp_text value "GD CSSRM2.14 445nm" (at 0 -4.3 90) (layer F.Fab))
    (pad NC thru_hole circle (at 1 -0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 -0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -0.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 -0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 smd rect (at 0 -1.65 90) (size 2.8 1.6) (layers F.Cu)
      (net 27 "Net-(D105-Pad1)") (solder_paste_margin -0.1))
    (pad 2 smd rect (at 0 1.65 90) (size 2.8 1.6) (layers F.Cu)
      (net 26 "Net-(D104-Pad1)") (solder_paste_margin -0.1))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CAD_GD_CSSRM2_14_20170907-db/Gx_CSSRM2_20170907_geometry.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module 1_Custom_Footprints:OSRAM_CSS (layer F.Cu) (tedit 5DEEFC1C)
    (at 89 81 90)
    (descr "OSRAM Opto 3030 SMD High-power LED")
    (attr smd)
    (fp_text reference D107 (at 0.5 -2.3 90) (layer F.SilkS))
    (fp_text value "GH CSSRM3.24 660nm" (at 0 -4.3 90) (layer F.Fab))
    (pad NC thru_hole circle (at 1 -0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 -0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -0.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 -0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 smd rect (at 0 -1.65 90) (size 2.8 1.6) (layers F.Cu)
      (net 28 "Net-(D107-Pad1)") (solder_paste_margin -0.1))
    (pad 2 smd rect (at 0 1.65 90) (size 2.8 1.6) (layers F.Cu)
      (net 15 "Net-(C15-Pad1)") (solder_paste_margin -0.1))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CAD_GD_CSSRM2_14_20170907-db/Gx_CSSRM2_20170907_geometry.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module 1_Custom_Footprints:OSRAM_CSS (layer F.Cu) (tedit 5DEEFC1C)
    (at 79 81 90)
    (descr "OSRAM Opto 3030 SMD High-power LED")
    (attr smd)
    (fp_text reference D108 (at 0.5 -2.3 90) (layer F.SilkS))
    (fp_text value "GH CSSRM3.24 660nm" (at 0 -4.3 90) (layer F.Fab))
    (pad NC thru_hole circle (at 1 -0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 -0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -0.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -0.7 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -2.1 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 -0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0.5 0.25 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -1.4 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -2.75 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 smd rect (at 0 -1.65 90) (size 2.8 1.6) (layers F.Cu)
      (net 29 "Net-(D108-Pad1)") (solder_paste_margin -0.1))
    (pad 2 smd rect (at 0 1.65 90) (size 2.8 1.6) (layers F.Cu)
      (net 28 "Net-(D107-Pad1)") (solder_paste_margin -0.1))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CAD_GD_CSSRM2_14_20170907-db/Gx_CSSRM2_20170907_geometry.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module 1_Custom_Footprints:OSRAM_CSS (layer F.Cu) (tedit 5DEEFC1C)
    (at 79 71 270)
    (descr "OSRAM Opto 3030 SMD High-power LED")
    (attr smd)
    (fp_text reference D109 (at 0.5 -2.3 90) (layer F.SilkS))
    (fp_text value "GH CSSRM3.24 660nm" (at 0 -4.3 90) (layer F.Fab))
    (pad NC thru_hole circle (at 1 -0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 -0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -0.5 0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1.5 0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -0.7 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 0.7 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 2.1 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -2.1 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 2.1 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 0.7 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -0.7 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -2.1 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 -0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1.5 0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0.5 0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -1.4 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 1.4 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 1.4 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -1.4 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 2.75 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -2.75 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 0 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 2.75 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 0 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -2.75 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 smd rect (at 0 -1.65 270) (size 2.8 1.6) (layers F.Cu)
      (net 30 "Net-(D109-Pad1)") (solder_paste_margin -0.1))
    (pad 2 smd rect (at 0 1.65 270) (size 2.8 1.6) (layers F.Cu)
      (net 29 "Net-(D108-Pad1)") (solder_paste_margin -0.1))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CAD_GD_CSSRM2_14_20170907-db/Gx_CSSRM2_20170907_geometry.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module 1_Custom_Footprints:OSRAM_CSS (layer F.Cu) (tedit 5DEEFC1C)
    (at 89 71 270)
    (descr "OSRAM Opto 3030 SMD High-power LED")
    (attr smd)
    (fp_text reference D110 (at 0.5 -2.3 90) (layer F.SilkS))
    (fp_text value "GH CSSRM3.24 660nm" (at 0 -4.3 90) (layer F.Fab))
    (pad NC thru_hole circle (at 1 -0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 -0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -0.5 0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1.5 0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -0.7 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 0.7 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 2.1 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -2.1 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 2.1 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 0.7 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -0.7 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -2.1 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 -0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1.5 0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0.5 0.25 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -1.4 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 1.4 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 1.4 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -1.4 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 2.75 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -2.75 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 0 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 2.75 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 0 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -2.75 270) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 smd rect (at 0 -1.65 270) (size 2.8 1.6) (layers F.Cu)
      (net 16 "Net-(C16-Pad2)") (solder_paste_margin -0.1))
    (pad 2 smd rect (at 0 1.65 270) (size 2.8 1.6) (layers F.Cu)
      (net 30 "Net-(D109-Pad1)") (solder_paste_margin -0.1))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CAD_GD_CSSRM2_14_20170907-db/Gx_CSSRM2_20170907_geometry.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module 1_Custom_Footprints:OSRAM_CSS (layer F.Cu) (tedit 5DEEFC1C)
    (at 79 120)
    (descr "OSRAM Opto 3030 SMD High-power LED")
    (attr smd)
    (fp_text reference D106 (at 0.5 -2.3 180) (layer F.SilkS))
    (fp_text value "GD CSSRM2.14 445nm" (at 0 -4.3 180) (layer F.Fab))
    (pad NC thru_hole circle (at 1 -0.25) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 -0.25) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -0.5 0.25) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1.5 0.25) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -0.7) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 0.7) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 2.1) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -2.1) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 2.1) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 0.7) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -0.7) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -2.1) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 -0.25) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1.5 0.25) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0.5 0.25) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -1.4) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 1.4) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 1.4) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -1.4) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 2.75) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -2.75) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 2.75) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -2.75) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 smd rect (at 0 -1.65) (size 2.8 1.6) (layers F.Cu)
      (net 12 "Net-(C12-Pad2)") (solder_paste_margin -0.1))
    (pad 2 smd rect (at 0 1.65) (size 2.8 1.6) (layers F.Cu)
      (net 27 "Net-(D105-Pad1)") (solder_paste_margin -0.1))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CAD_GD_CSSRM2_14_20170907-db/Gx_CSSRM2_20170907_geometry.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module 1_Custom_Footprints:OSRAM_CSS (layer F.Cu) (tedit 5DEEFC1C)
    (at 89 120 180)
    (descr "OSRAM Opto 3030 SMD High-power LED")
    (attr smd)
    (fp_text reference D104 (at 0.5 -2.3) (layer F.SilkS))
    (fp_text value "GD CSSRM2.14 445nm" (at 0 -4.3) (layer F.Fab))
    (pad NC thru_hole circle (at 1 -0.25 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0 -0.25 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -0.5 0.25 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1.5 0.25 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -0.7 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 0.7 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 2.1 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -4 -2.1 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 2.1 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 0.7 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -0.7 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 4 -2.1 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -1 -0.25 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 1.5 0.25 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 0.5 0.25 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -1.4 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 1.4 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 1.4 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -1.4 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 2.75 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 -2.75 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at -2.75 0 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 2.75 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 0 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad NC thru_hole circle (at 2.75 -2.75 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 2))
    (pad 1 smd rect (at 0 -1.65 180) (size 2.8 1.6) (layers F.Cu)
      (net 26 "Net-(D104-Pad1)") (solder_paste_margin -0.1))
    (pad 2 smd rect (at 0 1.65 180) (size 2.8 1.6) (layers F.Cu)
      (net 11 "Net-(C11-Pad1)") (solder_paste_margin -0.1))
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/CAD_GD_CSSRM2_14_20170907-db/Gx_CSSRM2_20170907_geometry.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 105.521 111.522 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 2.397 0.016) (layer F.SilkS))
    (fp_text value 10k (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /DISP_~RST))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 105.752 115.817 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3V3))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /I2C2_SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 104.482 115.817 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0.023 1.27 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3V3))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /I2C2_SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical (layer F.Cu) (tedit 5A29CEA9)
    (at 97.266 116.928 270)
    (descr "Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC-NL.pdf")
    (tags "tag connect programming header pogo pins")
    (attr virtual)
    (fp_text reference DBG1 (at -1.524 -2.032 90) (layer F.SilkS))
    (fp_text value TC2030-CTX-NL (at 0 -2.3 90) (layer F.Fab))
    (fp_text user KEEPOUT (at 0 0 90) (layer Cmts.User))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 6 connect circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 55 "Net-(DBG1-Pad6)"))
    (pad 5 connect circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 4 connect circle (at 0 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 37 /SWCLK))
    (pad 3 connect circle (at 0 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 20 /NRST))
    (pad 2 connect circle (at -1.27 -0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 38 /SWDIO))
    (pad 1 connect circle (at -1.27 0.635 270) (size 0.7874 0.7874) (layers F.Cu F.Mask)
      (net 19 +3V3))
    (pad "" np_thru_hole circle (at -2.54 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  )
  (module 1_Custom_Footprints:NHD-C0216CiZ-FN-FBW-3V (layer B.Cu) (tedit 5DF06743)
    (at 113.8936 113.5634 180)
    (fp_text reference U8 (at 8.5 2) (layer B.SilkS))
    (fp_text value NHD-C0216CiZ-FN-FBW-3V (at 5.1 16.9) (layer B.Fab))
    (pad 8 thru_hole circle (at 0 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(C26-Pad2)"))
    (pad 7 thru_hole circle (at 1.5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(C26-Pad1)"))
    (pad 6 thru_hole circle (at 3 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(C25-Pad1)"))
    (pad 5 thru_hole circle (at 4.5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 +3V3))
    (pad 4 thru_hole circle (at 6 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2) (thermal_width 0.2))
    (pad 3 thru_hole circle (at 7.5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /I2C2_SDA))
    (pad 2 thru_hole circle (at 9 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /I2C2_SCL))
    (pad 1 thru_hole circle (at 10.5 0 180) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /DISP_~RST))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 113.118 115.586)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C26 (at 0 1.524) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(C26-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(C26-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.5365 115.586 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at -0.0255 -1.524) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(C25-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 108.5205 111.522)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0.0255 -1.27) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm_ThermalVias (layer F.Cu) (tedit 5DEF12D2)
    (at 99.2895 72.587)
    (descr "MSOP, 8 Pin (http://www.ti.com/lit/ds/symlink/lm25085.pdf#page=32), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (attr smd)
    (fp_text reference U7 (at 1.9085 -2.499) (layer F.SilkS))
    (fp_text value LM3405A (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.1625 -0.975) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /DEEP_RED_CTRL))
    (pad 7 smd roundrect (at 2.1625 -0.325) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at 2.1625 0.325) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +12V))
    (pad 5 smd roundrect (at 2.1625 0.975) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C17-Pad2)"))
    (pad 4 smd roundrect (at -2.1625 0.975) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C17-Pad1)"))
    (pad 3 smd roundrect (at -2.1625 0.325) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(U7-Pad3)"))
    (pad 2 smd roundrect (at -2.1625 -0.325) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.1625 -0.975) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C16-Pad2)"))
    (pad "" smd roundrect (at 0.43 0.46) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.43 -0.46) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.43 0.46) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.43 -0.46) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at 0 0) (size 1.6 1.8) (layers B.Cu) (roundrect_rratio 0.15625)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0.55 0.65) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at -0.55 0.65) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0.55 -0.65) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at -0.55 -0.65) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND))
    (pad 9 smd roundrect (at 0 0) (size 1.73 1.85) (layers F.Cu F.Mask) (roundrect_rratio 0.144509)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/DGN0008A.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm_ThermalVias (layer F.Cu) (tedit 5DF067A0)
    (at 80.595 110.6455 90)
    (descr "MSOP, 8 Pin (http://www.ti.com/lit/ds/symlink/lm25085.pdf#page=32), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (attr smd)
    (fp_text reference U6 (at 1.9015 -2.469 90) (layer F.SilkS))
    (fp_text value LM3405A (at 0 2.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.1625 -0.975 90) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /DEEP_BLUE_CTRL))
    (pad 7 smd roundrect (at 2.1625 -0.325 90) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at 2.1625 0.325 90) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +12V))
    (pad 5 smd roundrect (at 2.1625 0.975 90) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C13-Pad2)"))
    (pad 4 smd roundrect (at -2.1625 0.975 90) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C13-Pad1)"))
    (pad 3 smd roundrect (at -2.1625 0.325 90) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(U6-Pad3)"))
    (pad 2 smd roundrect (at -2.1625 -0.325 90) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.1625 -0.975 90) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C12-Pad2)"))
    (pad "" smd roundrect (at 0.43 0.46 90) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.43 -0.46 90) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.43 0.46 90) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.43 -0.46 90) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at 0 0 90) (size 1.6 1.8) (layers B.Cu) (roundrect_rratio 0.15625)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0.55 0.65 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 9 thru_hole circle (at -0.55 0.65 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 9 thru_hole circle (at 0.55 -0.65 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 9 thru_hole circle (at -0.55 -0.65 90) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
    (pad 9 smd roundrect (at 0 0 90) (size 1.73 1.85) (layers F.Cu F.Mask) (roundrect_rratio 0.144509)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/DGN0008A.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm_ThermalVias (layer F.Cu) (tedit 5DEF1325)
    (at 124.0225 128.491 180)
    (descr "MSOP, 8 Pin (http://www.ti.com/lit/ds/symlink/lm25085.pdf#page=32), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (attr smd)
    (fp_text reference U5 (at 1.9085 -2.45) (layer F.SilkS))
    (fp_text value LM3405A (at 0 2.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.1625 -0.975 180) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /FAR_RED_CTRL))
    (pad 7 smd roundrect (at 2.1625 -0.325 180) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at 2.1625 0.325 180) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +12V))
    (pad 5 smd roundrect (at 2.1625 0.975 180) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C9-Pad2)"))
    (pad 4 smd roundrect (at -2.1625 0.975 180) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C9-Pad1)"))
    (pad 3 smd roundrect (at -2.1625 0.325 180) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(U5-Pad3)"))
    (pad 2 smd roundrect (at -2.1625 -0.325 180) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.1625 -0.975 180) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C8-Pad2)"))
    (pad "" smd roundrect (at 0.43 0.46 180) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.43 -0.46 180) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.43 0.46 180) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.43 -0.46 180) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at 0 0 180) (size 1.6 1.8) (layers B.Cu) (roundrect_rratio 0.15625)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0.55 0.65 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at -0.55 0.65 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0.55 -0.65 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at -0.55 -0.65 180) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND))
    (pad 9 smd roundrect (at 0 0 180) (size 1.73 1.85) (layers F.Cu F.Mask) (roundrect_rratio 0.144509)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/DGN0008A.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm_ThermalVias (layer F.Cu) (tedit 5DEF134D)
    (at 137.187 91.2125 270)
    (descr "MSOP, 8 Pin (http://www.ti.com/lit/ds/symlink/lm25085.pdf#page=32), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (attr smd)
    (fp_text reference U4 (at 1.9015 -2.499 90) (layer F.SilkS))
    (fp_text value LM3405A (at 0 2.45 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.1625 -0.975 270) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /UV_CTRL))
    (pad 7 smd roundrect (at 2.1625 -0.325 270) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at 2.1625 0.325 270) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +12V))
    (pad 5 smd roundrect (at 2.1625 0.975 270) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C5-Pad2)"))
    (pad 4 smd roundrect (at -2.1625 0.975 270) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C5-Pad1)"))
    (pad 3 smd roundrect (at -2.1625 0.325 270) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(U4-Pad3)"))
    (pad 2 smd roundrect (at -2.1625 -0.325 270) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.1625 -0.975 270) (size 1.425 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C4-Pad2)"))
    (pad "" smd roundrect (at 0.43 0.46 270) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.43 -0.46 270) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.43 0.46 270) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.43 -0.46 270) (size 0.72 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at 0 0 270) (size 1.6 1.8) (layers B.Cu) (roundrect_rratio 0.15625)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0.55 0.65 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at -0.55 0.65 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at 0.55 -0.65 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND))
    (pad 9 thru_hole circle (at -0.55 -0.65 270) (size 0.508 0.508) (drill 0.254) (layers *.Cu)
      (net 1 GND))
    (pad 9 smd roundrect (at 0 0 270) (size 1.73 1.85) (layers F.Cu F.Mask) (roundrect_rratio 0.144509)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/brady/Desktop/growLite LED Datasheets/CAD Files/DGN0008A.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 1_Custom_Footprints:SOT25-5 (layer F.Cu) (tedit 5DED9AB7)
    (at 114.3 106.934 180)
    (fp_text reference U3 (at 1 -1.2) (layer F.SilkS))
    (fp_text value AP7370-33W5 (at 1.1 -3.5) (layer F.Fab))
    (pad 5 smd rect (at 0 -2.4 180) (size 0.55 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 4 smd rect (at 1.9 -2.4 180) (size 0.55 0.8) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U3-Pad4)"))
    (pad 3 smd rect (at 1.9 0 180) (size 0.55 0.8) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U3-Pad3)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.55 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 180) (size 0.55 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 +12V))
  )
  (module 1_Custom_Footprints:4-Lead_AUA_2.5x2.0mm (layer F.Cu) (tedit 5DED95CB)
    (at 107.042 104.41 270)
    (fp_text reference U2 (at -1.5 -0.7) (layer F.SilkS))
    (fp_text value DSC6183JE2A (at 2 -3.6 90) (layer F.Fab))
    (pad 4 smd rect (at 0 -1.25 270) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 3 smd rect (at 1.65 -1.25 270) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U2-Pad3)"))
    (pad 2 smd rect (at 1.65 0 270) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 0.7 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 /LSE_MEMS))
  )
  (module 1_Custom_Footprints:ST-TSSOP20 (layer F.Cu) (tedit 5DED9F3D)
    (at 105.498 102.632 270)
    (fp_text reference U1 (at 2.85 2.8) (layer F.SilkS))
    (fp_text value STM32G03xF6 (at 2.55 -1.25 90) (layer F.Fab))
    (pad 20 smd rect (at 5.75 0 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-Pad20)"))
    (pad 19 smd rect (at 5.75 0.65 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 37 /SWCLK))
    (pad 18 smd rect (at 5.75 1.3 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 38 /SWDIO))
    (pad 17 smd rect (at 5.75 1.95 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 52 /I2C2_SDA))
    (pad 16 smd rect (at 5.75 2.6 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 /I2C2_SCL))
    (pad 15 smd rect (at 5.75 3.25 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 54 /DISP_~RST))
    (pad 14 smd rect (at 5.75 3.9 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 56 /UP_BUT))
    (pad 13 smd rect (at 5.75 4.55 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 58 /LEFT_BUT))
    (pad 12 smd rect (at 5.75 5.2 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 57 /DOWN_BUT))
    (pad 11 smd rect (at 5.75 5.85 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 59 /RIGHT_BUT))
    (pad 10 smd rect (at 0 5.85 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 /DEEP_BLUE_CTRL))
    (pad 9 smd rect (at 0 5.2 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 /DEEP_RED_CTRL))
    (pad 8 smd rect (at 0 4.55 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 /UV_CTRL))
    (pad 7 smd rect (at 0 3.9 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 /FAR_RED_CTRL))
    (pad 6 smd rect (at 0 3.25 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 /NRST))
    (pad 5 smd rect (at 0 2.6 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 1.95 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 +3V3))
    (pad 3 smd rect (at 0 1.3 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at 0 0.65 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 /LSE_MEMS))
    (pad 1 smd rect (at 0 0 270) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad1)"))
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 101.98 68.83 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -1.801 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /DEEP_RED_CTRL))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 76.692 107.973 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -1.801 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /DEEP_BLUE_CTRL))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 121.347 132.144)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -1.801 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /FAR_RED_CTRL))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 140.814 93.845 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -1.801 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /UV_CTRL))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 98.0715 69.58)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 200m (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C16-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 77.618 111.8705 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 200m (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 125.2405 131.498 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 200m (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 140.194 89.9875 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 200m (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 117.071 77.978 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 1.801 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(J1-Pad3)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 1_Custom_Footprints:Laird_TYS6045 (layer F.Cu) (tedit 5DED6C13)
    (at 101.452 80.756 180)
    (fp_text reference L4 (at 2.1 0 90) (layer F.SilkS))
    (fp_text value 15u (at 2 -3.9) (layer F.Fab))
    (pad 2 smd rect (at 4.2 0 180) (size 2 6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C15-Pad1)"))
    (pad 1 smd rect (at 0 0 180) (size 2 6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C17-Pad2)"))
  )
  (module 1_Custom_Footprints:Laird_TYS6045 (layer F.Cu) (tedit 5DED6C13)
    (at 88.794 108.49 270)
    (fp_text reference L3 (at 2.1 0) (layer F.SilkS))
    (fp_text value 15u (at 2 -3.9 90) (layer F.Fab))
    (pad 2 smd rect (at 4.2 0 270) (size 2 6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at 0 0 270) (size 2 6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C13-Pad2)"))
  )
  (module 1_Custom_Footprints:Laird_TYS6045 (layer F.Cu) (tedit 5DED6C13)
    (at 121.86 120.322)
    (fp_text reference L2 (at 2.1 0 90) (layer F.SilkS))
    (fp_text value 15u (at 2 -3.9) (layer F.Fab))
    (pad 2 smd rect (at 4.2 0) (size 2 6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (pad 1 smd rect (at 0 0) (size 2 6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad2)"))
  )
  (module 1_Custom_Footprints:Laird_TYS6045 (layer F.Cu) (tedit 5DED6C13)
    (at 129.018 93.368 90)
    (fp_text reference L1 (at 2.1 0) (layer F.SilkS))
    (fp_text value 15u (at 2 -3.9 90) (layer F.Fab))
    (pad 2 smd rect (at 4.2 0 90) (size 2 6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 1 smd rect (at 0 0 90) (size 2 6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)"))
  )
  (module Diode_SMD:D_SOT-23_ANK (layer F.Cu) (tedit 587CCEF9)
    (at 106.278 75.914 90)
    (descr "SOT-23, Single Diode")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D12 (at -2.314 0.02 180) (layer F.SilkS))
    (fp_text value "8.2V, 300mW" (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 1 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 +12V))
    (pad "" smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-523 (layer F.Cu) (tedit 586419F0)
    (at 103.484 76.884 270)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D11 (at 2.602 0 90) (layer F.SilkS))
    (fp_text value "0.35V, 0.2A" (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 100.052 75.93 180)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D10 (at -0.003 0 270) (layer F.SilkS))
    (fp_text value "0.5V, 2A" (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 "Net-(C17-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOT-23_ANK (layer F.Cu) (tedit 587CCEF9)
    (at 83.952 103.664 180)
    (descr "SOT-23, Single Diode")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D9 (at -2.392 0.032 270) (layer F.SilkS))
    (fp_text value "8.2V, 300mW" (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 +12V))
    (pad "" smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-523 (layer F.Cu) (tedit 586419F0)
    (at 84.922 106.458)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D8 (at 2.094 0) (layer F.SilkS))
    (fp_text value "0.35V, 0.2A" (at 0 1.4) (layer F.Fab))
    (fp_text user %R (at 0 -1.3) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.7 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 83.968 109.89 270)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D7 (at -0.13 0 180) (layer F.SilkS))
    (fp_text value "0.5V, 2A" (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 "Net-(C13-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOT-23_ANK (layer F.Cu) (tedit 587CCEF9)
    (at 117.034 125.164 270)
    (descr "SOT-23, Single Diode")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D6 (at 1.508 1.778 180) (layer F.SilkS))
    (fp_text value "8.2V, 300mW" (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 1 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 +12V))
    (pad "" smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-523 (layer F.Cu) (tedit 586419F0)
    (at 119.828 124.194 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D5 (at 2.094 0 90) (layer F.SilkS))
    (fp_text value "0.35V, 0.2A" (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 123.26 125.148)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at 0 0.110999 90) (layer F.SilkS))
    (fp_text value "0.5V, 2A" (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 "Net-(C9-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOT-23_ANK (layer F.Cu) (tedit 587CCEF9)
    (at 133.86 98.194)
    (descr "SOT-23, Single Diode")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D3 (at 1.508 1.778 270) (layer F.SilkS))
    (fp_text value "8.2V, 300mW" (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 +12V))
    (pad "" smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-523 (layer F.Cu) (tedit 586419F0)
    (at 132.89 95.4 180)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D2 (at 2.094 0) (layer F.SilkS))
    (fp_text value "0.35V, 0.2A" (at 0 1.4) (layer F.Fab))
    (fp_text user %R (at 0 -1.3) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 133.844 91.968 90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 0.008999) (layer F.SilkS))
    (fp_text value "0.5V, 2A" (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 "Net-(C5-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 103.235 100.854 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at -2.517 0) (layer F.SilkS))
    (fp_text value 100n (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 103.1865 99.076 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at -2.8195 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 97.536 105.664 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0.007 -1.182) (layer F.SilkS))
    (fp_text value 100n (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /NRST))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 109.816 104.895 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 -1.17 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 115.062 110.744)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at -2.8195 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.332 107.7215 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at 0 -1.58 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 103.484 74.429 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 2.309 0 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(C17-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(C17-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 94.594 72.6535 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 3.0615 0.02 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(C16-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 95.8895 75.93)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -3.0735 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 105.77 71.482 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 3.668 0.02 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 82.467 106.458 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 2.309 0) (layer F.SilkS))
    (fp_text value 10n (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C13-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 80.6915 115.348 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 2.9835 0.032) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C12-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 83.968 114.078 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at -3.0735 0 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 79.52 104.172 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 3.844 0.032) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 119.828 126.695 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 1.801 0 90) (layer F.SilkS))
    (fp_text value 10n (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C9-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.718 128.4755 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 2.3985 0.028 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C8-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 127.4225 125.148 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.5655 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 117.542 129.596 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 3.31 0.028 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 135.345 95.4)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 1.801 0) (layer F.SilkS))
    (fp_text value 10n (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C5-Pad2)"))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.1715 86.51)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.5145 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 133.844 87.8055 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.5655 0 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.292 97.686)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 3.284 -0.008) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_2816_7142Metric_Pad3.20x4.45mm_HandSolder (layer F.Cu) (tedit 5DF03E2D)
    (at 117.288 81.534 180)
    (descr "Capacitor SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100u (at 0 3.18) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.6 0 180) (size 3.2 4.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.078)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd roundrect (at -2.6 0 180) (size 3.2 4.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.078)
      (net 2 +12V) (zone_connect 2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_2816_7142Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "CAUTION\n! ! HOT ! !" (at 121.75 131 270) (layer B.SilkS))
  (gr_text 390-400nm (at 126 76 270) (layer F.SilkS))
  (gr_text UV-A (at 134 68 180) (layer F.SilkS))
  (gr_text "!! WARNING !!" (at 142 76 90) (layer F.SilkS))
  (gr_text "Deep Red" (at 94 88) (layer F.SilkS))
  (gr_text 660nm (at 80 88) (layer F.SilkS))
  (gr_text "Deep\nBlue" (at 92 128 90) (layer F.SilkS))
  (gr_text 445nm (at 77 129 270) (layer F.SilkS))
  (gr_text "Far Red" (at 141 118 90) (layer F.SilkS))
  (gr_text 12VDC (at 104.5 68.834) (layer B.SilkS))
  (gr_text - (at 107.95 66.802) (layer B.SilkS))
  (gr_text + (at 101.854 66.802) (layer B.SilkS))
  (gr_text "! ! CAUTION ! ! ! HOT ! ! " (at 94.996 76.454 90) (layer B.SilkS))
  (gr_text "! ! CAUTION ! ! ! HOT ! ! " (at 122.936 75.692 270) (layer B.SilkS))
  (gr_text v1.0 (at 101.854 82.804) (layer B.SilkS))
  (gr_text LITE (at 113.284 83.058) (layer B.SilkS))
  (gr_text grow (at 103.378 73.152) (layer B.SilkS))
  (gr_text "RIGHT/\nNEXT" (at 97.028 124.714) (layer B.SilkS))
  (gr_text "LEFT/\nBACK" (at 120.396 124.714) (layer B.SilkS))
  (gr_text DOWN (at 108.5 133.5) (layer B.SilkS))
  (gr_text UP (at 108.5 116.5) (layer B.SilkS))
  (gr_text "DEEP\nBLUE\n4.2W" (at 78 108.5) (layer B.SilkS))
  (gr_text "FAR\nRED\n0.77W" (at 138.5 108.5) (layer B.SilkS))
  (gr_text "UVA\n1W" (at 139 90.5) (layer B.SilkS))
  (gr_text "DEEP\nRED\n3.8W" (at 78 92.5) (layer B.SilkS))
  (gr_text "CAUTION\n! ! HOT ! !" (at 96 131 90) (layer B.SilkS))
  (gr_text 730nm (at 141 130 90) (layer F.SilkS))
  (gr_line (start 73 136) (end 73 65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145 136) (end 73 136) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145 65) (end 145 136) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73 65) (end 145 65) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.6))
    (min_thickness 0.5)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 74.5 86.5) (xy 74.49 66.64) (xy 94.605 66.64) (xy 123.815 66.64) (xy 143.49 66.64)
        (xy 143.5 86.5) (xy 143.5 114.5) (xy 143.5 134.5) (xy 123 134.5) (xy 94.5 134.5)
        (xy 74.5 134.5) (xy 74.5 114.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.6))
    (min_thickness 0.5)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 74.5 66.5) (xy 143.5 66.5) (xy 143.5 134.5) (xy 74.5 134.5)
      )
    )
  )
  (zone (net 19) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.6))
    (min_thickness 0.3)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86 101) (xy 86 116) (xy 94 116) (xy 94 120) (xy 114 120)
        (xy 118 116) (xy 118 110) (xy 115 110) (xy 115 108) (xy 113 108)
        (xy 113 105) (xy 104 96) (xy 86 96)
      )
    )
  )
)
