(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 17)
    (no_connects 0)
    (area 118.589999 91.125 152.922 120.9815)
    (thickness 1.6)
    (drawings 7)
    (tracks 51)
    (zones 0)
    (modules 7)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (user_trace_width 1.5)
    (user_trace_width 1.8)
    (user_trace_width 2.5)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(D2-Pad2)")
  (net 4 GP_GND)
  (net 5 RX)
  (net 6 TX)
  (net 7 GP_14)
  (net 8 +3V3)
  (net 9 GP_17)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net GP_14)
    (add_net GP_17)
    (add_net GP_GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net RX)
    (add_net TX)
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 141.25 106.25)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 1.75) (layer F.SilkS))
    (fp_text value LED (at 9.99 4.745) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 137.25 110.5)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at -0.057 1.7565) (layer F.SilkS))
    (fp_text value LED (at 0.193 9.5065) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 GP_GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05 (layer F.Cu) (tedit 0)
    (at 137 102.54 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 5.04 10.25 180) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 10.29 4.689 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 RX))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 TX))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GP_14))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3V3))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 GP_17))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 137 107 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -1.25 2.5 90) (layer F.SilkS))
    (fp_text value BSS138 (at -0.372 14.947 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 9 GP_17))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 GP_GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 145.25 106.25 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0.012 -2 180) (layer F.SilkS))
    (fp_text value R (at -4.75 0.255 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 141.25 110.5 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.0065 180) (layer F.SilkS))
    (fp_text value R (at -9.0045 -0.0065 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyKiCadLibs:QUECTEL-L80 (layer F.Cu) (tedit 593979B8)
    (at 126.365 104.901)
    (fp_text reference U1 (at 0.148 3) (layer F.SilkS))
    (fp_text value QUECTEL-L80 (at 0.048 -3) (layer F.Fab))
    (pad 6 smd rect (at -6.35 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 7 GP_14))
    (pad 5 smd rect (at -3.81 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 4 smd rect (at -1.27 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 3 smd rect (at 1.27 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 4 GP_GND))
    (pad 2 smd rect (at 3.81 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 5 RX))
    (pad 1 smd rect (at 6.35 -8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 6 TX))
    (pad 7 smd rect (at -6.35 8) (size 1 2) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -3.81 8) (size 1 2) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -1.27 8) (size 1 2) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 1.288 8) (size 1 2) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 3.81 8) (size 1 2) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 6.35 8) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 4 GP_GND))
  )
  (dimension 19.25 (width 0.3) (layer Cmts.User)
    (gr_text "19.250 mm" (at 156.35 104.875 270) (layer Cmts.User))
    (feature1 (pts (xy 150 114.5) (xy 157.7 114.5)))
    (feature2 (pts (xy 150 95.25) (xy 157.7 95.25)))
    (crossbar (pts (xy 155 95.25) (xy 155 114.5)))
    (arrow1a (pts (xy 155 114.5) (xy 154.413579 113.373496)))
    (arrow1b (pts (xy 155 114.5) (xy 155.586421 113.373496)))
    (arrow2a (pts (xy 155 95.25) (xy 154.413579 96.376504)))
    (arrow2b (pts (xy 155 95.25) (xy 155.586421 96.376504)))
  )
  (dimension 30.5 (width 0.3) (layer Cmts.User)
    (gr_text "30.500 mm" (at 134 89.15) (layer Cmts.User))
    (feature1 (pts (xy 149.25 94) (xy 149.25 87.8)))
    (feature2 (pts (xy 118.75 94) (xy 118.75 87.8)))
    (crossbar (pts (xy 118.75 90.5) (xy 149.25 90.5)))
    (arrow1a (pts (xy 149.25 90.5) (xy 148.123496 91.086421)))
    (arrow1b (pts (xy 149.25 90.5) (xy 148.123496 89.913579)))
    (arrow2a (pts (xy 118.75 90.5) (xy 119.876504 91.086421)))
    (arrow2b (pts (xy 118.75 90.5) (xy 119.876504 89.913579)))
  )
  (gr_text "GPS for AR150 \ngithub.com/takigama" (at 134 106.25 340) (layer B.SilkS))
  (gr_line (start 149.25 95.25) (end 118.75 95.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.25 114.5) (end 149.25 95.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.75 114.5) (end 149.25 114.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.75 95.25) (end 118.75 114.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GP_GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.75 95.5) (xy 118.75 114.25) (xy 134.75 114.25) (xy 134.75 95.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.25 95.5) (xy 135.25 114.25) (xy 149 114.25) (xy 149 95.5)
      )
    )
  )
  (zone (net 8) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119 95.5) (xy 119 114.25) (xy 149 114.25) (xy 149 95.5)
      )
    )
  )
)
