(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "User" 508 203.2)
  (title_block
    (title "Raspberry PiDal Switcher Switch Board")
    (date "2025-02-12")
    (rev "v1.2")
    (company "Slow Brewed Effects")
    (comment 1 "Created by Toni Wren")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user "plugins.config")
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )
  (net 0 "")
  (net 1 "Net-(SW1-S)")
  (net 2 "/ROW0")
  (net 3 "Net-(SW2-S)")
  (net 4 "Net-(SW3-S)")
  (net 5 "Net-(SW4-S)")
  (net 6 "/ROW1")
  (net 7 "Net-(SW5-S)")
  (net 8 "Net-(SW6-S)")
  (net 9 "Net-(SW7-S)")
  (net 10 "/ROW2")
  (net 11 "Net-(SW8-S)")
  (net 12 "Net-(SW9-S)")
  (net 13 "/RAW")
  (net 14 "/GND")
  (net 15 "/RESET")
  (net 16 "/VCC")
  (net 17 "/A3")
  (net 18 "/A2")
  (net 19 "/A1")
  (net 20 "/A0")
  (net 21 "/SCK")
  (net 22 "/MISO")
  (net 23 "/MOSI")
  (net 24 "/A10")
  (net 25 "/A9")
  (net 26 "Net-(SW10-S)")
  (net 27 "/COL2")
  (net 28 "/COL1")
  (net 29 "/COL0")
  (net 30 "/RXI")
  (net 31 "/TXO")
  (net 32 "/COL3")
  (footprint "pidal-switches:DO41-2" (layer "F.Cu")
    (at 312.4915 118.1282 180)
    (descr "<b>DO-41 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D6" (at -1.0922 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at -1.905 2.794) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(SW6-S)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "/ROW1") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:DO41-2" (layer "F.Cu")
    (at 264.9444 118.1282 180)
    (descr "<b>DO-41 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D5" (at -1.0922 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at -1.905 2.794) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(SW5-S)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "/ROW1") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:DO41-2" (layer "F.Cu")
    (at 360.0387 118.1282 180)
    (descr "<b>DO-41 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D7" (at -0.8658 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at -1.905 2.794) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(SW7-S)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "/ROW2") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:DO41-2" (layer "F.Cu")
    (at 81.915 135.255)
    (descr "<b>DO-41 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D10" (at -1.0922 0.635) (layer "F.SilkS"))
    (fp_text value "1N4148" (at -1.905 2.54) (layer "F.Fab"))
    (pad "A" thru_hole circle (at 2.54 0) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(SW10-S)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "/ROW0") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:SPST" (layer "F.Cu")
    (at 80.2585 138.43)
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SW10" (at -0.2485 0.635) (layer "F.SilkS"))
    (fp_text value "SPST" (at 0 0) (layer "F.Fab"))
    (fp_text user "1" (at -3.175 1.905) (layer "F.SilkS"))
    (fp_text user "2" (at 6.35 1.905) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -1.27 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 32 "/COL3") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole rect (at 5.08 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(SW10-S)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:DO41-2" (layer "F.Cu")
    (at 217.3972 118.1282 180)
    (descr "<b>DO-41 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D4" (at -1.0922 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at -1.905 2.794) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(SW4-S)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "/ROW1") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:DO41-2" (layer "F.Cu")
    (at 407.5858 118.1282 180)
    (descr "<b>DO-41 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D8" (at -0.9437 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at -1.905 2.794) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(SW8-S)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "/ROW2") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "Connector_Pin:Pin_D1.0mm_L10.0mm" (layer "F.Cu")
    (at 95.25 138.43 180)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "A1" (at 0 2.25) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "/A9") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "pidal-switches:1X12" (layer "F.Cu")
    (at 75.7895 138.4482 180)
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "JP6" (at -1.3462 -1.8288) (layer "F.SilkS"))
    (fp_text value "M12PTH" (at -1.27 3.175) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 13 "/RAW") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 14 "/GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 15 "/RESET") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 7.62 0 270) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 16 "/VCC") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 10.16 0 270) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 17 "/A3") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 12.7 0 270) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 18 "/A2") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at 15.24 0 270) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 19 "/A1") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at 17.78 0 270) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 20 "/A0") (pinfunction "8") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "9" thru_hole circle (at 20.32 0 270) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 21 "/SCK") (pinfunction "9") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "10" thru_hole circle (at 22.86 0 270) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 22 "/MISO") (pinfunction "10") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "11" thru_hole circle (at 25.4 0 270) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 23 "/MOSI") (pinfunction "11") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "12" thru_hole circle (at 27.94 0 270) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 24 "/A10") (pinfunction "12") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-switches:SPST" (layer "F.Cu")
    (at 286.813 118.1282)
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SW6" (at 0.4315 0) (layer "F.SilkS"))
    (fp_text value "SPST" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at -3.175 1.905) (layer "F.SilkS"))
    (fp_text user "2" (at 6.35 1.905) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -1.27 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 27 "/COL2") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole rect (at 5.08 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(SW6-S)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "LOGO" (layer "F.Cu")
    (at 107.058215 132.08)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS"))
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "pidal-switches:SPST" (layer "F.Cu")
    (at 447.2645 118.1282)
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SW9" (at 0.635 0) (layer "F.SilkS"))
    (fp_text value "SPST" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "2" (at 6.35 1.905) (layer "F.SilkS"))
    (fp_text user "1" (at -3.175 1.905) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -1.27 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 27 "/COL2") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole rect (at 5.08 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(SW9-S)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:1X12" (layer "F.Cu")
    (at 47.8495 123.2082)
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "JP7" (at -1.3462 -1.8288) (layer "F.SilkS"))
    (fp_text value "M12PTH" (at -1.27 3.175) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 25 "/A9") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 32 "/COL3") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 27 "/COL2") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 7.62 0 90) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 28 "/COL1") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 10.16 0 90) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 29 "/COL0") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 12.7 0 90) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 10 "/ROW2") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at 15.24 0 90) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 6 "/ROW1") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at 17.78 0 90) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 2 "/ROW0") (pinfunction "8") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "9" thru_hole circle (at 20.32 0 90) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 14 "/GND") (pinfunction "9") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "10" thru_hole circle (at 22.86 0 90) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 14 "/GND") (pinfunction "10") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "11" thru_hole circle (at 25.4 0 90) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 30 "/RXI") (pinfunction "11") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "12" thru_hole circle (at 27.94 0 90) (size 1.8796 1.8796) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 31 "/TXO") (pinfunction "12") (pintype "passive") (solder_mask_margin 0.1016))
  )
  (footprint "pidal-switches:DO41-2" (layer "F.Cu")
    (at 169.8501 118.1282 180)
    (descr "<b>DO-41 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D3" (at -0.5544 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at -1.905 2.794) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(SW3-S)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "/ROW0") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:SPST" (layer "F.Cu")
    (at 334.3601 118.1282)
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SW7" (at 0.5094 0) (layer "F.SilkS"))
    (fp_text value "SPST" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "2" (at 6.35 1.905) (layer "F.SilkS"))
    (fp_text user "1" (at -3.175 1.905) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -1.27 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 29 "/COL0") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole rect (at 5.08 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(SW7-S)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "Connector_Pin:Pin_D1.0mm_L10.0mm" (layer "F.Cu")
    (at 92.075 138.43 180)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "B1" (at 0 2.25) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "/A10") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "pidal-switches:DO41-2" (layer "F.Cu")
    (at 74.7558 118.1282 180)
    (descr "<b>DO-41 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D1" (at -1.0337 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at -5.4787 -9.525) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(SW1-S)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "/ROW0") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:SPST" (layer "F.Cu")
    (at 144.1715 118.1282)
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SW3" (at 0.198 0) (layer "F.SilkS"))
    (fp_text value "SPST" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at -3.175 1.905) (layer "F.SilkS"))
    (fp_text user "2" (at 6.35 1.905) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -1.27 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 27 "/COL2") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole rect (at 5.08 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(SW3-S)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:DO41-2" (layer "F.Cu")
    (at 428.8495 118.1282)
    (descr "<b>DO-41 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D9" (at -1.0922 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at -2.54 0) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(SW9-S)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "/ROW2") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:SPST" (layer "F.Cu")
    (at 239.2658 118.1282)
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SW5" (at 0.3537 0) (layer "F.SilkS"))
    (fp_text value "SPST" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at -3.175 1.905) (layer "F.SilkS"))
    (fp_text user "2" (at 6.35 1.905) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -1.27 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 28 "/COL1") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole rect (at 5.08 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(SW5-S)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "Connector_Pin:Pin_D1.0mm_L10.0mm" (layer "F.Cu")
    (at 88.9 138.43 180)
    (descr "solder Pin_ diameter 1.0mm, hole diameter 1.0mm (press fit), length 10.0mm")
    (tags "solder Pin_ press fit")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "GND1" (at 0 2.25) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 -2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "/GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Pin.3dshapes/Pin_D1.0mm_L10.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "pidal-switches:SPST" (layer "F.Cu")
    (at 96.6244 118.1282)
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SW2" (at 0.1201 0) (layer "F.SilkS"))
    (fp_text value "SPST" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at -3.175 1.905) (layer "F.SilkS"))
    (fp_text user "2" (at 6.35 1.905) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -1.27 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 28 "/COL1") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole rect (at 5.08 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(SW2-S)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:SPST" (layer "F.Cu")
    (at 49.0772 118.1282)
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SW1" (at 0.0423 0) (layer "F.SilkS"))
    (fp_text value "SPST" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "2" (at 6.35 1.905) (layer "F.SilkS"))
    (fp_text user "1" (at -3.175 1.905) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -1.27 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 29 "/COL0") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole rect (at 5.08 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(SW1-S)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:DO41-2" (layer "F.Cu")
    (at 122.3029 118.1282 180)
    (descr "<b>DO-41 0.2\" pad spacing</b>")
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "D2" (at -1.0922 0) (layer "F.SilkS"))
    (fp_text value "1N4148" (at -1.905 2.794) (layer "F.Fab") hide)
    (pad "A" thru_hole circle (at 2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(SW2-S)") (pinfunction "A") (pintype "passive") (solder_mask_margin 0.1016))
    (pad "C" thru_hole rect (at -2.54 0 180) (size 1.408 1.408) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "/ROW0") (pinfunction "C") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:SPST" (layer "F.Cu")
    (at 381.9073 118.1282)
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SW8" (at 0.5872 0) (layer "F.SilkS"))
    (fp_text value "SPST" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "2" (at 6.35 1.905) (layer "F.SilkS"))
    (fp_text user "1" (at -3.175 1.905) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -1.27 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 28 "/COL1") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole rect (at 5.08 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(SW8-S)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (footprint "pidal-switches:SPST" (layer "F.Cu")
    (at 191.7187 118.1282)
    (property "Sheetfile" "pidal-switches.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "SW4" (at 0.2758 0) (layer "F.SilkS"))
    (fp_text value "SPST" (at 0 0) (layer "F.Fab") hide)
    (fp_text user "1" (at -3.175 1.905) (layer "F.SilkS"))
    (fp_text user "2" (at 6.35 1.905) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -1.27 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 29 "/COL0") (pinfunction "P") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
    (pad "2" thru_hole rect (at 5.08 0) (size 1.905 1.905) (drill 1.27) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(SW4-S)") (pinfunction "S") (pintype "passive") (solder_mask_margin 0.1016) (thermal_bridge_angle 45))
  )
  (gr_line (start 455.477172 140.9882) (end 455.477172 115.5882)
    (layer "Edge.Cuts"))
  (gr_line (start 455.477172 115.5882) (end 45.267172 115.5882)
    (layer "Edge.Cuts"))
  (gr_line (start 45.267172 140.9882) (end 455.477172 140.9882)
    (layer "Edge.Cuts"))
  (gr_line (start 45.267172 115.5882) (end 45.267172 140.9882)
    (layer "Edge.Cuts"))
  (gr_text "Raspberry PiDal Switcher Switch Board" (at 116.84 135.640956) (layer "F.SilkS"))
  (gr_text "by Toni Wren" (at 118.677223 139.273404) (layer "F.SilkS"))
  (zone (net 14) (net_name "/GND") (layers "F&B.Cu") (name "stitch_zone_0") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 45.9445 116.2232)
        (xy 454.8845 116.2232)
        (xy 454.8845 140.3532)
        (xy 45.9445 140.3532)
      )
    )
  )
)
