(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~60~ubuntu17.10.1)
  (general
    (links 49)
    (no_connects 0)
    (area 80.949999 95.949999 155.050001 144.050001)
    (thickness 1.6)
    (drawings 23)
    (tracks 102)
    (zones 0)
    (modules 32)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.75 0.75)
    (mod_text_width 0.1)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 99.75 131.25)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 +15V)
  (net 4 GNDA)
  (net 5 "Net-(C6-Pad1)")
  (net 6 "Net-(C7-Pad1)")
  (net 7 -15V)
  (net 8 "Net-(R10-Pad1)")
  (net 9 "Net-(R22-Pad1)")
  (net 10 "Net-(C31-Pad1)")
  (net 11 "Net-(C31-Pad2)")
  (net 12 "Net-(J3-Pad1)")
  (net 13 "Net-(J3-Pad3)")
  (net 14 "Net-(J8-Pad2)")
  (net 15 "Net-(J10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 1)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +15V)
    (add_net -15V)
    (add_net GNDA)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C31-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R22-Pad1)")
  )
  (module custom:C_Rect_L4.0mm_W3.5mm_P2.50mm (layer F.Cu) (tedit 5A1F3E03)
    (at 121.25 125.4 90)
    (fp_text reference C13 (at 0.9 -2.5 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -2.75 0.8 180) (layer F.SilkS))
    (fp_text user %R (at 2.65 -0.8 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.25 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (pad 2 thru_hole circle (at 1.25 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 -15V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.5mm_W6.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5A1DE36B)
    (at 98 140)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference J4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5A1DE3D4)
    (at 138 140)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference J7 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5A1DE28F)
    (at 106.3 134.85 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C6 (at -3.55 -0.7 360) (layer F.SilkS))
    (fp_text value 100uF (at -3.55 2.05 360) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5A1DE2A0)
    (at 129.7 134.85 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C7 (at -3.55 -0.8 360) (layer F.SilkS))
    (fp_text value 100uF (at -3.55 1.95 360) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5A1DE432)
    (at 113.5 110.25 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (fp_text reference C31 (at 7.65 0.3 360) (layer F.SilkS))
    (fp_text value "220pF film" (at 9.75 1.6 360) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C31-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C31-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Conn_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5A1DE45A)
    (at 145.8 107.5)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 6 12) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Conn_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 5A1F368B)
    (at 106.75 114.18)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS) hide)
    (fp_text value LME49710 (at -2.45 1.67 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C31-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C31-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +15V))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 -15V))
    (pad 8 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 5A1F3694)
    (at 121.25 114.18)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U2 (at 3.81 -2.33) (layer F.SilkS) hide)
    (fp_text value LF356 (at 3.81 9.95) (layer F.SilkS))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R10-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R10-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C31-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +15V))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 -15V))
    (pad 8 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Conn_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A1DE3CF)
    (at 145.75 121.89 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J8-Pad2)"))
    (model ${KISYS3DMOD}/Conn_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5A1DE404)
    (at 138 100)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference J5 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 5A1DE27E)
    (at 98 100)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference J6 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Conn_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A1DEADB)
    (at 145.8 131.04 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Conn_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Conn_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5A1DE458)
    (at 145.8 104.85 180)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.33 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Conn_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F25E3)
    (at 117.55 111.17 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 2.42 -0.6 270) (layer F.SilkS))
    (fp_text value 49.9k (at 4.62 0.55 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F25CB)
    (at 131.73 119.35)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 2.67 -0.4) (layer F.SilkS))
    (fp_text value 100 (at 5.22 0.7) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R10-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(J8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F2602)
    (at 141.45 107.45 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 3.25 -0.55 180) (layer F.SilkS))
    (fp_text value 100 (at 3.25 0.45 180) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C31-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F2606)
    (at 141.45 110.45 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 3.25 -0.55 180) (layer F.SilkS))
    (fp_text value 10k (at 3.25 0.7 180) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C31-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F253B)
    (at 123.4 136.1 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R22 (at 10.15 -0.7 180) (layer F.SilkS))
    (fp_text value 475 (at 10.15 0.3 180) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R22-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F24F2)
    (at 123.35 130.45 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R23 (at 10.15 -0.8 180) (layer F.SilkS))
    (fp_text value 90.9 (at 10.4 0.2 180) (layer F.SilkS))
    (fp_text user %R (at 3.81 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R22-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F255D)
    (at 115.75 133.3)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R24 (at -2.5 0.75) (layer F.SilkS))
    (fp_text value 4.7K (at -2.75 -0.25) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F25AF)
    (at 106.93 106.25)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R31 (at 3.92 -0.6) (layer F.SilkS))
    (fp_text value 10k (at 3.82 0.4) (layer F.SilkS))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C31-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C31-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5A1F2506)
    (at 123.54 139.85 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference VREG1 (at 2.54 -3.56 180) (layer F.SilkS) hide)
    (fp_text value LM317 (at -0.96 -2.2 180) (layer F.SilkS))
    (fp_text user %R (at 2.54 -3.56 180) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +15V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R22-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W8.5mm_P5.00mm_FKP2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5A1F351D)
    (at 120.25 103.55)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, length*width=7.2*8.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 8.5mm Capacitor")
    (fp_text reference C1 (at -0.3 -4.8 180) (layer F.SilkS))
    (fp_text value "33nF film" (at 1.6 5.1 180) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W8.5mm_P5.00mm_FKP2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:C_Rect_L4.0mm_W3.5mm_P2.50mm (layer F.Cu) (tedit 5A1F3E33)
    (at 114.5 141.05 180)
    (fp_text reference C5 (at 2.7 -0.85 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.75 180) (layer F.SilkS))
    (fp_text user %R (at 0.25 -3.5 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.25 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +15V))
    (pad 2 thru_hole circle (at 1.25 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.5mm_W6.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:C_Rect_L5.5mm_W4.0mm_P2.50mm (layer F.Cu) (tedit 5A1F3D8F)
    (at 97.55 120.3)
    (fp_text reference C10 (at 3.5 -1.1 270) (layer F.SilkS))
    (fp_text value 1uF (at 1.75 2.65) (layer F.SilkS))
    (fp_text user %R (at 0.25 -2.75) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.25 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +15V))
    (pad 2 thru_hole circle (at 1.25 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.5mm_W6.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:C_Rect_L5.5mm_W4.0mm_P2.50mm (layer F.Cu) (tedit 5A1F3D82)
    (at 97.55 115.2)
    (fp_text reference C11 (at 3.35 1.1 90) (layer F.SilkS))
    (fp_text value 1uF (at 1.85 -2.65) (layer F.SilkS))
    (fp_text user %R (at 0.25 -2.75) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.25 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 -15V))
    (pad 2 thru_hole circle (at 1.25 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.5mm_W6.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:C_Rect_L4.0mm_W3.5mm_P2.50mm (layer F.Cu) (tedit 5A1F3E46)
    (at 132.25 115.55 270)
    (fp_text reference C12 (at -2.7 0.7 360) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.55 -2.45 270) (layer F.SilkS))
    (fp_text user %R (at 2.85 0.35 360) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.25 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (pad 2 thru_hole circle (at 1.25 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +15V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.5mm_W6.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:C_Rect_L4.0mm_W3.5mm_P2.50mm (layer F.Cu) (tedit 5A1F3E22)
    (at 117.55 115.55 270)
    (fp_text reference C22 (at -2.75 0.85 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.65 0.25 360) (layer F.SilkS))
    (fp_text user %R (at -2.75 0.85 360) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.25 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (pad 2 thru_hole circle (at 1.25 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +15V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.5mm_W6.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:C_Rect_L4.0mm_W3.5mm_P2.50mm (layer F.Cu) (tedit 5A1F3DF7)
    (at 106.75 125.35 90)
    (fp_text reference C23 (at 0.85 -2.5 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -2.95 0 180) (layer F.SilkS))
    (fp_text user %R (at 2.85 -0.4 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.25 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (pad 2 thru_hole circle (at 1.25 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 -15V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.5mm_W6.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Conn_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5A304E7A)
    (at 91.05 115.2)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 -15V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GNDA))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +15V))
    (model ${KISYS3DMOD}/Conn_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Conn_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5A304E77)
    (at 145.75 134.16)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J10-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Conn_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (gr_text "Microphone amplifier\n2017.12.18 revision\nBrad Buran\nLBHB@OHSU" (at 89.5 128.75 90) (layer B.SilkS))
  (gr_text V+ (at 88.05 120.3) (layer F.SilkS))
  (gr_arc (start 86 101) (end 81 101) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 86 139) (end 86 144) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 150 139) (end 155 139) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 150 101) (end 150 96) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150 96) (end 120 96) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155 139) (end 155 101) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 86 144) (end 150 144) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 81 101) (end 81 139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120 96) (end 86 96) (layer Edge.Cuts) (width 0.1))
  (gr_text Mic (at 148.65 105.05) (layer F.SilkS))
  (gr_text 40 (at 148.4 107.65) (layer F.SilkS))
  (gr_text 20 (at 148.55 112.65) (layer F.SilkS))
  (gr_text ⏚ (at 87.65 117.7) (layer F.SilkS))
  (gr_text 1.5V (at 149.45 128.5) (layer F.SilkS))
  (gr_text Vo (at 148.15 119.35 90) (layer F.SilkS))
  (gr_text ⏚ (at 148.2 122.05) (layer F.SilkS))
  (gr_text ⏚ (at 148.3 110.15) (layer F.SilkS))
  (gr_text ⏚ (at 148.6 131.05) (layer F.SilkS))
  (gr_text Ch (at 148.75 135.25) (layer F.SilkS))
  (gr_text V- (at 88.25 115.2) (layer F.SilkS))
  (gr_text V- (at 97 114.75) (layer F.Fab))
  (zone (net 4) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81 144) (xy 155 144) (xy 155 96) (xy 81 96)
      )
    )
  )
)
