(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 171)
    (no_connects 1)
    (area 108.225 50.024519 213.725001 146.075)
    (thickness 1.6)
    (drawings 15)
    (tracks 761)
    (zones 0)
    (modules 92)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 3.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 3)
    (pad_drill 2.25)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFFFF)
    (pcbplotparams
      (layerselection 0x00020_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(BNC_Out1-Pad1)")
  (net 3 Pulse)
  (net 4 "Net-(BNC_Out2-Pad1)")
  (net 5 12V)
  (net 6 "Net-(C_Boot1-Pad1)")
  (net 7 Out1)
  (net 8 "Net-(C_Boot2-Pad1)")
  (net 9 Out2)
  (net 10 Reg)
  (net 11 "Net-(C_HI1-Pad2)")
  (net 12 "Net-(C_HI2-Pad2)")
  (net 13 400VPower)
  (net 14 "Net-(C_LI1-Pad1)")
  (net 15 "Net-(C_LI2-Pad1)")
  (net 16 "Net-(C_VDD1-Pad1)")
  (net 17 "Net-(C_VDD3-Pad1)")
  (net 18 "Net-(D1-Pad1)")
  (net 19 "Net-(D3-Pad2)")
  (net 20 "Net-(D4-Pad2)")
  (net 21 "Net-(D6-Pad2)")
  (net 22 "Net-(D10-Pad2)")
  (net 23 "Net-(D11-Pad2)")
  (net 24 "Net-(D12-Pad2)")
  (net 25 "Net-(D14-Pad2)")
  (net 26 "Net-(D_Boot1-Pad2)")
  (net 27 "Net-(D_Boot2-Pad2)")
  (net 28 "Net-(G_AND1-Pad4)")
  (net 29 "Net-(G_AND2-Pad4)")
  (net 30 "Net-(G_NAND1-Pad4)")
  (net 31 "Net-(G_NAND2-Pad4)")
  (net 32 Enable)
  (net 33 "Net-(D7-Pad1)")
  (net 34 "Net-(D8-Pad2)")
  (net 35 "Net-(D15-Pad2)")
  (net 36 "Net-(D16-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 12V)
    (add_net 400VPower)
    (add_net Enable)
    (add_net GND)
    (add_net "Net-(BNC_Out1-Pad1)")
    (add_net "Net-(BNC_Out2-Pad1)")
    (add_net "Net-(C_Boot1-Pad1)")
    (add_net "Net-(C_Boot2-Pad1)")
    (add_net "Net-(C_HI1-Pad2)")
    (add_net "Net-(C_HI2-Pad2)")
    (add_net "Net-(C_LI1-Pad1)")
    (add_net "Net-(C_LI2-Pad1)")
    (add_net "Net-(C_VDD1-Pad1)")
    (add_net "Net-(C_VDD3-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D_Boot1-Pad2)")
    (add_net "Net-(D_Boot2-Pad2)")
    (add_net "Net-(G_AND1-Pad4)")
    (add_net "Net-(G_AND2-Pad4)")
    (add_net "Net-(G_NAND1-Pad4)")
    (add_net "Net-(G_NAND2-Pad4)")
    (add_net Out1)
    (add_net Out2)
    (add_net Pulse)
    (add_net Reg)
  )
  (module MyLibrary:2.2uF_HV_Cap (layer F.Cu) (tedit 5BBE3F77)
    (at 155.32 104.65 270)
    (fp_text reference C_HV1 (at 0.05 10.2 270) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 10 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -13.75 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 13.75 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 400VPower))
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP (layer F.Cu) (tedit 5BBE161D)
    (at 131.4 77)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference BNC_Out1 (at -9 0.2 270) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 10.89914 -9.6012 90) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366) (size 3.50012 5.00126) (drill 2.19964) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5.10032 0.7366) (size 3.50012 5.00126) (drill 2.19964) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 5.00126) (size 1.6002 1.6002) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 "Net-(BNC_Out1-Pad1)"))
    (pad 2 thru_hole circle (at -2.49936 5.00126) (size 1.6002 1.6002) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP (layer F.Cu) (tedit 5A68D122)
    (at 195.34 77)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference BNC_Out2 (at 0 8.25) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 10.89914 -9.6012 90) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366) (size 3.50012 5.00126) (drill 2.19964) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5.10032 0.7366) (size 3.50012 5.00126) (drill 2.19964) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 5.00126) (size 1.6002 1.6002) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 "Net-(BNC_Out2-Pad1)"))
    (pad 2 thru_hole circle (at -2.49936 5.00126) (size 1.6002 1.6002) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP (layer F.Cu) (tedit 5A68D11C)
    (at 152.44 77)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference BNC_SigGen1 (at 0 8.25) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 10.89914 -9.6012 90) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366) (size 3.50012 5.00126) (drill 2.19964) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5.10032 0.7366) (size 3.50012 5.00126) (drill 2.19964) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 5.00126) (size 1.6002 1.6002) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 Pulse))
    (pad 2 thru_hole circle (at -2.49936 5.00126) (size 1.6002 1.6002) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5BC0E6B8)
    (at 118.44 96.3 180)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q_HighSide1 (at 2.34 2.9 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 2.54 3.92 180) (layer F.Fab))
    (fp_text user %R (at 2.34 2.9 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(D6-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 13 400VPower))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5BC0E729)
    (at 180.42 96.43 180)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q_HighSide2 (at 7.3 3 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 2.54 3.92 180) (layer F.Fab))
    (fp_text user %R (at 7.3 3 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(D14-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 13 400VPower))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(D15-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5BC0E6FE)
    (at 133.5 96.3 180)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q_LowSide1 (at 2.1 2.8 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 2.54 3.92 180) (layer F.Fab))
    (fp_text user %R (at 2.1 2.8 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(D3-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(D7-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5BC48D7C)
    (at 195.42 96.53 180)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q_LowSide2 (at -3.4 1.95 450) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 2.54 3.92 180) (layer F.Fab))
    (fp_text user %R (at -3.4 1.95 450) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(D11-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(D16-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 0)
    (at 127.4 117 90)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value UCC27714 (at 0 1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C_HI1-Pad2)"))
    (pad 2 smd rect (at -2.54 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C_LI1-Pad1)"))
    (pad 3 smd rect (at -1.27 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 32 Enable))
    (pad 5 smd rect (at 1.27 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.54 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D1-Pad1)"))
    (pad 7 smd rect (at 3.81 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C_VDD1-Pad1)"))
    (pad 8 smd rect (at 3.81 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.54 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 Out1))
    (pad 12 smd rect (at -1.27 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad2)"))
    (pad 13 smd rect (at -2.54 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C_Boot1-Pad1)"))
    (pad 14 smd rect (at -3.81 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 1.27 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 0)
    (at 187.92 116.49 90)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U2 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value UCC27714 (at 0 1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C_HI2-Pad2)"))
    (pad 2 smd rect (at -2.54 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C_LI2-Pad1)"))
    (pad 3 smd rect (at -1.27 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 32 Enable))
    (pad 5 smd rect (at 1.27 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.54 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D10-Pad2)"))
    (pad 7 smd rect (at 3.81 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C_VDD3-Pad1)"))
    (pad 8 smd rect (at 3.81 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 2.54 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 Out2))
    (pad 12 smd rect (at -1.27 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D12-Pad2)"))
    (pad 13 smd rect (at -2.54 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C_Boot2-Pad1)"))
    (pad 14 smd rect (at -3.81 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 1.27 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5BC0E753)
    (at 161.24 136.05 180)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Reg (at 2.3 2.8 180) (layer F.SilkS))
    (fp_text value V_REG7805 (at 2.54 3.92 180) (layer F.Fab))
    (fp_text user %R (at 2.3 2.8 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 12V))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 Reg))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5BBF50C7)
    (at 161.4 127.7 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_12V1 (at -3.4 0 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at -3.4 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 5BC0DA6D)
    (at 111.2 108.9 90)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C_Boot1 (at 0.1 2.1 90) (layer F.SilkS))
    (fp_text value 68nF (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0.1 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C_Boot1-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 7 Out1))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 5BBE3F33)
    (at 173.27 106.39 90)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C_Boot2 (at 0 -2.25 90) (layer F.SilkS))
    (fp_text value 68nF (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C_Boot2-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 Out2))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5BBE3859)
    (at 132.4 132.7)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_G1 (at 0 1.6) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 1.6) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 Reg))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 139.6 132.7 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_G2 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 Reg))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 134 123.7 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_HI1 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 220pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C_HI1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58AA84E2)
    (at 123.67 91.02 180)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C_HV2 (at 0 -2.25 180) (layer F.SilkS))
    (fp_text value 68nF (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.5 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 13 400VPower))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 134.2 118.5 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_LI1 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 220pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C_LI1-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5BBCF99F)
    (at 118.11 81.09 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_Out1 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BNC_Out1-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 Out1))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 190.54 90.99 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_Out2 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(BNC_Out2-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 Out2))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 166.56 136.12 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_Reg1 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 151.79 135.94 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_Reg2 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 Reg))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 127.2 105.4)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_VDD1 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C_VDD1-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5BBCF9DD)
    (at 134.2 112.7 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_VDD2 (at 0 1.5 270) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C_VDD1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 199.07 111.2)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_VDD3 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C_VDD3-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5BBE39D4)
    (at 194.92 112.19 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_VDD4 (at 0 1.6 270) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 1.6 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C_VDD3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BBE38E0)
    (at 141.77 96.47 90)
    (fp_text reference D1 (at 0 -2.8 270) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 90) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 90) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2.392 0 90) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BBE173B)
    (at 127.4 128.75)
    (fp_text reference D2 (at 1 -2.5) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C_VDD1-Pad1)"))
    (pad 2 smd rect (at 2.392 0) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D1-Pad1)"))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BC0EE99)
    (at 135.59 106.51)
    (fp_text reference D3 (at -0.03 -2.41 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2.392 0) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D3-Pad2)"))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BBE1888)
    (at 111.4 128.3 90)
    (fp_text reference D4 (at -5 0 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 90) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 90) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C_Boot1-Pad1)"))
    (pad 2 smd rect (at 2.392 0 90) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad2)"))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BBE1899)
    (at 111.4 117.9 90)
    (fp_text reference D5 (at 4.8 0 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 90) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 90) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 2.392 0 90) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 7 Out1))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BBF48D1)
    (at 118.8 106.1 180)
    (fp_text reference D6 (at 0 -2.4 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 180) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 180) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 2.392 0 180) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D6-Pad2)"))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BBF50A7)
    (at 205.02 116.19 270)
    (fp_text reference D9 (at 0 -2.6 270) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 270) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 270) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at 2.392 0 270) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BBE3B40)
    (at 187.92 128.24)
    (fp_text reference D10 (at 2.2 -2.45) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C_VDD3-Pad1)"))
    (pad 2 smd rect (at 2.392 0) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D10-Pad2)"))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BC48EF2)
    (at 196.39 105.95)
    (fp_text reference D11 (at 0.07 2.54) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at 2.392 0) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D11-Pad2)"))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BBE3ECA)
    (at 173.27 126.99 90)
    (fp_text reference D12 (at -4.975 0.025 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 90) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 90) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C_Boot2-Pad1)"))
    (pad 2 smd rect (at 2.392 0 90) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D12-Pad2)"))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BBE3EFD)
    (at 173.27 115.39 90)
    (fp_text reference D13 (at 4.75 0 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 90) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 90) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D12-Pad2)"))
    (pad 2 smd rect (at 2.392 0 90) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 9 Out2))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BBF48F7)
    (at 180.81 106.57 180)
    (fp_text reference D14 (at 0 -2.4 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 180) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 180) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D12-Pad2)"))
    (pad 2 smd rect (at 2.392 0 180) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D14-Pad2)"))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BBCF762)
    (at 118.41 125.51 270)
    (fp_text reference D_Boot1 (at 0 2.5 270) (layer F.SilkS))
    (fp_text value D (at 0 3 270) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 270) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C_Boot1-Pad1)"))
    (pad 2 smd rect (at 2.392 0 270) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D_Boot1-Pad2)"))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BBF4C82)
    (at 179.65 123.61 270)
    (fp_text reference D_Boot2 (at 0 2.4 270) (layer F.SilkS))
    (fp_text value D (at 0 3 270) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 270) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C_Boot2-Pad1)"))
    (pad 2 smd rect (at 2.392 0 270) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D_Boot2-Pad2)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5BBE3875)
    (at 136 128.5 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference G_AND1 (at 0.8 -2.6 180) (layer F.SilkS))
    (fp_text value SOT_23 (at 0 2.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 Pulse))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 Pulse))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(G_AND1-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 Reg))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5BBE386C)
    (at 142.2 128.5 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference G_NAND1 (at -1.8 -2.6 180) (layer F.SilkS))
    (fp_text value SOT_23 (at 0 2.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 Pulse))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 Pulse))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(G_NAND1-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 Reg))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLibrary:1pin_1p6mm (layer F.Cu) (tedit 5BBF4FFE)
    (at 165 127.4 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P1 (at 0.1 -2 180) (layer F.SilkS))
    (fp_text value GND_Pin (at 0 3 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0.25 0 180) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MyLibrary:1pin_1p6mm (layer F.Cu) (tedit 5BBF5004)
    (at 152.3 127.3 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P2 (at 0 -2 180) (layer F.SilkS))
    (fp_text value +400V_Pin (at 0 3 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask)
      (net 13 400VPower))
  )
  (module MyLibrary:1pin_1p6mm (layer F.Cu) (tedit 5BBF5000)
    (at 157.6 127.35 180)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P3 (at 0 -1.95 180) (layer F.SilkS))
    (fp_text value +12V_Pin (at 0 3 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 12V))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 131.8 137.4 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 Enable))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5BC0E28E)
    (at 111.06 86.75 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference RMos1 (at -1.8 0 360) (layer F.SilkS))
    (fp_text value 1 (at 1.27 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 Out1))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 34 "Net-(D8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5BBE1609)
    (at 130.1 88.25 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference RMos2 (at -1.75 0.75 360) (layer F.SilkS))
    (fp_text value 1 (at 1.27 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 Out1))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 33 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5BBE6F1A)
    (at 183.95 92.06 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference RMos3 (at 1.2 -2 360) (layer F.SilkS))
    (fp_text value 1 (at 1.27 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 Out2))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 35 "Net-(D15-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5BC48D2C)
    (at 193.86 91.94)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference RMos4 (at 1.17 1.84) (layer F.SilkS))
    (fp_text value 1 (at 1.27 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 Out2))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 "Net-(D16-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BBF4B4B)
    (at 127.2 108.5)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_Bias1 (at 0 1.6) (layer F.SilkS))
    (fp_text value 2.1 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C_VDD1-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BBF4DA6)
    (at 199.02 115.06)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_Bias2 (at 0 -1.6) (layer F.SilkS))
    (fp_text value 2.1 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C_VDD3-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 125.65 125)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_Boot1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 500 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D_Boot1-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C_VDD1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 186.17 124.49)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_Boot2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 500 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D_Boot2-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C_VDD3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BBCF4A2)
    (at 138.6 123.9 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_HI1 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 51 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(G_AND1-Pad4)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C_HI1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 118.8 116.5)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_HO1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 3 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 180.02 115.49)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_HO2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 3 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D14-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BC0DA70)
    (at 118.8 113.3 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_HoS1 (at 0 1.8 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 Out1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BBE3F4F)
    (at 180.02 111.74 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_HoS2 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D14-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 Out2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BBCF518)
    (at 138.6 119.3 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_LI1 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 51 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(G_NAND1-Pad4)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C_LI1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 199.12 118.79 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_LI2 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 51 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(G_AND2-Pad4)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C_LI2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BBE356E)
    (at 138.6 115.5 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_LO1 (at 0 1.6 180) (layer F.SilkS))
    (fp_text value 3 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BC0EB5E)
    (at 188.17 108.39 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_LO2 (at -0.07 -1.51 180) (layer F.SilkS))
    (fp_text value 3 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BBE16EC)
    (at 138.6 112.3 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_LoS1 (at 0 1.75 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BBE34C7)
    (at 188.17 105.13 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_LoS2 (at 0 1.6 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BC0F0AB)
    (at 113.69 78.07 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_Out1 (at -2.36 -0.22 360) (layer F.SilkS))
    (fp_text value 5M (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 Out1))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BC0F0AE)
    (at 119.25 76.45 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_Out2 (at 2.16 0.39 180) (layer F.SilkS))
    (fp_text value 1.5M (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BNC_Out1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BC48D9F)
    (at 187.3 88.13 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_Out3 (at 2.13 -0.27 450) (layer F.SilkS))
    (fp_text value 5M (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 Out2))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5BC48DA2)
    (at 195.15 87.72)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_Out4 (at 2.21 -0.16 90) (layer F.SilkS))
    (fp_text value 1.5M (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(BNC_Out2-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLibrary:SwitchFootprint (layer F.Cu) (tedit 5BBF501E)
    (at 137.7 137.4 180)
    (fp_text reference SW1 (at 0.1 -1.7 180) (layer F.SilkS))
    (fp_text value SW_DPST_x2 (at 0 2.4 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -1 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 12V))
    (pad 2 thru_hole circle (at 1 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 Enable))
  )
  (module MyLibrary:CSM221-28AE (layer F.Cu) (tedit 5BBF49F3)
    (at 123.4 100.7)
    (fp_text reference H1 (at 0 -2.8) (layer F.SilkS))
    (fp_text value CSM221-28AE (at 0 4) (layer F.Fab))
    (pad 1 thru_hole circle (at -12 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 12 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module MyLibrary:CSM221-28AE (layer F.Cu) (tedit 5BCA0B3B)
    (at 185.32 100.83)
    (fp_text reference H2 (at -2.06 2.57) (layer F.SilkS))
    (fp_text value CSM221-28AE (at 0 4) (layer F.Fab))
    (pad 1 thru_hole circle (at -12 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 12 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5BBE3B07)
    (at 194.12 132.59)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_G3 (at 0 1.6) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 1.6) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 Reg))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5BBE3B1D)
    (at 200.92 132.59 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_G4 (at 0 -1.6 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 Reg))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 194.92 123.19 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_HI2 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 220pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C_HI2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 194.92 117.99 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C_LI2 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 220pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C_LI2-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5BBE3AEF)
    (at 202.72 127.99 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference G_AND2 (at -0.8 -2.8 180) (layer F.SilkS))
    (fp_text value SOT_23 (at 0 2.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 Pulse))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 Pulse))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(G_AND2-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 Reg))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5BBE3AED)
    (at 196.52 127.99 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference G_NAND2 (at 0.8 -2.8 180) (layer F.SilkS))
    (fp_text value SOT_23 (at 0 2.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 Pulse))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 Pulse))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(G_NAND2-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 Reg))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 199.12 123.39 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R_HI2 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 51 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(G_NAND2-Pad4)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C_HI2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BC0DBEC)
    (at 138.44 88.6 180)
    (fp_text reference D7 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 180) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 180) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 2.392 0 180) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BC3CBFC)
    (at 118.52 85.94 180)
    (fp_text reference D8 (at 0.03 2.44 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 180) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 180) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 13 400VPower))
    (pad 2 smd rect (at 2.392 0 180) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D8-Pad2)"))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BC0DBD0)
    (at 175.27 89.8 180)
    (fp_text reference D15 (at 0 2.7 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 180) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 180) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 13 400VPower))
    (pad 2 smd rect (at 2.392 0 180) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D15-Pad2)"))
  )
  (module MyLibrary:GB01SLT12-214 (layer F.Cu) (tedit 5BC48EDB)
    (at 203.708 98.552 270)
    (fp_text reference D16 (at -0.02 2.6 270) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 3 270) (layer F.Fab))
    (pad 1 smd rect (at -2.392 0 270) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 2.392 0 270) (size 2.592 2.712) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module MyLibrary:Drill_Footprint (layer F.Cu) (tedit 5BC0DCCB)
    (at 111.1 72.2)
    (fp_text reference D18 (at 0 2.5) (layer F.SilkS))
    (fp_text value Drill (at 0 5.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2.25) (layers *.Cu *.Mask))
  )
  (module MyLibrary:Drill_Footprint (layer F.Cu) (tedit 5BCA039A)
    (at 211.425 139.1)
    (fp_text reference D19 (at 0 -2.6) (layer F.SilkS))
    (fp_text value Drill (at 0 5.9) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.425 -1.5) (size 3 3) (drill 2.25) (layers *.Cu *.Mask))
  )
  (module MyLibrary:Drill_Footprint (layer F.Cu) (tedit 5BCF3A66)
    (at 200.9 72.2)
    (fp_text reference D20 (at 9.41 2.64) (layer F.SilkS))
    (fp_text value Drill (at 0 5.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 9.1 0) (size 3 3) (drill 2.25) (layers *.Cu *.Mask))
  )
  (module MyLibrary:Drill_Footprint (layer F.Cu) (tedit 5BC0DCB1)
    (at 110.9 137.6)
    (fp_text reference D17 (at 3 1.6) (layer F.SilkS))
    (fp_text value Drill (at 0 5.9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2.25) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 58AA84E2)
    (at 168.63 97.03)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C_HV3 (at 0 -2.25) (layer F.SilkS))
    (fp_text value 68nF (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 13 400VPower))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_TE-Connectivity:BNC_Socket_TYCO-AMP (layer F.Cu) (tedit 5BC9FFFA)
    (at 175.34 77)
    (descr "BNC Socket TYCO AMP")
    (tags "BNC Socket TYCO AMP")
    (fp_text reference BNC_GND1 (at -0.32 8.05) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 10.89914 -9.6012 90) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.09778 0.7366) (size 3.50012 5.00126) (drill 2.19964) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 5.10032 0.7366) (size 3.50012 5.00126) (drill 2.19964) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 5.00126) (size 1.6002 1.6002) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.49936 5.00126) (size 1.6002 1.6002) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Sockets_BNC.3dshapes/BNC_Socket_TYCO-AMP.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLibrary:1pin_1p6mm (layer F.Cu) (tedit 5BBCB66D)
    (at 206.25 84.99)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P4 (at 0 -3.048) (layer F.SilkS))
    (fp_text value GND_Pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MyLibrary:Zapping_Armidillos (layer F.Cu) (tedit 5A69049C)
    (at 121.43 136.18)
    (fp_text reference UNCG (at 0 -2.2) (layer F.SilkS))
    (fp_text value "Zapping Armidillos" (at 0 2.2) (layer F.Fab))
    (fp_text user UNCG (at 0 -2.2) (layer F.SilkS))
  )
  (gr_line (start 210.575 140.1) (end 202.375 140.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 213.675 137.05) (end 213.675 72.725) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 213.675 144.2) (end 213.65 144.2) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 201.425 69.7) (end 201.4 69.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 210.6 69.7) (end 201.425 69.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 210.625 137.05) (end 213.675 137.075) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 210.625 72.75) (end 210.6 69.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 202.4 140.1) (end 201.4 140.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 192.4 69.7) (end 201.4 69.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110 140.1) (end 201.4 140.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 109.8 138.7) (end 110 140.1) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.4 131.7) (end 108.4 138.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.4 72.7) (end 108.4 131.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 111.4 72.7) (end 108.4 72.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 192.4 69.7) (end 111.4 69.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 213.5 72.5) (xy 213.5 137.5) (xy 211.5 139.5) (xy 110 139.5) (xy 109 138.5)
        (xy 109 71.5) (xy 110.5 70) (xy 211 70)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.46 70.01) (xy 211 70) (xy 213.5 72.5) (xy 213.5 137.5) (xy 211.48 139.51)
        (xy 109.99 139.5) (xy 109 138.51) (xy 108.99 71.52)
      )
    )
  )
)
