(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 0.1016)
    (drawings 61)
    (tracks 205)
    (zones 0)
    (modules 20)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7EFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 VCC)
  (net 4 MISO)
  (net 5 SCK)
  (net 6 MOSI)
  (net 7 ~RST)
  (net 8 LED_OUT)
  (net 9 "Net-(U2-Pad3)")
  (net 10 "Net-(U2-Pad4)")
  (net 11 "Net-(U2-Pad6)")
  (net 12 "Net-(U2-Pad7)")
  (net 13 "Net-(U2-Pad9)")
  (net 14 "Net-(U2-Pad10)")
  (net 15 "Net-(U2-Pad13)")
  (net 16 "Net-(U2-Pad16)")
  (net 17 "Net-(U2-Pad17)")
  (net 18 "Net-(U2-Pad18)")
  (net 19 "Net-(U2-Pad19)")
  (net 20 "Net-(U2-Pad20)")
  (net 21 "Net-(U3-Pad4)")
  (net 22 "Net-(U3-Pad9)")
  (net 23 "Net-(U3-Pad10)")
  (net 24 "Net-(U3-Pad11)")
  (net 25 "Net-(U1-Pad5)")
  (net 26 "Net-(D1-Pad1)")
  (net 27 "Net-(D2-Pad1)")
  (net 28 "Net-(D3-Pad1)")
  (net 29 "Net-(D4-Pad1)")
  (net 30 "Net-(D5-Pad1)")
  (net 31 "Net-(D6-Pad1)")
  (net 32 "Net-(D7-Pad1)")
  (net 33 "Net-(D8-Pad1)")
  (net 34 "Net-(U2-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net +BATT)
    (add_net GND)
    (add_net LED_OUT)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad9)")
    (add_net SCK)
    (add_net VCC)
    (add_net ~RST)
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at -0.8 0)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference - (at 0.8 1.025 90) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 2 GND))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 1.6 0)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference + (at -0.775 1.025 90) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 1 +BATT))
  )
  (module earringHookWire:earringHookWire (layer F.Cu) (tedit 5E73830F)
    (at -8.1 0 90)
    (fp_text reference H1 (at 0 1.6 90) (layer F.SilkS) hide)
    (fp_text value earringHookWire (at 0 -1.6 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/components/earringHookWire/earringHookWire.stp
      (offset (xyz 0 1.3 -0.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module WS2812B-2020:WS2812B-2020 (layer F.Cu) (tedit 5E7233D6)
    (at 26 0)
    (descr "Addressable 24b color LED")
    (tags "WS2812 Ws2812B 2020 Led NeoPixel Addressable")
    (fp_text reference D8 (at 0 0) (layer B.SilkS))
    (fp_text value WS2812B-2020 (at 0 -1.8) (layer F.Fab))
    (pad 4 smd rect (at -0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd rect (at -0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D8-Pad1)"))
    (model ${KIPRJMOD}/components/WS2812B-2020/WS2812B-2020.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module WS2812B-2020:WS2812B-2020 (layer F.Cu) (tedit 5E7233D6)
    (at 23 0)
    (descr "Addressable 24b color LED")
    (tags "WS2812 Ws2812B 2020 Led NeoPixel Addressable")
    (fp_text reference D7 (at 0 0) (layer B.SilkS))
    (fp_text value WS2812B-2020 (at 0 -1.8) (layer F.Fab))
    (pad 4 smd rect (at -0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd rect (at -0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D7-Pad1)"))
    (model ${KIPRJMOD}/components/WS2812B-2020/WS2812B-2020.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module WS2812B-2020:WS2812B-2020 (layer F.Cu) (tedit 5E7233D6)
    (at 20 0)
    (descr "Addressable 24b color LED")
    (tags "WS2812 Ws2812B 2020 Led NeoPixel Addressable")
    (fp_text reference D6 (at 0 0) (layer B.SilkS))
    (fp_text value WS2812B-2020 (at 0 -1.8) (layer F.Fab))
    (pad 4 smd rect (at -0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd rect (at -0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D6-Pad1)"))
    (model ${KIPRJMOD}/components/WS2812B-2020/WS2812B-2020.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module WS2812B-2020:WS2812B-2020 (layer F.Cu) (tedit 5E7233D6)
    (at 17 0)
    (descr "Addressable 24b color LED")
    (tags "WS2812 Ws2812B 2020 Led NeoPixel Addressable")
    (fp_text reference D5 (at 0 0) (layer B.SilkS))
    (fp_text value WS2812B-2020 (at 0 -1.8) (layer F.Fab))
    (pad 4 smd rect (at -0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd rect (at -0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D5-Pad1)"))
    (model ${KIPRJMOD}/components/WS2812B-2020/WS2812B-2020.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module WS2812B-2020:WS2812B-2020 (layer F.Cu) (tedit 5E7233D6)
    (at 14 0)
    (descr "Addressable 24b color LED")
    (tags "WS2812 Ws2812B 2020 Led NeoPixel Addressable")
    (fp_text reference D4 (at 0 0) (layer B.SilkS))
    (fp_text value WS2812B-2020 (at 0 -1.8) (layer F.Fab))
    (pad 4 smd rect (at -0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd rect (at -0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D4-Pad1)"))
    (model ${KIPRJMOD}/components/WS2812B-2020/WS2812B-2020.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module WS2812B-2020:WS2812B-2020 (layer F.Cu) (tedit 5E7233D6)
    (at 11 0)
    (descr "Addressable 24b color LED")
    (tags "WS2812 Ws2812B 2020 Led NeoPixel Addressable")
    (fp_text reference D3 (at 0 0) (layer B.SilkS))
    (fp_text value WS2812B-2020 (at 0 -1.8) (layer F.Fab))
    (pad 4 smd rect (at -0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd rect (at -0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D3-Pad1)"))
    (model ${KIPRJMOD}/components/WS2812B-2020/WS2812B-2020.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module WS2812B-2020:WS2812B-2020 (layer F.Cu) (tedit 5E7233D6)
    (at 8 0)
    (descr "Addressable 24b color LED")
    (tags "WS2812 Ws2812B 2020 Led NeoPixel Addressable")
    (fp_text reference D2 (at 0 0) (layer B.SilkS))
    (fp_text value WS2812B-2020 (at 0 -1.8) (layer F.Fab))
    (pad 4 smd rect (at -0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd rect (at -0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D2-Pad1)"))
    (model ${KIPRJMOD}/components/WS2812B-2020/WS2812B-2020.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module WS2812B-2020:WS2812B-2020 (layer F.Cu) (tedit 5E7233D6)
    (at 5 0)
    (descr "Addressable 24b color LED")
    (tags "WS2812 Ws2812B 2020 Led NeoPixel Addressable")
    (fp_text reference D1 (at 0 0) (layer B.SilkS))
    (fp_text value WS2812B-2020 (at 0 -1.8) (layer F.Fab))
    (pad 4 smd rect (at -0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 3 smd rect (at -0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 8 LED_OUT))
    (pad 2 smd rect (at 0.915 -0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.915 0.5) (size 0.7 0.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D1-Pad1)"))
    (model ${KIPRJMOD}/components/WS2812B-2020/WS2812B-2020.stp
      (offset (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module MIC5365:MIC5365 (layer F.Cu) (tedit 5E7275CB)
    (at 3.05 -0.1 180)
    (fp_text reference U1 (at 0 0 180) (layer B.SilkS))
    (fp_text value MIC5365-3.3YD5 (at 0 -1.2 180) (layer F.Fab))
    (pad 1 smd custom (at -0.3125 0.375 180) (size 0.08 0.08) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.138 0.15) (xy 0.138 0.15) (xy 0.138 0.045) (xy -0.057 -0.15) (xy -0.138 -0.15)
) (width 0))
      ))
    (pad 2 smd custom (at 0.3125 0.375 180) (size 0.08 0.08) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.138 0.15) (xy -0.138 0.15) (xy -0.138 0.045) (xy 0.057 -0.15) (xy 0.138 -0.15)
) (width 0))
      ))
    (pad 3 smd custom (at 0.3125 -0.375) (size 0.08 0.08) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.138 0.15) (xy 0.138 0.15) (xy 0.138 0.045) (xy -0.057 -0.15) (xy -0.138 -0.15)
) (width 0))
      ))
    (pad 4 smd custom (at -0.3125 -0.375) (size 0.08 0.08) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.138 0.15) (xy -0.138 0.15) (xy -0.138 0.045) (xy 0.057 -0.15) (xy 0.138 -0.15)
) (width 0))
      ))
    (pad 5 smd rect (at 0 0 225) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad5)") (zone_connect 0))
    (model ${KIPRJMOD}/components/MIC5365/MLF-4.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 3.25 -1.575 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 1.45 1.4 180) (layer F.SilkS))
    (fp_text value 2u2 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TC2030-IDC-NL:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical (layer B.Cu) (tedit 5E72069C)
    (at -5.0165 0 270)
    (descr "Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC-NL.pdf")
    (tags "tag connect programming header pogo pins")
    (attr virtual)
    (fp_text reference J1 (at -2.4765 1.016 270) (layer B.SilkS))
    (fp_text value TC2030-IDC-NL (at 0 2.3 270) (layer B.Fab))
    (fp_text user KEEPOUT (at 0 0 270) (layer Cmts.User))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 6 connect circle (at 1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 5 connect circle (at 1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 7 ~RST))
    (pad 4 connect circle (at 0 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 6 MOSI))
    (pad 3 connect circle (at 0 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 5 SCK))
    (pad 2 connect circle (at -1.27 0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 3 VCC))
    (pad 1 connect circle (at -1.27 -0.635 270) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 4 MISO))
    (pad "" np_thru_hole circle (at -2.54 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  )
  (module LSM6DSM:LGA-14_3x2.5mm_6-6 (layer F.Cu) (tedit 5E72055A)
    (at -4.953 0 270)
    (descr "LGA, 14 Pin (http://www.st.com/resource/en/datasheet/lsm6ds3.pdf), generated with kicad-footprint-generator ipc_lga_layoutBorder_generator.py")
    (tags "LGA LGA")
    (attr smd)
    (fp_text reference U3 (at 0 0 90) (layer F.SilkS))
    (fp_text value LSM6DSM (at 0 2.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 14 smd rect (at -0.5 -0.8875 90) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 6 MOSI) (zone_connect 0))
    (pad 13 smd rect (at 0 -0.8875 180) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 SCK))
    (pad 12 smd rect (at 0.5 -0.8875 90) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (zone_connect 0))
    (pad 11 smd rect (at 1.1375 -0.75) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U3-Pad11)") (zone_connect 0))
    (pad 10 smd rect (at 1.1375 -0.25 270) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U3-Pad10)"))
    (pad 9 smd rect (at 1.1375 0.25 270) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U3-Pad9)"))
    (pad 8 smd rect (at 1.1375 0.75) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (zone_connect 0))
    (pad 7 smd rect (at 0.5 0.8875 90) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 0))
    (pad 6 smd rect (at 0 0.8875) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -0.5 0.8875 90) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (zone_connect 0))
    (pad 4 smd rect (at -1.1375 0.75) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U3-Pad4)") (zone_connect 0))
    (pad 3 smd rect (at -1.1375 0.25 270) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at -1.1375 -0.25 270) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 1 smd custom (at -1.1375 -0.75 270) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.3375 -0.125) (xy 0.2125 -0.125) (xy 0.3375 0) (xy 0.3375 0.125) (xy -0.3375 0.125)
) (width 0))
      ))
    (model ${KIPRJMOD}/components/LSM6DSM/LGA-14_3x2.5mm_P0.5mm_LayoutBorder3x4y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ATtiny85-20MU:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm (layer F.Cu) (tedit 5E7203F7)
    (at 0 0 180)
    (descr "QFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf#page=164), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U2 (at -1.65 -1.775) (layer F.SilkS))
    (fp_text value ATtiny85-20MU (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 21 smd roundrect (at 0 0 180) (size 2.6 2.6) (layers F.Cu F.Mask) (roundrect_rratio 0.096154)
      (net 2 GND))
    (pad "" smd roundrect (at -0.65 -0.65 180) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -0.65 0.65 180) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 -0.65 180) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 0.65 180) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad 1 smd roundrect (at -1.925 -1 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 ~RST))
    (pad 2 smd roundrect (at -1.925 -0.5 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 LED_OUT))
    (pad 3 smd roundrect (at -1.925 0 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(U2-Pad3)"))
    (pad 4 smd roundrect (at -1.925 0.5 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(U2-Pad4)"))
    (pad 5 smd roundrect (at -1.925 1 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(U2-Pad5)"))
    (pad 6 smd roundrect (at -1 1.925 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(U2-Pad6)"))
    (pad 7 smd roundrect (at -0.5 1.925 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(U2-Pad7)"))
    (pad 8 smd roundrect (at 0 1.925 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 0.5 1.925 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(U2-Pad9)"))
    (pad 10 smd roundrect (at 1 1.925 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(U2-Pad10)"))
    (pad 11 smd roundrect (at 1.925 1 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 MOSI))
    (pad 12 smd roundrect (at 1.925 0.5 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 MISO))
    (pad 13 smd roundrect (at 1.925 0 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(U2-Pad13)"))
    (pad 14 smd roundrect (at 1.925 -0.5 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 SCK))
    (pad 15 smd roundrect (at 1.925 -1 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 16 smd roundrect (at 1 -1.925 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(U2-Pad16)"))
    (pad 17 smd roundrect (at 0.5 -1.925 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(U2-Pad17)"))
    (pad 18 smd roundrect (at 0 -1.925 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(U2-Pad18)"))
    (pad 19 smd roundrect (at -0.5 -1.925 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(U2-Pad19)"))
    (pad 20 smd roundrect (at -1 -1.925 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(U2-Pad20)"))
    (model ${KIPRJMOD}/components/ATtiny85-20MU/qfn20-4x4.stp
      (offset (xyz 0 0 0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at -3.048 1.15 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -1.15 0.127 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 SCK))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at -3.1012 -1.6256)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0.1802 -0.6744 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 MOSI))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at -6.858 0.6985 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 1.9685 0 270) (layer F.SilkS))
    (fp_text value 0u1 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 3.3 1.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 1.5 -1.4 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +BATT))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start -7.3 3.3) (end -7.3 1.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 2.3 3.3) (end -7.3 3.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 2.3 2.1) (end 2.3 3.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 2.3 -3.3) (end 2.3 -2.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -7.3 -3.3) (end 2.3 -3.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -7.3 -1.6) (end -7.3 -3.3) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -8.1 0) (end -8.599999 -0.599999) (angle -100.3888578) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -8.6 -0.6) (end -7.3 -1.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -7.3 1.6) (end -8.6 0.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 30 0) (end 27.5 -1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 27.5 1) (end 30 0) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 2.3 2.1) (end 27.5 1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 2.3 -2.1) (end 27.5 -1) (layer Edge.Cuts) (width 0.05))
  (gr_text 2020 (at 5.8 1.5) (layer B.SilkS))
  (gr_text 0V1 (at 27.432 0 90) (layer B.SilkS))
  (gr_text sawaiz (at 5.9 -1.4 180) (layer B.SilkS))
)
