(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 189)
    (zones 0)
    (modules 23)
    (nets 33)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad16)")
  (net 2 "Net-(A1-Pad15)")
  (net 3 +12V)
  (net 4 "Net-(A1-Pad14)")
  (net 5 GND)
  (net 6 "Net-(A1-Pad13)")
  (net 7 "Net-(A1-Pad28)")
  (net 8 "Net-(A1-Pad12)")
  (net 9 +5V)
  (net 10 "Net-(A1-Pad11)")
  (net 11 "Net-(A1-Pad26)")
  (net 12 "Net-(A1-Pad10)")
  (net 13 "Net-(A1-Pad25)")
  (net 14 "Net-(A1-Pad9)")
  (net 15 "Net-(A1-Pad24)")
  (net 16 "Net-(A1-Pad8)")
  (net 17 "Net-(A1-Pad23)")
  (net 18 "Net-(A1-Pad7)")
  (net 19 "Net-(A1-Pad22)")
  (net 20 "Net-(A1-Pad6)")
  (net 21 "Net-(A1-Pad21)")
  (net 22 "Net-(A1-Pad5)")
  (net 23 "Net-(A1-Pad20)")
  (net 24 "Net-(A1-Pad19)")
  (net 25 "Net-(A1-Pad3)")
  (net 26 "Net-(A1-Pad18)")
  (net 27 "Net-(A1-Pad2)")
  (net 28 "Net-(A1-Pad17)")
  (net 29 "Net-(A1-Pad1)")
  (net 30 "Net-(J8-Pad3)")
  (net 31 "Net-(J8-Pad1)")
  (net 32 "Net-(J8-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad19)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad22)")
    (add_net "Net-(A1-Pad23)")
    (add_net "Net-(A1-Pad24)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad26)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A1-Pad7)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(J8-Pad8)")
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 107.95 50.8 90)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R11 (at 0.09906 -3.0988 90) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J8-Pad8)"))
    (pad 2 smd trapezoid (at 2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(A1-Pad28)"))
    (pad 1 thru_hole rect (at -5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 32 "Net-(J8-Pad8)"))
    (pad 2 thru_hole rect (at 5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad28)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 74.93 52.92)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R10 (at 0.09906 -3.0988) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J8-Pad3)"))
    (pad 2 smd trapezoid (at 2.413 0 180) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(A1-Pad1)"))
    (pad 1 thru_hole rect (at -5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 30 "Net-(J8-Pad3)"))
    (pad 2 thru_hole rect (at 5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 29 "Net-(A1-Pad1)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 74.93 49.53)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R9 (at 0.09906 -3.0988) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J8-Pad1)"))
    (pad 2 smd trapezoid (at 2.413 0 180) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(A1-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 31 "Net-(J8-Pad1)"))
    (pad 2 thru_hole rect (at 5.00126 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad2)"))
  )
  (module Modules:Arduino_Nano (layer F.Cu) (tedit 58ACAF70)
    (at 74.93 58.42 90)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (fp_text reference A1 (at 7.62 -5.08 90) (layer F.SilkS))
    (fp_text value Arduino_Nano_v3.x (at 8.89 19.05) (layer F.Fab))
    (fp_text user %R (at 6.35 19.05) (layer F.Fab))
    (pad 16 thru_hole oval (at 15.24 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad16)"))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad15)"))
    (pad 30 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad14)"))
    (pad 29 thru_hole oval (at 15.24 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad13)"))
    (pad 28 thru_hole oval (at 15.24 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad28)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad12)"))
    (pad 27 thru_hole oval (at 15.24 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad11)"))
    (pad 26 thru_hole oval (at 15.24 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad26)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad10)"))
    (pad 25 thru_hole oval (at 15.24 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad25)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad9)"))
    (pad 24 thru_hole oval (at 15.24 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad24)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad8)"))
    (pad 23 thru_hole oval (at 15.24 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad23)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad7)"))
    (pad 22 thru_hole oval (at 15.24 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad22)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad6)"))
    (pad 21 thru_hole oval (at 15.24 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad21)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad5)"))
    (pad 20 thru_hole oval (at 15.24 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad20)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 19 thru_hole oval (at 15.24 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad19)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad3)"))
    (pad 18 thru_hole oval (at 15.24 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad18)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-Pad2)"))
    (pad 17 thru_hole oval (at 15.24 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-Pad17)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(A1-Pad1)"))
  )
  (module digikey-footprints:Term_Block_1x8_P5.08mm (layer F.Cu) (tedit 5D419A27)
    (at 109.22 67.31 180)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J1 (at 18.05 -5.05) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x08 (at 18.65 5.2) (layer F.Fab))
    (fp_text user %R (at 17.75 0.15) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad12)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad11)"))
    (pad 3 thru_hole circle (at 10.16 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad10)"))
    (pad 4 thru_hole circle (at 15.24 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad9)"))
    (pad 5 thru_hole circle (at 20.32 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad8)"))
    (pad 6 thru_hole circle (at 25.4 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad7)"))
    (pad 7 thru_hole circle (at 30.48 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad6)"))
    (pad 8 thru_hole circle (at 35.56 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad5)"))
  )
  (module digikey-footprints:Term_Block_1x2_P5.08MM (layer F.Cu) (tedit 5D4199A2)
    (at 128.27 40.64 90)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J2 (at 2.794 -4.826 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 2.032 5.09 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
  )
  (module digikey-footprints:TERM_BLOCK_1x3_P5.08MM (layer F.Cu) (tedit 5D4199C5)
    (at 128.27 68.58 90)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J3 (at 5.16 -4.85 90) (layer F.SilkS))
    (fp_text value TriggerTerminal (at 4.53 5.09 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad14)"))
    (pad 3 thru_hole circle (at 10.16 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 +5V))
  )
  (module digikey-footprints:Term_Block_1x2_P5.08MM (layer F.Cu) (tedit 5D4199A2)
    (at 120.65 35.56 180)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J4 (at 2.794 -4.826) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 2.032 5.09) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module digikey-footprints:Term_Block_1x2_P5.08MM (layer F.Cu) (tedit 5D4199A2)
    (at 92.71 35.56 180)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J5 (at 2.794 -4.826) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 2.032 5.09) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
  )
  (module digikey-footprints:Term_Block_1x2_P5.08MM (layer F.Cu) (tedit 5D4199A2)
    (at 80.01 35.56 180)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J6 (at 2.794 -4.826) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 2.032 5.09) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
  )
  (module digikey-footprints:Term_Block_1x2_P5.08MM (layer F.Cu) (tedit 5D4199A2)
    (at 115.57 67.31)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J7 (at 2.794 -4.826) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 2.032 5.09) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module Connectors:RJ45_8 (layer F.Cu) (tedit 0)
    (at 66.04 58.42 270)
    (tags RJ45)
    (fp_text reference J8 (at 4.7 11.18 90) (layer F.SilkS))
    (fp_text value RJ45 (at 4.59 6.25 90) (layer F.Fab))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(J8-Pad8)"))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(J8-Pad3)"))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(J8-Pad3)"))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 "Net-(J8-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 "Net-(J8-Pad1)"))
    (pad Hole np_thru_hole circle (at -1.49 6.35 270) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at 10.38 6.35 270) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (model ${KISYS3DMOD}/Connectors.3dshapes/RJ45_8.wrl
      (offset (xyz 4.571999931335449 -6.349999904632568 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Term_Block_1x2_P5.08MM (layer F.Cu) (tedit 5D4199A2)
    (at 128.27 52.07 90)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J9 (at 2.794 -4.826 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 2.032 5.09 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 +12V))
  )
  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5861378E)
    (at 63.5 45.72 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J10 (at -8.45 5.75 270) (layer F.SilkS))
    (fp_text value Barrel_Jack (at -6.2 -5.5 90) (layer F.Fab))
    (pad 3 thru_hole rect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole rect (at -6 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 85.09 50.73904 270)
    (descr "Resistor, SMD+THT, universal, 1206, RM10, HandSoldering,")
    (tags "Resistor, SMD+THT, universal, 1206, RM10, Hand soldering,")
    (fp_text reference R1 (at 0.09906 -2.4003 90) (layer F.SilkS))
    (fp_text value R (at 2.70002 2.70002 90) (layer F.Fab))
    (pad 2 thru_hole rect (at 5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad5)"))
    (pad 1 thru_hole rect (at -5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at 2.60096 0 270) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(A1-Pad5)"))
    (pad 1 smd rect (at -2.60096 0 270) (size 2.99974 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 102.87 50.927 90)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R2 (at 0.09906 -3.0988 90) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(A1-Pad12)"))
    (pad 2 smd trapezoid (at 2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 1 thru_hole rect (at -5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad12)"))
    (pad 2 thru_hole rect (at 5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 +5V))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 87.63 50.87874 270)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R3 (at 0.09906 -3.0988 90) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116 90) (layer F.Fab))
    (pad 2 thru_hole rect (at 5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad6)"))
    (pad 1 thru_hole rect (at -5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 2 smd trapezoid (at 2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(A1-Pad6)"))
    (pad 1 smd trapezoid (at -2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 100.33 50.87874 90)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R4 (at 0.09906 -3.0988 90) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116 90) (layer F.Fab))
    (pad 2 thru_hole rect (at 5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 1 thru_hole rect (at -5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad11)"))
    (pad 2 smd trapezoid (at 2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 1 smd trapezoid (at -2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(A1-Pad11)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 90.17 50.72126 270)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R5 (at 0.09906 -3.0988 90) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 2 smd trapezoid (at 2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(A1-Pad7)"))
    (pad 1 thru_hole rect (at -5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 2 thru_hole rect (at 5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad7)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 97.79 50.927 90)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R6 (at 0.09906 -3.0988 90) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(A1-Pad10)"))
    (pad 2 smd trapezoid (at 2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 1 thru_hole rect (at -5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad10)"))
    (pad 2 thru_hole rect (at 5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 +5V))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 92.71 50.927 270)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R7 (at 0.09906 -3.0988 90) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116 90) (layer F.Fab))
    (pad 2 thru_hole rect (at 5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad8)"))
    (pad 1 thru_hole rect (at -5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 2 smd trapezoid (at 2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(A1-Pad8)"))
    (pad 1 smd trapezoid (at -2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 0)
    (at 95.25 50.927 90)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R8 (at 0.09906 -3.0988 90) (layer F.SilkS))
    (fp_text value R (at -0.39878 4.20116 90) (layer F.Fab))
    (pad 2 thru_hole rect (at 5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 1 thru_hole rect (at -5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad9)"))
    (pad 2 smd trapezoid (at 2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (pad 1 smd trapezoid (at -2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(A1-Pad9)"))
  )
  (module digikey-footprints:TERM_BLOCK_1x3_P5.08MM (layer F.Cu) (tedit 5D4199C5)
    (at 109.22 35.56 180)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J11 (at 5.16 -4.85) (layer F.SilkS))
    (fp_text value "Pot Term" (at 4.53 5.09) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad19)"))
    (pad 3 thru_hole circle (at 10.16 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 +5V))
  )
  (gr_text USB (at 113.03 50.8 270) (layer F.SilkS))
  (gr_text "ARDUINO\nNANO" (at 119.38 50.8 90) (layer F.SilkS))
  (gr_line (start 50.8 73.66) (end 50.8 72.39) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.62 73.66) (end 50.8 73.66) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.62 29.21) (end 134.62 73.66) (layer Edge.Cuts) (width 0.05))
  (gr_text "RELAY POWER" (at 118.11 72.39) (layer F.SilkS))
  (gr_text POT (at 104.14 30.48 180) (layer F.SilkS))
  (gr_text TRIGGER (at 133.35 63.5 90) (layer F.SilkS))
  (gr_text "RELAY BOARD" (at 91.44 72.39) (layer F.SilkS))
  (gr_line (start 50.8 29.21) (end 134.62 29.21) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50.8 72.39) (end 50.8 29.21) (layer Edge.Cuts) (width 0.05))
)
