(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 100 105.2)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-PadA5)")
  (net 2 "+5V")
  (net 3 "GND")
  (net 4 "Net-(J1-PadB5)")
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 99.1 96.3 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "usb-c performance mx.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 2.2 0 180) (layer "F.SilkS"))
    (fp_text value "5.1K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "Net-(J1-PadA5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.9 96.3 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "usb-c performance mx.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 2.2 0 180) (layer "F.SilkS"))
    (fp_text value "5.1K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(J1-PadB5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.7mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 95.55 84)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.7mm" (at 0 4.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.8 3.8) (drill 3.8) (layers F&B.Cu *.Mask))
  )
  (footprint "Custom_Library:USB_C_Receptable_DENKE_Power_Only" (layer "F.Cu")
    (tedit 0)
    (at 100 100)
    (property "Sheetfile" "usb-c performance mx.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -5.5 1.9 90 unlocked) (layer "F.SilkS"))
    (fp_text value "USB_C_Receptacle_Power_Only" (at 0 -5.08 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "F.Fab"))
    (pad "A5" smd roundrect (at -0.5 0) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 1 "Net-(J1-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A9" smd roundrect (at 1.5 0) (size 0.8 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 2 "+5V") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" smd roundrect (at 2.7 0) (size 0.8 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 3 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B5" smd roundrect (at 0.5 0) (size 0.7 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 4 "Net-(J1-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B9" smd roundrect (at -1.5 0) (size 0.8 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 2 "+5V") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" smd roundrect (at -2.7 0) (size 0.8 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 3 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 3.85) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 0.05) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 3.85) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 0.05) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "H:/KiCAD Projects/3D Models/USB Connector Type C female 6pin/USB Connector Type C female 6pin.STEP"
      (offset (xyz 0 -6.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.7mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 95.55 97.45)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.8mm" (at 0 4.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.8 3.8) (drill 3.8) (layers F&B.Cu *.Mask))
  )
  (footprint "kibuzzard-63334861" (layer "F.Cu")
    (tedit 63334861)
    (at 102 78.2 90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiTGVmdCIsICJDYXBMZWZ0Q2hvaWNlIjogIigiLCAiQ2FwUmlnaHRDaG9pY2UiOiAiXSIsICJGb250Q29tYm9Cb3giOiAibXBsdXMtMW1uLW1lZGl1bSIsICJIZWlnaHRDdHJsIjogIjEuMSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJHTkQiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAiMiIsICJQYWRkaW5nTGVmdEN0cmwiOiAiMCIsICJQYWRkaW5nUmlnaHRDdHJsIjogIjY1IiwgIlBhZGRpbmdUb3BDdHJsIjogIjIiLCAiV2lkdGhDdHJsIjogIjMifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-63334861" (at 0 -3.848365 90) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 3.848365 90) (layer "F.SilkS") hide)
  )
  (footprint "kibuzzard-63334844" (layer "F.Cu")
    (tedit 63334844)
    (at 98 78.2 90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiTGVmdCIsICJDYXBMZWZ0Q2hvaWNlIjogIigiLCAiQ2FwUmlnaHRDaG9pY2UiOiAiXSIsICJGb250Q29tYm9Cb3giOiAibXBsdXMtMW1uLW1lZGl1bSIsICJIZWlnaHRDdHJsIjogIjEuMSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICI1ViIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICIyIiwgIlBhZGRpbmdMZWZ0Q3RybCI6ICIwIiwgIlBhZGRpbmdSaWdodEN0cmwiOiAiNzgiLCAiUGFkZGluZ1RvcEN0cmwiOiAiMiIsICJXaWR0aEN0cmwiOiAiMyJ9")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-63334844" (at 0 -3.839633 90) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 3.839633 90) (layer "F.SilkS") hide)
  )
  (footprint "kibuzzard-63334861" (layer "B.Cu")
    (tedit 63334861)
    (at 102 78.2 90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiTGVmdCIsICJDYXBMZWZ0Q2hvaWNlIjogIigiLCAiQ2FwUmlnaHRDaG9pY2UiOiAiXSIsICJGb250Q29tYm9Cb3giOiAibXBsdXMtMW1uLW1lZGl1bSIsICJIZWlnaHRDdHJsIjogIjEuMSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJHTkQiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAiMiIsICJQYWRkaW5nTGVmdEN0cmwiOiAiMCIsICJQYWRkaW5nUmlnaHRDdHJsIjogIjY1IiwgIlBhZGRpbmdUb3BDdHJsIjogIjIiLCAiV2lkdGhDdHJsIjogIjMifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-63334861" (at 0 3.848365 90) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 -3.848365 90) (layer "F.SilkS") hide)
  )
  (footprint "kibuzzard-63334844" (layer "B.Cu")
    (tedit 63334844)
    (at 98 78.2 90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiTGVmdCIsICJDYXBMZWZ0Q2hvaWNlIjogIigiLCAiQ2FwUmlnaHRDaG9pY2UiOiAiXSIsICJGb250Q29tYm9Cb3giOiAibXBsdXMtMW1uLW1lZGl1bSIsICJIZWlnaHRDdHJsIjogIjEuMSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICI1ViIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICIyIiwgIlBhZGRpbmdMZWZ0Q3RybCI6ICIwIiwgIlBhZGRpbmdSaWdodEN0cmwiOiAiNzgiLCAiUGFkZGluZ1RvcEN0cmwiOiAiMiIsICJXaWR0aEN0cmwiOiAiMyJ9")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-63334844" (at 0 3.839633 90) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 -3.839633 90) (layer "F.SilkS") hide)
  )
  (gr_arc (start 105.3 99.7) (mid 105.607538 98.957538) (end 106.35 98.65) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.25 93.85) (end 92.35 93.85) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 96.25 87.45) (mid 98.512742 88.387258) (end 99.45 90.65) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 107.65 98.65) (end 107.65 82.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 106.35 98.65) (end 107.65 98.65) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 105.9 105.2) (end 105.9 103.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 92.35 82.2) (end 96.75 74.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 107.65 103.2) (end 107.65 100.9) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 103.35 74.2) (end 107.65 82.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.75 74.2) (end 103.35 74.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 105.9 105.2) (end 94.1 105.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 92.35 87.45) (end 92.35 82.2) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 106.35 100.9) (mid 105.607538 100.592462) (end 105.3 99.85) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 96.25 87.45) (end 92.35 87.45) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 105.9 103.2) (end 107.65 103.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 107.65 100.9) (end 106.35 100.9) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 94.1 103.2) (end 92.35 103.2) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 99.45 90.65) (mid 98.512742 92.912742) (end 96.25 93.85) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 92.35 103.2) (end 92.35 93.85) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 94.1 105.2) (end 94.1 103.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 105.3 99.85) (end 105.3 99.7) (layer "Edge.Cuts") (width 0.1))
  (gr_text "USB-C PERFORMANCE MX\nCHARGE ADAPTER" (at 105.6 88.7 90) (layer "F.SilkS"))
  (gr_text "5.1K" (at 102.1 96.3 90) (layer "F.SilkS"))
  (gr_text "5.1K" (at 97.9 96.3 90) (layer "F.SilkS"))
  (zone (net 3) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 108.1 106.3)
        (xy 92 106.3)
        (xy 91.8 73.2)
        (xy 108.1 73.2)
      )
    )
  )
  (zone (net 3) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 108.1 106.3)
        (xy 92 106.3)
        (xy 91.8 73.2)
        (xy 108.1 73.2)
      )
    )
  )
)
