(kicad_pcb (version 4) (host pcbnew 0.201412131231+5320~19~ubuntu14.04.1-product)
  (general
    (links 98)
    (no_connects 0)
    (area 114.749999 58.949999 169.450001 129.950001)
    (thickness 1.6)
    (drawings 58)
    (tracks 349)
    (zones 0)
    (modules 22)
    (nets 114)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.289)
    (user_trace_width 0.35)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8128)
    (via_drill 0.508)
    (via_min_size 0.654)
    (via_min_drill 0.4)
    (user_via 0.762 0.508)
    (user_via 0.8 0.508)
    (uvia_size 0.558)
    (uvia_drill 0.3048)
    (uvias_allowed no)
    (uvia_min_size 0.558)
    (uvia_min_drill 0.3048)
    (pcb_text_width 0.3)
    (pcb_text_size 1.2 1.2)
    (mod_edge_width 0.15)
    (mod_text_size 0.7 0.7)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_80000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory trial))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3.3V)
  (net 3 "Net-(Q1-Pad3)")
  (net 4 "Net-(Q1-Pad1)")
  (net 5 "Net-(R8-Pad1)")
  (net 6 "Net-(R9-Pad1)")
  (net 7 "Net-(U1-Pad1)")
  (net 8 "Net-(U1-Pad9)")
  (net 9 "Net-(U1-Pad7)")
  (net 10 "Net-(U1-Pad5)")
  (net 11 "Net-(U1-Pad3)")
  (net 12 "Net-(U1-Pad37)")
  (net 13 "Net-(U1-Pad35)")
  (net 14 "Net-(U1-Pad38)")
  (net 15 "Net-(U1-Pad36)")
  (net 16 "Net-(U1-Pad34)")
  (net 17 "Net-(U1-Pad32)")
  (net 18 "Net-(U1-Pad33)")
  (net 19 "Net-(U1-Pad26)")
  (net 20 "Net-(U1-Pad24)")
  (net 21 "Net-(U1-Pad31)")
  (net 22 "Net-(U1-Pad22)")
  (net 23 "Net-(U1-Pad18)")
  (net 24 "Net-(U1-Pad25)")
  (net 25 "Net-(U1-Pad16)")
  (net 26 "Net-(U1-Pad23)")
  (net 27 "Net-(U1-Pad14)")
  (net 28 "Net-(U1-Pad12)")
  (net 29 "Net-(U1-Pad19)")
  (net 30 "Net-(U1-Pad10)")
  (net 31 "Net-(U1-Pad17)")
  (net 32 "Net-(U1-Pad8)")
  (net 33 "Net-(U1-Pad15)")
  (net 34 "Net-(U1-Pad6)")
  (net 35 "Net-(U1-Pad13)")
  (net 36 "Net-(U1-Pad4)")
  (net 37 "Net-(U1-Pad11)")
  (net 38 "Net-(U1-Pad2)")
  (net 39 "Net-(U1-Pad911)")
  (net 40 "Net-(U1-Pad913)")
  (net 41 "Net-(U1-Pad906)")
  (net 42 "Net-(U1-Pad915)")
  (net 43 "Net-(U1-Pad908)")
  (net 44 "Net-(U1-Pad917)")
  (net 45 "Net-(U1-Pad912)")
  (net 46 "Net-(U1-Pad921)")
  (net 47 "Net-(U1-Pad914)")
  (net 48 "Net-(U1-Pad923)")
  (net 49 "Net-(U1-Pad916)")
  (net 50 "Net-(U1-Pad925)")
  (net 51 "Net-(U1-Pad918)")
  (net 52 "Net-(U1-Pad927)")
  (net 53 "Net-(U1-Pad929)")
  (net 54 "Net-(U1-Pad922)")
  (net 55 "Net-(U1-Pad931)")
  (net 56 "Net-(U1-Pad924)")
  (net 57 "Net-(U1-Pad926)")
  (net 58 "Net-(U1-Pad933)")
  (net 59 "Net-(U1-Pad928)")
  (net 60 "Net-(U1-Pad932)")
  (net 61 "Net-(U1-Pad934)")
  (net 62 "Net-(U1-Pad936)")
  (net 63 "Net-(U1-Pad938)")
  (net 64 "Net-(U1-Pad935)")
  (net 65 "Net-(U1-Pad937)")
  (net 66 "Net-(U1-Pad905)")
  (net 67 "Net-(U1-Pad907)")
  (net 68 "Net-(U1-Pad909)")
  (net 69 "Net-(U1-Pad939)")
  (net 70 "Net-(U1-Pad940)")
  (net 71 "Net-(U1-Pad930)")
  (net 72 "Net-(U1-Pad941)")
  (net 73 "Net-(U1-Pad942)")
  (net 74 "Net-(U2-Pad2)")
  (net 75 "Net-(U2-Pad3)")
  (net 76 "Net-(U2-Pad46)")
  (net 77 "Net-(U2-Pad47)")
  (net 78 /CH2)
  (net 79 /CH1)
  (net 80 /CH4)
  (net 81 /CH3)
  (net 82 /CH6)
  (net 83 /CH5)
  (net 84 /CH12)
  (net 85 /CH8)
  (net 86 /CH7)
  (net 87 /CH11)
  (net 88 /CH10)
  (net 89 /CH14)
  (net 90 /CH9)
  (net 91 /CH13)
  (net 92 /IN1)
  (net 93 /IN2)
  (net 94 /IN3)
  (net 95 /IN4)
  (net 96 /IN5)
  (net 97 /IN6)
  (net 98 /IN7)
  (net 99 /IN8)
  (net 100 /IN9)
  (net 101 /IN10)
  (net 102 /IN11)
  (net 103 /IN12)
  (net 104 /IN13)
  (net 105 /IN14)
  (net 106 /EP_SDA)
  (net 107 /EP_SCL)
  (net 108 /SYS_RESETn)
  (net 109 "Net-(C2-Pad1)")
  (net 110 "Net-(R10-Pad2)")
  (net 111 "Net-(R5-Pad1)")
  (net 112 "Net-(R12-Pad2)")
  (net 113 "Net-(R13-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.508)
    (uvia_dia 0.558)
    (uvia_drill 0.3048)
    (add_net /EP_SCL)
    (add_net /EP_SDA)
    (add_net GND)
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R5-Pad1)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.35)
    (via_dia 0.8128)
    (via_drill 0.508)
    (uvia_dia 0.558)
    (uvia_drill 0.3048)
    (add_net +3.3V)
    (add_net /SYS_RESETn)
    (add_net "Net-(C2-Pad1)")
  )
  (net_class Signal ""
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.508)
    (uvia_dia 0.558)
    (uvia_drill 0.3048)
    (add_net /CH1)
    (add_net /CH10)
    (add_net /CH11)
    (add_net /CH12)
    (add_net /CH13)
    (add_net /CH14)
    (add_net /CH2)
    (add_net /CH3)
    (add_net /CH4)
    (add_net /CH5)
    (add_net /CH6)
    (add_net /CH7)
    (add_net /CH8)
    (add_net /CH9)
    (add_net /IN1)
    (add_net /IN10)
    (add_net /IN11)
    (add_net /IN12)
    (add_net /IN13)
    (add_net /IN14)
    (add_net /IN2)
    (add_net /IN3)
    (add_net /IN4)
    (add_net /IN5)
    (add_net /IN6)
    (add_net /IN7)
    (add_net /IN8)
    (add_net /IN9)
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U1-Pad905)")
    (add_net "Net-(U1-Pad906)")
    (add_net "Net-(U1-Pad907)")
    (add_net "Net-(U1-Pad908)")
    (add_net "Net-(U1-Pad909)")
    (add_net "Net-(U1-Pad911)")
    (add_net "Net-(U1-Pad912)")
    (add_net "Net-(U1-Pad913)")
    (add_net "Net-(U1-Pad914)")
    (add_net "Net-(U1-Pad915)")
    (add_net "Net-(U1-Pad916)")
    (add_net "Net-(U1-Pad917)")
    (add_net "Net-(U1-Pad918)")
    (add_net "Net-(U1-Pad921)")
    (add_net "Net-(U1-Pad922)")
    (add_net "Net-(U1-Pad923)")
    (add_net "Net-(U1-Pad924)")
    (add_net "Net-(U1-Pad925)")
    (add_net "Net-(U1-Pad926)")
    (add_net "Net-(U1-Pad927)")
    (add_net "Net-(U1-Pad928)")
    (add_net "Net-(U1-Pad929)")
    (add_net "Net-(U1-Pad930)")
    (add_net "Net-(U1-Pad931)")
    (add_net "Net-(U1-Pad932)")
    (add_net "Net-(U1-Pad933)")
    (add_net "Net-(U1-Pad934)")
    (add_net "Net-(U1-Pad935)")
    (add_net "Net-(U1-Pad936)")
    (add_net "Net-(U1-Pad937)")
    (add_net "Net-(U1-Pad938)")
    (add_net "Net-(U1-Pad939)")
    (add_net "Net-(U1-Pad940)")
    (add_net "Net-(U1-Pad941)")
    (add_net "Net-(U1-Pad942)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad46)")
    (add_net "Net-(U2-Pad47)")
  )
  (module "Custom libs:BBB" locked (layer B.Cu) (tedit 54AD0BFD)
    (at 169.4 134 90)
    (descr "Beagle Bone Black")
    (tags Beagle)
    (fp_text reference U1 (at 44.8945 -23.9395 90) (layer B.SilkS) hide)
    (fp_text value bbb (at 44.7675 -26.67 90) (layer B.SilkS) hide)
    (pad 1 thru_hole circle (at 71.4248 -4.4196 270) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask B.SilkS)
      (net 7 "Net-(U1-Pad1)"))
    (pad 46 thru_hole circle (at 15.5448 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 78 /CH2))
    (pad 45 thru_hole circle (at 15.5448 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 79 /CH1))
    (pad 44 thru_hole circle (at 18.0848 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 80 /CH4))
    (pad 43 thru_hole circle (at 18.0848 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 81 /CH3))
    (pad 42 thru_hole circle (at 20.6248 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 82 /CH6))
    (pad 41 thru_hole circle (at 20.6248 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 83 /CH5))
    (pad 30 thru_hole circle (at 35.8648 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 84 /CH12))
    (pad 40 thru_hole circle (at 23.1648 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 85 /CH8))
    (pad 39 thru_hole circle (at 23.1648 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 86 /CH7))
    (pad 9 thru_hole circle (at 61.2648 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(U1-Pad9)"))
    (pad 7 thru_hole circle (at 63.8048 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(U1-Pad7)"))
    (pad 5 thru_hole circle (at 66.3448 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 10 "Net-(U1-Pad5)"))
    (pad 3 thru_hole circle (at 68.8848 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 11 "Net-(U1-Pad3)"))
    (pad 37 thru_hole circle (at 25.7048 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(U1-Pad37)"))
    (pad 35 thru_hole circle (at 28.2448 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 13 "Net-(U1-Pad35)"))
    (pad 38 thru_hole circle (at 25.7048 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 14 "Net-(U1-Pad38)"))
    (pad 36 thru_hole circle (at 28.2448 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 15 "Net-(U1-Pad36)"))
    (pad 34 thru_hole circle (at 30.7848 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 16 "Net-(U1-Pad34)"))
    (pad 32 thru_hole circle (at 33.3248 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 17 "Net-(U1-Pad32)"))
    (pad 28 thru_hole circle (at 38.4048 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 87 /CH11))
    (pad 33 thru_hole circle (at 30.7848 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 18 "Net-(U1-Pad33)"))
    (pad 26 thru_hole circle (at 40.9448 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 19 "Net-(U1-Pad26)"))
    (pad 24 thru_hole circle (at 43.4848 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 20 "Net-(U1-Pad24)"))
    (pad 31 thru_hole circle (at 33.3248 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 "Net-(U1-Pad31)"))
    (pad 22 thru_hole circle (at 46.0248 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 22 "Net-(U1-Pad22)"))
    (pad 29 thru_hole circle (at 35.8648 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 88 /CH10))
    (pad 20 thru_hole circle (at 48.5648 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 89 /CH14))
    (pad 27 thru_hole circle (at 38.4048 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 90 /CH9))
    (pad 18 thru_hole circle (at 51.1048 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 23 "Net-(U1-Pad18)"))
    (pad 25 thru_hole circle (at 40.9448 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 24 "Net-(U1-Pad25)"))
    (pad 16 thru_hole circle (at 53.6448 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 25 "Net-(U1-Pad16)"))
    (pad 23 thru_hole circle (at 43.4848 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 26 "Net-(U1-Pad23)"))
    (pad 14 thru_hole circle (at 56.1848 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 27 "Net-(U1-Pad14)"))
    (pad 21 thru_hole circle (at 46.0248 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 91 /CH13))
    (pad 12 thru_hole circle (at 58.7248 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 28 "Net-(U1-Pad12)"))
    (pad 19 thru_hole circle (at 48.5648 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 29 "Net-(U1-Pad19)"))
    (pad 10 thru_hole circle (at 61.2648 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 30 "Net-(U1-Pad10)"))
    (pad 17 thru_hole circle (at 51.1048 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 31 "Net-(U1-Pad17)"))
    (pad 8 thru_hole circle (at 63.8048 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 32 "Net-(U1-Pad8)"))
    (pad 15 thru_hole circle (at 53.6448 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 33 "Net-(U1-Pad15)"))
    (pad 6 thru_hole circle (at 66.3448 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 34 "Net-(U1-Pad6)"))
    (pad 13 thru_hole circle (at 56.1848 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 35 "Net-(U1-Pad13)"))
    (pad 4 thru_hole circle (at 68.8848 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 36 "Net-(U1-Pad4)"))
    (pad 11 thru_hole circle (at 58.7248 -4.4196 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 37 "Net-(U1-Pad11)"))
    (pad 2 thru_hole circle (at 71.4248 -1.8796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 38 "Net-(U1-Pad2)"))
    (pad 902 thru_hole circle (at 71.4248 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 911 thru_hole circle (at 58.7248 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 39 "Net-(U1-Pad911)"))
    (pad 904 thru_hole circle (at 68.8848 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 +3.3V))
    (pad 913 thru_hole circle (at 56.1848 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 40 "Net-(U1-Pad913)"))
    (pad 906 thru_hole circle (at 66.3448 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 41 "Net-(U1-Pad906)"))
    (pad 915 thru_hole circle (at 53.6448 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 42 "Net-(U1-Pad915)"))
    (pad 908 thru_hole circle (at 63.8048 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 43 "Net-(U1-Pad908)"))
    (pad 917 thru_hole circle (at 51.1048 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 44 "Net-(U1-Pad917)"))
    (pad 910 thru_hole circle (at 61.2648 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 108 /SYS_RESETn))
    (pad 919 thru_hole circle (at 48.5648 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 107 /EP_SCL))
    (pad 912 thru_hole circle (at 58.7248 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 45 "Net-(U1-Pad912)"))
    (pad 921 thru_hole circle (at 46.0248 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 46 "Net-(U1-Pad921)"))
    (pad 914 thru_hole circle (at 56.1848 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 47 "Net-(U1-Pad914)"))
    (pad 923 thru_hole circle (at 43.4848 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 48 "Net-(U1-Pad923)"))
    (pad 916 thru_hole circle (at 53.6448 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 49 "Net-(U1-Pad916)"))
    (pad 925 thru_hole circle (at 40.9448 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 50 "Net-(U1-Pad925)"))
    (pad 918 thru_hole circle (at 51.1048 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 51 "Net-(U1-Pad918)"))
    (pad 927 thru_hole circle (at 38.4048 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 52 "Net-(U1-Pad927)"))
    (pad 920 thru_hole circle (at 48.5648 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 106 /EP_SDA))
    (pad 929 thru_hole circle (at 35.8648 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 53 "Net-(U1-Pad929)"))
    (pad 922 thru_hole circle (at 46.0248 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 54 "Net-(U1-Pad922)"))
    (pad 931 thru_hole circle (at 33.3248 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 55 "Net-(U1-Pad931)"))
    (pad 924 thru_hole circle (at 43.4848 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 56 "Net-(U1-Pad924)"))
    (pad 926 thru_hole circle (at 40.9448 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 57 "Net-(U1-Pad926)"))
    (pad 933 thru_hole circle (at 30.7848 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 58 "Net-(U1-Pad933)"))
    (pad 928 thru_hole circle (at 38.4048 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 59 "Net-(U1-Pad928)"))
    (pad 932 thru_hole circle (at 33.3248 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 60 "Net-(U1-Pad932)"))
    (pad 934 thru_hole circle (at 30.7848 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 61 "Net-(U1-Pad934)"))
    (pad 936 thru_hole circle (at 28.2448 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 62 "Net-(U1-Pad936)"))
    (pad 938 thru_hole circle (at 25.7048 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 63 "Net-(U1-Pad938)"))
    (pad 935 thru_hole circle (at 28.2448 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 64 "Net-(U1-Pad935)"))
    (pad 937 thru_hole circle (at 25.7048 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 65 "Net-(U1-Pad937)"))
    (pad 903 thru_hole circle (at 68.8848 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 +3.3V))
    (pad 905 thru_hole circle (at 66.3448 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 66 "Net-(U1-Pad905)"))
    (pad 907 thru_hole circle (at 63.8048 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 67 "Net-(U1-Pad907)"))
    (pad 909 thru_hole circle (at 61.2648 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 68 "Net-(U1-Pad909)"))
    (pad 939 thru_hole circle (at 23.1648 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 69 "Net-(U1-Pad939)"))
    (pad 940 thru_hole circle (at 23.1648 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 70 "Net-(U1-Pad940)"))
    (pad 930 thru_hole circle (at 35.8648 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 71 "Net-(U1-Pad930)"))
    (pad 941 thru_hole circle (at 20.6248 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 72 "Net-(U1-Pad941)"))
    (pad 942 thru_hole circle (at 20.6248 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 73 "Net-(U1-Pad942)"))
    (pad 943 thru_hole circle (at 18.0848 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 944 thru_hole circle (at 18.0848 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 945 thru_hole circle (at 15.5448 -52.6796 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 946 thru_hole circle (at 15.5448 -50.1396 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 901 thru_hole circle (at 71.4248 -52.6796 270) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
  )
  (module Pin_Headers:Pin_Header_Angled_2x14 (layer F.Cu) (tedit 548DE101)
    (at 142.3 116.95 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -19.5 -4.25 180) (layer F.SilkS) hide)
    (fp_text value CONN_02X14 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -16.51 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 92 /IN1))
    (pad 2 thru_hole oval (at -16.51 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at -13.97 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 93 /IN2))
    (pad 4 thru_hole oval (at -13.97 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at -11.43 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 94 /IN3))
    (pad 6 thru_hole oval (at -11.43 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole oval (at -8.89 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 95 /IN4))
    (pad 8 thru_hole oval (at -8.89 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9 thru_hole oval (at -6.35 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 96 /IN5))
    (pad 10 thru_hole oval (at -6.35 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 11 thru_hole oval (at -3.81 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 97 /IN6))
    (pad 12 thru_hole oval (at -3.81 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 13 thru_hole oval (at -1.27 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 98 /IN7))
    (pad 14 thru_hole oval (at -1.27 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole oval (at 1.27 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 99 /IN8))
    (pad 16 thru_hole oval (at 1.27 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 17 thru_hole oval (at 3.81 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 100 /IN9))
    (pad 18 thru_hole oval (at 3.81 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 19 thru_hole oval (at 6.35 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 101 /IN10))
    (pad 20 thru_hole oval (at 6.35 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 21 thru_hole oval (at 8.89 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 102 /IN11))
    (pad 22 thru_hole oval (at 8.89 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 23 thru_hole oval (at 11.43 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 103 /IN12))
    (pad 24 thru_hole oval (at 11.43 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 25 thru_hole oval (at 13.97 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 104 /IN13))
    (pad 26 thru_hole oval (at 13.97 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 27 thru_hole oval (at 16.51 1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 105 /IN14))
    (pad 28 thru_hole oval (at 16.51 -1.27 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers/Pin_Header_Angled_2x14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOT-23 (layer B.Cu) (tedit 548DA1AC)
    (at 140.9192 104.4956 270)
    (tags SOT23)
    (fp_text reference Q1 (at 0.0044 -0.0058 270) (layer B.SilkS))
    (fp_text value BSS138 (at 0.0635 0 270) (layer B.SilkS) hide)
    (pad 3 smd rect (at 0 1.09982 270) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 0.9525 -1.09982 270) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 -1.09982 270) (size 0.8001 1.00076) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (model smd\SOT23_3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_SSOP:TSSOP-48_6.1x12.5mm_Pitch0.5mm (layer B.Cu) (tedit 548DE205)
    (at 152.15 104.95 225)
    (descr "TSSOP48: plastic thin shrink small outline package; 48 leads; body width 6.1 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot362-1_po.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U2 (at -3.058237 -7.05339 225) (layer B.SilkS) hide)
    (fp_text value 74LVCH16245 (at -0.070711 0.247487 315) (layer B.SilkS))
    (pad 1 smd rect (at -3.75 5.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (pad 2 smd rect (at -3.75 5.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -3.75 4.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -3.75 4.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -3.75 3.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(R8-Pad1)"))
    (pad 6 smd rect (at -3.75 3.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(R9-Pad1)"))
    (pad 7 smd rect (at -3.75 2.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (pad 8 smd rect (at -3.75 2.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 87 /CH11))
    (pad 9 smd rect (at -3.75 1.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 88 /CH10))
    (pad 10 smd rect (at -3.75 1.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -3.75 0.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 90 /CH9))
    (pad 12 smd rect (at -3.75 0.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 84 /CH12))
    (pad 13 smd rect (at -3.75 -0.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 85 /CH8))
    (pad 14 smd rect (at -3.75 -0.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 86 /CH7))
    (pad 15 smd rect (at -3.75 -1.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -3.75 -1.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 82 /CH6))
    (pad 17 smd rect (at -3.75 -2.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 83 /CH5))
    (pad 18 smd rect (at -3.75 -2.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (pad 19 smd rect (at -3.75 -3.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 80 /CH4))
    (pad 20 smd rect (at -3.75 -3.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 81 /CH3))
    (pad 21 smd rect (at -3.75 -4.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 22 smd rect (at -3.75 -4.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 78 /CH2))
    (pad 23 smd rect (at -3.75 -5.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 79 /CH1))
    (pad 24 smd rect (at -3.75 -5.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (pad 25 smd rect (at 3.75 -5.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(Q1-Pad3)"))
    (pad 26 smd rect (at 3.75 -5.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 92 /IN1))
    (pad 27 smd rect (at 3.75 -4.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 93 /IN2))
    (pad 28 smd rect (at 3.75 -4.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 29 smd rect (at 3.75 -3.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 94 /IN3))
    (pad 30 smd rect (at 3.75 -3.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 95 /IN4))
    (pad 31 smd rect (at 3.75 -2.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 109 "Net-(C2-Pad1)"))
    (pad 32 smd rect (at 3.75 -2.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 96 /IN5))
    (pad 33 smd rect (at 3.75 -1.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 97 /IN6))
    (pad 34 smd rect (at 3.75 -1.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 35 smd rect (at 3.75 -0.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 98 /IN7))
    (pad 36 smd rect (at 3.75 -0.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 99 /IN8))
    (pad 37 smd rect (at 3.75 0.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 103 /IN12))
    (pad 38 smd rect (at 3.75 0.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 100 /IN9))
    (pad 39 smd rect (at 3.75 1.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 40 smd rect (at 3.75 1.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 101 /IN10))
    (pad 41 smd rect (at 3.75 2.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 102 /IN11))
    (pad 42 smd rect (at 3.75 2.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 109 "Net-(C2-Pad1)"))
    (pad 43 smd rect (at 3.75 3.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 104 /IN13))
    (pad 44 smd rect (at 3.75 3.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 105 /IN14))
    (pad 45 smd rect (at 3.75 4.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 46 smd rect (at 3.75 4.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(U2-Pad46)"))
    (pad 47 smd rect (at 3.75 5.25 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(U2-Pad47)"))
    (pad 48 smd rect (at 3.75 5.75 225) (size 1 0.285) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(Q1-Pad3)"))
    (model Housings_SSOP/TSSOP-48_6.1x12.5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 54AD1EF1)
    (at 125.4506 85.1408 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at -3.9592 -3.4506 90) (layer B.SilkS) hide)
    (fp_text value EEPROM (at 0 -3.5 90) (layer B.SilkS))
    (pad 1 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 113 "Net-(R13-Pad2)"))
    (pad 2 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 112 "Net-(R12-Pad2)"))
    (pad 3 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 111 "Net-(R5-Pad1)"))
    (pad 4 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 106 /EP_SDA))
    (pad 6 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 107 /EP_SCL))
    (pad 7 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 110 "Net-(R10-Pad2)"))
    (pad 8 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (model Housings_SOIC/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DA24A)
    (at 143.5354 101.1936 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.8186 0.9354 450) (layer B.SilkS))
    (fp_text value 100K (at 0.0814 -0.0146 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(Q1-Pad3)"))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DA347)
    (at 124.7902 79.7052 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.3302 0.0348 90) (layer B.SilkS))
    (fp_text value 4K7 (at 0.0052 -0.0152 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 107 /EP_SCL))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DA34B)
    (at 123.063 79.7306 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.3306 0.062 90) (layer B.SilkS))
    (fp_text value 4K7 (at -0.0194 0.037 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 106 /EP_SDA))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DA343)
    (at 126.5174 79.7306 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.3306 0.0826 90) (layer B.SilkS))
    (fp_text value 10K (at -0.0194 0.0076 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 110 "Net-(R10-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DC58E)
    (at 130.175 85.2932)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.225 0.1068) (layer B.SilkS))
    (fp_text value 10K (at 0.05 -0.0432) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 111 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DC4AC)
    (at 130.175 86.9188)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 2.325 -0.0438) (layer B.SilkS) hide)
    (fp_text value 10K (at 0.025 0.0062) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 112 "Net-(R12-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DC4B0)
    (at 130.2004 88.6714)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.3246 0.0036) (layer B.SilkS) hide)
    (fp_text value 10K (at 0.0746 0.0036) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 113 "Net-(R13-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DA261)
    (at 161.55 87.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -0.025 -1.425) (layer B.SilkS))
    (fp_text value 0R (at -2.3 2.025) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 89 /CH14))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DA25D)
    (at 161.55 89.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 1.5) (layer B.SilkS))
    (fp_text value 0R (at -2.25 -1.925) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 91 /CH13))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DA359)
    (at 130.0734 80.5434 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -2.5516 -0.0816 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.9 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 110 "Net-(R10-Pad2)"))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DC484)
    (at 125.0442 91.2368 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -2.6882 0.0808 90) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.9 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 112 "Net-(R12-Pad2)"))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DC480)
    (at 126.9746 91.2368 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -2.6632 0.1504 90) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.9 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 113 "Net-(R13-Pad2)"))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DC894)
    (at 141.625 101.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 2.475 -0.05 90) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.9 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 108 /SYS_RESETn))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DA232)
    (at 147.05 99.225 45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.174353 0.053033 45) (layer B.SilkS))
    (fp_text value "0.1 uF" (at 0 -1.9 135) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0 45) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 45) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 548DA239)
    (at 157.2 110.9 45)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.209709 0.123744 45) (layer B.SilkS))
    (fp_text value "0.1 uF" (at 0 -1.9 45) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.75 0 45) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 109 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 45) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 548DA1E5)
    (at 145.475 100.625 135)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at 1.962221 0.159099 135) (layer B.SilkS))
    (fp_text value 0R (at -2.616295 -0.035355 135) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.45 0 135) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 109 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.45 0 135) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 +3.3V))
    (model Resistors_SMD/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module logo:logo (layer F.Cu) (tedit 548DD7FB)
    (at 142.85 75.925)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (dimension 71 (width 0.3) (layer Margin)
    (gr_text "71.000 mm" (at 173.6 94.5 90) (layer Margin))
    (feature1 (pts (xy 141.4 59) (xy 174.8 59)))
    (feature2 (pts (xy 141.4 130) (xy 174.8 130)))
    (crossbar (pts (xy 172.4 130) (xy 172.4 59)))
    (arrow1a (pts (xy 172.4 59) (xy 172.986421 60.126504)))
    (arrow1b (pts (xy 172.4 59) (xy 171.813579 60.126504)))
    (arrow2a (pts (xy 172.4 130) (xy 172.986421 128.873496)))
    (arrow2b (pts (xy 172.4 130) (xy 171.813579 128.873496)))
  )
  (dimension 54.6 (width 0.3) (layer Margin)
    (gr_text "54.600 mm" (at 142.1 133.9) (layer Margin))
    (feature1 (pts (xy 169.4 100.9) (xy 169.4 135.1)))
    (feature2 (pts (xy 114.8 100.9) (xy 114.8 135.1)))
    (crossbar (pts (xy 114.8 132.7) (xy 169.4 132.7)))
    (arrow1a (pts (xy 169.4 132.7) (xy 168.273496 133.286421)))
    (arrow1b (pts (xy 169.4 132.7) (xy 168.273496 132.113579)))
    (arrow2a (pts (xy 114.8 132.7) (xy 115.926504 133.286421)))
    (arrow2b (pts (xy 114.8 132.7) (xy 115.926504 132.113579)))
  )
  (gr_arc (start 157.2 117.7) (end 157.2 129.9) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.4 99) (end 169.4 117.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.4 59) (end 169.4 99) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.6 59) (end 169.4 59) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153.5 63.8) (end 155.6 59) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.7 63.8) (end 153.5 63.8) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127.8 129.9) (end 157.2 129.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 127.8 116.9) (end 114.8 116.9) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8 59) (end 114.8 116.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.6 59) (end 114.8 59) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.7 63.8) (end 128.6 59) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text www.beaglelogic.net (at 143 90.6) (layer F.SilkS))
  (gr_text "Cape version 1.1" (at 143 88.2) (layer F.SilkS))
  (gr_text P9 (at 118.2 120.8) (layer F.SilkS))
  (gr_text P9 (at 122.2 65.2) (layer F.SilkS))
  (gr_text P8 (at 162 65.2) (layer F.SilkS))
  (gr_text P8 (at 166.4 121) (layer F.SilkS))
  (gr_text 1 (at 163 62.6) (layer F.SilkS))
  (gr_text 19 (at 162.4 85.4) (layer F.SilkS))
  (gr_text 29 (at 162.4 98.2) (layer F.SilkS))
  (gr_text 39 (at 162.4 111) (layer F.SilkS))
  (gr_text 45 (at 162.4 118.6) (layer F.SilkS))
  (gr_text 9 (at 163.4 72.8) (layer F.SilkS))
  (gr_text 10 (at 120.8 72.8) (layer F.SilkS))
  (gr_text 46 (at 121.6 118.6) (layer F.SilkS))
  (gr_text 40 (at 121.6 110.8) (layer F.SilkS))
  (gr_text 30 (at 121.8 98.2) (layer F.SilkS))
  (gr_text 20 (at 121.8 85.4) (layer F.SilkS))
  (gr_text 2 (at 121.2 62.6) (layer F.SilkS))
  (gr_text Inputs (at 142.8 105.7) (layer F.SilkS))
  (gr_text P8_22* (at 126 110.6 90) (layer F.SilkS))
  (gr_text P8_30 (at 131.1 111.1 90) (layer F.SilkS))
  (gr_text P8_21* (at 128.6 110.6 90) (layer F.SilkS))
  (gr_text P8_28 (at 133.6 111.1 90) (layer F.SilkS))
  (gr_text P8_41 (at 148.6 111.1 90) (layer F.SilkS))
  (gr_text P8_42 (at 146.2 111.1 90) (layer F.SilkS))
  (gr_text P8_39 (at 143.6 111.1 90) (layer F.SilkS))
  (gr_text P8_40 (at 141.1 111.1 90) (layer F.SilkS))
  (gr_text P8_29 (at 136 111.1 90) (layer F.SilkS))
  (gr_text P8_27 (at 138.6 111.1 90) (layer F.SilkS))
  (gr_text P8_44 (at 151.2 111.1 90) (layer F.SilkS))
  (gr_text P8_43 (at 153.8 111.1 90) (layer F.SilkS))
  (gr_text P8_46 (at 156.5 111.1 90) (layer F.SilkS))
  (gr_text "Up to 5V" (at 142.3 102.9) (layer F.SilkS))
  (gr_text P8_45 (at 159 111.1 90) (layer F.SilkS))
  (gr_text "All bottom pins GND" (at 142.2 100) (layer F.SilkS))
  (gr_text CH14 (at 122 125) (layer F.SilkS))
  (gr_text CH1 (at 162.4 125) (layer F.SilkS))
  (gr_text "Remove R15 for 1.8 V logic\nConnect its bottom pad\nto VDD_ADC (1V8)\n" (at 146 95.4) (layer B.SilkS))
  (gr_text "CH13&14 Enable using 0R\nWARNING:Disable eMMC first" (at 162.4 84) (layer B.SilkS))
  (gr_text A1 (at 125.2 93.8) (layer B.SilkS))
  (gr_text A0 (at 127 93.8) (layer B.SilkS))
  (gr_text "Shunt to '0'\nCape Address" (at 126 95.4) (layer B.SilkS))
  (gr_text A1 (at 132.4 87) (layer B.SilkS))
  (gr_text A0 (at 132.4 88.8) (layer B.SilkS))
  (gr_text "(c) 2014-15 Kumar Abhishek\nwww.theembeddedkitchen.net\nwww.beaglelogic.net" (at 142.7 69.6) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 128.1 59.5) (xy 130.2 64.3) (xy 154 64.3) (xy 156.1 59.5) (xy 169 59.5)
        (xy 169 66.9) (xy 169 69.1) (xy 169 71.7) (xy 169 75.6) (xy 169 81.9)
        (xy 169 85.8) (xy 169 94.2) (xy 169 98.3) (xy 169 108.6) (xy 169 119.1)
        (xy 168.8 120.5) (xy 168 122.6) (xy 167.2 124) (xy 166 125.5) (xy 165.1 126.4)
        (xy 164.2 127.2) (xy 163.3 127.8) (xy 162.2 128.4) (xy 161.2 128.8) (xy 160.5 129.1)
        (xy 159.7 129.3) (xy 159.1 129.4) (xy 158.3 129.5) (xy 157.6 129.6) (xy 156.6 129.6)
        (xy 150.1 129.6) (xy 144 129.6) (xy 126.9 129.6) (xy 126.5 129.6) (xy 126.1 129.6)
        (xy 125.4 129.5) (xy 124.5 129.3) (xy 123.8 129.1) (xy 123.2 128.9) (xy 122.2 128.5)
        (xy 121.4 128) (xy 120.8 127.7) (xy 120.2 127.3) (xy 119.7 126.9) (xy 118.8 126.1)
        (xy 118.4 125.7) (xy 118 125.2) (xy 117.7 124.8) (xy 117.4 124.4) (xy 116.9 123.7)
        (xy 116.3 122.7) (xy 115.6 121) (xy 115.3 119.9) (xy 115.1 118.6) (xy 115.1 117.8)
        (xy 115.1 114.6) (xy 115.1 110.9) (xy 115.1 105.2) (xy 115.1 101.5) (xy 115.1 96.1)
        (xy 115.1 81.1) (xy 115.1 73.5) (xy 115.1 64.7) (xy 115.1 59.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 128.1 59.5) (xy 130.2 64.3) (xy 154 64.3) (xy 156.1 59.5) (xy 169 59.5)
        (xy 169 66.9) (xy 169 69.1) (xy 169 71.7) (xy 169 75.6) (xy 169 81.9)
        (xy 169 85.8) (xy 169 94.2) (xy 169 98.3) (xy 169 108.6) (xy 169 119.1)
        (xy 168.8 120.5) (xy 168 122.6) (xy 167.2 124) (xy 166 125.5) (xy 165.1 126.4)
        (xy 164.2 127.2) (xy 163.3 127.8) (xy 162.2 128.4) (xy 161.2 128.8) (xy 160.5 129.1)
        (xy 159.7 129.3) (xy 159.1 129.4) (xy 158.3 129.5) (xy 157.6 129.6) (xy 156.6 129.6)
        (xy 150.1 129.6) (xy 144 129.6) (xy 126.9 129.6) (xy 126.5 129.6) (xy 126.1 129.6)
        (xy 125.4 129.5) (xy 124.5 129.3) (xy 123.8 129.1) (xy 123.2 128.9) (xy 122.2 128.5)
        (xy 121.4 128) (xy 120.8 127.7) (xy 120.2 127.3) (xy 119.7 126.9) (xy 118.8 126.1)
        (xy 118.4 125.7) (xy 118 125.2) (xy 117.7 124.8) (xy 117.4 124.4) (xy 116.9 123.7)
        (xy 116.3 122.7) (xy 115.6 121) (xy 115.3 119.9) (xy 115.1 118.6) (xy 115.1 117.8)
        (xy 115.1 114.6) (xy 115.1 110.9) (xy 115.1 105.2) (xy 115.1 101.5) (xy 115.1 96.1)
        (xy 115.1 81.1) (xy 115.1 73.5) (xy 115.1 64.7) (xy 115.1 59.5)
      )
    )
  )
)
