<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="40.64" y1="21.59" x2="0" y2="21.59" width="0.254" layer="20"/>
<wire x1="0" y1="21.59" x2="0" y2="10.16" width="0.254" layer="20"/>
<wire x1="6.35" y1="0" x2="34.29" y2="0" width="0.254" layer="20"/>
<text>KD0GLS 2018</text>
<text>VRP</text>
<text>GND</text>
<text>S8</text>
<text>S7</text>
<text>S6</text>
<text>S5</text>
<text>S4</text>
<text>S3</text>
<text>S2</text>
<text>S1</text>
<wire x1="40.64" y1="10.16" x2="40.64" y2="21.59" width="0.254" layer="20"/>
<wire x1="0" y1="10.16" x2="6.35" y2="10.16" width="0.254" layer="20"/>
<wire x1="6.35" y1="10.16" x2="6.35" y2="0" width="0.254" layer="20"/>
<wire x1="40.64" y1="10.16" x2="34.29" y2="10.16" width="0.254" layer="20"/>
<wire x1="34.29" y1="10.16" x2="34.29" y2="0" width="0.254" layer="20"/>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="CONN_BREAKAWAY_1X10_100">
</package>
<package name="SWITCH_CK_PTS635">
<description>C&amp;K P/N PTS635SL50 LFS
Digi-Key P/N CKN9102-ND</description>
</package>
<package name="RESISTOR_PACK_SIP_10">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="kd0gls" package="CONN_BREAKAWAY_1X10_100" value="CONN_BREAKAWAY_1X10_100"/>
<element name="SW1" library="kd0gls" package="SWITCH_CK_PTS635" value="SWITCH_PUSHBUTTON"/>
<element name="SW2" library="kd0gls" package="SWITCH_CK_PTS635" value="SWITCH_PUSHBUTTON"/>
<element name="SW3" library="kd0gls" package="SWITCH_CK_PTS635" value="SWITCH_PUSHBUTTON"/>
<element name="SW4" library="kd0gls" package="SWITCH_CK_PTS635" value="SWITCH_PUSHBUTTON"/>
<element name="SW5" library="kd0gls" package="SWITCH_CK_PTS635" value="SWITCH_PUSHBUTTON"/>
<element name="SW6" library="kd0gls" package="SWITCH_CK_PTS635" value="SWITCH_PUSHBUTTON"/>
<element name="SW7" library="kd0gls" package="SWITCH_CK_PTS635" value="SWITCH_PUSHBUTTON"/>
<element name="SW8" library="kd0gls" package="SWITCH_CK_PTS635" value="SWITCH_PUSHBUTTON"/>
<element name="RP1" library="kd0gls" package="RESISTOR_PACK_SIP_10" value="10K"/>
</elements>
<signals>
<signal name="S1">
<contactref element="RP1" pad="9"/>
<contactref element="J1" pad="2"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="S2">
<contactref element="RP1" pad="8"/>
<contactref element="J1" pad="3"/>
<contactref element="SW2" pad="2"/>
</signal>
<signal name="S3">
<contactref element="RP1" pad="7"/>
<contactref element="J1" pad="4"/>
<contactref element="SW3" pad="2"/>
</signal>
<signal name="S4">
<contactref element="RP1" pad="6"/>
<contactref element="J1" pad="5"/>
<contactref element="SW4" pad="2"/>
</signal>
<signal name="S5">
<contactref element="RP1" pad="5"/>
<contactref element="J1" pad="6"/>
<contactref element="SW5" pad="2"/>
</signal>
<signal name="S6">
<contactref element="RP1" pad="4"/>
<contactref element="J1" pad="7"/>
<contactref element="SW6" pad="2"/>
</signal>
<signal name="S7">
<contactref element="RP1" pad="3"/>
<contactref element="J1" pad="8"/>
<contactref element="SW7" pad="2"/>
</signal>
<signal name="S8">
<contactref element="RP1" pad="2"/>
<contactref element="J1" pad="9"/>
<contactref element="SW8" pad="2"/>
</signal>
<signal name="COM">
<contactref element="SW1" pad="1"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW3" pad="1"/>
<contactref element="SW4" pad="1"/>
<contactref element="SW5" pad="1"/>
<contactref element="SW6" pad="1"/>
<contactref element="SW7" pad="1"/>
<contactref element="SW8" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="RP1" pad="1"/>
<contactref element="J1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
