(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 6)
    (zones 0)
    (modules 6)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(U5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(U5-Pad1)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Horizontal (layer F.Cu) (tedit 5E313B8D)
    (at 69.85 53.34 90)
    (descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 4.385 -2.27 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Male (at 4.385 9.89 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.77 3.81 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module comps:wireholes (layer F.Cu) (tedit 5E313B85)
    (at 69.85 57.785)
    (fp_text reference U1 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value A (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.0414 1.0414) (drill 0.508) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (module comps:wireholes (layer F.Cu) (tedit 5E313B83)
    (at 72.39 56.515)
    (fp_text reference U2 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value A (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.0414 1.0414) (drill 0.508) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
  )
  (module comps:wireholes (layer F.Cu) (tedit 5E313B7F)
    (at 74.93 56.515)
    (fp_text reference U3 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value A (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.0414 1.0414) (drill 0.508) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
  )
  (module comps:wireholes (layer F.Cu) (tedit 5E313B7C)
    (at 77.47 57.785)
    (fp_text reference U4 (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value A (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.0414 1.0414) (drill 0.508) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
  )
  (module comps:hole (layer F.Cu) (tedit 5E313B90)
    (at 73.66 60.325)
    (fp_text reference U5 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text value H (at 0 -5.08) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.175) (layers *.Cu *.Mask)
      (net 5 "Net-(U5-Pad1)"))
  )
  (gr_line (start 77.47 61.976) (end 79.121 61.976) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.199 61.976) (end 68.199 63.246) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 69.85 61.976) (end 68.199 61.976) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 69.85 60.96) (end 69.85 61.976) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.199 60.96) (end 69.85 60.96) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.121 61.976) (end 79.121 63.246) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.47 60.96) (end 77.47 61.976) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.121 60.96) (end 77.47 60.96) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.199 60.96) (end 68.199 48.895) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 79.121 63.246) (end 68.199 63.246) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 79.121 48.895) (end 79.121 60.96) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 68.199 48.895) (end 79.121 48.895) (layer Edge.Cuts) (width 0.2))
)
