(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 214)
    (no_connects 0)
    (area 66.424999 66.424999 131.575001 122.575001)
    (thickness 1.6)
    (drawings 24)
    (tracks 756)
    (zones 0)
    (modules 80)
    (nets 93)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 GND.Cu power hide)
    (2 PWR.Cu power hide)
    (31 B.Cu signal hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.127)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (user_via 0.762 0.508)
    (user_via 1.143 0.762)
    (uvia_size 0.4572)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 70 70)
    (grid_origin 68 69.5)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P2-Pad2)")
  (net 2 GND)
  (net 3 +5V)
  (net 4 Depth)
  (net 5 WaterTemp)
  (net 6 Flow)
  (net 7 "Net-(P3-Pad2)")
  (net 8 AirTemp)
  (net 9 "Net-(J2-Pad2)")
  (net 10 "Net-(J2-Pad1)")
  (net 11 "Net-(J3-Pad2)")
  (net 12 "Net-(J3-Pad1)")
  (net 13 "Net-(U1-Pad10)")
  (net 14 "Net-(U1-Pad2)")
  (net 15 "Net-(U1-Pad9)")
  (net 16 "Net-(U1-Pad7)")
  (net 17 "Net-(U2-Pad10)")
  (net 18 "Net-(U2-Pad2)")
  (net 19 "Net-(U2-Pad9)")
  (net 20 "Net-(U2-Pad7)")
  (net 21 "Net-(P5-Pad3)")
  (net 22 "Net-(P5-Pad5)")
  (net 23 "Net-(P5-Pad7)")
  (net 24 "Net-(P5-Pad11)")
  (net 25 "Net-(P5-Pad12)")
  (net 26 "Net-(P5-Pad13)")
  (net 27 "Net-(P5-Pad15)")
  (net 28 "Net-(P5-Pad16)")
  (net 29 "Net-(P5-Pad18)")
  (net 30 "Net-(P5-Pad19)")
  (net 31 "Net-(P5-Pad21)")
  (net 32 "Net-(P5-Pad22)")
  (net 33 "Net-(P5-Pad23)")
  (net 34 "Net-(P5-Pad24)")
  (net 35 "Net-(P5-Pad26)")
  (net 36 "Net-(P5-Pad27)")
  (net 37 "Net-(P5-Pad28)")
  (net 38 "Net-(P5-Pad29)")
  (net 39 "Net-(P5-Pad31)")
  (net 40 "Net-(P5-Pad32)")
  (net 41 "Net-(P5-Pad33)")
  (net 42 "Net-(P5-Pad35)")
  (net 43 "Net-(P5-Pad36)")
  (net 44 "Net-(P5-Pad37)")
  (net 45 "Net-(P5-Pad38)")
  (net 46 "Net-(P5-Pad40)")
  (net 47 "Net-(D1-Pad1)")
  (net 48 "Net-(U7-Pad2)")
  (net 49 "Net-(U7-Pad19)")
  (net 50 "Net-(U7-Pad22)")
  (net 51 "Net-(U7-Pad30)")
  (net 52 "Net-(U7-Pad31)")
  (net 53 "Net-(P7-Pad3)")
  (net 54 "Net-(C3-Pad1)")
  (net 55 "Net-(C4-Pad1)")
  (net 56 "Net-(C7-Pad1)")
  (net 57 "Net-(C11-Pad1)")
  (net 58 "Net-(C19-Pad1)")
  (net 59 "Net-(R1-Pad2)")
  (net 60 "Net-(R2-Pad2)")
  (net 61 "Net-(R3-Pad2)")
  (net 62 "Net-(R4-Pad2)")
  (net 63 +12V)
  (net 64 GND-pH)
  (net 65 3V3-pH)
  (net 66 GND-EC)
  (net 67 3V3-EC)
  (net 68 Motor1-out)
  (net 69 Motor2-out)
  (net 70 Motor3-out)
  (net 71 Motor4-out)
  (net 72 Light)
  (net 73 LightRelay)
  (net 74 WaterRelay)
  (net 75 Motor1)
  (net 76 Motor2)
  (net 77 Motor3)
  (net 78 Motor4)
  (net 79 Reset-5V)
  (net 80 SCL)
  (net 81 SDA)
  (net 82 Motor12-en)
  (net 83 Motor34-en)
  (net 84 RXD)
  (net 85 TXD)
  (net 86 +3V3)
  (net 87 "Net-(R11-Pad2)")
  (net 88 "Net-(D2-Pad1)")
  (net 89 "Net-(D3-Pad1)")
  (net 90 LED1)
  (net 91 "Net-(D4-Pad1)")
  (net 92 LED2)
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.4572)
    (uvia_drill 0.254)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net 3V3-EC)
    (add_net 3V3-pH)
    (add_net AirTemp)
    (add_net Depth)
    (add_net Flow)
    (add_net GND)
    (add_net GND-EC)
    (add_net GND-pH)
    (add_net LED1)
    (add_net LED2)
    (add_net Light)
    (add_net LightRelay)
    (add_net Motor1)
    (add_net Motor1-out)
    (add_net Motor12-en)
    (add_net Motor2)
    (add_net Motor2-out)
    (add_net Motor3)
    (add_net Motor3-out)
    (add_net Motor34-en)
    (add_net Motor4)
    (add_net Motor4-out)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P5-Pad11)")
    (add_net "Net-(P5-Pad12)")
    (add_net "Net-(P5-Pad13)")
    (add_net "Net-(P5-Pad15)")
    (add_net "Net-(P5-Pad16)")
    (add_net "Net-(P5-Pad18)")
    (add_net "Net-(P5-Pad19)")
    (add_net "Net-(P5-Pad21)")
    (add_net "Net-(P5-Pad22)")
    (add_net "Net-(P5-Pad23)")
    (add_net "Net-(P5-Pad24)")
    (add_net "Net-(P5-Pad26)")
    (add_net "Net-(P5-Pad27)")
    (add_net "Net-(P5-Pad28)")
    (add_net "Net-(P5-Pad29)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P5-Pad31)")
    (add_net "Net-(P5-Pad32)")
    (add_net "Net-(P5-Pad33)")
    (add_net "Net-(P5-Pad35)")
    (add_net "Net-(P5-Pad36)")
    (add_net "Net-(P5-Pad37)")
    (add_net "Net-(P5-Pad38)")
    (add_net "Net-(P5-Pad40)")
    (add_net "Net-(P5-Pad5)")
    (add_net "Net-(P5-Pad7)")
    (add_net "Net-(P7-Pad3)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U7-Pad19)")
    (add_net "Net-(U7-Pad2)")
    (add_net "Net-(U7-Pad22)")
    (add_net "Net-(U7-Pad30)")
    (add_net "Net-(U7-Pad31)")
    (add_net RXD)
    (add_net Reset-5V)
    (add_net SCL)
    (add_net SDA)
    (add_net TXD)
    (add_net WaterRelay)
    (add_net WaterTemp)
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 5C5AA197)
    (at 70 70)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference MK1 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 5C5AA1D8)
    (at 70 119)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference MK2 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 5C5AA1BC)
    (at 128 70)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference MK3 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 5C5AA1CC)
    (at 128 119)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference MK4 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module CloudHydroponics:CUI_PJ-102A (layer F.Cu) (tedit 5C623370)
    (at 78.25 120.5 270)
    (fp_text reference J1 (at -5.4 5.85 270) (layer F.SilkS) hide)
    (fp_text value PJ-102A (at -4.01634 5.77692 270) (layer F.SilkS) hide)
    (fp_line (start -2.7 -4.2) (end -4.3 -4.2) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -2.7 -5.2) (end -2.7 -4.2) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -4.3 -5.2) (end -2.7 -5.2) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -4.3 -4.2) (end -4.3 -5.2) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start 0 -0.8) (end 0 0.8) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -1 -0.8) (end 0 -0.8) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -1 0.8) (end -1 -0.8) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start 0 0.8) (end -1 0.8) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -6 -0.8) (end -6 0.8) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -7 -0.8) (end -6 -0.8) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -7 0.8) (end -7 -0.8) (layer Edge.Cuts) (width 0.0001))
    (fp_line (start -6 0.8) (end -7 0.8) (layer Edge.Cuts) (width 0.0001))
    (pad 3 thru_hole oval (at -3.5 -4.7 90) (size 3.016 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at -0.5 0) (size 3.016 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole oval (at -6.5 0) (size 3.016 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 63 +12V))
  )
  (module CloudHydroponics:TE_1-1634612-0 (layer F.Cu) (tedit 5C61FA72)
    (at 102 115 270)
    (fp_text reference J2 (at 1.9 8.6 270) (layer F.SilkS) hide)
    (fp_text value 1-1634612-0 (at 2.1787 8.62968 270) (layer F.SilkS) hide)
    (pad S2 thru_hole circle (at 5.08 5.08 180) (size 3.015 3.015) (drill 2.01) (layers *.Cu *.Mask))
    (pad S1 thru_hole circle (at 5.08 -5.08 180) (size 3.015 3.015) (drill 2.01) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad1)"))
  )
  (module CloudHydroponics:TE_1-1634612-0 (layer F.Cu) (tedit 5C61FABE)
    (at 117.5 115 270)
    (fp_text reference J3 (at 0.4 -8.7 270) (layer F.SilkS) hide)
    (fp_text value 1-1634612-0 (at 2.1787 8.62968 270) (layer F.SilkS) hide)
    (pad S2 thru_hole circle (at 5.08 5.08 180) (size 3.015 3.015) (drill 2.01) (layers *.Cu *.Mask))
    (pad S1 thru_hole circle (at 5.08 -5.08 180) (size 3.015 3.015) (drill 2.01) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad1)"))
  )
  (module CloudHydroponics:Atlas (layer F.Cu) (tedit 5C62333F)
    (at 99.75 104.75 90)
    (descr "Atlas Scientific Pads")
    (tags "HDR DIL")
    (attr smd)
    (fp_text reference U1 (at -8.2 -5.85 270) (layer F.SilkS))
    (fp_text value ph-SM (at -0.55 6.55 270) (layer F.SilkS))
    (fp_text user ○ (at -7.95 -4.9 90) (layer F.SilkS))
    (pad 1 smd rect (at -6 -4.6 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R1-Pad2)"))
    (pad 10 smd rect (at 6 -4.6 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad10)"))
    (pad 2 smd rect (at -6 -2.3 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad2)"))
    (pad 9 smd rect (at 6 -2.3 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad9)"))
    (pad 3 smd rect (at -6 0 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 65 3V3-pH))
    (pad 8 smd rect (at 6 0 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R3-Pad2)"))
    (pad 4 smd rect (at -6 2.3 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad1)"))
    (pad 7 smd rect (at 6 2.3 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad7)"))
    (pad 5 smd rect (at -6 4.6 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad2)"))
    (pad 6 smd rect (at 6 4.6 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 64 GND-pH))
    (model Atlas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module CloudHydroponics:Atlas (layer F.Cu) (tedit 5C623323)
    (at 115.25 104.75 90)
    (descr "Atlas Scientific Pads")
    (tags "HDR DIL")
    (attr smd)
    (fp_text reference U2 (at -8.25 -5.6 270) (layer F.SilkS))
    (fp_text value EC-SM (at -0.65 6.55 270) (layer F.SilkS))
    (fp_text user ○ (at -8 -4.6 90) (layer F.SilkS))
    (pad 1 smd rect (at -6 -4.6 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(R2-Pad2)"))
    (pad 10 smd rect (at 6 -4.6 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad10)"))
    (pad 2 smd rect (at -6 -2.3 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad2)"))
    (pad 9 smd rect (at 6 -2.3 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad9)"))
    (pad 3 smd rect (at -6 0 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 67 3V3-EC))
    (pad 8 smd rect (at 6 0 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R4-Pad2)"))
    (pad 4 smd rect (at -6 2.3 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J3-Pad1)"))
    (pad 7 smd rect (at 6 2.3 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad7)"))
    (pad 5 smd rect (at -6 4.6 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad2)"))
    (pad 6 smd rect (at 6 4.6 90) (size 2.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 66 GND-EC))
    (model Atlas.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module CloudHydroponics:SI8600AC-B-IS (layer B.Cu) (tedit 5C623044)
    (at 105.05 100.3 180)
    (fp_text reference U3 (at -4.5 3.5 180) (layer B.SilkS))
    (fp_text value SI8600AC-B-IS (at 0 0 180) (layer B.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 180) (layer Cmts.User))
    (fp_text user * (at -4.35 1.6 180) (layer B.SilkS))
    (fp_text user * (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (pad 2 smd oval (at -2.7 0.635 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 81 SDA))
    (pad 3 smd oval (at -2.7 -0.635 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 80 SCL))
    (pad 4 smd oval (at -2.7 -1.905 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd oval (at 2.7 -1.905 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 64 GND-pH))
    (pad 6 smd oval (at 2.7 -0.635 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R3-Pad2)"))
    (pad 7 smd oval (at 2.7 0.635 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R1-Pad2)"))
    (pad 8 smd oval (at 2.7 1.905 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 65 3V3-pH))
  )
  (module CloudHydroponics:SI8600AC-B-IS (layer B.Cu) (tedit 5C62324A)
    (at 110.45 107.45)
    (fp_text reference U4 (at -5.7 2.15) (layer B.SilkS))
    (fp_text value SI8600AC-B-IS (at 0 0) (layer B.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at -4.35 2.15) (layer B.SilkS))
    (fp_text user * (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (pad 2 smd oval (at -2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 81 SDA))
    (pad 3 smd oval (at -2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 80 SCL))
    (pad 4 smd oval (at -2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd oval (at 2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 66 GND-EC))
    (pad 6 smd oval (at 2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(R4-Pad2)"))
    (pad 7 smd oval (at 2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(R2-Pad2)"))
    (pad 8 smd oval (at 2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 3V3-EC))
  )
  (module CloudHydroponics:AP1509-50SG-13 (layer F.Cu) (tedit 5C623818)
    (at 87 94.75 90)
    (fp_text reference U5 (at -5.45 -0.55 90) (layer F.SilkS))
    (fp_text value AP1509-50SG-13 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at -4.05 -1.75 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 63 +12V))
    (pad 2 smd oval (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D1-Pad1)"))
    (pad 3 smd oval (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 4 smd oval (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd oval (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd oval (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd oval (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd oval (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module CloudHydroponics:CONV_RM-0505S (layer F.Cu) (tedit 5C621787)
    (at 115.1 91.8 180)
    (fp_text reference PS2 (at -6.7 -2.3 270) (layer F.SilkS))
    (fp_text value RM-0505S (at -3.175 2.286 180) (layer F.SilkS) hide)
    (pad 4 thru_hole circle (at 3.81 0 180) (size 1.228 1.228) (drill 0.72) (layers *.Cu *.Mask)
      (net 57 "Net-(C11-Pad1)"))
    (pad 1 thru_hole rect (at -3.81 0 180) (size 1.228 1.228) (drill 0.72) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 1.27 0 180) (size 1.228 1.228) (drill 0.72) (layers *.Cu *.Mask)
      (net 66 GND-EC))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1.228 1.228) (drill 0.72) (layers *.Cu *.Mask)
      (net 3 +5V))
  )
  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 5C62335D)
    (at 88.5 117.75 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (attr smd)
    (fp_text reference C1 (at -3.75 4.2 270) (layer F.SilkS))
    (fp_text value "220uF 35V" (at 0 -4.43 270) (layer F.Fab) hide)
    (fp_text user + (at -1.73 -0.08 270) (layer F.Fab))
    (fp_text user + (at -4.3 2.2 270) (layer F.SilkS))
    (fp_text user %R (at 0 4.43 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 63 +12V))
    (pad 2 smd rect (at 2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 5C623352)
    (at 90 104.75 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x7.7")
    (attr smd)
    (fp_text reference C2 (at -4.35 -2.5 360) (layer F.SilkS))
    (fp_text value "470uF 10V" (at 0 -4.43 270) (layer F.Fab) hide)
    (fp_text user + (at -1.73 -0.08 270) (layer F.Fab))
    (fp_text user + (at -4.3 2.1 270) (layer F.SilkS))
    (fp_text user %R (at 0 4.43 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module CloudHydroponics:ATMEGA328P-AUR (layer F.Cu) (tedit 5C624A5C)
    (at 83.3 80.6)
    (fp_text reference U7 (at -0.15 6.2 180) (layer F.SilkS))
    (fp_text value ATMEGA328P-AUR (at 0 0) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at -5.8 -2.5) (layer F.SilkS))
    (fp_text user * (at -2.9972 -2.819) (layer F.Fab))
    (pad 1 smd rect (at -4.2418 -2.799999 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 74 WaterRelay))
    (pad 2 smd rect (at -4.2418 -2.000001 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U7-Pad2)"))
    (pad 3 smd rect (at -4.2418 -1.2 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.2418 -0.399999 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 5 smd rect (at -4.2418 0.399999 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.2418 1.2 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 7 smd rect (at -4.2418 1.999999 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C3-Pad1)"))
    (pad 8 smd rect (at -4.2418 2.799999 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C4-Pad1)"))
    (pad 9 smd rect (at -2.799999 4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 92 LED2))
    (pad 10 smd rect (at -2.000001 4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 82 Motor12-en))
    (pad 11 smd rect (at -1.2 4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 83 Motor34-en))
    (pad 12 smd rect (at -0.399999 4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 5 WaterTemp))
    (pad 13 smd rect (at 0.399999 4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 90 LED1))
    (pad 14 smd rect (at 1.2 4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 78 Motor4))
    (pad 15 smd rect (at 1.999999 4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 77 Motor3))
    (pad 16 smd rect (at 2.799999 4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 76 Motor2))
    (pad 17 smd rect (at 4.2418 2.799999 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 75 Motor1))
    (pad 18 smd rect (at 4.2418 2.000001 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 19 smd rect (at 4.2418 1.2 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U7-Pad19)"))
    (pad 20 smd rect (at 4.2418 0.399999 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C19-Pad1)"))
    (pad 21 smd rect (at 4.2418 -0.399999 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.2418 -1.2 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U7-Pad22)"))
    (pad 23 smd rect (at 4.2418 -1.999999 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 6 Flow))
    (pad 24 smd rect (at 4.2418 -2.799999 90) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 4 Depth))
    (pad 25 smd rect (at 2.799999 -4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 72 Light))
    (pad 26 smd rect (at 2.000001 -4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 8 AirTemp))
    (pad 27 smd rect (at 1.2 -4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 81 SDA))
    (pad 28 smd rect (at 0.399999 -4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 80 SCL))
    (pad 29 smd rect (at -0.399999 -4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 79 Reset-5V))
    (pad 30 smd rect (at -1.2 -4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U7-Pad30)"))
    (pad 31 smd rect (at -1.999999 -4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U7-Pad31)"))
    (pad 32 smd rect (at -2.799999 -4.2418) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 73 LightRelay))
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5C61F9F6)
    (at 98.2 85.7 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P6 (at 1.27 -2.33 180) (layer F.SilkS) hide)
    (fp_text value ISP (at 1.27 7.41 180) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 Motor2))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 Motor1))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 Motor3))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 Reset-5V))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CloudHydroponics:NLSX4373DR2G (layer F.Cu) (tedit 5C621724)
    (at 96.3 75.9)
    (fp_text reference U8 (at -5.55 -1.9) (layer F.SilkS))
    (fp_text value NLSX4373 (at 0 0) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at -4.2 -1.65) (layer F.SilkS))
    (fp_text user * (at -1.5748 -2.3749) (layer F.Fab))
    (pad 1 smd rect (at -2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at -2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U7-Pad31)"))
    (pad 3 smd rect (at -2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U7-Pad30)"))
    (pad 4 smd rect (at -2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(R11-Pad2)"))
    (pad 6 smd rect (at 2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 84 RXD))
    (pad 7 smd rect (at 2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 85 TXD))
    (pad 8 smd rect (at 2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 86 +3V3))
  )
  (module CloudHydroponics:XTAL_ECS-160-18-30B-AGN-TR (layer F.Cu) (tedit 5C624B8E)
    (at 75.5 82.9 270)
    (attr smd)
    (fp_text reference Y1 (at -0.1 2.85 270) (layer F.SilkS))
    (fp_text value "16.0 MHz" (at -0.769903 2.56059 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.85 1.1 90) (size 1.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.85 1.1 90) (size 1.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.85 -1.1 90) (size 1.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C4-Pad1)"))
    (pad 4 smd rect (at -1.85 -1.1 90) (size 1.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module CloudHydroponics:MCP1754ST-3302E_CB (layer B.Cu) (tedit 5C61FD4D)
    (at 95.85 97.8 270)
    (fp_text reference U9 (at 3 -0.2 270) (layer B.SilkS))
    (fp_text value MCP1754ST-3302E/CB (at 0 0 270) (layer B.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 270) (layer Cmts.User))
    (fp_text user * (at 0 0 270) (layer B.SilkS))
    (fp_text user * (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.950001 -1.1952 270) (size 0.5588 1.3208) (layers B.Cu B.Paste B.Mask)
      (net 64 GND-pH))
    (pad 2 smd rect (at 0.950001 -1.1952 270) (size 0.5588 1.3208) (layers B.Cu B.Paste B.Mask)
      (net 65 3V3-pH))
    (pad 3 smd rect (at 0 1.1952 270) (size 0.5588 1.3208) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C7-Pad1)"))
  )
  (module CloudHydroponics:MCP1754ST-3302E_CB (layer B.Cu) (tedit 5C61FCF3)
    (at 111.7 98.8 180)
    (fp_text reference U10 (at -3.6 -0.1 180) (layer B.SilkS))
    (fp_text value MCP1754ST-3302E/CB (at 0 0 180) (layer B.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 180) (layer Cmts.User))
    (fp_text user * (at 0 0 180) (layer B.SilkS))
    (fp_text user * (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.950001 -1.1952 180) (size 0.5588 1.3208) (layers B.Cu B.Paste B.Mask)
      (net 66 GND-EC))
    (pad 2 smd rect (at 0.950001 -1.1952 180) (size 0.5588 1.3208) (layers B.Cu B.Paste B.Mask)
      (net 67 3V3-EC))
    (pad 3 smd rect (at 0 1.1952 180) (size 0.5588 1.3208) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(C11-Pad1)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5C650ADE)
    (at 75.3 79.1)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.25 0.05) (layer F.SilkS))
    (fp_text value "18 pF" (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5C5DC034)
    (at 75.5 86.7 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value "18 pF" (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C4-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5C61FB18)
    (at 91 96.9 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 2.6 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5C61FB10)
    (at 92.4 96.9 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2.65 0.05 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C61FD3D)
    (at 97.2 93.4)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -2.65 -0.05) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.5) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 64 GND-pH))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C7-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C61FD45)
    (at 97.2 94.8)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -2.55 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 64 GND-pH))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(C7-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C61FD57)
    (at 98.9 97.65 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -2.6 0.1 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 64 GND-pH))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 65 3V3-pH))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C61FD5F)
    (at 100.35 97.65 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at -3.1 0.1 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 64 GND-pH))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 65 3V3-pH))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C61FCBE)
    (at 112.45 93.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -3.05 0) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 66 GND-EC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(C11-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C62302F)
    (at 112.45 95.15)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -2.8 -0.1) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 66 GND-EC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(C11-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C61FCFD)
    (at 111.95 102)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 3.35 -0.15) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 66 GND-EC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 67 3V3-EC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C61FD06)
    (at 111.95 103.55)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 3.3 0.05) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 66 GND-EC))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 67 3V3-EC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5C624A84)
    (at 78.8 86.3 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0.85 1.2 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 88 86.3 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5C632585)
    (at 78.7 75.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 0.75 -1.4 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5C621680)
    (at 88.1 75.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at -0.1 1.35 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5C62397F)
    (at 90 82.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at -2.95 -0.15 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C19-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C61FD2B)
    (at 102.2 93.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 3.25 0) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C61FCCE)
    (at 117.7 93.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 3.15 0) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 96.25 113.3 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 65 3V3-pH))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 111.4 113.25 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 67 3V3-EC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5C622FFC)
    (at 103.45 95.55)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.3 -0.15) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 65 3V3-pH))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5C62325C)
    (at 115.25 95.35 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.25 -1.65 270) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 67 3V3-EC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C61FBB5)
    (at 81.9 73.9)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.9 0.1 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C61FBF4)
    (at 85.85 73.9 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 1.9 0.05 270) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5C623298)
    (at 115.3 75.8)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -2.65 0.05) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 WaterTemp))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 125.85 86.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 1.45) (layer B.SilkS))
    (fp_text value 4.7K (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 72 Light))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C61F9AD)
    (at 89.35 88.95 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0.1 1.4 270) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(P5-Pad12)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C61FB31)
    (at 95.75 89.15 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -3.05 0.05 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 Reset-5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CloudHydroponics:SOT-23 (layer F.Cu) (tedit 5C61D537)
    (at 92.15 89.15)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value DMN60H080DS (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(P5-Pad12)"))
    (pad 3 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 79 Reset-5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C61EA2B)
    (at 102.8 74.75 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -3.1 0 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CloudHydroponics:Grove_1x04 (layer F.Cu) (tedit 5C61EBE1)
    (at 105.75 78.5)
    (descr https://statics3.seeedstudio.com/images/opl/datasheet/3470130P1.pdf)
    (tags Grove-1x04)
    (fp_text reference P1 (at -1.5 -4) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 4.19 2.83 90) (layer F.Fab) hide)
    (fp_text user 1 (at -1.775 0.075) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 2) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 3 thru_hole circle (at 0 4) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 Depth))
    (pad 4 thru_hole circle (at 0 6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 Depth))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Grove_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 -90))
    )
  )
  (module CloudHydroponics:Grove_1x04 (layer F.Cu) (tedit 5C61EE41)
    (at 117.25 78.5 270)
    (descr https://statics3.seeedstudio.com/images/opl/datasheet/3470130P1.pdf)
    (tags Grove-1x04)
    (fp_text reference P2 (at -1.5 -4 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 4.19 2.83 360) (layer F.Fab) hide)
    (fp_text user 1 (at -1.775 0.075 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 WaterTemp))
    (pad 2 thru_hole circle (at 0 2 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P2-Pad2)"))
    (pad 3 thru_hole circle (at 0 4 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 4 thru_hole circle (at 0 6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Grove_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 -90))
    )
  )
  (module CloudHydroponics:Grove_1x04 (layer F.Cu) (tedit 5C61EE63)
    (at 128.7 78.5 270)
    (descr https://statics3.seeedstudio.com/images/opl/datasheet/3470130P1.pdf)
    (tags Grove-1x04)
    (fp_text reference P3 (at -1.5 -4 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 4.19 2.83 360) (layer F.Fab) hide)
    (fp_text user 1 (at -1.775 0.075 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 Flow))
    (pad 2 thru_hole circle (at 0 2 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P3-Pad2)"))
    (pad 3 thru_hole circle (at 0 4 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 4 thru_hole circle (at 0 6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Grove_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 -90))
    )
  )
  (module CloudHydroponics:Grove_1x04 (layer F.Cu) (tedit 5C61EE49)
    (at 111.2 84 90)
    (descr https://statics3.seeedstudio.com/images/opl/datasheet/3470130P1.pdf)
    (tags Grove-1x04)
    (fp_text reference P4 (at -1.5 -4 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 4.19 2.83 180) (layer F.Fab) hide)
    (fp_text user 1 (at -1.775 0.075 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 0 2 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 8 AirTemp))
    (pad 3 thru_hole circle (at 0 4 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole circle (at 0 6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Grove_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 -90))
    )
  )
  (module CloudHydroponics:Grove_1x04 (layer F.Cu) (tedit 5C61EE56)
    (at 122.7 84 90)
    (descr https://statics3.seeedstudio.com/images/opl/datasheet/3470130P1.pdf)
    (tags Grove-1x04)
    (fp_text reference P7 (at -1.5 -4 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 4.19 2.83 180) (layer F.Fab) hide)
    (fp_text user 1 (at -1.775 0.075 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 72 Light))
    (pad 2 thru_hole circle (at 0 2 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 3 thru_hole circle (at 0 4 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(P7-Pad3)"))
    (pad 4 thru_hole circle (at 0 6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Grove_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 -90))
    )
  )
  (module CloudHydroponics:Grove_1x04 (layer F.Cu) (tedit 5C61FAEE)
    (at 126.1 98.3 180)
    (descr https://statics3.seeedstudio.com/images/opl/datasheet/3470130P1.pdf)
    (tags Grove-1x04)
    (fp_text reference P8 (at -1.5 -4 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 4.19 2.83 270) (layer F.Fab) hide)
    (fp_text user 1 (at -1.775 0.075 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 73 LightRelay))
    (pad 2 thru_hole circle (at 0 2 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 4 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole circle (at 0 6 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Grove_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 -90))
    )
  )
  (module CloudHydroponics:Grove_1x04 (layer F.Cu) (tedit 5C61FAE3)
    (at 126.1 109.8 180)
    (descr https://statics3.seeedstudio.com/images/opl/datasheet/3470130P1.pdf)
    (tags Grove-1x04)
    (fp_text reference P9 (at -1.5 -4 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 4.19 2.83 270) (layer F.Fab) hide)
    (fp_text user 1 (at -1.775 0.075 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 74 WaterRelay))
    (pad 2 thru_hole circle (at 0 2 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 4 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole circle (at 0 6 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Grove_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C621542)
    (at 80.45 87)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at 0.05 -1.55) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 63 +12V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C62153B)
    (at 85.4 102.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C23 (at -0.2 -1.75 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5C623034)
    (at 107 96.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at 0 -1.25) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 107.25 111.1)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C25 (at 0 1.5) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CloudHydroponics:CONV_RM-0505S (layer F.Cu) (tedit 5C6232EC)
    (at 99.8 91.8 180)
    (fp_text reference PS1 (at -4.05 2.35 180) (layer F.SilkS))
    (fp_text value RM-0505S (at -3.175 2.286 180) (layer F.SilkS) hide)
    (pad 4 thru_hole circle (at 3.81 0 180) (size 1.228 1.228) (drill 0.72) (layers *.Cu *.Mask)
      (net 56 "Net-(C7-Pad1)"))
    (pad 1 thru_hole rect (at -3.81 0 180) (size 1.228 1.228) (drill 0.72) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 1.27 0 180) (size 1.228 1.228) (drill 0.72) (layers *.Cu *.Mask)
      (net 64 GND-pH))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1.228 1.228) (drill 0.72) (layers *.Cu *.Mask)
      (net 3 +5V))
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm (layer F.Cu) (tedit 5C6233EC)
    (at 74.8 71.4 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference P5 (at 1.27 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_02X20 (at 1.27 50.59 90) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P5-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P5-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P5-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 RXD))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 TXD))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P5-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P5-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P5-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(P5-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(P5-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 +3V3))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P5-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P5-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P5-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P5-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(P5-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P5-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P5-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(P5-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(P5-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P5-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(P5-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(P5-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(P5-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(P5-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(P5-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(P5-Pad37)"))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(P5-Pad38)"))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(P5-Pad40)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CloudHydroponics:2106091-1 (layer B.Cu) (tedit 5C6237CE)
    (at 73.25 111.5 270)
    (fp_text reference J4 (at -0.75 0 270) (layer F.SilkS) hide)
    (fp_text value 2106091-1 (at -0.75 0 270) (layer B.SilkS) hide)
    (fp_line (start -3.75412 1.73736) (end -3.75412 6.70052) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 2.25044 1.73736) (end -3.75412 1.73736) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 2.25044 6.73608) (end 2.25044 1.73736) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -3.75412 6.73608) (end 2.25044 6.73608) (layer Edge.Cuts) (width 0.15))
    (fp_text user * (at 0 0 270) (layer B.Fab))
    (fp_text user * (at -1.5 -1.95 270) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 270) (layer Cmts.User) hide)
    (pad 8 smd rect (at 3.3394 4.2418 270) (size 0.9906 3.2512) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -4.8394 4.2418 270) (size 0.9906 3.2512) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.000001 0 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 68 Motor1-out))
    (pad 1 smd rect (at -1.500001 0 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module CloudHydroponics:2106091-1 (layer B.Cu) (tedit 5C6237B4)
    (at 73.25 100.85 270)
    (fp_text reference J5 (at -0.75 0 270) (layer F.SilkS) hide)
    (fp_text value 2106091-1 (at -0.75 0 270) (layer B.SilkS) hide)
    (fp_line (start -3.75412 1.73736) (end -3.75412 6.70052) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 2.25044 1.73736) (end -3.75412 1.73736) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 2.25044 6.73608) (end 2.25044 1.73736) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -3.75412 6.73608) (end 2.25044 6.73608) (layer Edge.Cuts) (width 0.15))
    (fp_text user * (at 0 0 270) (layer B.Fab))
    (fp_text user * (at -1.5 -1.8 270) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 270) (layer Cmts.User) hide)
    (pad 8 smd rect (at 3.3394 4.2418 270) (size 0.9906 3.2512) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -4.8394 4.2418 270) (size 0.9906 3.2512) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.000001 0 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 69 Motor2-out))
    (pad 1 smd rect (at -1.500001 0 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module CloudHydroponics:2106091-1 (layer B.Cu) (tedit 5C6237BF)
    (at 73.25 90.2 270)
    (fp_text reference J6 (at -0.75 0 270) (layer F.SilkS) hide)
    (fp_text value 2106091-1 (at -0.75 0 270) (layer B.SilkS) hide)
    (fp_line (start -3.75412 1.73736) (end -3.75412 6.70052) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 2.25044 1.73736) (end -3.75412 1.73736) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 2.25044 6.73608) (end 2.25044 1.73736) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -3.75412 6.73608) (end 2.25044 6.73608) (layer Edge.Cuts) (width 0.15))
    (fp_text user * (at 0 0 270) (layer B.Fab))
    (fp_text user * (at -1.55 -1.75 270) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 270) (layer Cmts.User) hide)
    (pad 8 smd rect (at 3.3394 4.2418 270) (size 0.9906 3.2512) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -4.8394 4.2418 270) (size 0.9906 3.2512) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.000001 0 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 70 Motor3-out))
    (pad 1 smd rect (at -1.500001 0 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module CloudHydroponics:2106091-1 (layer B.Cu) (tedit 5C62379B)
    (at 73.25 79.5 270)
    (fp_text reference J7 (at -0.75 0 270) (layer F.SilkS) hide)
    (fp_text value 2106091-1 (at -0.75 0 270) (layer B.SilkS) hide)
    (fp_line (start -3.75412 1.73736) (end -3.75412 6.70052) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 2.25044 1.73736) (end -3.75412 1.73736) (layer Edge.Cuts) (width 0.15))
    (fp_line (start 2.25044 6.73608) (end 2.25044 1.73736) (layer Edge.Cuts) (width 0.15))
    (fp_line (start -3.75412 6.73608) (end 2.25044 6.73608) (layer Edge.Cuts) (width 0.15))
    (fp_text user * (at 0 0 270) (layer B.Fab))
    (fp_text user * (at -1.45 -1.95 270) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 270) (layer Cmts.User) hide)
    (pad 8 smd rect (at 3.3394 4.2418 270) (size 0.9906 3.2512) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -4.8394 4.2418 270) (size 0.9906 3.2512) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0.000001 0 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 71 Motor4-out))
    (pad 1 smd rect (at -1.500001 0 270) (size 0.8128 1.4986) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module CloudHydroponics:L293DD (layer B.Cu) (tedit 5C6238AA)
    (at 82.25 94.75)
    (fp_text reference U6 (at -4.6 8) (layer B.SilkS))
    (fp_text value L293DD (at 0 0) (layer B.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at -6.45 6) (layer B.SilkS))
    (fp_text user * (at -6.45 6) (layer B.Fab))
    (pad 1 smd rect (at -4.6863 5.715) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 82 Motor12-en))
    (pad 2 smd rect (at -4.6863 4.445) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 75 Motor1))
    (pad 3 smd rect (at -4.6863 3.175) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 68 Motor1-out))
    (pad 4 smd rect (at -4.6863 1.905) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -4.6863 0.635) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.6863 -0.635) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -4.6863 -1.905) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -4.6863 -3.175) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 69 Motor2-out))
    (pad 9 smd rect (at -4.6863 -4.445) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 76 Motor2))
    (pad 10 smd rect (at -4.6863 -5.715) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 63 +12V))
    (pad 11 smd rect (at 4.6863 -5.715) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 83 Motor34-en))
    (pad 12 smd rect (at 4.6863 -4.445) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 77 Motor3))
    (pad 13 smd rect (at 4.6863 -3.175) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 70 Motor3-out))
    (pad 14 smd rect (at 4.6863 -1.905) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 15 smd rect (at 4.6863 -0.635) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 16 smd rect (at 4.6863 0.635) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 4.6863 1.905) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 18 smd rect (at 4.6863 3.175) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 71 Motor4-out))
    (pad 19 smd rect (at 4.6863 4.445) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 78 Motor4))
    (pad 20 smd rect (at 4.6863 5.715) (size 1.9812 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 3 +5V))
  )
  (module CloudHydroponics:Wurth_7447 (layer F.Cu) (tedit 5C650A8F)
    (at 79 105.75)
    (fp_text reference L1 (at 7.4 5.25 180) (layer F.SilkS))
    (fp_text value "47uH 3A" (at 0 4.6) (layer F.Fab))
    (pad 2 smd rect (at 4.95 0) (size 2.9 5.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -4.95 0) (size 2.9 5.4) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D1-Pad1)"))
  )
  (module CloudHydroponics:D_SMC (layer F.Cu) (tedit 5C624B2B)
    (at 77.45 95.35)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D1 (at -5.7 -3.2 90) (layer F.SilkS))
    (fp_text value B340 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.9) (layer F.Fab))
    (pad 1 smd rect (at -3.4 0 90) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 3.4 0 90) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C650AA8)
    (at 90.8 112.05)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 1.1 -1.25) (layer F.SilkS))
    (fp_text value 470 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C650B0E)
    (at 72.85 75.1 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 2.3 -0.05 270) (layer F.SilkS))
    (fp_text value 470 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5C650B32)
    (at 74.35 75.1 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 2.4 0 270) (layer F.SilkS))
    (fp_text value 470 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CloudHydroponics:D_0603 (layer F.Cu) (tedit 5C650B88)
    (at 75.8 75.05 270)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D4 (at 2.05 0.1 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.4 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.4 270) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.85 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 92 LED2))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CloudHydroponics:D_0603 (layer F.Cu) (tedit 5C650B7E)
    (at 77.25 75.1 270)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D3 (at 2 0.35 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.4 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.4 270) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.85 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 90 LED1))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CloudHydroponics:D_0603 (layer F.Cu) (tedit 5C632B6F)
    (at 72.75 113.9 90)
    (descr "Diode SMD in 0603 package http://datasheets.avx.com/schottky.pdf")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D2 (at 0 -1.4 90) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.4 90) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.85 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5C650070)
    (at 83.15 96.7 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at 3.15 0.15 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 63 +12V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5C650A87)
    (at 87.9 110.45 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C27 (at -0.55 1.15 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 63 +12V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Intelligent EDGE Hydroponics" (at 107.65 100.45 90) (layer F.SilkS))
  (gr_text ISP (at 93 83.2 90) (layer F.SilkS))
  (gr_text EC (at 126.15 114.9 90) (layer F.SilkS))
  (gr_text pH (at 93.3 119.4 90) (layer F.SilkS))
  (gr_text Motor4 (at 69.45 74.85) (layer F.SilkS))
  (gr_text Motor3 (at 69.35 85.65) (layer F.SilkS))
  (gr_text Motor2 (at 69.4 96.3) (layer F.SilkS))
  (gr_text Motor1 (at 69.45 106.9) (layer F.SilkS))
  (gr_text 12VDC (at 69.35 115.1) (layer F.SilkS))
  (gr_text WaterRelay (at 130 106.7 90) (layer F.SilkS))
  (gr_text LightRelay (at 130.15 95.5 90) (layer F.SilkS))
  (gr_text Light (at 125.8 87.85) (layer F.SilkS))
  (gr_text AirTemp (at 114.5 87.95) (layer F.SilkS))
  (gr_text Flow (at 125.45 74.5) (layer F.SilkS))
  (gr_text WaterTemp (at 114.4 74.45) (layer F.SilkS))
  (gr_text Depth (at 101.7 81.35 90) (layer F.SilkS))
  (gr_arc (start 70 119) (end 70 122.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128 119) (end 131.5 119) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128 70) (end 128 66.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 70 70) (end 66.5 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70 122.5) (end 128 122.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.5 70) (end 131.5 119) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70 66.5) (end 128 66.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 66.5 119) (end 66.5 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer GND.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61.8 64.5) (xy 135.6 64.5) (xy 135.6 113) (xy 123.9 113) (xy 123.9 93.4)
        (xy 117.5 93.4) (xy 117.5 89.6) (xy 108.95 89.6) (xy 108.95 113.25) (xy 106.75 113.25)
        (xy 106.75 93.4) (xy 102.2 93.4) (xy 102.2 89.7) (xy 93.5 89.7) (xy 93.4 126.6)
        (xy 61.4 126.3) (xy 61.4 64.5) (xy 61.7 64.5) (xy 61.9 64.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.1 87.45) (xy 94.1 96.7) (xy 89.3 96.7) (xy 89.3 97.4) (xy 88.6 97.4)
        (xy 88.6 95.9) (xy 80 95.85) (xy 80 93.2) (xy 75.95 93.2) (xy 80 87.45)
      )
    )
  )
  (zone (net 3) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.7 104.6) (xy 87 104.6) (xy 87 109.3) (xy 83.7 109.3) (xy 83.7 102.1)
        (xy 87.3 102.1) (xy 87.3 97.3) (xy 88 97.3) (xy 88 98.8) (xy 90.5 98.8)
        (xy 90.5 97.7) (xy 92.7 97.7)
      )
    )
  )
  (zone (net 47) (net_name "Net-(D1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.6 98.6) (xy 85.9 98.7) (xy 85.9 97.6) (xy 86.7 97.6) (xy 86.7 101.4)
        (xy 79.5 101.4) (xy 79.5 106.8) (xy 72.2 106.8) (xy 72.2 94.4) (xy 77.6 94.4)
      )
    )
  )
  (zone (net 63) (net_name +12V) (layer PWR.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.25 115.7) (xy 75.7 115.7) (xy 75.7 103.15) (xy 78.3 103.1) (xy 78.4 88.3)
        (xy 84.7 88.3) (xy 84.7 105.5) (xy 89.3 105.5)
      )
    )
  )
  (zone (net 63) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.2 111.8) (xy 88.8 111.9) (xy 88.8 116.5) (xy 75.2 116.4)
      )
    )
  )
  (zone (net 3) (net_name +5V) (layer PWR.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71.9 64.9) (xy 132.2 64.8) (xy 132.1 112.8) (xy 123.8 112.8) (xy 123.8 89.6)
        (xy 117.8 89.6) (xy 117.8 93.4) (xy 114.9 93.4) (xy 114.9 89.6) (xy 108.95 89.6)
        (xy 108.95 111.5) (xy 106.2 111.5) (xy 106.2 89.6) (xy 102.5 89.6) (xy 102.5 93.3)
        (xy 99.6 93.3) (xy 99.6 89.6) (xy 93.7 89.6) (xy 93.7 104.7) (xy 85.6 104.6)
        (xy 85.6 85.45) (xy 71.9 85.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.2 117.6) (xy 88.8 117.6) (xy 88.8 123.2) (xy 75.2 123.1)
      )
    )
  )
  (zone (net 64) (net_name GND-pH) (layer GND.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.1 94.3) (xy 106.1 94.3) (xy 106.1 103.7) (xy 99.85 103.7) (xy 99.85 116.9)
        (xy 94.35 116.9) (xy 94.3 90.6) (xy 101.1 90.6)
      )
    )
  )
  (zone (net 66) (net_name GND-EC) (layer GND.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.3 94.2) (xy 121.6 94.2) (xy 121.6 103.45) (xy 115.25 103.45) (xy 115.25 117)
        (xy 109.5 117) (xy 109.5 90.7) (xy 116.3 90.7)
      )
    )
  )
  (zone (net 9) (net_name "Net-(J2-Pad2)") (layer GND.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.1 116.9) (xy 100.5 116.9) (xy 100.5 104.25) (xy 106.1 104.25)
      )
    )
  )
  (zone (net 11) (net_name "Net-(J3-Pad2)") (layer GND.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.6 116.9) (xy 116 116.9) (xy 116 104.1) (xy 121.6 104.1)
      )
    )
  )
  (zone (net 11) (net_name "Net-(J3-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.2 104.1) (xy 121.2 116.8) (xy 116 116.8) (xy 116.1 104.1)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.6 92.45) (xy 86.95 92.5) (xy 86.95 97.15) (xy 85.15 97.15) (xy 85.1 103.2)
        (xy 82.05 103.2) (xy 82.05 99.25) (xy 79.95 97.15) (xy 77.45 97.15)
      )
    )
  )
  (zone (net 9) (net_name "Net-(J2-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.45 104.4) (xy 105.9 104.4) (xy 105.9 117) (xy 100.5 117)
      )
    )
  )
)
