(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 18)
    (no_connects 0)
    (area 126.924999 76.124999 144.855001 94.055001)
    (thickness 1.6)
    (drawings 29)
    (tracks 60)
    (zones 0)
    (modules 10)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.7366)
    (user_trace_width 0.4826)
    (user_trace_width 0.7366)
    (trace_clearance 0.2)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(HOLE1-Pad1)")
  (net 6 "Net-(HOLE2-Pad1)")
  (net 7 /SCL)
  (net 8 /SDA)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(HOLE1-Pad1)")
    (add_net "Net-(HOLE2-Pad1)")
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A384CF4)
    (at 129.54 87.63 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 1.27 1.5875 180) (layer F.SilkS))
    (fp_text value 1uF (at -1.5875 1.5875 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A384CE3)
    (at 129.54 84.455 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 1.27 1.5875 180) (layer F.SilkS))
    (fp_text value 1uF (at -1.5875 1.5875 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A3860A4)
    (at 138.43 86.0425 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 1.7145 -1.27 270) (layer F.SilkS))
    (fp_text value DNP (at 0 -7.62 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Hole_2.5mm (layer F.Cu) (tedit 5A38488C)
    (at 129.54 78.74)
    (descr "Mounting Hole, 2.5mm")
    (tags "HOLE 2.5MM")
    (fp_text reference HOLE1 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value M2.5 (at 0 -3.4925) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(HOLE1-Pad1)"))
  )
  (module my_components:Hole_2.5mm (layer F.Cu) (tedit 5A384893)
    (at 142.24 78.74)
    (descr "Mounting Hole, 2.5mm")
    (tags "HOLE 2.5MM")
    (fp_text reference HOLE2 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value M2.5 (at 0 -3.4925) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(HOLE2-Pad1)"))
  )
  (module my_components:Conn_Pin_Header_5x1_2.54mm (layer F.Cu) (tedit 5A383928)
    (at 135.89 91.44)
    (descr "Pin Header, 5x1, 2.54mm pitch")
    (tags "CONN 5x1")
    (fp_text reference P1 (at -7.3025 0 90) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 3.4925) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 3 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SCL))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SDA))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A384D20)
    (at 142.24 87.63 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 1.5875 1.5875 180) (layer F.SilkS))
    (fp_text value 10k (at -0.9525 1.5875 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /SDA))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A384D31)
    (at 142.24 84.455 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 1.4605 1.5875 180) (layer F.SilkS))
    (fp_text value 10k (at -0.9525 1.5875 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCL))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_SOT23-5_Hand_Soldering (layer F.Cu) (tedit 5A385F92)
    (at 134.62 86.0425 90)
    (descr "5-pin SOT23 package - Hand Soldering")
    (tags IC_SOT23-5_Hand_Soldering)
    (attr smd)
    (fp_text reference U2 (at 3.302 0 180) (layer F.SilkS))
    (fp_text value MIC5225 (at 0.254 2.3495 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.5 0 90) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.5 0.95 90) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 1.5 0.95 90) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 5 smd rect (at 1.5 -0.95 90) (size 1.8 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_TO-46-4 (layer F.Cu) (tedit 5A384D28)
    (at 135.89 79.375 90)
    (descr TO-46-4)
    (tags "TO-46-4, TO-46, 4Pin")
    (fp_text reference U1 (at 0 -3.4925 90) (layer F.SilkS))
    (fp_text value MLX90615 (at -0.635 3.3655 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 1.27 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SDA))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 3 thru_hole circle (at 0 -1.27 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SCL))
    (pad 4 thru_hole circle (at -1.27 0 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (gr_text "MLX90615\nInfrared Temperature\nSensor V2 (C) 2017\nSergey Kiselev" (at 135.89 84.455) (layer B.SilkS))
  (gr_text SDA (at 140.97 89.3445) (layer F.SilkS))
  (gr_text SCL (at 138.43 89.3445) (layer F.SilkS))
  (gr_text GND (at 135.89 89.3445) (layer F.SilkS))
  (gr_text 3.3V (at 133.0325 89.3445) (layer F.SilkS))
  (gr_text 5V (at 130.4925 89.3445) (layer F.SilkS))
  (gr_line (start 127 77.47) (end 127 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 77.47) (end 144.78 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.51 76.2) (end 128.27 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 93.98) (end 143.51 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 143.51 92.71) (end 144.78 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128.27 92.71) (end 128.27 93.98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128.27 77.47) (end 127 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 143.51 77.47) (end 143.51 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.78 93.98) (xy 127 93.98) (xy 127 76.2) (xy 144.78 76.2) (xy 144.78 93.98)
      )
    )
  )
)
