(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(U1-BIAS)")
	(net 2 "GND")
	(net 3 "Net-(U1-SS)")
	(net 4 "Net-(U1-VCC)")
	(net 5 "Net-(C4-Pad1)")
	(net 6 "Net-(U1-COMP)")
	(net 7 "Net-(D1-A)")
	(net 8 "Net-(D1-K)")
	(net 9 "Net-(U1-RT)")
	(net 10 "Net-(U1-MODE)")
	(net 11 "Net-(R4-Pad2)")
	(net 12 "Net-(U1-PGOOD)")
	(net 13 "Net-(C11-Pad1)")
	(net 14 "unconnected-(U1-NC-Pad15)")
	(net 15 "Net-(C6-Pad1)")
	(net 16 "unconnected-(U1-NC-Pad12)")
	(net 17 "unconnected-(U2-PWMTG-Pad20)")
	(net 18 "Net-(C12-Pad1)")
	(net 19 "Net-(C13-Pad1)")
	(net 20 "Net-(U2-BST1)")
	(net 21 "Net-(U2-BST2)")
	(net 22 "Net-(C14-Pad1)")
	(net 23 "/Vref_A")
	(net 24 "Net-(U2-SS)")
	(net 25 "Net-(U2-Vin)")
	(net 26 "Net-(U2-ISN)")
	(net 27 "Net-(C19-Pad1)")
	(net 28 "Net-(U2-Vc)")
	(net 29 "Net-(U2-INTVcc)")
	(net 30 "Net-(U4-BST1)")
	(net 31 "Net-(U4-SW1)")
	(net 32 "Net-(U4-SW2)")
	(net 33 "Net-(U4-BST2)")
	(net 34 "Net-(U4-PVIN)")
	(net 35 "Net-(U3-SW1)")
	(net 36 "Net-(U3-BST1)")
	(net 37 "Net-(U3-SW2)")
	(net 38 "Net-(U3-BST2)")
	(net 39 "Net-(U3-PVIN)")
	(net 40 "Net-(U4-PVOUT)")
	(net 41 "Net-(U3-VOUT)")
	(net 42 "Net-(U4-PVcc)")
	(net 43 "Net-(C37-Pad1)")
	(net 44 "Net-(U4-VC)")
	(net 45 "Net-(U4-RT)")
	(net 46 "/VOUT")
	(net 47 "/VIN")
	(net 48 "Net-(U1-EN_UVLO_SYNC)")
	(net 49 "Net-(R8-Pad1)")
	(net 50 "Net-(R9-Pad2)")
	(net 51 "Net-(U2-OVLO)")
	(net 52 "Net-(U2-EN{slash}ULO)")
	(net 53 "Net-(U2-RT)")
	(net 54 "Net-(U2-RP)")
	(net 55 "Net-(U2-ISP)")
	(net 56 "Net-(U2-FB)")
	(net 57 "Net-(U2-CRTL)")
	(net 58 "Net-(U3-RUN)")
	(net 59 "Net-(U3-MODE)")
	(net 60 "unconnected-(U3-NC-Pad17)")
	(net 61 "/Vcc_B")
	(net 62 "Net-(U3-VS2{slash}FB)")
	(net 63 "Net-(U3-VS1{slash}ILIM)")
	(net 64 "Net-(U4-FB)")
	(net 65 "Net-(U4-RUN)")
	(net 66 "Net-(U2-ISMON)")
	(net 67 "Net-(U2-~{FAULT})")
	(net 68 "Net-(U2-SYNC{slash}SPREAD)")
	(net 69 "Net-(U3-PGOOD)")
	(net 70 "Net-(U1-FB)")
	(net 71 "Net-(U4-PWM{slash}SYNC)")
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 151.765 83.185)
		(property "Reference" "TP7"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 151.13 71.374)
		(property "Reference" "TP9"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Vout"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(C11-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 169.418 54.608 -90)
		(descr "SMT capacitor, 0603")
		(property "Reference" "C7"
			(at 2.034 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.016 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(D1-A)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 168.021 54.598 -90)
		(descr "SMT capacitor, 0603")
		(property "Reference" "C6"
			(at 1.917 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.016 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 0.0635 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(D1-A)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "DRM_KLibrary:RTE0016K-IPC_A"
		(layer "F.Cu")
		(at 166.624 58.674)
		(tags "LM5158QRTERQ1 ")
		(property "Reference" "U1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LM5158QRTERQ1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "DRM_KLibrary:RTE0016K-IPC_A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5158-q1.pdf?HQS=dis-dk-null-digikeymode-dsf-pf-null-wwe&ts=1731935599625&ref_url=https%253A%252F%252Fic-online.com%252F"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMPS Boost Regulator 60V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RTE0016K-IPC_A RTE0016K-IPC_B RTE0016K-IPC_C RTE0016K-MFG")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.504554 -0.749998 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -1.504554 -0.25 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U1-VCC)")
			(pinfunction "VCC")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at -1.504554 0.25 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-BIAS)")
			(pinfunction "BIAS")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.504554 0.750001 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(U1-PGOOD)")
			(pinfunction "PGOOD")
			(pintype "open_collector")
		)
		(pad "5" smd rect
			(at -0.749998 1.504554)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(U1-RT)")
			(pinfunction "RT")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -0.25 1.504554)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "Net-(U1-EN_UVLO_SYNC)")
			(pinfunction "EN_UVLO_SYNC")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 0.25 1.504554)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 0.750001 1.504554)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U1-COMP)")
			(pinfunction "COMP")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at 1.504554 0.750001 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "Net-(U1-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
		)
		(pad "10" smd rect
			(at 1.504554 0.25 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(U1-SS)")
			(pinfunction "SS")
			(pintype "unspecified")
		)
		(pad "11" smd rect
			(at 1.504554 -0.25 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-MODE)")
			(pinfunction "MODE")
			(pintype "unspecified")
		)
		(pad "12" smd rect
			(at 1.504554 -0.749998 90)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "unconnected-(U1-NC-Pad12)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
		)
		(pad "13" smd rect
			(at 0.750001 -1.504554)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(C6-Pad1)")
			(pinfunction "SW")
			(pintype "unspecified")
		)
		(pad "14" smd rect
			(at 0.25 -1.504554)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(C6-Pad1)")
			(pinfunction "SW")
			(pintype "unspecified")
		)
		(pad "15" smd rect
			(at -0.25 -1.504554)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "unconnected-(U1-NC-Pad15)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
		)
		(pad "16" smd rect
			(at -0.749998 -1.504554)
			(size 0.239283 0.949109)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at 0 0)
			(size 1.6002 1.6002)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "power_in")
		)
		(model "${T_LIBS}/3d/t_qfn/LM5158QRTERQ1.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 181.864 79.629 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C12"
			(at 3.048 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(C12-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 170.011 93.067 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R23"
			(at -0.042 -0.151 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "Net-(U3-MODE)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "/Vcc_B")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 172.72 75.946 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C19"
			(at -0.127 1.143 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.47uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(C19-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 162.56 78.74)
		(descr "SMT capacitor, 0603")
		(property "Reference" "C15"
			(at -0.762 1.397 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 0.0635 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/Vref_A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(layer "F.Cu")
		(at 188.595 52.07)
		(property "Reference" "TP5"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 173.736 60.198)
		(property "Reference" "TP2"
			(at 1.8 0.18 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(R4-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_coilcraft:Coilcraft_XAL4020"
		(layer "F.Cu")
		(at 166.582 67.818)
		(property "Reference" "L2"
			(at -3.006 -2.032 0)
			(layer "F.SilkS")
		)
		(property "Value" "8.2uH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:Coilcraft_XAL4020"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.1811 0)
			(size 0.9652 3.4036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(C13-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.1811 0)
			(size 0.9652 3.4036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(C14-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-XEL4020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 159.385 63.5)
		(property "Reference" "TP22"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 146.685 83.185)
		(property "Reference" "TP6"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Vin"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(R8-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 170.434 67.588 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C18"
			(at 2.945 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U2-ISN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 160.274 69.977 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C17"
			(at 3.175 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U2-Vin)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_so:SOD-123"
		(layer "F.Cu")
		(at 170.053 51.816 180)
		(property "Reference" "D1"
			(at 0.127 1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "SS36FA"
			(at 0.0635 1.8415 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_so:SOD-123"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.42 -0.02 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.025 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.025 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 171.196 103.505 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C32"
			(at 3.024 0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(U4-PVOUT)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 172.847 90.4 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R24"
			(at -2.31 1.397 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "Net-(U3-VOUT)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "Net-(U3-VS2{slash}FB)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 174.371 103.505 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C33"
			(at 3.151 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(U4-PVOUT)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 166.37 61.54 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R1"
			(at -1.651 -1.452 90)
			(layer "F.SilkS")
		)
		(property "Value" "13.3k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(U1-RT)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 170.9 60.579 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C4"
			(at -1.78 -0.762 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.47uF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 184.15 64.135)
		(property "Reference" "TP24"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 171.027 74.422 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R15"
			(at 0.085 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "Net-(U2-RT)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 169.037 80.137)
		(property "Reference" "TP15"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(U2-~{FAULT})")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 171.069 90.273)
		(property "Reference" "TP18"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "Net-(U3-PGOOD)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 162.306 97.409 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C39"
			(at -2.286 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "Net-(U4-PVcc)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 170.815 86.868 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C34"
			(at 2.921 0.381 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "Net-(U3-VOUT)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 167.471 70.612)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C14"
			(at 2.032 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(C14-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(U2-BST2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 166.624 80.137)
		(property "Reference" "TP14"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(U2-ISMON)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "DRM_KLibrary:cap_1210"
		(layer "F.Cu")
		(at 171.831 55.348 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C8"
			(at 0.532 -5.842 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "DRM_KLibrary:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 148.59 71.374)
		(property "Reference" "TP8"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Vout"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(R8-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 163.576 89.511 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R21"
			(at -2.056 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(U3-PVIN)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "Net-(U3-RUN)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 162.052 76.073)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R11"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "Net-(U2-OVLO)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 158.073 97.663)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R33"
			(at -2.117 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "Net-(U4-PWM{slash}SYNC)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(layer "F.Cu")
		(at 145.415 107.95)
		(property "Reference" "TP21"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 167.513 104.14)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C24"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Net-(U4-SW2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "Net-(U4-BST2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "DRM_KLibrary:UDC_20_ADI"
		(layer "F.Cu")
		(at 166.624 90.019)
		(tags "LTC3130EUDC-PBF ")
		(property "Reference" "U3"
			(at -1.905 3.072 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LTC3130EUDC-PBF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "DRM_KLibrary:UDC_20_ADI"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/3130f.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "UDC_20_ADI UDC_20_ADI-M UDC_20_ADI-L")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.4384 -1.25 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.4384 -1.25 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -0.3556 -1.25 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.3556 -1.25 0)
			(layer "F.Fab")
		)
		(pad "1" smd oval
			(at -1.397 -1.25 90)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "Net-(U3-BST1)")
			(pinfunction "BST1")
			(pintype "unspecified")
		)
		(pad "2" smd oval
			(at -1.397 -0.750001 90)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(U3-PVIN)")
			(pinfunction "PVIN")
			(pintype "input")
		)
		(pad "3" smd oval
			(at -1.397 -0.25 90)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(U3-PVIN)")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "4" smd oval
			(at -1.397 0.25 90)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "Net-(U3-RUN)")
			(pinfunction "RUN")
			(pintype "input")
		)
		(pad "5" smd oval
			(at -1.397 0.750001 90)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "/Vcc_B")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "6" smd oval
			(at -1.397 1.25 90)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "/Vcc_B")
			(pinfunction "MPPC")
			(pintype "unspecified")
		)
		(pad "7" smd oval
			(at -0.750001 1.905)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "8" smd oval
			(at -0.25 1.905)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "9" smd oval
			(at 0.25 1.905)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "Net-(U3-VS2{slash}FB)")
			(pinfunction "VS2/FB")
			(pintype "bidirectional")
		)
		(pad "10" smd oval
			(at 0.750001 1.905)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "Net-(U3-VS1{slash}ILIM)")
			(pinfunction "VS1/ILIM")
			(pintype "bidirectional")
		)
		(pad "11" smd oval
			(at 1.397 1.25 90)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "Net-(U3-MODE)")
			(pinfunction "MODE")
			(pintype "unspecified")
		)
		(pad "12" smd oval
			(at 1.397 0.750001 90)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "EXTVCC")
			(pintype "input")
		)
		(pad "13" smd oval
			(at 1.397 0.25 90)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 69 "Net-(U3-PGOOD)")
			(pinfunction "PGOOD")
			(pintype "output")
		)
		(pad "14" smd oval
			(at 1.397 -0.25 90)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "Net-(U3-VOUT)")
			(pinfunction "VOUT")
			(pintype "output")
		)
		(pad "15" smd oval
			(at 1.397 -0.750001 90)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "Net-(U3-SW2)")
			(pinfunction "SW2")
			(pintype "unspecified")
		)
		(pad "16" smd oval
			(at 1.397 -1.25 90)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "Net-(U3-BST2)")
			(pinfunction "BST2")
			(pintype "unspecified")
		)
		(pad "17" smd oval
			(at 0.750001 -1.905)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "unconnected-(U3-NC-Pad17)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "18" smd oval
			(at 0.25 -1.905)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "power_out")
		)
		(pad "19" smd oval
			(at -0.25 -1.905)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "power_out")
		)
		(pad "20" smd oval
			(at -0.750001 -1.905)
			(size 0.254 0.8128)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(U3-SW1)")
			(pinfunction "SW1")
			(pintype "unspecified")
		)
		(pad "21" smd rect
			(at 0 0)
			(size 1.5 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "PAD")
			(pintype "power_out")
			(thermal_bridge_angle 45)
		)
		(model "D:/Dan/Eng Projects/Assualter/KiCAD/Library/3D/UDC_20_ADI.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/Dan/EngProjects/Assaulter/KiCAD/Library/3D/UDC_20_ADI.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 170.011 94.083 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R26"
			(at 0 -1.04 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "Net-(U3-VS1{slash}ILIM)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "/Vcc_B")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "DRM_KLibrary:cap_1210"
		(layer "F.Cu")
		(at 160.23 53.999 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C10"
			(at 2.921 0.044 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "DRM_KLibrary:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-BIAS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "DRM_KLibrary:DFN-16_DHC_LIT-M"
		(layer "F.Cu")
		(at 166.2638 100.357998 180)
		(tags "LTC3114EDHC-1-TRPBF ")
		(property "Reference" "U4"
			(at 1.5448 3.456998 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LTC3115EDHD-1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "DRM_KLibrary:DFN-16_DHC_LIT-M"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LTC3115-1.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DFN-16_DHC_LIT DFN-16_DHC_LIT-M DFN-16_DHC_LIT-L")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5032 -1.750002 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "Net-(U4-RUN)")
			(pinfunction "RUN")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.5032 -1.25 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Net-(U4-SW2)")
			(pinfunction "SW2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at -1.5032 -0.750001 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(U4-PVOUT)")
			(pinfunction "PVOUT")
			(pintype "output")
		)
		(pad "4" smd rect
			(at -1.5032 -0.25 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at -1.5032 0.25 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" smd rect
			(at -1.5032 0.749998 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "Net-(U4-VC)")
			(pinfunction "VC")
			(pintype "output")
		)
		(pad "7" smd rect
			(at -1.5032 1.25 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "Net-(U4-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "8" smd rect
			(at -1.5032 1.749999 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "Net-(U4-RT)")
			(pinfunction "RT")
			(pintype "output")
		)
		(pad "9" smd rect
			(at 1.5032 1.750002 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "Net-(U4-PVcc)")
			(pinfunction "Vcc")
			(pintype "input")
		)
		(pad "10" smd rect
			(at 1.5032 1.25 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(U4-PVIN)")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 1.5032 0.750001 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "Net-(U4-PVcc)")
			(pinfunction "PVcc")
			(pintype "output")
		)
		(pad "12" smd rect
			(at 1.5032 0.25 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "Net-(U4-BST2)")
			(pinfunction "BST2")
			(pintype "unspecified")
		)
		(pad "13" smd rect
			(at 1.5032 -0.25 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(U4-BST1)")
			(pinfunction "BST1")
			(pintype "unspecified")
		)
		(pad "14" smd rect
			(at 1.5032 -0.749998 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(U4-PVIN)")
			(pinfunction "PVIN")
			(pintype "input")
		)
		(pad "15" smd rect
			(at 1.5032 -1.25 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(U4-SW1)")
			(pinfunction "SW1")
			(pintype "unspecified")
		)
		(pad "16" smd rect
			(at 1.5032 -1.749999 180)
			(size 0.9064 0.2492)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "Net-(U4-PWM{slash}SYNC)")
			(pinfunction "PWM/SYNC")
			(pintype "input")
		)
		(pad "17" smd rect
			(at 0 0 180)
			(size 1.75 4.500001)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(model "D:/Dan/Eng Projects/Assualter/KiCAD/Library/3D/DFN-16_DHC_LIT.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/Dan/EngProjects/Assaulter/KiCAD/Library/3D/DFN-16_DHC_LIT.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 182.88 84.455)
		(property "Reference" "TP13"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 173.44 58.547)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R5"
			(at 0 -1.047 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "220"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(R4-Pad2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "Net-(U1-FB)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 153.035 104.14)
		(property "Reference" "TP25"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 159.639 103.759 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C26"
			(at 1.651 -2.794 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(U4-PVIN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 163.703 57.658 -90)
		(descr "SMT capacitor, 0603")
		(property "Reference" "C3"
			(at 1.905 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.016 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 0.0635 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U1-VCC)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 163.576 60.96)
		(property "Reference" "TP3"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(U1-PGOOD)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 157.607 102.574 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R32"
			(at -0.042 -1.016 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(U4-PVIN)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "Net-(U4-RUN)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "DRM_KLibrary:cap_1210"
		(layer "F.Cu")
		(at 175.133 55.348 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C9"
			(at -1.246 -2.413 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "DRM_KLibrary:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 162.179 73.787)
		(descr "SMT capacitor, 0603")
		(property "Reference" "C21"
			(at -0.889 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 0.0635 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(U2-INTVcc)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "DRM_KLibrary:QFN-28_EP_4x5_Pitch0.5mm"
		(layer "F.Cu")
		(at 166.444 74.29)
		(property "Reference" "U2"
			(at -3.376 -1.646 0)
			(layer "F.SilkS")
		)
		(property "Value" "LT3942"
			(at 0 4.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "DRM_KLibrary:QFN-28_EP_4x5_Pitch0.5mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/lt3942.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -0.9 -1.275)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at -0.9 -0.425)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at -0.9 0.425)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at -0.9 1.275)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at -0.3 -1.275)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at -0.3 -0.425)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at -0.3 0.425)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at -0.3 1.275)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0.3 -1.275)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0.3 -0.425)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0.3 0.425)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0.3 1.275)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0.9 -1.275)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0.9 -0.425)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0.9 0.425)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "" smd rect
			(at 0.9 1.275)
			(size 0.000001 0.250001)
			(layers "F.Paste")
			(thermal_bridge_angle 45)
		)
		(pad "1" smd rect
			(at -1.95 -1.75 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U2-Vin)")
			(pinfunction "PVin")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -1.95 -1.25 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U2-Vin)")
			(pinfunction "PVin")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -1.95 -0.75 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U2-Vin)")
			(pinfunction "Vin")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -1.95 -0.25 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(U2-INTVcc)")
			(pinfunction "INTVcc")
			(pintype "power_out")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at -1.95 0.25 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "Net-(U2-EN{slash}ULO)")
			(pinfunction "EN/ULO")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at -1.95 0.75 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "Net-(U2-OVLO)")
			(pinfunction "OVLO")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at -1.95 1.25 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "Net-(U2-RP)")
			(pinfunction "RP")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at -1.95 1.75 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/Vref_A")
			(pinfunction "PWM")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at -1.25 2.45)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/Vref_A")
			(pinfunction "Vref")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at -0.75 2.45)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "Net-(U2-CRTL)")
			(pinfunction "CRTL")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "11" smd rect
			(at -0.25 2.45)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "Net-(U2-ISP)")
			(pinfunction "ISP")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "12" smd rect
			(at 0.25 2.45)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U2-ISN)")
			(pinfunction "ISN")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "13" smd rect
			(at 0.75 2.45)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "Net-(U2-ISMON)")
			(pinfunction "ISMON")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "14" smd rect
			(at 1.25 2.45)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "Net-(U2-~{FAULT})")
			(pinfunction "~{FAULT}")
			(pintype "open_collector")
			(thermal_bridge_angle 45)
		)
		(pad "15" smd rect
			(at 1.95 1.75 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(U2-SS)")
			(pinfunction "SS")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "16" smd rect
			(at 1.95 1.25 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "Net-(U2-FB)")
			(pinfunction "FB")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "17" smd rect
			(at 1.95 0.75 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(U2-Vc)")
			(pinfunction "Vc")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "18" smd rect
			(at 1.95 0.25 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "Net-(U2-RT)")
			(pinfunction "RT")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "19" smd rect
			(at 1.95 -0.25 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "Net-(U2-SYNC{slash}SPREAD)")
			(pinfunction "SYNC/SPREAD")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "20" smd rect
			(at 1.95 -0.75 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "unconnected-(U2-PWMTG-Pad20)")
			(pinfunction "PWMTG")
			(pintype "input+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "21" smd rect
			(at 1.95 -1.25 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "Net-(U2-ISP)")
			(pinfunction "PVout")
			(pintype "power_out")
			(thermal_bridge_angle 45)
		)
		(pad "22" smd rect
			(at 1.95 -1.75 90)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "Net-(U2-ISP)")
			(pinfunction "PVout")
			(pintype "power_out")
			(thermal_bridge_angle 45)
		)
		(pad "23" smd rect
			(at 1.25 -2.45)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(C14-Pad1)")
			(pinfunction "SW2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "24" smd rect
			(at 0.75 -2.45)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(C14-Pad1)")
			(pinfunction "SW2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "25" smd rect
			(at 0.25 -2.45)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(U2-BST2)")
			(pinfunction "BST2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "26" smd rect
			(at -0.25 -2.45)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(U2-BST1)")
			(pinfunction "BST1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "27" smd rect
			(at -0.75 -2.45)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(C13-Pad1)")
			(pinfunction "SW1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "28" smd rect
			(at -1.25 -2.45)
			(size 0.27 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(C13-Pad1)")
			(pinfunction "SW1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "29" smd rect
			(at 0 0)
			(size 2.4 3.4)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "D:/Dan/Eng Projects/Assualter/KiCAD/Library/3D/UFD-28_QFN.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/Dan/EngProjects/Assaulter/KiCAD/Library/3D/UFD-28_QFN.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 172.847 92.517 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R25"
			(at -2.098 0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "Net-(U3-VS2{slash}FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 171.027 76.327 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C20"
			(at 0.085 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(U2-Vc)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 158.120838 95.218838)
		(property "Reference" "TP4"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(U4-PWM{slash}SYNC)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 167.217 96.774)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R28"
			(at 0 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "Net-(U4-RT)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 172.212 99.949 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C37"
			(at 0 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.47uF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "Net-(C37-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_1206"
		(layer "F.Cu")
		(at 157.861 100.076)
		(descr "SMT capacitor, 1206")
		(property "Reference" "FB5"
			(at -3.556 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -1.6002 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:fb_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(U4-PVIN)")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/VIN")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 170.011 59.309 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C2"
			(at 0 -0.381 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(U1-SS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:Coilcraft_XAL4020"
		(layer "F.Cu")
		(at 166.243 106.934)
		(property "Reference" "L3"
			(at -3.048 1.143 0)
			(layer "F.SilkS")
		)
		(property "Value" "8.2uH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:Coilcraft_XAL4020"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.1811 0)
			(size 0.9652 3.4036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(U4-SW1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.1811 0)
			(size 0.9652 3.4036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Net-(U4-SW2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-XEL4020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 162.052 77.47)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R16"
			(at -2.032 0.635 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "Net-(U2-RP)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_1206"
		(layer "F.Cu")
		(at 175.387 71.247)
		(descr "SMT capacitor, 1206")
		(property "Reference" "FB4"
			(at 3.556 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -1.6002 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:fb_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/VOUT")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U2-ISN)")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 165.608 86.717)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C28"
			(at 0 -0.381 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(U3-SW1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "Net-(U3-BST1)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0805"
		(layer "F.Cu")
		(at 170.876 71.247 180)
		(descr "SMT resistor, 0805")
		(property "Reference" "R17"
			(at -0.066 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.01"
			(at 0 1.3208 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.95 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "Net-(U2-ISP)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.95 0 180)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U2-ISN)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 163.576 63.246)
		(property "Reference" "TP16"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(U1-EN_UVLO_SYNC)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 185.42 72.39)
		(property "Reference" "TP10"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Vout"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(C12-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 165.269 104.14 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C23"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(U4-SW1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(U4-BST1)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 170.519 73.025 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R18"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "Net-(U2-ISP)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "Net-(U2-FB)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 161.925 57.973 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C1"
			(at 2.352 1.016 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-BIAS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_1206"
		(layer "F.Cu")
		(at 176.276 90.527)
		(descr "SMT capacitor, 1206")
		(property "Reference" "FB8"
			(at 3.683 0.024 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -1.6002 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:fb_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/VOUT")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "Net-(U3-VOUT)")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 176.784 80.137 180)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C40"
			(at 0.381 2.032 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 360)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/VOUT")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 172.212 98.679 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C38"
			(at -1.27 1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "Net-(U4-VC)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "DRM_KLibrary:cap_1210"
		(layer "F.Cu")
		(at 155.956 68.199)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C41"
			(at 0.127 -2.286 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 360)
			(layer "F.Fab")
		)
		(property "Footprint" "DRM_KLibrary:cap_1210"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/VIN")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_1206"
		(layer "F.Cu")
		(at 155.321 76.327)
		(descr "SMT capacitor, 1206")
		(property "Reference" "FB1"
			(at 1.905 1.778 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -1.6002 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:fb_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/VIN")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(C11-Pad1)")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 170.815 77.851 180)
		(descr "SMT capacitor, 0603")
		(property "Reference" "C16"
			(at 0 -1.397 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.016 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 0.0635 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(U2-SS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 154.305 80.01 -90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C11"
			(at 3.175 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(C11-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_1206"
		(layer "F.Cu")
		(at 156.591 72.644 90)
		(descr "SMT capacitor, 1206")
		(property "Reference" "FB3"
			(at 0.508 -1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -1.6002 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:fb_1206"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0 90)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U2-Vin)")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0 90)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/VIN")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 160.274 73.914 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R12"
			(at -2.159 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U2-Vin)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "Net-(U2-EN{slash}ULO)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 169.21 61 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R3"
			(at 1.865 -0.335 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U1-COMP)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(C4-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 187.96 84.455)
		(property "Reference" "TP12"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Vout"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(R9-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:fb_1206"
		(layer "F.Cu")
		(at 176.403 51.689)
		(descr "SMT capacitor, 1206")
		(property "Reference" "FB9"
			(at 3.556 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -1.6002 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:fb_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/VOUT")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(D1-K)")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 170.18 98.679)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R30"
			(at -0.127 -2.159 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(U4-PVOUT)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "Net-(U4-FB)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(layer "F.Cu")
		(at 188.595 107.95)
		(property "Reference" "TP20"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:fb_1206"
		(layer "F.Cu")
		(at 158.369 57.658)
		(descr "SMT capacitor, 1206")
		(property "Reference" "FB10"
			(at -1.905 -1.778 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -1.6002 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:fb_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-BIAS)")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/VIN")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 167.005 93.218)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R27"
			(at -0.127 1.143 360)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "Net-(U3-VS1{slash}ILIM)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 176.149 60.198)
		(property "Reference" "TP1"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(D1-K)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 159.258 73.914 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R10"
			(at -2.159 -0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U2-Vin)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "Net-(U2-OVLO)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 174.117 86.868 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C35"
			(at 2.921 0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "Net-(U3-VOUT)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:Coilcraft_XAL4020"
		(layer "F.Cu")
		(at 166.624 83.923)
		(property "Reference" "L4"
			(at 3.048 -1.246 0)
			(layer "F.SilkS")
		)
		(property "Value" "8.2uH"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:Coilcraft_XAL4020"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.1811 0)
			(size 0.9652 3.4036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(U3-SW1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.1811 0)
			(size 0.9652 3.4036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "Net-(U3-SW2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-XEL4020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 171.577 58.8 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R6"
			(at -0.507 -1.123 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "220"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "Net-(U1-FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 170.91 61.58 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C5"
			(at -1.937 -0.904 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U1-COMP)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 174.625 74.422)
		(property "Reference" "TP17"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(U2-SYNC{slash}SPREAD)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(layer "F.Cu")
		(at 145.415 52.07)
		(property "Reference" "TP19"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res2512W"
		(layer "F.Cu")
		(at 186.539 78.486 -90)
		(property "Reference" "R9"
			(at -4.318 -0.024 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 -0.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res2512W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0 1.5 270)
			(size 7 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(C12-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 -1.5 270)
			(size 7 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "Net-(R9-Pad2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/R2512W.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_1206"
		(layer "F.Cu")
		(at 159.893 89.511)
		(descr "SMT capacitor, 1206")
		(property "Reference" "FB6"
			(at -0.127 2.056 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -1.6002 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:fb_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(U3-PVIN)")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/VIN")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 166.412 62.611 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R7"
			(at -1.609 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "Net-(U1-EN_UVLO_SYNC)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_1206"
		(layer "F.Cu")
		(at 180.086 75.946)
		(descr "SMT capacitor, 1206")
		(property "Reference" "FB2"
			(at 0 -1.778 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -1.6002 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:fb_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(C12-Pad1)")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/VOUT")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res2512W"
		(layer "F.Cu")
		(at 149.884 76.708 -90)
		(property "Reference" "R8"
			(at -4.572 3.453 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 -0.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res2512W"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0 1.5 270)
			(size 7 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "Net-(R8-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 -1.5 270)
			(size 7 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(C11-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/R2512W.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 160.655 85.828 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C30"
			(at 2.897 0.254 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(U3-PVIN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 182.88 97.155)
		(property "Reference" "TP23"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 187.96 72.39)
		(property "Reference" "TP11"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Vout"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(R9-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 164.973 78.486 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R20"
			(at 0.508 -1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "100K"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/Vref_A")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "Net-(U2-CRTL)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 162.179 103.1 90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C27"
			(at -3.58 -2.667 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(U4-PVIN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 170.18 99.949 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R29"
			(at 0.127 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "Net-(U4-VC)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "Net-(C37-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 168.021 86.717)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C29"
			(at 0.127 0.024 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "Net-(U3-SW2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "Net-(U3-BST2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 172.678 73.025 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R19"
			(at -2.201 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "Net-(U2-FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 170.18 97.536 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R31"
			(at 0 -0.9144 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "Net-(U4-FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 170.053 58.22 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R2"
			(at 0.73 0.97 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(U1-MODE)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "DRM_KLibrary:LPD4012"
		(layer "F.Cu")
		(at 164.48 53.721 90)
		(property "Reference" "L1"
			(at 3.3 -0.13 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LPD40xx"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "DRM_KLibrary:LPD4012"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1:1 Coupled Inductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd oval
			(at -1.5 -1.5 225)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-BIAS)")
			(pinfunction "1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd oval
			(at -1.5 1.5 315)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(C6-Pad1)")
			(pinfunction "2")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd oval
			(at 1.5 1.5 45)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(D1-A)")
			(pinfunction "3")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd oval
			(at 1.5 -1.5 135)
			(size 1 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "4")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "C:/Dan/EngProjects/Assaulter/KiCAD/Library/3D/Coilcraft-LPD4012.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 175.641 58.547)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R4"
			(at 2.032 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(D1-K)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(R4-Pad2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 170.053 91.821 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R22"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "Net-(U3-MODE)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 162.814 70.419 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C25"
			(at -2.474 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U2-Vin)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_1210"
		(layer "F.Cu")
		(at 173.609 67.588 90)
		(descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 1210")
		(property "Reference" "C22"
			(at 2.945 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:cap_1210"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U2-ISN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/C_1210.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 165.439 70.612 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C13"
			(at 0 0.381 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(C13-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(U2-BST1)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 162.052 75.184)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R13"
			(at 0 -0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "Net-(U2-EN{slash}ULO)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "F.Cu")
		(at 163.322 86.402 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C31"
			(at -2.328 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.3462 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(U3-PVIN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 171.027 75.311 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R14"
			(at 0.085 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(U2-Vc)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(C19-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_1206"
		(layer "F.Cu")
		(at 175.895 99.822)
		(descr "SMT capacitor, 1206")
		(property "Reference" "FB7"
			(at 3.429 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -1.6002 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_passive_smd:fb_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "SepicTest1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.1 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/VOUT")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.397 0)
			(size 1.6002 1.8034)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(U4-PVOUT)")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 141.732 48.26)
		(end 192.532 111.76)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "GND"
		(at 180.848 87.757 0)
		(layer "F.SilkS")
	)
	(gr_text "SEPIC\nBUCK/BOOST\nTest Board\n27 Jan 2025\nDRM"
		(at 142.875 99.06 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 149.733 86.487 0)
		(layer "F.SilkS")
	)
	(gr_text "VOUT\n"
		(at 186.309 87.757 0)
		(layer "F.SilkS")
	)
	(gr_text "VIN"
		(at 144.907 86.614 0)
		(layer "F.SilkS")
	)
	(zone
		(net 55)
		(net_name "Net-(U2-ISP)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.044 72.405) (xy 168.744 72.405) (xy 169.291 72.009) (xy 169.291 70.485) (xy 169.418 70.358)
				(xy 170.434 70.358) (xy 170.434 73.406) (xy 170.307 73.533) (xy 169.545 73.533) (xy 169.291 73.152)
				(xy 168.044 73.175)
			)
		)
	)
	(zone
		(net 25)
		(net_name "Net-(U2-Vin)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 164.844 73.675) (xy 164.844 72.405) (xy 163.564 70.869) (xy 156.591 70.866) (xy 156.591 72.0471)
				(xy 158.369 73.406) (xy 160.782 73.406) (xy 161.163 73.025) (xy 163.449 73.025) (xy 164.144 73.675)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(D1-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 165.1 51.435) (xy 165.1 52.197) (xy 167.259 54.356) (xy 169.926 54.356) (xy 169.926 51.562)
				(xy 169.545 51.181) (xy 165.354 51.181)
			)
		)
	)
	(zone
		(net 19)
		(net_name "Net-(C13-Pad1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 165.829 72.19) (xy 165.862 71.247) (xy 165.608 70.866) (xy 165.608 69.977) (xy 165.8835 69.5198)
				(xy 165.862 66.548) (xy 164.592 66.548) (xy 164.592 71.247) (xy 165.059 72.19)
			)
		)
	)
	(zone
		(net 8)
		(net_name "Net-(D1-K)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.581 54.448) (xy 176.383 54.448) (xy 176.403 50.8) (xy 171.323 50.8) (xy 170.561 51.562)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(C6-Pad1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 166.754358 57.644001) (xy 167.493643 57.644001) (xy 168.656 56.261) (xy 169.164 55.626) (xy 169.926 55.626)
				(xy 169.926 54.737) (xy 165.354 54.737) (xy 164.973 55.245) (xy 164.973 56.007) (xy 165.227 56.261)
				(xy 166.497 56.261) (xy 166.751 56.515)
			)
		)
	)
	(zone
		(net 22)
		(net_name "Net-(C14-Pad1)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 167.059 72.19) (xy 167.829 72.19) (xy 168.402 70.993) (xy 168.402 66.548) (xy 167.259 66.548)
				(xy 167.259 70.993) (xy 167.059 71.49)
			)
		)
	)
	(zone
		(net 39)
		(net_name "Net-(U3-PVIN)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 165.481 89.916) (xy 165.481 89.154) (xy 164.592 89.154) (xy 164.211 88.773) (xy 164.211 86.868)
				(xy 159.766 86.868) (xy 159.766 88.138) (xy 160.274 88.646) (xy 160.274 90.297) (xy 162.433 90.297)
				(xy 163.195 89.535) (xy 163.957 89.535) (xy 164.338 89.916)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads thru_hole_only
			(clearance 0.254)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 142.24 48.895) (xy 191.77 48.895) (xy 191.77 111.125) (xy 142.24 111.125)
			)
		)
	)
)
