(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "MDM1")
	(net 2 "MDM2")
	(net 3 "MDM3")
	(net 4 "MDM4")
	(net 5 "MDM5")
	(net 6 "MDM6")
	(net 7 "MDM7")
	(net 8 "MDM8")
	(net 9 "MDM9")
	(net 10 "MDM10")
	(net 11 "MDM11")
	(net 12 "MDM12")
	(net 13 "MDM14")
	(net 14 "MDM15")
	(net 15 "MDM17")
	(net 16 "MDM16")
	(net 17 "MDM18")
	(net 18 "MDM19")
	(net 19 "MDM20")
	(net 20 "MDM21")
	(net 21 "MDM22")
	(net 22 "MDM23")
	(net 23 "MDM24")
	(net 24 "MDM25")
	(net 25 "GND")
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 178.3334 62.738)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "REF**"
			(at 0 -3.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 3.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 128.7272 62.7634)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "REF**"
			(at 0 -3.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 3.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:MICRO-D-RIGHT-ANGLE"
		(layer "F.Cu")
		(at 127.658 99.786)
		(property "Reference" "U$1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RIGHT-ANGLE-MICRO-D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "3"
			(at 2.032 -10.541 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "21"
			(at 7.112 -0.381 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "6"
			(at 2.032 -5.461 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "19"
			(at 7.112 -5.461 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "14"
			(at 7.112 -13.081 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "11"
			(at 2.032 2.159 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "9"
			(at 4.572 -1.651 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "10"
			(at 2.032 -0.381 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "8"
			(at 2.032 -2.921 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "12"
			(at 2.032 4.699 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "20"
			(at 7.112 -2.921 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 2.032 -13.081 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "16"
			(at 7.112 -10.541 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "22"
			(at 4.572 0.889 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "25"
			(at 7.112 4.699 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Glenair MWDM 2L 25S CBR P .110"
			(at -0.508 -4.826 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "4"
			(at 2.032 -8.001 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "18"
			(at 7.112 -8.001 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "13"
			(at 4.572 5.969 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "5"
			(at 4.572 -6.731 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "7"
			(at 4.572 -4.191 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "23"
			(at 7.112 2.159 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "24"
			(at 4.572 3.429 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "15"
			(at 4.572 -11.811 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "17"
			(at 4.572 -9.271 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 4.572 -14.351 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "" np_thru_hole circle
			(at 3.81 -17.0815 90)
			(size 2.4384 2.4384)
			(drill 2.4384)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 3.81 7.4295 90)
			(size 2.4384 2.4384)
			(drill 2.4384)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at 3.302 -14.986 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "MDM1")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 0.762 -13.716 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "MDM2")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at 0.762 -11.176 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "MDM3")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at 0.762 -8.636 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "MDM4")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 3.302 -7.366 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "MDM5")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 0.762 -6.096 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "MDM6")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at 3.302 -4.826 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "MDM7")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at 0.762 -3.556 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "MDM8")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at 3.302 -2.286 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "MDM9")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole circle
			(at 0.762 -1.016 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "MDM10")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "11" thru_hole circle
			(at 0.762 1.524 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "MDM11")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "12" thru_hole circle
			(at 0.762 4.064 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "MDM12")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole circle
			(at 3.302 5.334 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "14" thru_hole circle
			(at 5.842 -13.716 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "MDM14")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "15" thru_hole circle
			(at 3.302 -12.446 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "MDM15")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "16" thru_hole circle
			(at 5.842 -11.176 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "MDM16")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "17" thru_hole circle
			(at 3.302 -9.906 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "MDM17")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "18" thru_hole circle
			(at 5.842 -8.636 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "MDM18")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "19" thru_hole circle
			(at 5.842 -6.096 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "MDM19")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "20" thru_hole circle
			(at 5.842 -3.556 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "MDM20")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "21" thru_hole circle
			(at 5.842 -1.016 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "MDM21")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "22" thru_hole circle
			(at 3.302 0.254 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "MDM22")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "23" thru_hole circle
			(at 5.842 1.524 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "MDM23")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "24" thru_hole circle
			(at 3.302 2.794 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "MDM24")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "25" thru_hole circle
			(at 5.842 4.064 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "MDM25")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 146 70)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "MDM1")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 166 120)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "MDM12")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 128.6764 127.2794)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "REF**"
			(at 0 -3.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 3.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 145.96 100.04)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "MDM4")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 176 110)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "MDM24")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 166 100)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "MDM10")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 156 90)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "MDM16")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 176 70)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "MDM20")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 166 90)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "MDM9")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 176 90)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "MDM22")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 145.96 120.04)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "MDM6")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 146 90)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "MDM3")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 156 80)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "MDM15")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 145.96 80.04)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "MDM2")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 176 80)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "MDM21")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 176 100)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "MDM23")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 156 70)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "MDM14")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 156 110)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "MDM18")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 156 120)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "MDM19")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 166 80)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "MDM8")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 156 100)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "MDM17")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 166 70)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "MDM7")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 176 120)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "MDM25")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 166 110)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "MDM11")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Foolib:SMA"
		(layer "F.Cu")
		(at 145.96 110.04)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "GND")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "MDM5")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 178.2826 127.2286)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "REF**"
			(at 0 -3.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 3.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 180 131)
		(end 182 129)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182 129)
		(end 182 61)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127 59)
		(end 125 61)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 125 129)
		(end 125 61)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127 131)
		(end 180 131)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127 59)
		(end 180 59)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180 59)
		(end 182 61)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 125 129)
		(end 127 131)
		(layer "Edge.Cuts")
	)
	(gr_text "4"
		(at 141 97.04 0)
		(layer "F.SilkS")
	)
	(gr_text "23"
		(at 170.1 97 0)
		(layer "F.SilkS")
	)
	(gr_text "14"
		(at 150.1 66.825 0)
		(layer "F.SilkS")
	)
	(gr_text "17"
		(at 150.1 97.04 0)
		(layer "F.SilkS")
	)
	(gr_text "22"
		(at 170.1 87 0)
		(layer "F.SilkS")
	)
	(gr_text "24"
		(at 170.1 107 0)
		(layer "F.SilkS")
	)
	(gr_text "11"
		(at 160.1 107 0)
		(layer "F.SilkS")
	)
	(gr_text "16"
		(at 150.1 87 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 141 76.865 0)
		(layer "F.SilkS")
	)
	(gr_text "9"
		(at 161 87 0)
		(layer "F.SilkS")
	)
	(gr_text "15"
		(at 150.1 76.865 0)
		(layer "F.SilkS")
	)
	(gr_text "SMA Breakout\nDesign by AN 09.17.25"
		(at 126 79.5 0)
		(layer "F.SilkS")
	)
	(gr_text "21"
		(at 170.1 76.825 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 141 87 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 141 66.825 0)
		(layer "F.SilkS")
	)
	(gr_text "19"
		(at 150.1 117.04 0)
		(layer "F.SilkS")
	)
	(gr_text "8"
		(at 161 76.825 0)
		(layer "F.SilkS")
	)
	(gr_text "18"
		(at 150.1 107 0)
		(layer "F.SilkS")
	)
	(gr_text "25"
		(at 170.1 117 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 141 107 0)
		(layer "F.SilkS")
	)
	(gr_text "12"
		(at 160.1 117 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 161 66.825 0)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 141 117.04 0)
		(layer "F.SilkS")
	)
	(gr_text "20"
		(at 170.1 66.825 0)
		(layer "F.SilkS")
	)
	(gr_text "10"
		(at 160.1 97 0)
		(layer "F.SilkS")
	)
	(zone
		(net 25)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125 61) (xy 127 59) (xy 180 59) (xy 182 61) (xy 182 129) (xy 180 131) (xy 127 131) (xy 125 129)
			)
		)
	)
	(zone
		(net 25)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125 61) (xy 127 59) (xy 180 59) (xy 182 61) (xy 182 129) (xy 180 131) (xy 127 131) (xy 125 129)
			)
		)
	)
	(embedded_fonts no)
)
