(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 50)
    (tracks 16)
    (zones 0)
    (modules 2)
    (nets 56)
  )
  (page A)
  (title_block
    (title "WeMos D1 Mini to GBS 8200 via PLCC socket")
    (date 2019-11-20)
    (rev 3.0)
    (comment 1 "Original by jmuzi")
    (comment 2 "Modified by MrFreeman")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad2)")
  (net 2 "Net-(U1-Pad1)")
  (net 3 "Net-(U1-Pad3)")
  (net 4 "Net-(U1-Pad4)")
  (net 5 "Net-(U1-Pad5)")
  (net 6 "Net-(U1-Pad6)")
  (net 7 "Net-(U1-Pad7)")
  (net 8 "Net-(U1-Pad8)")
  (net 9 "Net-(U1-Pad9)")
  (net 10 "Net-(U1-Pad10)")
  (net 11 "Net-(U1-Pad11)")
  (net 12 "Net-(U1-Pad12)")
  (net 13 "Net-(U1-Pad13)")
  (net 14 "Net-(U1-Pad14)")
  (net 15 "Net-(U1-Pad15)")
  (net 16 "Net-(U1-Pad16)")
  (net 17 "Net-(U2-Pad1)")
  (net 18 "Net-(U2-Pad3)")
  (net 19 "Net-(U2-Pad5)")
  (net 20 "Net-(U2-Pad43)")
  (net 21 "Net-(U2-Pad41)")
  (net 22 "Net-(U2-Pad2)")
  (net 23 "Net-(U2-Pad4)")
  (net 24 "Net-(U2-Pad6)")
  (net 25 "Net-(U2-Pad44)")
  (net 26 "Net-(U2-Pad42)")
  (net 27 "Net-(U2-Pad8)")
  (net 28 "Net-(U2-Pad10)")
  (net 29 "Net-(U2-Pad12)")
  (net 30 "Net-(U2-Pad14)")
  (net 31 "Net-(U2-Pad16)")
  (net 32 "Net-(U2-Pad7)")
  (net 33 "Net-(U2-Pad9)")
  (net 34 "Net-(U2-Pad11)")
  (net 35 "Net-(U2-Pad13)")
  (net 36 "Net-(U2-Pad15)")
  (net 37 "Net-(U2-Pad17)")
  (net 38 "Net-(U2-Pad19)")
  (net 39 "Net-(U2-Pad21)")
  (net 40 "Net-(U2-Pad25)")
  (net 41 "Net-(U2-Pad29)")
  (net 42 "Net-(U2-Pad22)")
  (net 43 "Net-(U2-Pad28)")
  (net 44 "Net-(U2-Pad32)")
  (net 45 "Net-(U2-Pad36)")
  (net 46 "Net-(U2-Pad38)")
  (net 47 "Net-(U2-Pad40)")
  (net 48 "Net-(U2-Pad31)")
  (net 49 "Net-(U2-Pad33)")
  (net 50 "Net-(U2-Pad35)")
  (net 51 "Net-(U2-Pad37)")
  (net 52 "Net-(U2-Pad39)")
  (net 53 "Net-(U2-Pad30)")
  (net 54 "Net-(U2-Pad24)")
  (net 55 "Net-(U2-Pad23)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad31)")
    (add_net "Net-(U2-Pad32)")
    (add_net "Net-(U2-Pad33)")
    (add_net "Net-(U2-Pad35)")
    (add_net "Net-(U2-Pad36)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad38)")
    (add_net "Net-(U2-Pad39)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad40)")
    (add_net "Net-(U2-Pad41)")
    (add_net "Net-(U2-Pad42)")
    (add_net "Net-(U2-Pad43)")
    (add_net "Net-(U2-Pad44)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
  )
  (module Package_LCC:PLCC-44_THT-Socket (layer F.Cu) (tedit 5DD5F773)
    (at 43.18 21.59)
    (descr "PLCC, 44 pins, through hole")
    (tags "plcc leaded")
    (fp_text reference U2 (at -10.16 -3.81) (layer F.SilkS) hide)
    (fp_text value MTV230M (at -1.27 19.1) (layer F.Fab) hide)
    (fp_text user GBS (at -1.27 6.35 90) (layer F.SilkS))
    (pad 39 thru_hole circle (at 7.62 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(U2-Pad39)"))
    (pad 37 thru_hole circle (at 7.62 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(U2-Pad37)"))
    (pad 35 thru_hole circle (at 7.62 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(U2-Pad35)"))
    (pad 33 thru_hole circle (at 7.62 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(U2-Pad33)"))
    (pad 31 thru_hole circle (at 7.62 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(U2-Pad31)"))
    (pad 40 thru_hole circle (at 5.08 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U2-Pad40)"))
    (pad 38 thru_hole circle (at 5.08 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U2-Pad38)"))
    (pad 36 thru_hole circle (at 5.08 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U2-Pad36)"))
    (pad 34 thru_hole circle (at 5.08 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad5)"))
    (pad 32 thru_hole circle (at 5.08 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U2-Pad32)"))
    (pad 30 thru_hole circle (at 5.08 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(U2-Pad30)"))
    (pad 28 thru_hole circle (at 5.08 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U2-Pad28)"))
    (pad 26 thru_hole circle (at 2.54 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad13)"))
    (pad 24 thru_hole circle (at 0 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(U2-Pad24)"))
    (pad 22 thru_hole circle (at -2.54 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U2-Pad22)"))
    (pad 20 thru_hole rect (at -5.08 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad10)"))
    (pad 18 thru_hole circle (at -7.62 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad8)"))
    (pad 29 thru_hole circle (at 7.62 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U2-Pad29)"))
    (pad 27 thru_hole circle (at 2.54 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad14)"))
    (pad 25 thru_hole circle (at 0 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U2-Pad25)"))
    (pad 23 thru_hole circle (at -2.54 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(U2-Pad23)"))
    (pad 21 thru_hole circle (at -5.08 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U2-Pad21)"))
    (pad 19 thru_hole circle (at -7.62 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(U2-Pad19)"))
    (pad 17 thru_hole circle (at -10.16 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U2-Pad17)"))
    (pad 15 thru_hole circle (at -10.16 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U2-Pad15)"))
    (pad 13 thru_hole circle (at -10.16 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U2-Pad13)"))
    (pad 11 thru_hole circle (at -10.16 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U2-Pad11)"))
    (pad 9 thru_hole circle (at -10.16 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U2-Pad9)"))
    (pad 7 thru_hole circle (at -10.16 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U2-Pad7)"))
    (pad 16 thru_hole circle (at -7.62 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U2-Pad16)"))
    (pad 14 thru_hole circle (at -7.62 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U2-Pad14)"))
    (pad 12 thru_hole circle (at -7.62 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U2-Pad12)"))
    (pad 10 thru_hole circle (at -7.62 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U2-Pad10)"))
    (pad 8 thru_hole circle (at -7.62 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(U2-Pad8)"))
    (pad 42 thru_hole circle (at 2.54 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(U2-Pad42)"))
    (pad 44 thru_hole circle (at 0 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U2-Pad44)"))
    (pad 6 thru_hole circle (at -7.62 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(U2-Pad6)"))
    (pad 4 thru_hole circle (at -5.08 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(U2-Pad4)"))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U2-Pad2)"))
    (pad 41 thru_hole circle (at 5.08 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(U2-Pad41)"))
    (pad 43 thru_hole circle (at 2.54 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(U2-Pad43)"))
    (pad 5 thru_hole circle (at -5.08 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(U2-Pad5)"))
    (pad 3 thru_hole circle (at -2.54 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(U2-Pad3)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad1)"))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-44_THT-Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:WEMOS_D1_mini_light (layer F.Cu) (tedit 5DD61F1C)
    (at 50.8 41.91 270)
    (descr "16-pin module, column spacing 22.86 mm (900 mils), https://wiki.wemos.cc/products:d1:d1_mini, https://c1.staticflickr.com/1/734/31400410271_f278b087db_z.jpg")
    (tags "ESP8266 WiFi microcontroller")
    (fp_text reference U1 (at 0 24.13 90) (layer F.SilkS) hide)
    (fp_text value "WeMos D1 Mini" (at 11.43 2.54 90) (layer F.SilkS))
    (fp_text user "No copper" (at 11.43 -3.81 90) (layer Cmts.User))
    (fp_text user "KEEP OUT" (at 11.43 -6.35 90) (layer Cmts.User))
    (pad 16 thru_hole oval (at 22.86 0 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad16)"))
    (pad 15 thru_hole oval (at 22.86 2.54 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad15)"))
    (pad 14 thru_hole oval (at 22.86 5.08 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad14)"))
    (pad 13 thru_hole oval (at 22.86 7.62 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad13)"))
    (pad 12 thru_hole oval (at 22.86 10.16 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad12)"))
    (pad 11 thru_hole oval (at 22.86 12.7 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad11)"))
    (pad 10 thru_hole rect (at 22.86 15.24 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad10)"))
    (pad 9 thru_hole oval (at 22.86 17.78 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(U1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad3)"))
    (pad 1 thru_hole oval (at 0 0 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad2)"))
    (model ${KISYS3DMOD}/Module.3dshapes/WEMOS_D1_mini_light.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (offset (xyz 0 0 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (offset (xyz 22.86 0 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (offset (xyz 22.86 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text SCLSDA (at 44.45 62.865) (layer B.SilkS))
  (gr_text GND (at 35.56 62.865) (layer B.SilkS))
  (gr_text 3.3V (at 33.02 44.45) (layer B.SilkS))
  (gr_text DEBUG (at 40.64 44.45) (layer B.SilkS))
  (gr_line (start 54.61 66.675) (end 29.21 66.675) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 54.61 15.24) (end 54.61 66.675) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 29.21 17.145) (end 29.21 66.675) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 31.115 15.24) (end 29.21 17.145) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 54.61 15.24) (end 31.115 15.24) (layer Edge.Cuts) (width 0.05))
  (gr_text SDA (at 45.72 38.735) (layer F.SilkS))
  (gr_text SCL (at 45.72 32.385) (layer F.SilkS))
  (gr_text GND (at 38.1 38.735) (layer F.SilkS))
  (gr_text 3.3V (at 32.385 36.83) (layer F.SilkS))
  (gr_text DBG (at 46.355 29.21 90) (layer F.SilkS))
  (gr_text SDASCL (at 44.45 62.865) (layer F.SilkS))
  (gr_text GND (at 35.56 62.865) (layer F.SilkS))
  (gr_text DEBUG (at 40.64 44.45) (layer F.SilkS))
  (gr_text 3.3V (at 33.02 44.45) (layer F.SilkS))
)
