(kicad_pcb (version 20170123) (host pcbnew no-vcs-found-4bdac4d~58~ubuntu17.04.1)
  (general
    (links 148)
    (no_connects 0)
    (area 29.949999 79.320137 90.091466 126.957162)
    (thickness 1.6)
    (drawings 11)
    (tracks 1127)
    (zones 0)
    (modules 53)
    (nets 53)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 1)
    (via_drill 0.6)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 51.873969 90.432637)
    (grid_origin 63.066065 98.828362)
    (visible_elements FFFCEF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory pdf))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 LOAD1)
  (net 4 LOAD2)
  (net 5 +3V3)
  (net 6 LOAD_SW2)
  (net 7 LOAD_SW1)
  (net 8 RF_CSN)
  (net 9 SPI_CLK)
  (net 10 SPI_MOSI)
  (net 11 SPI_MISO)
  (net 12 RF_IRQ)
  (net 13 USBDP)
  (net 14 USBDM)
  (net 15 NRST)
  (net 16 SWDCLK)
  (net 17 SWDIO)
  (net 18 "Net-(C9-Pad2)")
  (net 19 "Net-(C8-Pad2)")
  (net 20 I2C_CLK)
  (net 21 I2C_DATA)
  (net 22 "Net-(D2-Pad2)")
  (net 23 "Net-(D1-Pad2)")
  (net 24 +5V)
  (net 25 VFB)
  (net 26 "Net-(J2-Pad13)")
  (net 27 "Net-(J1-Pad13)")
  (net 28 PA1)
  (net 29 OC_CHARGE_FAULT)
  (net 30 ESP_UART_TX)
  (net 31 ESP_UART_RX)
  (net 32 AN_BATTERY)
  (net 33 LED2)
  (net 34 LED1)
  (net 35 RF_CE_ESP_RST)
  (net 36 OC_CHARGING)
  (net 37 AN_SOLARY)
  (net 38 "Net-(P3-Pad3)")
  (net 39 "Net-(C9-Pad1)")
  (net 40 "Net-(C5-Pad1)")
  (net 41 "Net-(C7-Pad2)")
  (net 42 "Net-(P5-Pad2)")
  (net 43 "Net-(P5-Pad5)")
  (net 44 "Net-(R9-Pad1)")
  (net 45 "Net-(P3-Pad5)")
  (net 46 "Net-(J4-Pad1)")
  (net 47 "Net-(J3-Pad1)")
  (net 48 "Net-(J6-Pad1)")
  (net 49 "Net-(R10-Pad1)")
  (net 50 "Net-(J5-Pad1)")
  (net 51 BAT_VCC)
  (net 52 "Net-(J7-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(R10-Pad1)")
    (add_net VFB)
  )
  (net_class 12v ""
    (clearance 0.4)
    (trace_width 0.9)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net BAT_VCC)
    (add_net LOAD1)
    (add_net LOAD2)
  )
  (net_class 3v ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
  )
  (net_class data ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net AN_BATTERY)
    (add_net AN_SOLARY)
    (add_net ESP_UART_RX)
    (add_net ESP_UART_TX)
    (add_net I2C_CLK)
    (add_net I2C_DATA)
    (add_net LED1)
    (add_net LED2)
    (add_net LOAD_SW1)
    (add_net LOAD_SW2)
    (add_net NRST)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad5)")
    (add_net "Net-(R9-Pad1)")
    (add_net OC_CHARGE_FAULT)
    (add_net OC_CHARGING)
    (add_net PA1)
    (add_net RF_CE_ESP_RST)
    (add_net RF_CSN)
    (add_net RF_IRQ)
    (add_net SPI_CLK)
    (add_net SPI_MISO)
    (add_net SPI_MOSI)
    (add_net SWDCLK)
    (add_net SWDIO)
    (add_net USBDM)
    (add_net USBDP)
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 594CE798)
    (at 42.568265 111.261662 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 3.556 0.127 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at -1.27 -0.0635 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 PA1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 0)
    (at 47.330765 109.674162 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -2.4257 -0.635 270) (layer F.SilkS))
    (fp_text value NRF24LO+ (at 0 -3.1 180) (layer F.Fab))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 RF_IRQ))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 SPI_MISO))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 SPI_MOSI))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SPI_CLK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 RF_CSN))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 RF_CE_ESP_RST))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 +3V3))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 50.881969 87.257637)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value MCP1702T (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 +5V))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 86.700765 103.895662)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J7 (at 0 -3.048) (layer F.SilkS))
    (fp_text value Hole (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 52 "Net-(J7-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 86.970765 111.706162)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0.873 1.8415) (layer F.SilkS))
    (fp_text value SI2319 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 51 BAT_VCC))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5861332C)
    (at 81.303265 86.179162)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J5 (at 0 -3.048) (layer F.SilkS))
    (fp_text value Hole (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 50 "Net-(J5-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 594BC1F2)
    (at 40.155265 102.028762)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J8 (at 0.0635 -2.794) (layer F.SilkS))
    (fp_text value MAX31855 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 SPI_MISO))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 PA1))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SPI_CLK))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 594BC670)
    (at 57.236765 107.113662 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0.6555 1.4605 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at -0.1905 0.1905 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 LOAD_SW2))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 60.284765 107.070662 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -0.6985 -1.397 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at -0.353001 -2.7345 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 LOAD_SW1))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 84.076765 108.404162)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0.5285 -1.397) (layer F.SilkS))
    (fp_text value 1M (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5905F349)
    (at 33.551265 99.958662)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J6 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value Hole (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 48 "Net-(J6-Pad1)"))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5905F354)
    (at 53.172765 120.723162)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J3 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value Hole (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.3) (layers *.Cu *.Mask)
      (net 47 "Net-(J3-Pad1)"))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5905F35E)
    (at 33.678265 120.723162)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J4 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value Hole (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask)
      (net 46 "Net-(J4-Pad1)"))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 82.402765 112.722162 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 3.322 -0.127 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 0)
    (at 87.687969 97.671637 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at -2.76493 -1.110997 270) (layer F.SilkS))
    (fp_text value "NUCLEO CN4" (at -7.047475 0.034704 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 NRST))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 +5V))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 RF_CE_ESP_RST))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 LOAD_SW1))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 LED2))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 LED1))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 RF_CSN))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 RF_IRQ))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 PA1))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 AN_BATTERY))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 +3V3))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SPI_CLK))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_QFP:LQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 66.927969 89.956637)
    (descr "LQFP32: plastic low profile quad flat package; 32 leads; body 7 x 7 x 1.4 mm (see NXP sot358-1_po.pdf and sot358-1_fr.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U4 (at 0 -0.032) (layer F.SilkS))
    (fp_text value STM32F042 (at 0 5.85) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R9-Pad1)"))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 I2C_DATA))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 I2C_CLK))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 SPI_MOSI))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 SPI_MISO))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 SPI_CLK))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 AN_SOLARY))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 SWDCLK))
    (pad 23 smd rect (at 4.25 -2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 SWDIO))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 USBDP))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 USBDM))
    (pad 20 smd rect (at 4.25 0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 ESP_UART_TX))
    (pad 19 smd rect (at 4.25 1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 ESP_UART_RX))
    (pad 18 smd rect (at 4.25 2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 OC_CHARGE_FAULT))
    (pad 17 smd rect (at 4.25 2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at 2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 OC_CHARGING))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 LOAD_SW2))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 LOAD_SW1))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 LED2))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 LED1))
    (pad 10 smd rect (at -2 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 RF_CSN))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 RF_IRQ))
    (pad 8 smd rect (at -4.25 2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 RF_CE_ESP_RST))
    (pad 7 smd rect (at -4.25 2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 PA1))
    (pad 6 smd rect (at -4.25 1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 AN_BATTERY))
    (pad 5 smd rect (at -4.25 0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 NRST))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at -4.25 -2) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C8-Pad2)"))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Housings_QFP.3dshapes/LQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer B.Cu) (tedit 0)
    (at 44.854265 122.564662)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 5.1435 0.254 90) (layer F.SilkS))
    (fp_text value "ESP8266 - 1" (at 0 3.1) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 30 ESP_UART_TX))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 38 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 +3V3))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 45 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 35 RF_CE_ESP_RST))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 31 ESP_UART_RX))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 43.711265 87.957162 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.9415 -0.0635 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 I2C_DATA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 43.661969 86.305137)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 3.005 0.0635) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0.0635) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 I2C_CLK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 57.461969 94.115637)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.25) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C7-Pad2)"))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 58.162969 85.987637)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 0.127) (layer B.SilkS))
    (fp_text value 10pF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0.95 -0.635) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 81.210969 100.084637 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -2.667 -0.127 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C9-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C9-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 51.492969 90.559637)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 1.425796 -1.395975) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 24 +5V))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 70.889265 103.402637 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -3.667 -0.127 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at -3.731525 -0.127 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 24 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 79.906265 110.690162 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 3.3655 -0.0635 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.02 1.8415 180) (layer F.Fab))
    (fp_text user %R (at 0.889 0.127 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 68.857265 101.609662 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -4.318 0.127 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at -4.3815 0.0635 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 24 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 50.095969 92.591637)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -1.050704 1.588525) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 54.837969 84.590637)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -0.522204 1.398025) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at -0.508 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R9-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 81.210969 104.148637 90)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at -0.254 -0.127 90) (layer F.SilkS))
    (fp_text value MCP16311/2 (at -2.096525 3.330796 90) (layer F.Fab))
    (fp_text user %R (at 0.168 -0.041 90) (layer F.Fab))
    (pad 8 smd rect (at 2.2 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 2.2 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C9-Pad2)"))
    (pad 6 smd rect (at 2.2 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C9-Pad1)"))
    (pad 5 smd rect (at 2.2 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.2 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (pad 3 smd rect (at -2.2 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at -2.2 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -2.2 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 VFB))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/MSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 60.284765 111.917162 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.186 -1.524 90) (layer F.SilkS))
    (fp_text value R (at -0.3175 2.3495 90) (layer F.Fab))
    (fp_text user %R (at 0.127 -0.0635 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 AN_BATTERY))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 57.236765 111.917162 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.1225 -1.524 90) (layer F.SilkS))
    (fp_text value R (at -0.014204 1.842525 90) (layer F.Fab))
    (fp_text user %R (at 0.0205 -0.1905 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 AN_BATTERY))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 79.781765 108.467662 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 1.0185 1.27 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 59024CD7)
    (at 72.701969 93.988637 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0.635 1.524 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0.127 1.524 270) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 563007E4)
    (at 81.637265 120.024662)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P6 (at 2.714 -3.8735) (layer F.SilkS))
    (fp_text value BAT (at 2.5 -6.6) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 51 BAT_VCC))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA)
    (at 43.745969 91.829637)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -0.542704 -0.443475) (layer F.SilkS))
    (fp_text value 24LC01B (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 I2C_CLK))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 I2C_DATA))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 43.364969 82.431637 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -2.223525 -0.161704 180) (layer F.SilkS))
    (fp_text value SWD (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 SWDCLK))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 SWDIO))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:SO-8 (layer F.Cu) (tedit 0)
    (at 65.174265 108.086662 180)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U5 (at 0 0 180) (layer F.SilkS))
    (fp_text value FDS6930 (at 0 0 180) (layer F.Fab))
    (pad 8 smd oval (at -1.905 -2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 4 LOAD2))
    (pad 7 smd oval (at -0.635 -2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 4 LOAD2))
    (pad 6 smd oval (at 0.635 -2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 3 LOAD1))
    (pad 5 smd oval (at 1.905 -2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 3 LOAD1))
    (pad 4 smd oval (at 1.905 2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 7 LOAD_SW1))
    (pad 3 smd oval (at 0.635 2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd oval (at -0.635 2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 6 LOAD_SW2))
    (pad 1 smd oval (at -1.905 2.794 180) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57FE943C)
    (at 39.046969 82.177637 180)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 2.193704 1.586475 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.7 180) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.65 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57FE943C)
    (at 33.679265 82.177637 180)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 1.9695 1.459475) (layer F.SilkS))
    (fp_text value LED (at 0 1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.65 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Crystals:Crystal_SMD_5032-4pin_5.0x3.2mm (layer F.Cu) (tedit 58CD2E9C)
    (at 57.477969 89.796637 270)
    (descr "SMD Crystal SERIES SMD2520/4 http://www.icbase.com/File/PDF/HKC/HKC00061008.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 1.652 2.683 270) (layer F.SilkS))
    (fp_text value Crystal_GND24_Small (at 0 2.8 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 4 smd rect (at -1.65 -1 270) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.65 -1 270) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 1.65 1 270) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.65 1 270) (size 1.6 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C8-Pad2)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_5032-4pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58FCB213)
    (at 60.890969 90.117637 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0 0 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0.254 0 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 0)
    (at 87.687969 82.431637 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 2.82307 -0.475997 270) (layer F.SilkS))
    (fp_text value "NUCLEO CN3" (at 6.287525 0.987204 270) (layer F.Fab))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 SPI_MISO))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 SPI_MOSI))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J2-Pad13)"))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 OC_CHARGE_FAULT))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 SWDIO))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 SWDCLK))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 OC_CHARGING))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 I2C_CLK))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 I2C_DATA))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 LOAD_SW1))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 AN_SOLARY))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 NRST))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 ESP_UART_TX))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 ESP_UART_RX))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58FC826E)
    (at 61.144969 85.987637 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 2.159 0.127) (layer B.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at -5.334 -10.541 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Wurth_HCI-5040 (layer F.Cu) (tedit 5745AE01)
    (at 75.334265 103.133662 180)
    (descr "Inductor, Wurth Elektronik, Wurth_HCI-5040, 5.5mmx5.2mm")
    (tags "inductor wurth hci smd")
    (attr smd)
    (fp_text reference L1 (at 0.127 -1.778 180) (layer F.SilkS))
    (fp_text value 22uH (at 0 4.1 180) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0 180) (size 1.9 1.6) (layers F.Cu F.Paste F.Mask)
      (net 24 +5V))
    (pad 1 smd rect (at -2.05 0 180) (size 1.9 1.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C9-Pad1)"))
    (model Inductors.3dshapes/Inductor_Wurth_HCI-5040.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5418A00F)
    (at 72.837265 111.007662 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 3.0275 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 VFB))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5418A00F)
    (at 75.440765 108.213662)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -3.091 0) (layer F.SilkS))
    (fp_text value 52.3k (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 VFB))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 +5V))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58724819)
    (at 32.823969 85.733637)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0.092296 9.970525 180) (layer F.SilkS))
    (fp_text value OLED (at 2.961035 3.911771 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 I2C_DATA))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 I2C_CLK))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 +3V3))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5870E92E)
    (at 36.887969 84.717637 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.043 -1.651 180) (layer F.SilkS))
    (fp_text value R (at 0 1.9 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 LED1))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58FC7949)
    (at 36.896265 87.576162 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -0.084 -1.778 180) (layer F.SilkS))
    (fp_text value R (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 LED2))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5870C605)
    (at 61.017969 93.988637 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0.254 -0.127 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 32 AN_BATTERY))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 563007E4)
    (at 59.983765 120.088162)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P8 (at 1.952 -3.81) (layer F.SilkS))
    (fp_text value OUT2 (at 2.5 -6.6) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 4 LOAD2))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 5870C4E7)
    (at 70.905765 120.024662)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P7 (at 2.54 -3.81) (layer F.SilkS))
    (fp_text value OUT1 (at 2.5 -6.6) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 LOAD1))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 54EA0684)
    (at 74.860969 84.844637)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 2.921 0) (layer F.SilkS))
    (fp_text value USB (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P5-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 USBDP))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 USBDM))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P5-Pad5)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text MAX31855 (at 42.695265 105.419662 90) (layer F.SilkS))
  (gr_text ESP8266 (at 49.756465 117.014762 90) (layer F.SilkS))
  (gr_text NRF24LO+ (at 49.654865 104.619562 90) (layer F.SilkS))
  (gr_text GND/CLK/IO (at 45.650969 84.782162 180) (layer B.SilkS))
  (gr_text "I2C OLED" (at 35.202265 92.783162 90) (layer F.SilkS))
  (gr_text "USB addon\ncard" (at 87.018265 89.989162 90) (layer F.SilkS))
  (gr_text "STM32Coolboard\nDesigned \nby Mike7b4\nv2.1" (at 33.703665 110.055162 270) (layer F.SilkS))
  (gr_line (start 30 79.8) (end 30 125) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30 125) (end 90 125) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90 79.8) (end 90 125) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30 79.8) (end 90 79.8) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29.995265 79.829162) (xy 30.249265 95.958162) (xy 30.249265 96.212162) (xy 89.939265 96.085162) (xy 89.939265 79.829162)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29.995265 79.829162) (xy 29.995265 96.339162) (xy 89.939265 96.085162) (xy 89.939265 79.829162)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.440765 96.275662) (xy 37.996265 125.041162) (xy 72.476765 124.850662) (xy 72.667265 96.085162) (xy 42.695265 96.212162)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.128265 95.577162) (xy 78.826765 124.850662) (xy 89.748765 124.723662) (xy 89.939265 96.212162) (xy 89.812265 95.450162)
        (xy 77.366265 95.577162) (xy 77.493265 96.085162) (xy 78.128265 95.958162)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.349765 105.356162) (xy 72.349765 125.041162) (xy 78.890265 124.787162) (xy 78.636265 105.610162)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.440765 96.148662) (xy 37.996265 124.914162) (xy 72.349765 124.723662) (xy 72.286265 95.704162)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.159265 105.229162) (xy 72.413265 119.961162) (xy 82.065265 119.834162) (xy 81.811265 105.229162)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.001265 95.577162) (xy 79.144265 117.738662) (xy 72.032265 117.929162) (xy 72.095765 124.660162) (xy 89.748765 124.406162)
        (xy 89.812265 95.704162) (xy 78.128265 96.085162) (xy 78.128265 95.958162)
      )
    )
  )
)
