<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="58.725" y1="2.02324375" x2="58.725" y2="77.4336125" width="0" layer="20"/>
<wire x1="58.725" y1="77.4336125" x2="57.4286125" y2="78.73" width="0" layer="20" curve="90"/>
<wire x1="57.4286125" y1="78.73" x2="1.78899375" y2="78.73" width="0" layer="20"/>
<wire x1="1.78899375" y1="78.73" x2="0" y2="76.94100625" width="0" layer="20" curve="90"/>
<wire x1="0" y1="76.94100625" x2="0" y2="4.10980625" width="0" layer="20"/>
<wire x1="0" y1="4.10980625" x2="2.83980625" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.83980625" y1="0" x2="55.43175625" y2="0" width="0" layer="20"/>
<wire x1="55.43175625" y1="0" x2="58.725" y2="2.02324375" width="0" layer="20" curve="90"/>
<text>bat+</text>
<text>bat-</text>
<text>ArduBadBoy</text>
<text>FX</text>
<text>tx</text>
<text>rx</text>
<text>ok</text>
<text>charge</text>
<text>ch-curr</text>
<text>development edition</text>
<text>Attiny</text>
<text>Fx</text>
<text>rgb</text>
<text>rgb</text>
<text>64mb</text>
<text>64mb</text>
<text>Design</text>
<text>by</text>
<text>Duncan Young</text>
<text>reset</text>
<text>Limited 1st Edition</text>
</plain>
<libraries>
<library name="libavr-hvsp-programmer">
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
<package name="AVRISP">
</package>
<package name="SMT-0540-S-R">
</package>
<package name="RGBLED5050">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="blinkinlabs">
<description>Library of parts that we use for our Blinkinlabs designs. Some parts copied (and modified) from the excellent
Sparkfun and Adafruit libraries.</description>
<packages>
<package name="TEST_PAD_SMT">
</package>
</packages>
</library>
<library name="oled_spi_154">
<packages>
<package name="OLED">
</package>
</packages>
</library>
<library name="Dunks_tact">
<packages>
<package name="KPS-1290">
</package>
</packages>
</library>
<library name="DUNK">
<packages>
<package name="USB_MICRO_THRUHOLE">
</package>
</packages>
</library>
<library name="adafruit (2)">
<packages>
<package name="TQFP44">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-SMD-5X3">
</package>
</packages>
</library>
<library name="Ai_LED">
<description>&lt;h3&gt;Ai LED&lt;/h3&gt;
&lt;p&gt;
This library includes LEDs of all shapes and sizes.
&lt;/p&gt;</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD_4.6X2.8MM">
<description>&lt;h3&gt;4.6 x 2.8mm Tactile Switch&lt;/h3&gt;

&lt;p&gt;&lt;a href="http://www.digikey.com/product-detail/en/KMR231NG%20LFS/CKN10246CT-ND/2176497"&gt;Example&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="W25Q64FVZPIG">
<packages>
<package name="SON127P600X500X80-9N">
</package>
</packages>
</library>
<library name="cap-master">
<description>&lt;b&gt;CAP MASTER! v4.02 - Electrolytic, Film and Tantalum&lt;/b&gt;&lt;br&gt;
&lt;p&gt;This library is a collection of SMD and through hole capacitors by various manufacturers. Some of these include types from Panasonic, Kemet, BC Components and others. Many of the packages were adapted from &lt;b&gt;rcl.lbr&lt;/b&gt; and &lt;b&gt;cap-pan40.lbr&lt;/b&gt; and have been renamed and grouped in a more logical form.&lt;/p&gt;&lt;p&gt;Silkscreen elements are a minimum of 8 mils in width with larger components using 10 mil widths. Most of the SMD components have text sizes of 0 .04" and thru-hole components are 0.05" in size.  A text ratio of 14 is used in both cases. Where practical, the elements are aligned on a 12.5 mil or 6.25 mil grid depending on the pad size and spacing.&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All capacitors are grouped by the following naming conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CNP-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP-&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;
&lt;small&gt;DISCLAIMER: The author does not warrant that this library is free from error or that it will meet your specific requirements.&lt;/small&gt;&lt;/p&gt;
&lt;author&gt;by Bob Starr (rtzaudio@mindspring.com)&lt;br&gt;
Updated 05/28/2005 - Rev 4.02&lt;/author&gt;&lt;br&gt;&lt;br&gt;</description>
<packages>
<package name="3528-21W/T">
<description>&lt;b&gt;SMD CHIP TANT&lt;/b&gt; - KEMET B / EIA 3528-21 Wave solder&lt;p&gt;
KEMET T / EIA 3528-12</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BTN_A" library="libavr-hvsp-programmer" package="TACTILE_SWITCH_PTH_6.0MM" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BTN_B" library="libavr-hvsp-programmer" package="TACTILE_SWITCH_PTH_6.0MM" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="100uf">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DOWN" library="libavr-hvsp-programmer" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="adafruit" package="SOT23-5L" value="MCP73831/OT"/>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6">
<attribute name="NAME"/>
</element>
<element name="LEFT" library="libavr-hvsp-programmer" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="0.3">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="150">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0805" value="150">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="2k">
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="2k">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="2k">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="2k">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RECT_PAD1" library="blinkinlabs" package="TEST_PAD_SMT" value="TEST_PAD_SMTRECT_PAD"/>
<element name="RECT_PAD2" library="blinkinlabs" package="TEST_PAD_SMT" value="TEST_PAD_SMTRECT_PAD"/>
<element name="RIGHT" library="libavr-hvsp-programmer" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPK1" library="adafruit" package="SMT-0540-S-R" value="SMT-0540-S-R"/>
<element name="U$1" library="oled_spi_154" package="OLED" value="OLED"/>
<element name="U$2" library="Dunks_tact" package="KPS-1290" value="SWITCH_SPDT">
<attribute name="PROD_ID" value="SWCH-10651"/>
</element>
<element name="U$4" library="DUNK" package="USB_MICRO_THRUHOLE" value="USB_MICROSMT+THRUHULE"/>
<element name="U$5" library="adafruit (2)" package="TQFP44" value="ATMEGA32U4-AU"/>
<element name="UP" library="libavr-hvsp-programmer" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="Ai_LED" package="LED-0603" value=""/>
<element name="LED2" library="Ai_LED" package="LED-0603" value=""/>
<element name="LED3" library="Ai_LED" package="LED-0603" value="power"/>
<element name="LED4" library="Ai_LED" package="LED-0603" value=""/>
<element name="SW1" library="SparkFun-Electromechanical" package="TACTILE_SWITCH_SMD_4.6X2.8MM" value="">
<attribute name="PROD_ID" value="SWCH-13065"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="SparkFun-FreqCtrl" package="CRYSTAL-SMD-5X3" value="CRYSTAL-GROUNDED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="Ai_LED" package="LED-0603" value="power"/>
<element name="R7" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="avr-7" package="SOIC8" value="TINY25/45/85-20SU"/>
<element name="R17" library="SparkFun-Resistors" package="0805" value="0.3">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="SparkFun-Resistors" package="0805" value="0.3">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="SparkFun-Resistors" package="0805" value="0.3">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="0.3">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="SparkFun-Resistors" package="0805" value="0.3">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED9" library="Ai_LED" package="LED-0603" value="power"/>
<element name="LED10" library="Ai_LED" package="LED-0603" value="power"/>
<element name="LED11" library="Ai_LED" package="LED-0603" value="power"/>
<element name="LED12" library="Ai_LED" package="LED-0603" value="power"/>
<element name="LED13" library="Ai_LED" package="LED-0603" value="power"/>
<element name="U2" library="W25Q64FVZPIG" package="SON127P600X500X80-9N" value="W25Q64FVZPIG">
<attribute name="PACKAGE" value="WSON-8 Winbond"/>
<attribute name="MF" value="Winbond"/>
<attribute name="PRICE" value="None"/>
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Ic Flash 64mbit 104mhz 8wson "/>
<attribute name="MP" value="W25Q64FVZPIG"/>
</element>
<element name="R23" library="SparkFun-Resistors" package="0805" value="0.3">
<attribute name="PROD_ID" value="RES-11622"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED14" library="adafruit" package="RGBLED5050" value="RGBLED5050"/>
<element name="LED15" library="adafruit" package="RGBLED5050" value="RGBLED5050"/>
<element name="C1" library="cap-master" package="3528-21W/T" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="DOWN">
<contactref element="DOWN" pad="1"/>
<contactref element="DOWN" pad="2"/>
<contactref element="U$5" pad="39"/>
</signal>
<signal name="LEFT">
<contactref element="LEFT" pad="3"/>
<contactref element="LEFT" pad="4"/>
<contactref element="U$5" pad="38"/>
</signal>
<signal name="RIGHT">
<contactref element="RIGHT" pad="1"/>
<contactref element="RIGHT" pad="2"/>
<contactref element="U$5" pad="37"/>
</signal>
<signal name="A">
<contactref element="BTN_A" pad="1"/>
<contactref element="BTN_A" pad="2"/>
<contactref element="U$5" pad="1"/>
</signal>
<signal name="B">
<contactref element="BTN_B" pad="1"/>
<contactref element="BTN_B" pad="2"/>
<contactref element="U$5" pad="28"/>
</signal>
<signal name="VCC">
<contactref element="U$5" pad="14"/>
<contactref element="U$5" pad="34"/>
<contactref element="U$5" pad="44"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$5" pad="24"/>
<contactref element="ISP1" pad="2"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="R5" pad="1"/>
<contactref element="U$2" pad="S"/>
<contactref element="R6" pad="2"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="R7" pad="2"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="7"/>
<contactref element="R23" pad="1"/>
<contactref element="LED14" pad="3"/>
<contactref element="LED15" pad="2"/>
<contactref element="LED15" pad="1"/>
<contactref element="LED15" pad="3"/>
<contactref element="LED14" pad="2"/>
<contactref element="LED14" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="U$6" pad="8"/>
<contactref element="R9" pad="2"/>
<contactref element="R22" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="SCK"/>
<contactref element="ISP1" pad="3"/>
<contactref element="U$5" pad="9"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="SDA"/>
<contactref element="ISP1" pad="4"/>
<contactref element="U$5" pad="10"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="RX_LED">
<contactref element="R16" pad="1"/>
<contactref element="U$5" pad="8"/>
</signal>
<signal name="MISO">
<contactref element="ISP1" pad="1"/>
<contactref element="U$5" pad="11"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="TX_LED">
<contactref element="R14" pad="1"/>
<contactref element="U$5" pad="22"/>
</signal>
<signal name="GND">
<contactref element="LEFT" pad="1"/>
<contactref element="UP" pad="3"/>
<contactref element="DOWN" pad="3"/>
<contactref element="RIGHT" pad="3"/>
<contactref element="BTN_A" pad="3"/>
<contactref element="BTN_B" pad="3"/>
<contactref element="BTN_A" pad="4"/>
<contactref element="BTN_B" pad="4"/>
<contactref element="LEFT" pad="2"/>
<contactref element="UP" pad="4"/>
<contactref element="DOWN" pad="4"/>
<contactref element="RIGHT" pad="4"/>
<contactref element="IC3" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U$4" pad="PIN$5"/>
<contactref element="U$5" pad="5"/>
<contactref element="U$5" pad="15"/>
<contactref element="U$5" pad="23"/>
<contactref element="U$5" pad="35"/>
<contactref element="U$5" pad="43"/>
<contactref element="ISP1" pad="6"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U$5" pad="42"/>
<contactref element="C4" pad="2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="LED3" pad="C"/>
<contactref element="RECT_PAD1" pad="P$1"/>
<contactref element="SW1" pad="3"/>
<contactref element="SW1" pad="4"/>
<contactref element="U$3" pad="4"/>
<contactref element="U$3" pad="2"/>
<contactref element="LED7" pad="C"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="9"/>
<contactref element="C1" pad="-"/>
<contactref element="C5" pad="1"/>
<contactref element="U$6" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="R13" pad="2"/>
<contactref element="LED14" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="R15" pad="2"/>
<contactref element="LED14" pad="6"/>
</signal>
<signal name="N$12">
<contactref element="R19" pad="2"/>
<contactref element="LED14" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="R12" pad="2"/>
<contactref element="LED15" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="R11" pad="2"/>
<contactref element="LED15" pad="6"/>
</signal>
<signal name="N$16">
<contactref element="R10" pad="2"/>
<contactref element="LED15" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="U$5" pad="19"/>
<contactref element="U2" pad="1"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="VUSB">
<contactref element="IC3" pad="4"/>
<contactref element="C4" pad="1"/>
<contactref element="U$4" pad="PIN$1"/>
<contactref element="U$5" pad="7"/>
<contactref element="U$5" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="BTN_RST">
<contactref element="U$5" pad="13"/>
<contactref element="R5" pad="2"/>
<contactref element="ISP1" pad="5"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="BLUE">
<contactref element="R12" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="U$5" pad="30"/>
</signal>
<signal name="RED">
<contactref element="R10" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="U$5" pad="29"/>
</signal>
<signal name="GREEN">
<contactref element="R11" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="U$5" pad="12"/>
</signal>
<signal name="TX_LED_R">
<contactref element="R14" pad="2"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="RX_LED_R">
<contactref element="R16" pad="2"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="D+">
<contactref element="U$4" pad="PIN$3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="D-">
<contactref element="U$4" pad="PIN$2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC3" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="CS">
<contactref element="U$1" pad="CS"/>
<contactref element="U$5" pad="26"/>
</signal>
<signal name="N$22">
<contactref element="U$5" pad="17"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="U$5" pad="16"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="UCAP">
<contactref element="U$5" pad="6"/>
<contactref element="C1" pad="+"/>
</signal>
<signal name="SPK1+">
<contactref element="SPK1" pad="+"/>
<contactref element="U$5" pad="31"/>
</signal>
<signal name="N$28">
<contactref element="U$5" pad="33"/>
</signal>
<signal name="UP">
<contactref element="U$5" pad="36"/>
<contactref element="UP" pad="1"/>
<contactref element="UP" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U$5" pad="20"/>
</signal>
<signal name="N$7">
<contactref element="U$5" pad="21"/>
</signal>
<signal name="DC">
<contactref element="U$5" pad="25"/>
<contactref element="U$1" pad="DC"/>
</signal>
<signal name="OLED_RES">
<contactref element="U$5" pad="27"/>
<contactref element="U$1" pad="RES"/>
</signal>
<signal name="N$5">
<contactref element="U$5" pad="18"/>
</signal>
<signal name="SPK2+">
<contactref element="U$5" pad="32"/>
<contactref element="SPK1" pad="-"/>
</signal>
<signal name="N$38">
<contactref element="U$5" pad="41"/>
</signal>
<signal name="N$39">
<contactref element="U$5" pad="40"/>
</signal>
<signal name="VBATT">
<contactref element="IC3" pad="3"/>
<contactref element="RECT_PAD2" pad="P$1"/>
<contactref element="U$2" pad="P"/>
</signal>
<signal name="N$25">
<contactref element="U$5" pad="3"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="U$5" pad="4"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R6" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="LED4" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="LED7" pad="A"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U$6" pad="3"/>
<contactref element="LED9" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="U$6" pad="2"/>
<contactref element="LED10" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="U$6" pad="7"/>
<contactref element="LED11" pad="A"/>
</signal>
<signal name="N$21">
<contactref element="U$6" pad="6"/>
<contactref element="LED12" pad="A"/>
</signal>
<signal name="N$24">
<contactref element="U$6" pad="5"/>
<contactref element="LED13" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="R9" pad="1"/>
<contactref element="LED9" pad="C"/>
</signal>
<signal name="N$26">
<contactref element="R22" pad="1"/>
<contactref element="LED10" pad="C"/>
</signal>
<signal name="N$29">
<contactref element="R21" pad="1"/>
<contactref element="LED11" pad="C"/>
</signal>
<signal name="N$30">
<contactref element="R20" pad="1"/>
<contactref element="LED12" pad="C"/>
</signal>
<signal name="N$32">
<contactref element="R17" pad="1"/>
<contactref element="LED13" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
