(kicad_pcb (version 20171130) (host pcbnew 5.1.5)
  (general
    (thickness 1.6)
    (drawings 46)
    (tracks 381)
    (zones 0)
    (modules 8)
    (nets 58)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(A0-Pad16)")
  (net 2 "Net-(A0-Pad15)")
  (net 3 "Net-(A0-Pad30)")
  (net 4 "Net-(A0-Pad14)")
  (net 5 GND)
  (net 6 "Net-(A0-Pad13)")
  (net 7 "Net-(A0-Pad28)")
  (net 8 "Net-(A0-Pad12)")
  (net 9 +5V)
  (net 10 "Net-(A0-Pad11)")
  (net 11 "Net-(A0-Pad26)")
  (net 12 "Net-(A0-Pad10)")
  (net 13 "Net-(A0-Pad25)")
  (net 14 "Net-(A0-Pad9)")
  (net 15 "Net-(A0-Pad24)")
  (net 16 "Net-(A0-Pad8)")
  (net 17 "Net-(A0-Pad23)")
  (net 18 "Net-(A0-Pad7)")
  (net 19 "Net-(A0-Pad22)")
  (net 20 "Net-(A0-Pad6)")
  (net 21 "Net-(A0-Pad21)")
  (net 22 "Net-(A0-Pad5)")
  (net 23 "Net-(A0-Pad20)")
  (net 24 "Net-(A0-Pad19)")
  (net 25 "Net-(A0-Pad3)")
  (net 26 "Net-(A0-Pad18)")
  (net 27 "Net-(A0-Pad2)")
  (net 28 "Net-(A0-Pad17)")
  (net 29 "Net-(A0-Pad1)")
  (net 30 "Net-(U0-Pad7)")
  (net 31 "Net-(U0-Pad14)")
  (net 32 "Net-(U0-Pad6)")
  (net 33 "Net-(U0-Pad13)")
  (net 34 "Net-(U0-Pad5)")
  (net 35 "Net-(U0-Pad12)")
  (net 36 "Net-(U0-Pad4)")
  (net 37 "Net-(U0-Pad11)")
  (net 38 "Net-(U0-Pad10)")
  (net 39 "Net-(U0-Pad9)")
  (net 40 "Net-(U1-Pad7)")
  (net 41 "Net-(U1-Pad14)")
  (net 42 "Net-(U1-Pad6)")
  (net 43 "Net-(U1-Pad13)")
  (net 44 "Net-(U1-Pad5)")
  (net 45 "Net-(U1-Pad12)")
  (net 46 "Net-(U1-Pad4)")
  (net 47 "Net-(U1-Pad11)")
  (net 48 "Net-(U1-Pad10)")
  (net 49 "Net-(U1-Pad9)")
  (net 50 "Net-(U2-Pad15)")
  (net 51 "Net-(U2-Pad14)")
  (net 52 "Net-(U2-Pad13)")
  (net 53 "Net-(U2-Pad5)")
  (net 54 "Net-(U2-Pad12)")
  (net 55 "Net-(U2-Pad4)")
  (net 56 "Net-(U2-Pad2)")
  (net 57 "Net-(U2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(A0-Pad1)")
    (add_net "Net-(A0-Pad10)")
    (add_net "Net-(A0-Pad11)")
    (add_net "Net-(A0-Pad12)")
    (add_net "Net-(A0-Pad13)")
    (add_net "Net-(A0-Pad14)")
    (add_net "Net-(A0-Pad15)")
    (add_net "Net-(A0-Pad16)")
    (add_net "Net-(A0-Pad17)")
    (add_net "Net-(A0-Pad18)")
    (add_net "Net-(A0-Pad19)")
    (add_net "Net-(A0-Pad2)")
    (add_net "Net-(A0-Pad20)")
    (add_net "Net-(A0-Pad21)")
    (add_net "Net-(A0-Pad22)")
    (add_net "Net-(A0-Pad23)")
    (add_net "Net-(A0-Pad24)")
    (add_net "Net-(A0-Pad25)")
    (add_net "Net-(A0-Pad26)")
    (add_net "Net-(A0-Pad28)")
    (add_net "Net-(A0-Pad3)")
    (add_net "Net-(A0-Pad30)")
    (add_net "Net-(A0-Pad5)")
    (add_net "Net-(A0-Pad6)")
    (add_net "Net-(A0-Pad7)")
    (add_net "Net-(A0-Pad8)")
    (add_net "Net-(A0-Pad9)")
    (add_net "Net-(U0-Pad10)")
    (add_net "Net-(U0-Pad11)")
    (add_net "Net-(U0-Pad12)")
    (add_net "Net-(U0-Pad13)")
    (add_net "Net-(U0-Pad14)")
    (add_net "Net-(U0-Pad4)")
    (add_net "Net-(U0-Pad5)")
    (add_net "Net-(U0-Pad6)")
    (add_net "Net-(U0-Pad7)")
    (add_net "Net-(U0-Pad9)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
  )
  (module fourteenSegDisplay-OnACard:LTP-3784 (layer F.Cu) (tedit 5DE732E6)
    (at 111.252 25.908)
    (fp_text reference U3 (at -9.652 0 180) (layer F.SilkS))
    (fp_text value LTP-3784 (at 0 0) (layer F.Fab))
    (pad 18 thru_hole oval (at -8.636 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 33 "Net-(U0-Pad13)"))
    (pad 1 thru_hole oval (at -8.636 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 31 "Net-(U0-Pad14)"))
    (pad 17 thru_hole oval (at -6.096 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad13)"))
    (pad 2 thru_hole oval (at -6.096 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad7)"))
    (pad 16 thru_hole oval (at -3.556 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 51 "Net-(U2-Pad14)"))
    (pad 3 thru_hole oval (at -3.556 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at -1.016 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 35 "Net-(U0-Pad12)"))
    (pad 4 thru_hole oval (at -1.016 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad6)"))
    (pad 14 thru_hole oval (at 1.524 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 37 "Net-(U0-Pad11)"))
    (pad 5 thru_hole oval (at 1.524 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 44 "Net-(U1-Pad5)"))
    (pad 13 thru_hole oval (at 4.064 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad14)"))
    (pad 6 thru_hole oval (at 4.064 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 46 "Net-(U1-Pad4)"))
    (pad 12 thru_hole oval (at 6.604 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 36 "Net-(U0-Pad4)"))
    (pad 7 thru_hole oval (at 6.604 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 30 "Net-(U0-Pad7)"))
    (pad 11 thru_hole oval (at 9.144 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 52 "Net-(U2-Pad13)"))
    (pad 8 thru_hole oval (at 9.144 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 11.684 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 34 "Net-(U0-Pad5)"))
    (pad 9 thru_hole oval (at 11.684 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 32 "Net-(U0-Pad6)"))
  )
  (module fourteenSegDisplay-OnACard:LTP-3784 (layer F.Cu) (tedit 5DE732E6)
    (at 85.344 25.908)
    (fp_text reference U4 (at -9.652 0 180) (layer F.SilkS))
    (fp_text value LTP-3784 (at 0 0) (layer F.Fab))
    (pad 18 thru_hole oval (at -8.636 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 33 "Net-(U0-Pad13)"))
    (pad 1 thru_hole oval (at -8.636 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 31 "Net-(U0-Pad14)"))
    (pad 17 thru_hole oval (at -6.096 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad13)"))
    (pad 2 thru_hole oval (at -6.096 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad7)"))
    (pad 16 thru_hole oval (at -3.556 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 54 "Net-(U2-Pad12)"))
    (pad 3 thru_hole oval (at -3.556 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at -1.016 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 35 "Net-(U0-Pad12)"))
    (pad 4 thru_hole oval (at -1.016 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad6)"))
    (pad 14 thru_hole oval (at 1.524 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 37 "Net-(U0-Pad11)"))
    (pad 5 thru_hole oval (at 1.524 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 44 "Net-(U1-Pad5)"))
    (pad 13 thru_hole oval (at 4.064 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad14)"))
    (pad 6 thru_hole oval (at 4.064 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 46 "Net-(U1-Pad4)"))
    (pad 12 thru_hole oval (at 6.604 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 36 "Net-(U0-Pad4)"))
    (pad 7 thru_hole oval (at 6.604 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 30 "Net-(U0-Pad7)"))
    (pad 11 thru_hole oval (at 9.144 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 50 "Net-(U2-Pad15)"))
    (pad 8 thru_hole oval (at 9.144 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 11.684 -5.588) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 34 "Net-(U0-Pad5)"))
    (pad 9 thru_hole oval (at 11.684 9.652) (size 1.25 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 32 "Net-(U0-Pad6)"))
  )
  (module MountingHole:MountingHole_2mm (layer F.Cu) (tedit 5B924920)
    (at 122.936 14.732)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2mm (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2mm (layer F.Cu) (tedit 5B924920)
    (at 76.2 14.732)
    (descr "Mounting Hole 2mm, no annular")
    (tags "mounting hole 2mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2mm (at 0 3.1) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 113.284 47.244)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 0.508) (layer F.SilkS))
    (fp_text value 4051 (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(U2-Pad15)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(U2-Pad14)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(U2-Pad13)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(U2-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(U2-Pad12)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(U2-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U1-Pad12)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U1-Pad11)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(U2-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(U2-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 98.044 47.244)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 0.508) (layer F.SilkS))
    (fp_text value 4094 (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad7)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad14)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad13)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U1-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U1-Pad12)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U1-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U1-Pad11)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(A0-Pad6)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(U1-Pad10)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U0-Pad9)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(U1-Pad9)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(A0-Pad7)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 82.804 47.244)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U0 (at 3.81 0.508) (layer F.SilkS))
    (fp_text value 4094 (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U0-Pad7)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U0-Pad14)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U0-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U0-Pad13)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U0-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U0-Pad12)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U0-Pad4)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U0-Pad11)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(A0-Pad6)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(U0-Pad10)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(A0-Pad5)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U0-Pad9)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(A0-Pad7)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:Arduino_Nano (layer F.Cu) (tedit 58ACAF70)
    (at 118.364 73.152 270)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (fp_text reference A0 (at 7.62 40.64) (layer F.SilkS))
    (fp_text value Arduino_Nano_v3.x (at 8.89 19.05) (layer F.Fab))
    (fp_text user %R (at 6.35 19.05) (layer F.Fab))
    (pad 16 thru_hole oval (at 15.24 35.56 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(A0-Pad16)"))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(A0-Pad15)"))
    (pad 30 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(A0-Pad30)"))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(A0-Pad14)"))
    (pad 29 thru_hole oval (at 15.24 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(A0-Pad13)"))
    (pad 28 thru_hole oval (at 15.24 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(A0-Pad28)"))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(A0-Pad12)"))
    (pad 27 thru_hole oval (at 15.24 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(A0-Pad11)"))
    (pad 26 thru_hole oval (at 15.24 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(A0-Pad26)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(A0-Pad10)"))
    (pad 25 thru_hole oval (at 15.24 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(A0-Pad25)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(A0-Pad9)"))
    (pad 24 thru_hole oval (at 15.24 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(A0-Pad24)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(A0-Pad8)"))
    (pad 23 thru_hole oval (at 15.24 17.78 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(A0-Pad23)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(A0-Pad7)"))
    (pad 22 thru_hole oval (at 15.24 20.32 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(A0-Pad22)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(A0-Pad6)"))
    (pad 21 thru_hole oval (at 15.24 22.86 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(A0-Pad21)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(A0-Pad5)"))
    (pad 20 thru_hole oval (at 15.24 25.4 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(A0-Pad20)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 19 thru_hole oval (at 15.24 27.94 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(A0-Pad19)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(A0-Pad3)"))
    (pad 18 thru_hole oval (at 15.24 30.48 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(A0-Pad18)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(A0-Pad2)"))
    (pad 17 thru_hole oval (at 15.24 33.02 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(A0-Pad17)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(A0-Pad1)"))
    (model ${KISYS3DMOD}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "www.cculysses.com\nwww.cs.uml.edu/~~ccook\ngithub.com/cSquaerd (not a typo)\ncook.char.p@gmail.com" (at 111.76 80.264) (layer B.SilkS))
  (gr_text "Attach Headers or Pins to these\npoints if you want to keep your\nArduino separate from the board." (at 81.788 84.328) (layer F.SilkS))
  (gr_text GND (at 115.824 85.344 90) (layer F.SilkS))
  (gr_text "VDD (+5V)" (at 110.744 82.804 90) (layer F.SilkS))
  (gr_text GND (at 110.744 76.2 270) (layer F.SilkS))
  (gr_text STROBE (at 103.124 77.724 270) (layer F.SilkS))
  (gr_text CLOCK (at 105.664 77.216 270) (layer F.SilkS))
  (gr_text DATA (at 108.204 76.708 270) (layer F.SilkS))
  (gr_text "Fourteen Segment Display Revolving Message Board\nDesigned by Charlie Cook\n" (at 101.6 40.132) (layer F.SilkS))
  (gr_text "VERSION 2" (at 75.184 55.88 90) (layer B.Cu))
  (gr_text "Arduino Nano" (at 100.584 70.612) (layer F.SilkS))
  (gr_text 4051-MUX (at 116.332 67.564) (layer F.SilkS))
  (gr_text 4094-HIGH (at 101.6 67.564) (layer F.SilkS))
  (gr_text 4094-LOW (at 85.852 67.564) (layer F.SilkS))
  (gr_line (start 73.66 89.916) (end 73.66 12.192) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.984 89.916) (end 73.66 89.916) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.984 12.192) (end 125.984 89.916) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 73.66 12.192) (end 125.984 12.192) (layer Edge.Cuts) (width 0.05))
  (zone (net 9) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 90.424) (xy 73.152 90.424) (xy 73.152 11.684) (xy 126.492 11.684)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 90.424) (xy 73.152 90.424) (xy 73.152 11.684) (xy 126.492 11.684)
      )
    )
  )
)
