(kicad_pcb (version 4) (host pcbnew 4.0.3-rc7-stable)
  (general
    (links 41)
    (no_connects 0)
    (area 99.924999 49.924999 142.575001 79.075001)
    (thickness 1.6)
    (drawings 26)
    (tracks 142)
    (zones 0)
    (modules 14)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.1)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.55 1)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 100 79)
    (grid_origin 100 50)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 GPIO12)
  (net 5 "Net-(U1-Pad9)")
  (net 6 "Net-(U1-Pad10)")
  (net 7 "Net-(U1-Pad11)")
  (net 8 "Net-(U1-Pad13)")
  (net 9 "Net-(U1-Pad14)")
  (net 10 ADC)
  (net 11 GPIO14)
  (net 12 GPIO13)
  (net 13 "Net-(R3-Pad1)")
  (net 14 "Net-(U1-Pad17)")
  (net 15 GPIO0)
  (net 16 GPIO4)
  (net 17 GPIO5)
  (net 18 RXD)
  (net 19 TXD)
  (net 20 "Net-(P1-Pad2)")
  (net 21 "Net-(P1-Pad3)")
  (net 22 "Net-(P1-Pad4)")
  (net 23 "Net-(U1-Pad12)")
  (net 24 CH_PD)
  (net 25 RST)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net ADC)
    (add_net CH_PD)
    (add_net GND)
    (add_net GPIO0)
    (add_net GPIO12)
    (add_net GPIO13)
    (add_net GPIO14)
    (add_net GPIO4)
    (add_net GPIO5)
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad9)")
    (add_net RST)
    (add_net RXD)
    (add_net TXD)
  )
  (net_class 5v ""
    (clearance 0.2)
    (trace_width 0.75)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57810DC1)
    (at 111.2 61.3 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 0 -2.25 90) (layer F.SilkS))
    (fp_text value AP1117D15 (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 570ABF3C)
    (at 107.75 61 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.75 0 360) (layer F.SilkS))
    (fp_text value 10uf (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 570ABF50)
    (at 114.25 61 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.75 0 180) (layer F.SilkS))
    (fp_text value 10uf (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 570ABDC3)
    (at 122.5 58.5 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -3 0 90) (layer F.SilkS))
    (fp_text value 100nf (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 570AFC4E)
    (at 115.5 70.25 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 3 0 180) (layer F.SilkS))
    (fp_text value 100nf (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 GPIO4))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP8266:ESP-12E (layer F.Cu) (tedit 570ABEEB)
    (at 140.75 56 270)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U1 (at 8.75 7.5 270) (layer F.SilkS))
    (fp_text value ESP-12E (at 8 1 270) (layer F.Fab))
    (fp_text user "No Copper" (at 7.9 -5.4 270) (layer F.CrtYd))
    (pad 9 smd oval (at 2.99 15.75) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad9)"))
    (pad 10 smd oval (at 4.99 15.75) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad10)"))
    (pad 11 smd oval (at 6.99 15.75) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad11)"))
    (pad 12 smd oval (at 8.99 15.75) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad12)"))
    (pad 13 smd oval (at 10.99 15.75) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad13)"))
    (pad 14 smd oval (at 12.99 15.75) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad14)"))
    (pad 1 smd rect (at 0 0 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 RST))
    (pad 2 smd oval (at 0 2 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 10 ADC))
    (pad 3 smd oval (at 0 4 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 24 CH_PD))
    (pad 4 smd oval (at 0 6 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 25 RST))
    (pad 5 smd oval (at 0 8 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 11 GPIO14))
    (pad 6 smd oval (at 0 10 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 GPIO12))
    (pad 7 smd oval (at 0 12 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 12 GPIO13))
    (pad 8 smd oval (at 0 14 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 15 smd oval (at 16 14 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 16 smd oval (at 16 12 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (pad 17 smd oval (at 16 10 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad17)"))
    (pad 18 smd oval (at 16 8 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 15 GPIO0))
    (pad 19 smd oval (at 16 6 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 16 GPIO4))
    (pad 20 smd oval (at 16 4 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 17 GPIO5))
    (pad 21 smd oval (at 16 2 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 18 RXD))
    (pad 22 smd oval (at 16 0 270) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 19 TXD))
    (model ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0.04 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:USB_Micro-B (layer F.Cu) (tedit 57811738)
    (at 102.5 64.225 270)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference P1 (at 0 -3.45 270) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at 0 4.8 270) (layer F.Fab))
    (pad 1 smd rect (at -1.3009 -1.56254) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -0.6509 -1.56254) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at -0.0009 -1.56254) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 0.6491 -1.56254) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P1-Pad4)"))
    (pad 5 smd rect (at 1.2991 -1.56254) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -2.5009 -1.56254) (size 1 1) (drill 0.55) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at 2.4991 -1.56254) (size 1 1) (drill 0.55) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole oval (at -3.5009 1.13746) (size 1.55 1) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 6 thru_hole oval (at 3.4991 1.13746) (size 1.55 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model "/Library/Application Support/kicad/packages3d/conn_pc/usb_B_micro_smd.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 570ABD21)
    (at 110.5 53.8 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value CONN_02X03 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 TXD))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 RXD))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 GPIO0))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 CH_PD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 570ABD40)
    (at 113.2 55.3 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 3 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 GPIO0))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 570ABDEA)
    (at 136.8 52.5 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.5 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 CH_PD))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 570ABDD4)
    (at 127.75 74.75 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -3 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 570ABDEC)
    (at 134.8 52.5 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 RST))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 570ABD60)
    (at 115.5 68.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 3 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 GPIO4))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_jst-ph:s8b-ph-kl (layer F.Cu) (tedit 578116CF)
    (at 115.5 72.5)
    (descr "JST PH series connector, S8B-PH-KL")
    (fp_text reference P3 (at -5.75 -3.75 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 7.80034) (layer F.Fab))
    (pad 1 thru_hole rect (at -7.00024 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole oval (at -5.00126 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 17 GPIO5))
    (pad 3 thru_hole oval (at -2.99974 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 4 thru_hole oval (at -1.00076 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 16 GPIO4))
    (pad 5 thru_hole oval (at 1.00076 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.99974 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 2))
    (pad 7 thru_hole oval (at 5.00126 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 12 GPIO13))
    (pad 8 thru_hole oval (at 7.00024 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model walter/conn_jst-ph/s8b-ph-kl.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 100.975 67.75) (end 101.8 67.75) (angle 90) (layer Edge.Cuts) (width 0.5))
  (gr_line (start 101.775 60.575) (end 101.775 60.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.95 60.75) (end 101.775 60.75) (angle 90) (layer Edge.Cuts) (width 0.5))
  (gr_line (start 101.875 60.775) (end 101.875 60.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.8 60.9) (end 100.8 60.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.9 60.6) (end 101.9 60.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "ESP HammondBox 0.4" (at 129.8 51.475 180) (layer B.SilkS))
  (gr_text z2amiller (at 115.325 77.5) (layer B.SilkS))
  (gr_text PROG (at 103.1 54.9 90) (layer F.SilkS))
  (gr_text "USB PWR" (at 106 64 270) (layer F.SilkS))
  (gr_line (start 142.5 79) (end 106.25 79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 50) (end 142.25 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.5 50) (end 100 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.5 50.5) (end 142.5 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 136.75 76.25) (end 136.5 77.5) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 117 52.75) (end 117 51.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 72.75) (end 100.25 72.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 50) (end 100 72.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.25 75.5) (end 106.25 79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 72.75) (end 102.75 72.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104 72.75) (end 100 72.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 103.75 75.25) (end 104 72.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 50.5) (end 100 50) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.5 79) (end 142.5 50.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.25 78.75) (xy 106.5 78.75) (xy 106.5 74) (xy 105 72.5) (xy 100.25 72.5)
        (xy 100.25 50.25) (xy 142.25 50.25) (xy 142.25 78.75)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.75 57.75) (xy 120.75 57.75) (xy 117.5 61) (xy 111.25 61) (xy 111.25 57.5)
        (xy 105.5 57.5) (xy 105.5 53.5) (xy 113.25 53.5) (xy 114.25 52.5) (xy 127.75 52.5)
        (xy 127.75 57.75)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.475 64.35) (xy 105.5 64.35) (xy 105.5 63.125) (xy 103.175 63.125) (xy 103.175 58.05)
        (xy 110.975 58.05) (xy 110.975 64.35)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.8 50.25) (xy 142.25 50.25) (xy 142.25 78.75) (xy 106.75 78.75) (xy 106.75 74.25)
        (xy 105 72.5) (xy 100 72.5) (xy 100 50.25) (xy 102.5 50.35) (xy 102.5 50.2)
        (xy 128.8 50.2) (xy 128.8 50.25)
      )
    )
    (polygon
      (pts        (xy 114.2 52.3) (xy 113.2 53.3) (xy 105.2 53.3) (xy 105.2 57.8) (xy 102.5 57.8)
        (xy 102.5 64) (xy 105.025 64) (xy 104.95 64.075) (xy 104.95 65.3) (xy 111.275 65.3)
        (xy 111.275 62) (xy 118.25 62) (xy 121 59.25) (xy 128.75 59.25) (xy 128.75 52.3)
        (xy 114.2 52.3)
      )
    )
  )
)
