<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<text>G</text>
<text>G</text>
<text>G</text>
<text>5V</text>
<text>5V</text>
<text>AC</text>
<text>AC</text>
<text>VRECT</text>
<text>www.smbaker.com</text>
<text>www.smbaker.com</text>
</plain>
<libraries>
<library name="resistor">
<packages>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="E2,5-7">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 7 mm</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="DO201-15">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 5.6 mm, horizontal, grid 15.24 mm</description>
</package>
</packages>
</library>
<library name="scott">
<packages>
<package name="DCJACK">
<description>&lt;b&gt;DC POWER JACK&lt;/b&gt;&lt;p&gt;
Source: DCJ0202.pdf</description>
</package>
</packages>
</library>
<library name="inductor-neosid">
<packages>
<package name="BS11">
<description>NOMINAL &lt;b&gt;INDUCTANCE&lt;/b&gt;&lt;p&gt;
grid 5 mm, diameter 10.5 mm, height 13.5 mm</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-17">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="scott-new">
<packages>
<package name="TO220-52">
<description>&lt;b&gt;Transistor Outline Package&lt;/b&gt;&lt;p&gt;
P-TO220-5-2 SIEMENS TLE4270</description>
</package>
</packages>
</library>
<library name="raspberrypi_bastelstube_v13">
<description>&lt;b&gt;Raspberry Pi&lt;/b&gt; by &lt;b&gt;Martin's Bastelstube&lt;/b&gt;
&lt;p&gt;
Different shapes of piggyback boards for the famous &amp;amp; fabulous
&lt;a href="http://www.raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt; computer.
&lt;p&gt;
The outline of the Raspberry Pi board is drawn on layer 52 bDocu, so you can make it invisible if necessary.&lt;br/&gt;
Recommendation: Start your design with RASPI_BOARD_*_FULL, so you are aware of all the big components and
connectors when you're drawing the dimensions of your board and placing your own components.&lt;br/&gt;
Later, you can simply change the package of your Raspberry Pi connector to the RASPI_BOARD_*_EDGES type,
so you can concentrate on your own design.
&lt;p&gt;
Most of my board packages don't have the outline drawn in layer 20 Dimension (except the HATs). This allows you to deviate from the original Raspberry Pi board shape, e.g. when you need more space behind the GPIO connector for the routing of the power supply lines. If you want to stick exactly to the Raspberry Pi board shape, then just draw the Dimension layer right on the lines in layer bDocu.

&lt;hr&gt;&lt;br/&gt;

Version 1.3
&lt;ul&gt;
&lt;li&gt;Added the shape and dimensions of the HAT board with &amp;amp; without the camera and display flex cutout&lt;/li&gt;
&lt;li&gt;New GPIO connector version (suffix &amp;quot;#&amp;quot;) with all pins connected (no more &amp;quot;n.c.&amp;quot; pins)&lt;/li&gt;
&lt;li&gt;Two more &amp;quot;AB-&amp;quot; boards with 5 and 6 drill holes / pads, mechanically compatible with all RasPi versions&lt;/li&gt;
&lt;/ul&gt;

Version 1.2
&lt;ul&gt;
&lt;li&gt;Added a 26-pin GPIO connector with board dimensions of model B+&lt;br/&gt;
       for backwards compatibility with models A and B, named &amp;quot;B-&amp;quot;&lt;/li&gt;
&lt;/ul&gt;

Version 1.1
&lt;ul&gt;
&lt;li&gt;New GPIO connector and board dimensions of model B+&lt;/li&gt;
&lt;li&gt;Old connector and board (for models A and B) renamed to AB&lt;/li&gt;
&lt;li&gt;GPIO pin numbers on connector changed to match Rev2 board design&lt;/li&gt;
&lt;/ul&gt;

Version 1.0
&lt;ul&gt;
&lt;li&gt;More detailed descriptions for all components&lt;/li&gt;
&lt;li&gt;Published on Cadsoft webpage&lt;/li&gt;
&lt;/ul&gt;

&lt;hr&gt;&lt;br/&gt;

Designed by &lt;a href="http://bastelstube.rocci.net/"&gt;Martin's Bastelstube&lt;/a&gt;&lt;br&gt;
Comments / complaints / bug reports / suggestions to &lt;author&gt;eightbit@web.de&lt;/author&gt;</description>
<packages>
<package name="RASPI_BOARD_B+_FULL">
<description>Raspberry Pi board model B+, full outline with position of big connectors &amp;amp; drill holes</description>
</package>
</packages>
</library>
<library name="con-wago-508">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-132">
<description>&lt;b&gt;WAGO SREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C10" library="resistor" package="E2,5-7" value="1000uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="resistor" package="E2,5-7" value="100uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="DO41-10" value="1n4005"/>
<element name="D2" library="diode" package="DO41-10" value="1n4005"/>
<element name="D3" library="diode" package="DO41-10" value="1N4005"/>
<element name="D4" library="diode" package="DO41-10" value="1n4005"/>
<element name="D5" library="diode" package="DO201-15" value="1n5822"/>
<element name="J1" library="scott" package="DCJACK" value="DCJACK">
<attribute name="NAME"/>
</element>
<element name="L2" library="inductor-neosid" package="BS11" value="100UH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="0204/7" value=""/>
<element name="R2" library="resistor" package="0204/7" value=""/>
<element name="SJ1" library="jumper" package="SJ" value=""/>
<element name="TP1" library="testpad" package="P1-17" value="PTR1PAD1-17">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP2" library="testpad" package="P1-13" value="PTR1PAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="U$1" library="scott-new" package="TO220-52" value="LM2576-THROUGHHOLEHORIZ">
<attribute name="NAME"/>
</element>
<element name="X1" library="raspberrypi_bastelstube_v13" package="RASPI_BOARD_B+_FULL" value="RASPI_BOARD_B+_F"/>
<element name="X2" library="con-wago-508" package="W237-132" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="JP1" library="jumper" package="JP1" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="jumper" package="SJ" value=""/>
<element name="L1" library="inductor-neosid" package="BS11" value="10UH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="resistor" package="E2,5-5" value="10uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="scott" package="DCJACK" value="DCJACK">
<attribute name="NAME"/>
</element>
<element name="JP2" library="jumper" package="JP1" value="">
<attribute name="VALUE"/>
</element>
<element name="X3" library="con-wago-508" package="W237-132" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="SJ3" library="jumper" package="SJ" value=""/>
<element name="SJ4" library="jumper" package="SJ" value=""/>
<element name="C2" library="resistor" package="E2,5-7" value="100uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="3V3">
<contactref element="X1" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="U$1" pad="1"/>
<contactref element="C9" pad="+"/>
<contactref element="D1" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="JP2" pad="2"/>
<contactref element="SJ3" pad="1"/>
<contactref element="C2" pad="+"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="3"/>
<contactref element="C9" pad="-"/>
<contactref element="D5" pad="A"/>
<contactref element="C10" pad="-"/>
<contactref element="R2" pad="1"/>
<contactref element="D4" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="TP1" pad="TP"/>
<contactref element="TP2" pad="TP"/>
<contactref element="JP1" pad="1"/>
<contactref element="X1" pad="6"/>
<contactref element="C1" pad="-"/>
<contactref element="JP2" pad="1"/>
<contactref element="X3" pad="1"/>
<contactref element="SJ4" pad="2"/>
<contactref element="C2" pad="-"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="2"/>
<contactref element="L2" pad="1"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="+5V">
<contactref element="JP1" pad="2"/>
<contactref element="SJ2" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="L1" pad="2"/>
<contactref element="X3" pad="2"/>
</signal>
<signal name="AC2">
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="C"/>
<contactref element="J1" pad="3"/>
<contactref element="X2" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="SJ4" pad="1"/>
</signal>
<signal name="AC1">
<contactref element="D3" pad="A"/>
<contactref element="D4" pad="C"/>
<contactref element="J1" pad="1"/>
<contactref element="X2" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="SJ3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="SJ1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="X1" pad="2"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="L2" pad="2"/>
<contactref element="SJ1" pad="2"/>
<contactref element="C10" pad="+"/>
<contactref element="R1" pad="2"/>
<contactref element="L1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
