(kicad_pcb (version 4) (host pcbnew "(2015-09-06 BZR 6161, Git 6b3ff2d)-product")
  (general
    (links 22)
    (no_connects 0)
    (area 29.794999 128.219999 81.330001 179.120001)
    (thickness 1.6)
    (drawings 8)
    (tracks 213)
    (zones 0)
    (modules 6)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gbr/))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 /JTAG_TMS)
  (net 3 /JTAG_TCK)
  (net 4 /JTAG_TDO)
  (net 5 /JTAG_TDI)
  (net 6 "Net-(J1-Pad12)")
  (net 7 "Net-(J1-Pad13)")
  (net 8 "Net-(J1-Pad14)")
  (net 9 GNDREF)
  (net 10 "Net-(J2-Pad6)")
  (net 11 "Net-(J2-Pad9)")
  (net 12 "Net-(J2-Pad12)")
  (net 13 /PIC_DRIVES_JTAG)
  (net 14 /VPP/~MCLR)
  (net 15 /VDDTarget)
  (net 16 /ICSPDAT/PGD)
  (net 17 /LVP)
  (net 18 /VCC_3V3)
  (net 19 /VCC_AUX)
  (net 20 /ICDPCLK/PGC)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /ICDPCLK/PGC)
    (add_net /ICSPDAT/PGD)
    (add_net /JTAG_TCK)
    (add_net /JTAG_TDI)
    (add_net /JTAG_TDO)
    (add_net /JTAG_TMS)
    (add_net /LVP)
    (add_net /PIC_DRIVES_JTAG)
    (add_net /VCC_3V3)
    (add_net /VCC_AUX)
    (add_net /VDDTarget)
    (add_net /VPP/~MCLR)
    (add_net GNDREF)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad9)")
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5BAD3CAB)
    (at 91.48 147.47 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /PIC_DRIVES_JTAG))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 GNDREF))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5BAD3CA0)
    (at 100.75 139.42 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value R (at -6.31 -2.4 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /LVP))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Parts:930853 (layer F.Cu) (tedit 5BAD3C80)
    (at 98.46 138.25 270)
    (fp_text reference J2 (at 4.191 6.731 270) (layer F.SilkS) hide)
    (fp_text value 930853 (at 11.38 -3.75 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 4.699 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 19 /VCC_AUX))
    (pad 2 smd rect (at 0 0.127 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 9 GNDREF))
    (pad 3 smd rect (at 1.27 4.699 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 3 /JTAG_TCK))
    (pad 4 smd rect (at 1.27 0.127 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 9 GNDREF))
    (pad 6 smd rect (at 2.54 0.127 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad6)"))
    (pad 5 smd rect (at 2.54 4.699 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 /JTAG_TMS))
    (pad 8 smd rect (at 3.81 0.127 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 4 /JTAG_TDO))
    (pad 7 smd rect (at 3.81 4.699 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 5 /JTAG_TDI))
    (pad 10 smd rect (at 5.08 0.127 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 16 /ICSPDAT/PGD))
    (pad 9 smd rect (at 5.08 4.699 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad9)"))
    (pad 12 smd rect (at 6.35 0.127 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad12)"))
    (pad 11 smd rect (at 6.35 4.699 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 14 /VPP/~MCLR))
    (pad 14 smd rect (at 7.62 0.127 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 20 /ICDPCLK/PGC))
    (pad 13 smd rect (at 7.62 4.699 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 13 /PIC_DRIVES_JTAG))
    (pad 16 smd rect (at 8.89 0.127 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 18 /VCC_3V3))
    (pad 15 smd rect (at 8.89 4.699 270) (size 0.7366 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 9 GNDREF))
  )
  (module Parts:930241 (layer B.Cu) (tedit 5BAD3C8B)
    (at 107.18 137.13 270)
    (fp_text reference J1 (at 6.477 -7.493 270) (layer B.SilkS) hide)
    (fp_text value 930241 (at 6.858 2.794 270) (layer B.Fab))
    (pad 1 smd rect (at 0 -4.445 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0 0.254 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 19 /VCC_AUX))
    (pad 4 smd rect (at 1.778 0.254 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /JTAG_TMS))
    (pad 3 smd rect (at 1.778 -4.445 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 9 GNDREF))
    (pad 6 smd rect (at 3.7465 0.254 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 3 /JTAG_TCK))
    (pad 5 smd rect (at 3.7465 -4.445 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 9 GNDREF))
    (pad 8 smd rect (at 5.715 0.254 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 4 /JTAG_TDO))
    (pad 7 smd rect (at 5.715 -4.445 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 9 GNDREF))
    (pad 10 smd rect (at 7.6835 0.254 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 5 /JTAG_TDI))
    (pad 9 smd rect (at 7.6835 -4.445 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 9 GNDREF))
    (pad 12 smd rect (at 9.779 0.254 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad12)"))
    (pad 11 smd rect (at 9.652 -4.445 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 9 GNDREF))
    (pad 14 smd rect (at 11.6205 0.254 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J1-Pad14)"))
    (pad 13 smd rect (at 11.6205 -4.445 270) (size 1 2.75) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad13)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5BAD3C83)
    (at 99.75 149.26)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1) (layer F.SilkS) hide)
    (fp_text value R (at 1.5 -16.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /VCC_3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /VDDTarget))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x06 (layer F.Cu) (tedit 5BAD3C46)
    (at 122.21 137.13)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J3 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value 6PINHEADER (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /VPP/~MCLR))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /VDDTarget))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 GNDREF))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /ICSPDAT/PGD))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /ICDPCLK/PGC))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /LVP))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text 1 (at 90.79 134.65) (layer F.SilkS))
  (gr_text PIN1 (at 121.54 134.42) (layer B.SilkS))
  (gr_text PIN1 (at 121.71 134.34) (layer F.SilkS))
  (gr_line (start 88.28 132.64) (end 88.63 132.64) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.28 153.62) (end 88.28 132.64) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.5 153.62) (end 88.28 153.62) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.5 132.64) (end 126.5 153.62) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.54 132.64) (end 126.5 132.64) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 9) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.12 132.32) (xy 126.85 132.32) (xy 126.85 154.12) (xy 87.68 154.12) (xy 87.68 132.27)
        (xy 88.18 132.27)
      )
    )
  )
  (zone (net 9) (net_name GNDREF) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.45 132.1) (xy 127.02 132.1) (xy 127.02 154.4) (xy 87.34 154.4) (xy 87.34 132.04)
        (xy 87.68 132.04)
      )
    )
  )
)
