(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 24)
    (no_connects 0)
    (area 152.578999 84.252999 174.319001 110.057001)
    (thickness 1.6)
    (drawings 9)
    (tracks 84)
    (zones 0)
    (modules 13)
    (nets 11)
  )
  (page A4)
  (title_block
    (title CVTriggerX2)
    (date 19/8/2017)
    (rev 1)
    (company "ALPES MACHINES")
    (comment 1 "designed by Julien Voirin")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.99898 1.99898)
    (pad_drill 1.27)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.152000)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CVTrigger_Gerber/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(P1-Pad5)")
  (net 4 IN_2)
  (net 5 IN_1)
  (net 6 "Net-(P1-Pad8)")
  (net 7 OUT_2)
  (net 8 OUT_1)
  (net 9 "Net-(Q1-Pad2)")
  (net 10 "Net-(Q2-Pad2)")
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net IN_1)
    (add_net IN_2)
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net OUT_1)
    (add_net OUT_2)
  )
  (net_class PSU ""
    (clearance 0.3)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
  )
  (module Pin_Headers:Pin_Header_Straight_2x05 placed (layer F.Cu) (tedit 5998493C)
    (at 162.56 93.345)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -2.6035 -0.762) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 1.27 -10.541) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 IN_2))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 IN_1))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 OUT_2))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 OUT_1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 placed (layer F.Cu) (tedit 5998441C)
    (at 165.1 90.805 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference PSU1 (at -5.715 1.27 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0.254 -13.716 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 placed (layer F.Cu) (tedit 5998492E)
    (at 155.575 90.17 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P_IN1 (at -0.4445 -2.286 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -7.239 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 IN_1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 IN_2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 placed (layer F.Cu) (tedit 59984018)
    (at 165.735 107.95 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P_OUT1 (at -2.032 1.905 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 3.81 1.651 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 OUT_1))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 OUT_2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Alpes_Machines:Transistor_NPN placed (layer F.Cu) (tedit 5998442A)
    (at 168.91 105.41 90)
    (fp_text reference Q1 (at -3.302 4.064 180) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.016 -0.762 90) (layer F.SilkS))
    (fp_text user "C B E" (at 0 1.27 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.286 1.27 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 OUT_1))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.286 1.27 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Alpes_Machines:Transistor_NPN placed (layer F.Cu) (tedit 599840EB)
    (at 156.845 107.95 180)
    (fp_text reference Q2 (at 2.667 -1.016 180) (layer F.SilkS))
    (fp_text value 2N3904 (at -1.651 -1.016 180) (layer F.SilkS))
    (fp_text user "C B E" (at 0 1.27 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.286 1.27 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 OUT_2))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole circle (at 2.286 1.27 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Alpes_Machines:Resistor_Horizontal_RM7mm placed (layer F.Cu) (tedit 5998491A)
    (at 154.94 101.6 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 0.4445 -1.651 90) (layer F.SilkS))
    (fp_text value 1K (at 3.81 -0.254 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 5 IN_1))
  )
  (module Alpes_Machines:Resistor_Horizontal_RM7mm placed (layer F.Cu) (tedit 599840CE)
    (at 162.56 86.995 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at 4.572 1.905 180) (layer F.SilkS))
    (fp_text value 1K (at 3.81 -0.254 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 4 IN_2))
  )
  (module Alpes_Machines:Resistor_Horizontal_RM7mm placed (layer F.Cu) (tedit 599840D1)
    (at 165.1 86.995)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R3 (at 5.334 -1.905) (layer F.SilkS))
    (fp_text value 10K (at 3.81 -0.254) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 8 OUT_1))
  )
  (module Alpes_Machines:Resistor_Horizontal_RM7mm placed (layer F.Cu) (tedit 599840C3)
    (at 157.988 93.98 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R4 (at 5.588 -2.159 270) (layer F.SilkS))
    (fp_text value 10K (at 3.81 -0.254 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 7 OUT_2))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 placed (layer F.Cu) (tedit 59984A03)
    (at 172.085 90.17 270)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference ZD1 (at 5.334 -0.127 270) (layer F.SilkS))
    (fp_text value "ZENER 5.1V" (at 4.37134 -3.55854 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 90) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 -0.00254 90) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(Q1-Pad2)"))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 placed (layer F.Cu) (tedit 599849FC)
    (at 168.91 90.17 270)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference ZD2 (at 5.588 0 270) (layer F.SilkS))
    (fp_text value "ZENER 5.1V" (at 4.572 -8.128 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 90) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 -0.00254 90) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(Q2-Pad2)"))
  )
  (module Alpes_Machines:LOGO_AM_Micro (layer B.Cu) (tedit 573D3D84)
    (at 170.434 94.996 180)
    (fp_text reference " " (at 0 -4.445 180) (layer B.SilkS) hide)
    (fp_text value " " (at 0 4.445 180) (layer B.SilkS) hide)
  )
  (gr_text "CV Trig v1" (at 157.48 108.458) (layer B.Cu))
  (gr_line (start 174.244 84.582) (end 174.244 109.728) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.908 84.328) (end 173.99 84.328) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.654 109.728) (end 152.654 84.582) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.99 109.982) (end 152.908 109.982) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.99 109.728) (end 174.244 109.728) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.99 84.582) (end 173.99 84.328) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.908 84.582) (end 152.654 84.582) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.908 109.728) (end 152.908 109.982) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 174.244 84.582) (xy 174.244 109.728) (xy 173.99 109.982) (xy 153.162 109.982) (xy 152.908 109.728)
        (xy 152.908 84.836) (xy 153.416 84.328) (xy 173.99 84.328) (xy 174.244 84.582)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.4)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 174.244 84.582) (xy 174.244 109.728) (xy 173.99 109.982) (xy 152.908 109.982) (xy 152.654 109.728)
        (xy 152.654 85.09) (xy 153.416 84.328) (xy 173.99 84.328) (xy 174.244 84.582)
      )
    )
  )
)
