(kicad_pcb (version 4) (host pcbnew 4.0.2+e4-6225~38~ubuntu14.04.1-stable)
  (general
    (links 36)
    (no_connects 0)
    (area 66.980999 84.760999 142.569001 120.979001)
    (thickness 1.6)
    (drawings 13)
    (tracks 155)
    (zones 0)
    (modules 10)
    (nets 125)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 3va)
  (net 2 tx1a)
  (net 3 "Net-(U1A1-Pad3)")
  (net 4 gnda)
  (net 5 3vb)
  (net 6 rx1b)
  (net 7 gndb)
  (net 8 tx1b)
  (net 9 "Net-(U1B1-Pad3)")
  (net 10 rx1a)
  (net 11 3vc)
  (net 12 tx1c)
  (net 13 "Net-(U1C1-Pad3)")
  (net 14 gndc)
  (net 15 rx2a)
  (net 16 3vd)
  (net 17 tx1d)
  (net 18 "Net-(U1D1-Pad3)")
  (net 19 gndd)
  (net 20 rx3a)
  (net 21 tx2a)
  (net 22 "Net-(U2A1-Pad3)")
  (net 23 rx1c)
  (net 24 tx3a)
  (net 25 "Net-(U3A1-Pad3)")
  (net 26 rx1d)
  (net 27 "Net-(UA1-Pad2)")
  (net 28 "Net-(UA1-Pad3)")
  (net 29 "Net-(UA1-Pad4)")
  (net 30 "Net-(UA1-Pad5)")
  (net 31 "Net-(UA1-Pad6)")
  (net 32 "Net-(UA1-Pad11)")
  (net 33 "Net-(UA1-Pad12)")
  (net 34 "Net-(UA1-Pad13)")
  (net 35 "Net-(UA1-Pad14)")
  (net 36 "Net-(UA1-Pad15)")
  (net 37 "Net-(UA1-Pad16)")
  (net 38 "Net-(UA1-Pad17)")
  (net 39 "Net-(UA1-Pad18)")
  (net 40 "Net-(UA1-Pad19)")
  (net 41 "Net-(UA1-Pad20)")
  (net 42 "Net-(UA1-Pad21)")
  (net 43 "Net-(UA1-Pad22)")
  (net 44 "Net-(UA1-Pad23)")
  (net 45 "Net-(UA1-Pad25)")
  (net 46 "Net-(UA1-Pad26)")
  (net 47 "Net-(UB1-Pad2)")
  (net 48 "Net-(UB1-Pad3)")
  (net 49 "Net-(UB1-Pad4)")
  (net 50 "Net-(UB1-Pad5)")
  (net 51 "Net-(UB1-Pad6)")
  (net 52 "Net-(UB1-Pad7)")
  (net 53 "Net-(UB1-Pad8)")
  (net 54 "Net-(UB1-Pad9)")
  (net 55 "Net-(UB1-Pad10)")
  (net 56 "Net-(UB1-Pad11)")
  (net 57 "Net-(UB1-Pad12)")
  (net 58 "Net-(UB1-Pad13)")
  (net 59 "Net-(UB1-Pad14)")
  (net 60 "Net-(UB1-Pad15)")
  (net 61 "Net-(UB1-Pad16)")
  (net 62 "Net-(UB1-Pad17)")
  (net 63 "Net-(UB1-Pad18)")
  (net 64 "Net-(UB1-Pad19)")
  (net 65 "Net-(UB1-Pad20)")
  (net 66 "Net-(UB1-Pad21)")
  (net 67 "Net-(UB1-Pad22)")
  (net 68 "Net-(UB1-Pad23)")
  (net 69 "Net-(UB1-Pad25)")
  (net 70 "Net-(UB1-Pad26)")
  (net 71 "Net-(UC1-Pad2)")
  (net 72 "Net-(UC1-Pad3)")
  (net 73 "Net-(UC1-Pad4)")
  (net 74 "Net-(UC1-Pad5)")
  (net 75 "Net-(UC1-Pad6)")
  (net 76 "Net-(UC1-Pad7)")
  (net 77 "Net-(UC1-Pad8)")
  (net 78 "Net-(UC1-Pad9)")
  (net 79 "Net-(UC1-Pad10)")
  (net 80 "Net-(UC1-Pad11)")
  (net 81 "Net-(UC1-Pad12)")
  (net 82 "Net-(UC1-Pad13)")
  (net 83 "Net-(UC1-Pad14)")
  (net 84 "Net-(UC1-Pad15)")
  (net 85 "Net-(UC1-Pad16)")
  (net 86 "Net-(UC1-Pad17)")
  (net 87 "Net-(UC1-Pad18)")
  (net 88 "Net-(UC1-Pad19)")
  (net 89 "Net-(UC1-Pad20)")
  (net 90 "Net-(UC1-Pad21)")
  (net 91 "Net-(UC1-Pad22)")
  (net 92 "Net-(UC1-Pad23)")
  (net 93 "Net-(UC1-Pad25)")
  (net 94 "Net-(UC1-Pad26)")
  (net 95 "Net-(UD1-Pad2)")
  (net 96 "Net-(UD1-Pad3)")
  (net 97 "Net-(UD1-Pad4)")
  (net 98 "Net-(UD1-Pad5)")
  (net 99 "Net-(UD1-Pad6)")
  (net 100 "Net-(UD1-Pad7)")
  (net 101 "Net-(UD1-Pad8)")
  (net 102 "Net-(UD1-Pad9)")
  (net 103 "Net-(UD1-Pad10)")
  (net 104 "Net-(UD1-Pad11)")
  (net 105 "Net-(UD1-Pad12)")
  (net 106 "Net-(UD1-Pad13)")
  (net 107 "Net-(UD1-Pad14)")
  (net 108 "Net-(UD1-Pad15)")
  (net 109 "Net-(UD1-Pad16)")
  (net 110 "Net-(UD1-Pad17)")
  (net 111 "Net-(UD1-Pad18)")
  (net 112 "Net-(UD1-Pad19)")
  (net 113 "Net-(UD1-Pad20)")
  (net 114 "Net-(UD1-Pad21)")
  (net 115 "Net-(UD1-Pad22)")
  (net 116 "Net-(UD1-Pad23)")
  (net 117 "Net-(UD1-Pad25)")
  (net 118 "Net-(UD1-Pad26)")
  (net 119 "Net-(U1A1-Pad7)")
  (net 120 "Net-(U1B1-Pad7)")
  (net 121 "Net-(U1C1-Pad7)")
  (net 122 "Net-(U1D1-Pad7)")
  (net 123 "Net-(U2A1-Pad7)")
  (net 124 "Net-(U3A1-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3va)
    (add_net 3vb)
    (add_net 3vc)
    (add_net 3vd)
    (add_net "Net-(U1A1-Pad3)")
    (add_net "Net-(U1A1-Pad7)")
    (add_net "Net-(U1B1-Pad3)")
    (add_net "Net-(U1B1-Pad7)")
    (add_net "Net-(U1C1-Pad3)")
    (add_net "Net-(U1C1-Pad7)")
    (add_net "Net-(U1D1-Pad3)")
    (add_net "Net-(U1D1-Pad7)")
    (add_net "Net-(U2A1-Pad3)")
    (add_net "Net-(U2A1-Pad7)")
    (add_net "Net-(U3A1-Pad3)")
    (add_net "Net-(U3A1-Pad7)")
    (add_net "Net-(UA1-Pad11)")
    (add_net "Net-(UA1-Pad12)")
    (add_net "Net-(UA1-Pad13)")
    (add_net "Net-(UA1-Pad14)")
    (add_net "Net-(UA1-Pad15)")
    (add_net "Net-(UA1-Pad16)")
    (add_net "Net-(UA1-Pad17)")
    (add_net "Net-(UA1-Pad18)")
    (add_net "Net-(UA1-Pad19)")
    (add_net "Net-(UA1-Pad2)")
    (add_net "Net-(UA1-Pad20)")
    (add_net "Net-(UA1-Pad21)")
    (add_net "Net-(UA1-Pad22)")
    (add_net "Net-(UA1-Pad23)")
    (add_net "Net-(UA1-Pad25)")
    (add_net "Net-(UA1-Pad26)")
    (add_net "Net-(UA1-Pad3)")
    (add_net "Net-(UA1-Pad4)")
    (add_net "Net-(UA1-Pad5)")
    (add_net "Net-(UA1-Pad6)")
    (add_net "Net-(UB1-Pad10)")
    (add_net "Net-(UB1-Pad11)")
    (add_net "Net-(UB1-Pad12)")
    (add_net "Net-(UB1-Pad13)")
    (add_net "Net-(UB1-Pad14)")
    (add_net "Net-(UB1-Pad15)")
    (add_net "Net-(UB1-Pad16)")
    (add_net "Net-(UB1-Pad17)")
    (add_net "Net-(UB1-Pad18)")
    (add_net "Net-(UB1-Pad19)")
    (add_net "Net-(UB1-Pad2)")
    (add_net "Net-(UB1-Pad20)")
    (add_net "Net-(UB1-Pad21)")
    (add_net "Net-(UB1-Pad22)")
    (add_net "Net-(UB1-Pad23)")
    (add_net "Net-(UB1-Pad25)")
    (add_net "Net-(UB1-Pad26)")
    (add_net "Net-(UB1-Pad3)")
    (add_net "Net-(UB1-Pad4)")
    (add_net "Net-(UB1-Pad5)")
    (add_net "Net-(UB1-Pad6)")
    (add_net "Net-(UB1-Pad7)")
    (add_net "Net-(UB1-Pad8)")
    (add_net "Net-(UB1-Pad9)")
    (add_net "Net-(UC1-Pad10)")
    (add_net "Net-(UC1-Pad11)")
    (add_net "Net-(UC1-Pad12)")
    (add_net "Net-(UC1-Pad13)")
    (add_net "Net-(UC1-Pad14)")
    (add_net "Net-(UC1-Pad15)")
    (add_net "Net-(UC1-Pad16)")
    (add_net "Net-(UC1-Pad17)")
    (add_net "Net-(UC1-Pad18)")
    (add_net "Net-(UC1-Pad19)")
    (add_net "Net-(UC1-Pad2)")
    (add_net "Net-(UC1-Pad20)")
    (add_net "Net-(UC1-Pad21)")
    (add_net "Net-(UC1-Pad22)")
    (add_net "Net-(UC1-Pad23)")
    (add_net "Net-(UC1-Pad25)")
    (add_net "Net-(UC1-Pad26)")
    (add_net "Net-(UC1-Pad3)")
    (add_net "Net-(UC1-Pad4)")
    (add_net "Net-(UC1-Pad5)")
    (add_net "Net-(UC1-Pad6)")
    (add_net "Net-(UC1-Pad7)")
    (add_net "Net-(UC1-Pad8)")
    (add_net "Net-(UC1-Pad9)")
    (add_net "Net-(UD1-Pad10)")
    (add_net "Net-(UD1-Pad11)")
    (add_net "Net-(UD1-Pad12)")
    (add_net "Net-(UD1-Pad13)")
    (add_net "Net-(UD1-Pad14)")
    (add_net "Net-(UD1-Pad15)")
    (add_net "Net-(UD1-Pad16)")
    (add_net "Net-(UD1-Pad17)")
    (add_net "Net-(UD1-Pad18)")
    (add_net "Net-(UD1-Pad19)")
    (add_net "Net-(UD1-Pad2)")
    (add_net "Net-(UD1-Pad20)")
    (add_net "Net-(UD1-Pad21)")
    (add_net "Net-(UD1-Pad22)")
    (add_net "Net-(UD1-Pad23)")
    (add_net "Net-(UD1-Pad25)")
    (add_net "Net-(UD1-Pad26)")
    (add_net "Net-(UD1-Pad3)")
    (add_net "Net-(UD1-Pad4)")
    (add_net "Net-(UD1-Pad5)")
    (add_net "Net-(UD1-Pad6)")
    (add_net "Net-(UD1-Pad7)")
    (add_net "Net-(UD1-Pad8)")
    (add_net "Net-(UD1-Pad9)")
    (add_net gnda)
    (add_net gndb)
    (add_net gndc)
    (add_net gndd)
    (add_net rx1a)
    (add_net rx1b)
    (add_net rx1c)
    (add_net rx1d)
    (add_net rx2a)
    (add_net rx3a)
    (add_net tx1a)
    (add_net tx1b)
    (add_net tx1c)
    (add_net tx1d)
    (add_net tx2a)
    (add_net tx3a)
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 54130A77)
    (at 95.25 110.49 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1A1 (at 0 3.5 270) (layer B.SilkS))
    (fp_text value opto (at 0 -3.5 270) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 3va))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 tx1a))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(U1A1-Pad3)"))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 gnda))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 gndb))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 rx1b))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 119 "Net-(U1A1-Pad7)"))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 3vb))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 54130A77)
    (at 95.25 96.52 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1B1 (at 0 3.5 270) (layer B.SilkS))
    (fp_text value opto (at 0 -3.5 270) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 3vb))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 8 tx1b))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(U1B1-Pad3)"))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 gndb))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 gnda))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 rx1a))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 120 "Net-(U1B1-Pad7)"))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 3va))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 54130A77)
    (at 114.3 96.52 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1C1 (at 0 3.5 270) (layer B.SilkS))
    (fp_text value opto (at 0 -3.5 270) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 11 3vc))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 tx1c))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(U1C1-Pad3)"))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 14 gndc))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 gnda))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 15 rx2a))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 121 "Net-(U1C1-Pad7)"))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 3va))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 54130A77)
    (at 133.35 96.52 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1D1 (at 0 3.5 270) (layer B.SilkS))
    (fp_text value opto (at 0 -3.5 270) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 16 3vd))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 17 tx1d))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(U1D1-Pad3)"))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 19 gndd))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 gnda))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 20 rx3a))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 122 "Net-(U1D1-Pad7)"))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 3va))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 54130A77)
    (at 114.3 110.49 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2A1 (at 0 3.5 270) (layer B.SilkS))
    (fp_text value opto (at 0 -3.5 270) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 3va))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 21 tx2a))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(U2A1-Pad3)"))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 gnda))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 14 gndc))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 23 rx1c))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 123 "Net-(U2A1-Pad7)"))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 11 3vc))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 54130A77)
    (at 133.35 110.49 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3A1 (at 0 3.5 270) (layer B.SilkS))
    (fp_text value opto (at 0 -3.5 270) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 3va))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 24 tx3a))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U3A1-Pad3)"))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 gnda))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 19 gndd))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 26 rx1d))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 124 "Net-(U3A1-Pad7)"))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 16 3vd))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Teensy-3:Teensy-3.1 (layer F.Cu) (tedit 5506D470)
    (at 83.82 116.84 90)
    (fp_text reference UA1 (at -5.08 -7.62 180) (layer F.SilkS))
    (fp_text value Teensy_3.1 (at 5.08 -10.16 90) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 rx1a))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 tx1a))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(UA1-Pad2)"))
    (pad 3 thru_hole circle (at 7.62 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(UA1-Pad3)"))
    (pad 4 thru_hole circle (at 10.16 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(UA1-Pad4)"))
    (pad 5 thru_hole circle (at 12.7 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(UA1-Pad5)"))
    (pad 6 thru_hole circle (at 15.24 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(UA1-Pad6)"))
    (pad 7 thru_hole circle (at 17.78 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 rx3a))
    (pad 8 thru_hole circle (at 20.32 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 tx3a))
    (pad 9 thru_hole circle (at 22.86 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 rx2a))
    (pad 10 thru_hole circle (at 25.4 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 tx2a))
    (pad 11 thru_hole circle (at 27.94 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(UA1-Pad11)"))
    (pad 12 thru_hole circle (at 30.48 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(UA1-Pad12)"))
    (pad 13 thru_hole circle (at 30.48 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(UA1-Pad13)"))
    (pad 14 thru_hole circle (at 27.94 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(UA1-Pad14)"))
    (pad 15 thru_hole circle (at 25.4 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(UA1-Pad15)"))
    (pad 16 thru_hole circle (at 22.86 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(UA1-Pad16)"))
    (pad 17 thru_hole circle (at 20.32 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(UA1-Pad17)"))
    (pad 18 thru_hole circle (at 17.78 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(UA1-Pad18)"))
    (pad 19 thru_hole circle (at 15.24 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(UA1-Pad19)"))
    (pad 20 thru_hole circle (at 12.7 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(UA1-Pad20)"))
    (pad 21 thru_hole circle (at 10.16 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(UA1-Pad21)"))
    (pad 22 thru_hole circle (at 7.62 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(UA1-Pad22)"))
    (pad 23 thru_hole circle (at 5.08 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(UA1-Pad23)"))
    (pad 24 thru_hole circle (at 2.54 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 3va))
    (pad 25 thru_hole circle (at 0 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(UA1-Pad25)"))
    (pad 26 thru_hole circle (at -2.54 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(UA1-Pad26)"))
    (pad 27 thru_hole circle (at -2.54 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 gnda))
  )
  (module Teensy-3:Teensy-3.1 (layer F.Cu) (tedit 5506D470)
    (at 102.87 116.84 90)
    (fp_text reference UB1 (at -5.08 -7.62 180) (layer F.SilkS))
    (fp_text value Teensy_3.1 (at 5.08 -10.16 90) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 rx1b))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 tx1b))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(UB1-Pad2)"))
    (pad 3 thru_hole circle (at 7.62 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(UB1-Pad3)"))
    (pad 4 thru_hole circle (at 10.16 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(UB1-Pad4)"))
    (pad 5 thru_hole circle (at 12.7 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(UB1-Pad5)"))
    (pad 6 thru_hole circle (at 15.24 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(UB1-Pad6)"))
    (pad 7 thru_hole circle (at 17.78 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(UB1-Pad7)"))
    (pad 8 thru_hole circle (at 20.32 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(UB1-Pad8)"))
    (pad 9 thru_hole circle (at 22.86 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(UB1-Pad9)"))
    (pad 10 thru_hole circle (at 25.4 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(UB1-Pad10)"))
    (pad 11 thru_hole circle (at 27.94 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(UB1-Pad11)"))
    (pad 12 thru_hole circle (at 30.48 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(UB1-Pad12)"))
    (pad 13 thru_hole circle (at 30.48 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(UB1-Pad13)"))
    (pad 14 thru_hole circle (at 27.94 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(UB1-Pad14)"))
    (pad 15 thru_hole circle (at 25.4 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(UB1-Pad15)"))
    (pad 16 thru_hole circle (at 22.86 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(UB1-Pad16)"))
    (pad 17 thru_hole circle (at 20.32 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(UB1-Pad17)"))
    (pad 18 thru_hole circle (at 17.78 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(UB1-Pad18)"))
    (pad 19 thru_hole circle (at 15.24 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(UB1-Pad19)"))
    (pad 20 thru_hole circle (at 12.7 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(UB1-Pad20)"))
    (pad 21 thru_hole circle (at 10.16 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(UB1-Pad21)"))
    (pad 22 thru_hole circle (at 7.62 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(UB1-Pad22)"))
    (pad 23 thru_hole circle (at 5.08 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(UB1-Pad23)"))
    (pad 24 thru_hole circle (at 2.54 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 3vb))
    (pad 25 thru_hole circle (at 0 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(UB1-Pad25)"))
    (pad 26 thru_hole circle (at -2.54 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(UB1-Pad26)"))
    (pad 27 thru_hole circle (at -2.54 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 gndb))
  )
  (module Teensy-3:Teensy-3.1 (layer F.Cu) (tedit 5506D470)
    (at 121.92 116.84 90)
    (fp_text reference UC1 (at -5.08 -7.62 180) (layer F.SilkS))
    (fp_text value Teensy_3.1 (at 5.08 -10.16 90) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 rx1c))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 tx1c))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(UC1-Pad2)"))
    (pad 3 thru_hole circle (at 7.62 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(UC1-Pad3)"))
    (pad 4 thru_hole circle (at 10.16 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(UC1-Pad4)"))
    (pad 5 thru_hole circle (at 12.7 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(UC1-Pad5)"))
    (pad 6 thru_hole circle (at 15.24 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(UC1-Pad6)"))
    (pad 7 thru_hole circle (at 17.78 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(UC1-Pad7)"))
    (pad 8 thru_hole circle (at 20.32 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(UC1-Pad8)"))
    (pad 9 thru_hole circle (at 22.86 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(UC1-Pad9)"))
    (pad 10 thru_hole circle (at 25.4 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(UC1-Pad10)"))
    (pad 11 thru_hole circle (at 27.94 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(UC1-Pad11)"))
    (pad 12 thru_hole circle (at 30.48 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(UC1-Pad12)"))
    (pad 13 thru_hole circle (at 30.48 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(UC1-Pad13)"))
    (pad 14 thru_hole circle (at 27.94 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(UC1-Pad14)"))
    (pad 15 thru_hole circle (at 25.4 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(UC1-Pad15)"))
    (pad 16 thru_hole circle (at 22.86 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(UC1-Pad16)"))
    (pad 17 thru_hole circle (at 20.32 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(UC1-Pad17)"))
    (pad 18 thru_hole circle (at 17.78 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(UC1-Pad18)"))
    (pad 19 thru_hole circle (at 15.24 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(UC1-Pad19)"))
    (pad 20 thru_hole circle (at 12.7 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 89 "Net-(UC1-Pad20)"))
    (pad 21 thru_hole circle (at 10.16 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(UC1-Pad21)"))
    (pad 22 thru_hole circle (at 7.62 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(UC1-Pad22)"))
    (pad 23 thru_hole circle (at 5.08 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(UC1-Pad23)"))
    (pad 24 thru_hole circle (at 2.54 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 3vc))
    (pad 25 thru_hole circle (at 0 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(UC1-Pad25)"))
    (pad 26 thru_hole circle (at -2.54 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(UC1-Pad26)"))
    (pad 27 thru_hole circle (at -2.54 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 gndc))
  )
  (module Teensy-3:Teensy-3.1 (layer F.Cu) (tedit 5506D470)
    (at 140.97 116.84 90)
    (fp_text reference UD1 (at -5.08 -7.62 180) (layer F.SilkS))
    (fp_text value Teensy_3.1 (at 5.08 -10.16 90) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 rx1d))
    (pad 1 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 tx1d))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(UD1-Pad2)"))
    (pad 3 thru_hole circle (at 7.62 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(UD1-Pad3)"))
    (pad 4 thru_hole circle (at 10.16 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(UD1-Pad4)"))
    (pad 5 thru_hole circle (at 12.7 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(UD1-Pad5)"))
    (pad 6 thru_hole circle (at 15.24 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(UD1-Pad6)"))
    (pad 7 thru_hole circle (at 17.78 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(UD1-Pad7)"))
    (pad 8 thru_hole circle (at 20.32 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(UD1-Pad8)"))
    (pad 9 thru_hole circle (at 22.86 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(UD1-Pad9)"))
    (pad 10 thru_hole circle (at 25.4 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(UD1-Pad10)"))
    (pad 11 thru_hole circle (at 27.94 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(UD1-Pad11)"))
    (pad 12 thru_hole circle (at 30.48 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(UD1-Pad12)"))
    (pad 13 thru_hole circle (at 30.48 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(UD1-Pad13)"))
    (pad 14 thru_hole circle (at 27.94 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(UD1-Pad14)"))
    (pad 15 thru_hole circle (at 25.4 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(UD1-Pad15)"))
    (pad 16 thru_hole circle (at 22.86 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(UD1-Pad16)"))
    (pad 17 thru_hole circle (at 20.32 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(UD1-Pad17)"))
    (pad 18 thru_hole circle (at 17.78 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(UD1-Pad18)"))
    (pad 19 thru_hole circle (at 15.24 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(UD1-Pad19)"))
    (pad 20 thru_hole circle (at 12.7 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(UD1-Pad20)"))
    (pad 21 thru_hole circle (at 10.16 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(UD1-Pad21)"))
    (pad 22 thru_hole circle (at 7.62 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(UD1-Pad22)"))
    (pad 23 thru_hole circle (at 5.08 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(UD1-Pad23)"))
    (pad 24 thru_hole circle (at 2.54 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 3vd))
    (pad 25 thru_hole circle (at 0 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(UD1-Pad25)"))
    (pad 26 thru_hole circle (at -2.54 -15.24 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(UD1-Pad26)"))
    (pad 27 thru_hole circle (at -2.54 0 90) (size 1.9 1.9) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 gndd))
  )
  (gr_text V2 (at 75.692 92.71) (layer B.SilkS))
  (gr_text "USB\n" (at 133.35 118.491) (layer F.SilkS))
  (gr_text "USB\n" (at 114.3 118.491) (layer F.SilkS))
  (gr_text "USB\n" (at 95.123 118.491) (layer F.SilkS))
  (gr_text USB (at 76.073 118.364) (layer F.SilkS))
  (gr_line (start 142.494 119.38) (end 142.494 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.58 120.904) (end 140.97 120.904) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.056 86.36) (end 67.056 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.97 84.836) (end 68.58 84.836) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 68.58 86.36) (end 67.056 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 68.58 119.38) (end 68.58 120.904) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 140.97 119.38) (end 142.494 119.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 140.97 86.36) (end 140.97 84.836) (angle 90) (layer Edge.Cuts) (width 0.15))
)
