<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="25.55875" y1="39.37" x2="25.55875" y2="36.67125" width="0" layer="20"/>
<wire x1="25.55875" y1="36.67125" x2="26.82875" y2="35.40125" width="0" layer="20" curve="90"/>
<wire x1="26.82875" y1="35.40125" x2="32.0675" y2="35.40125" width="0" layer="20"/>
<wire x1="32.0675" y1="35.40125" x2="33.3375" y2="34.13125" width="0" layer="20" curve="-90"/>
<wire x1="32.0675" y1="0" x2="1.27" y2="0" width="0" layer="20"/>
<wire x1="1.27" y1="0" x2="0" y2="1.27" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="1.27" x2="0" y2="34.13125" width="0" layer="20"/>
<wire x1="32.0675" y1="0" x2="33.3375" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="33.3375" y1="1.27" x2="33.3375" y2="34.13125" width="0" layer="20"/>
<wire x1="0" y1="34.13125" x2="1.27" y2="35.40125" width="0" layer="20" curve="-90"/>
<wire x1="1.27" y1="35.40125" x2="6.50875" y2="35.40125" width="0" layer="20"/>
<text>G</text>
<text>Germ-o-phobe</text>
<wire x1="6.50875" y1="35.40125" x2="7.77875" y2="36.67125" width="0" layer="20" curve="90"/>
<wire x1="7.77875" y1="36.67125" x2="7.77875" y2="39.37" width="0" layer="20"/>
<wire x1="7.77875" y1="39.37" x2="9.04875" y2="40.64" width="0" layer="20" curve="-90"/>
<wire x1="9.04875" y1="40.64" x2="24.28875" y2="40.64" width="0" layer="20"/>
<wire x1="24.28875" y1="40.64" x2="25.55875" y2="39.37" width="0" layer="20" curve="-90"/>
<text>Layout by Stomptown</text>
<text>G</text>
<text>G</text>
</plain>
<libraries>
<library name="mb_supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="SQUARE">
<description>&lt;b&gt;Square Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="mb_resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="mb_trans">
<description>&lt;b&gt;Transistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;small signal amps (e.g., 2N508x)
&lt;li&gt;switching transistors (e.g., 2N2222, 2N390x)
&lt;li&gt;JFETs (e.g., J201, 2N3819, 2N5457)
&lt;li&gt;MOSFETs (e.g., BS170, BS250)
&lt;li&gt;mostly copied from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="TO5">
<description>&lt;b&gt;TO-5&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mb_caps-electro">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020_1">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistors">
<description>&lt;b&gt;Transistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;small signal amps (e.g., 2N508x)
&lt;li&gt;switching transistors (e.g., 2N2222, 2N390x)
&lt;li&gt;JFETs (e.g., J201, 2N3819, 2N5457)
&lt;li&gt;MOSFETs (e.g., BS170, BS250)
&lt;li&gt;mostly copied from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="TO92-FLAT">
</package>
</packages>
</library>
<library name="potentiometers">
<packages>
<package name="9MM_W/MOUNTS">
</package>
</packages>
</library>
<library name="mb_caps-chicklet">
<description>&lt;b&gt;Capacitors, Film, Chicklet&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;100pF - 0.1uF (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors
&lt;li&gt;available from smallbearelec.com as Panasonic ECQ-B capacitors
&lt;li&gt;these become quite large for values near 1uF
&lt;/ul&gt;</description>
<packages>
<package name="075X030">
<description>&lt;b&gt;7.5mm x 3.0mm, 5mm lead spacing&lt;/b&gt;

&lt;p&gt;Panasonic ECQ-B</description>
</package>
</packages>
</library>
<library name="diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DO35-3">
<description>&lt;B&gt;DO-35 0.3" spacing&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="mb_diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="I" library="mb_supply" package="SQUARE" value="IN(T)">
<attribute name="NAME"/>
</element>
<element name="O" library="mb_supply" package="SQUARE" value="OUT(T)">
<attribute name="NAME"/>
</element>
<element name="9V" library="mb_supply" package="SQUARE" value="+9V(T)">
<attribute name="NAME"/>
</element>
<element name="G" library="mb_supply" package="SQUARE" value="GND(T)">
<attribute name="NAME"/>
</element>
<element name="R1" library="mb_resistors" package="R0207/3" value="51k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="mb_resistors" package="R0207/3" value="91k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="mb_resistors" package="R0207/3" value="3M9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="mb_resistors" package="R0207/3" value="91k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="mb_resistors" package="R0207/3" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="mb_trans" package="TO5" value="2n404a">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="mb_caps-electro" package="050_020_1" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="mb_caps-electro" package="050_020_1" value="2u2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="mb_caps-electro" package="050_020_1" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistors" package="TO92-FLAT" value="2n3565">
<attribute name="NAME"/>
</element>
<element name="HARM" library="potentiometers" package="9MM_W/MOUNTS" value="100KA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BAL" library="potentiometers" package="9MM_W/MOUNTS" value="50KA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diodes" package="DO35-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diodes" package="DO35-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="G2" library="mb_supply" package="SQUARE" value="GND(T)"/>
<element name="D3" library="diodes" package="DO35-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED" library="mb_diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
</element>
<element name="R6" library="mb_resistors" package="R0207/3" value="91k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW" library="mb_supply" package="SQUARE" value="">
<attribute name="NAME"/>
</element>
<element name="C1" library="mb_caps-chicklet" package="075X030" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="mb_caps-chicklet" package="075X030" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="mb_caps-chicklet" package="075X030" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="mb_caps-chicklet" package="075X030" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="mb_caps-chicklet" package="075X030" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="G1" library="mb_supply" package="SQUARE" value="GND(T)"/>
<element name="G3" library="mb_supply" package="SQUARE" value="GND(T)"/>
</elements>
<signals>
<signal name="GND">
<contactref element="G" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="-"/>
<contactref element="C6" pad="-"/>
<contactref element="HARM" pad="P$1"/>
<contactref element="BAL" pad="P$1"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="A"/>
<contactref element="G2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="G1" pad="1"/>
<contactref element="G3" pad="1"/>
</signal>
<signal name="OUT">
<contactref element="O" pad="1"/>
<contactref element="BAL" pad="P$2"/>
</signal>
<signal name="IN">
<contactref element="I" pad="1"/>
<contactref element="HARM" pad="P$3"/>
</signal>
<signal name="N$2">
<contactref element="HARM" pad="P$2"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C4" pad="-"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="1"/>
<contactref element="C3" pad="+"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="C4" pad="+"/>
<contactref element="R3" pad="1"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="BAL" pad="P$3"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R5" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="R4" pad="2"/>
<contactref element="C6" pad="+"/>
<contactref element="D3" pad="C"/>
<contactref element="R6" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="+9V">
<contactref element="9V" pad="1"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="LED" pad="A"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="LED" pad="K"/>
<contactref element="SW" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
