(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 476)
    (no_connects 0)
    (area 67.999499 81.999499 138.000501 100.000501)
    (thickness 1.6)
    (drawings 44)
    (tracks 2144)
    (zones 0)
    (modules 168)
    (nets 108)
  )
  (page A4 portrait)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.127)
    (zone_clearance 0.127)
    (zone_45_only yes)
    (trace_min 0.12)
    (segment_width 0.1)
    (edge_width 0.001)
    (via_size 0.56)
    (via_drill 0.3)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.2 5.2)
    (pad_drill 3)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.1)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFE609)
    (pcbplotparams
      (layerselection 0x010fc_80000007)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../../../../../../Desktop/MINI_VESC5/))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 "Net-(Q1-Pad1)")
  (net 3 "Net-(Q2-Pad1)")
  (net 4 VSS)
  (net 5 "Net-(Q3-Pad1)")
  (net 6 "Net-(Q5-Pad1)")
  (net 7 "Net-(Q6-Pad1)")
  (net 8 "Net-(C1-Pad1)")
  (net 9 "Net-(C2-Pad1)")
  (net 10 "Net-(C3-Pad1)")
  (net 11 "Net-(U4-Pad4)")
  (net 12 "Net-(U5-Pad4)")
  (net 13 "Net-(U6-Pad4)")
  (net 14 "Net-(U7-Pad4)")
  (net 15 "Net-(U7-Pad2)")
  (net 16 "Net-(U7-Pad3)")
  (net 17 "Net-(U7-Pad20)")
  (net 18 "Net-(U7-Pad23)")
  (net 19 "Net-(U7-Pad33)")
  (net 20 "Net-(U7-Pad40)")
  (net 21 "Net-(U7-Pad50)")
  (net 22 "Net-(U7-Pad51)")
  (net 23 "Net-(U7-Pad52)")
  (net 24 "Net-(U7-Pad53)")
  (net 25 "Net-(U7-Pad54)")
  (net 26 "Net-(U7-Pad55)")
  (net 27 "Net-(U7-Pad56)")
  (net 28 "Net-(U7-Pad25)")
  (net 29 "Net-(U7-Pad59)")
  (net 30 "Net-(U7-Pad28)")
  (net 31 "Net-(P1-Pad1)")
  (net 32 "Net-(P2-Pad1)")
  (net 33 "Net-(P3-Pad1)")
  (net 34 SH1)
  (net 35 SH2)
  (net 36 SH3)
  (net 37 C1)
  (net 38 C2)
  (net 39 C3)
  (net 40 "Net-(C17-Pad2)")
  (net 41 "Net-(C18-Pad2)")
  (net 42 VCC)
  (net 43 SENS_SUPPLY)
  (net 44 "Net-(R6-Pad2)")
  (net 45 "Net-(R8-Pad2)")
  (net 46 "Net-(R10-Pad2)")
  (net 47 SENS_1)
  (net 48 SENS_2)
  (net 49 SENS_3)
  (net 50 I1)
  (net 51 I2)
  (net 52 I3)
  (net 53 LI1)
  (net 54 HI1)
  (net 55 LI2)
  (net 56 HI2)
  (net 57 LI3)
  (net 58 HI3)
  (net 59 "Net-(C23-Pad1)")
  (net 60 "Net-(C23-Pad2)")
  (net 61 USB-DM)
  (net 62 USB-DP)
  (net 63 "Net-(D3-Pad1)")
  (net 64 "Net-(D4-Pad1)")
  (net 65 LED_GREEN)
  (net 66 LED_RED)
  (net 67 HALL_1)
  (net 68 HALL_2)
  (net 69 HALL_3)
  (net 70 SWCLK)
  (net 71 SWDIO)
  (net 72 "Net-(C30-Pad1)")
  (net 73 "Net-(C31-Pad1)")
  (net 74 SERVO)
  (net 75 TEMP_MOTOR)
  (net 76 RX)
  (net 77 TX)
  (net 78 EN)
  (net 79 servoi)
  (net 80 "Net-(C77-Pad2)")
  (net 81 "Net-(Q4-Pad1)")
  (net 82 +5V)
  (net 83 "Net-(R7-Pad1)")
  (net 84 "Net-(R9-Pad1)")
  (net 85 "Net-(R11-Pad1)")
  (net 86 "Net-(R21-Pad2)")
  (net 87 VAA)
  (net 88 "Net-(C20-Pad2)")
  (net 89 "Net-(P10-Pad4)")
  (net 90 ADC_EXT2)
  (net 91 "Net-(P10-Pad5)")
  (net 92 ADC_EXT1)
  (net 93 +12V)
  (net 94 "Net-(C92-Pad2)")
  (net 95 "Net-(C92-Pad1)")
  (net 96 "Net-(C93-Pad2)")
  (net 97 "Net-(C93-Pad1)")
  (net 98 DRIVER)
  (net 99 CANH)
  (net 100 CANL)
  (net 101 TXC)
  (net 102 RXC)
  (net 103 "Net-(D2-Pad2)")
  (net 104 "Net-(Q7-Pad7)")
  (net 105 "Net-(Q7-Pad5)")
  (net 106 "Net-(C94-Pad1)")
  (net 107 "Net-(L2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.3)
    (via_dia 0.56)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net ADC_EXT1)
    (add_net ADC_EXT2)
    (add_net C1)
    (add_net C2)
    (add_net C3)
    (add_net CANH)
    (add_net CANL)
    (add_net DRIVER)
    (add_net EN)
    (add_net HALL_1)
    (add_net HALL_2)
    (add_net HALL_3)
    (add_net HI1)
    (add_net HI2)
    (add_net HI3)
    (add_net I1)
    (add_net I2)
    (add_net I3)
    (add_net LED_GREEN)
    (add_net LED_RED)
    (add_net LI1)
    (add_net LI2)
    (add_net LI3)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C30-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C77-Pad2)")
    (add_net "Net-(C92-Pad1)")
    (add_net "Net-(C92-Pad2)")
    (add_net "Net-(C93-Pad1)")
    (add_net "Net-(C93-Pad2)")
    (add_net "Net-(C94-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P10-Pad4)")
    (add_net "Net-(P10-Pad5)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(Q7-Pad5)")
    (add_net "Net-(Q7-Pad7)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U6-Pad4)")
    (add_net "Net-(U7-Pad2)")
    (add_net "Net-(U7-Pad20)")
    (add_net "Net-(U7-Pad23)")
    (add_net "Net-(U7-Pad25)")
    (add_net "Net-(U7-Pad28)")
    (add_net "Net-(U7-Pad3)")
    (add_net "Net-(U7-Pad33)")
    (add_net "Net-(U7-Pad4)")
    (add_net "Net-(U7-Pad40)")
    (add_net "Net-(U7-Pad50)")
    (add_net "Net-(U7-Pad51)")
    (add_net "Net-(U7-Pad52)")
    (add_net "Net-(U7-Pad53)")
    (add_net "Net-(U7-Pad54)")
    (add_net "Net-(U7-Pad55)")
    (add_net "Net-(U7-Pad56)")
    (add_net "Net-(U7-Pad59)")
    (add_net RX)
    (add_net RXC)
    (add_net SENS_1)
    (add_net SENS_2)
    (add_net SENS_3)
    (add_net SENS_SUPPLY)
    (add_net SERVO)
    (add_net SH1)
    (add_net SH2)
    (add_net SH3)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net TEMP_MOTOR)
    (add_net TX)
    (add_net TXC)
    (add_net USB-DM)
    (add_net USB-DP)
    (add_net VAA)
    (add_net VCC)
    (add_net VDD)
    (add_net VSS)
    (add_net servoi)
  )
  (module kicad_subory:WSON10__ (layer B.Cu) (tedit 59B97A00)
    (at 94.63 86.25 270)
    (solder_paste_ratio -0.1)
    (fp_text reference U3 (at 0 -5 270) (layer B.SilkS) hide)
    (fp_text value LM5001 (at 0 3.81 270) (layer B.Fab))
    (pad 7 smd rect (at -0.8 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 58 HI3))
    (pad 9 smd rect (at 0 0 270) (size 3 2.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 6 smd rect (at -1.6 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -1.6 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 0 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 57 LI3))
    (pad 3 smd rect (at 0 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(R10-Pad2)"))
    (pad 2 smd rect (at 0.8 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C3-Pad1)"))
    (pad 1 smd rect (at 1.6 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 93 +12V))
    (pad 4 smd rect (at -0.8 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 36 SH3))
    (pad 9 smd rect (at 0.8 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 10 smd rect (at 1.6 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(R11-Pad1)"))
    (model ../../../../../../Users/anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/wson.wrl
      (at (xyz -0.07874 0.07874 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5A41)
    (at 96.65 94.9)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C13 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 594197CB)
    (at 129.55 97.55 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R34 (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 VAA))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 TEMP_MOTOR))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 594197D1)
    (at 130.85 97.55 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C78 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 75 TEMP_MOTOR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59416163)
    (at 126 83.95 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R33 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 78 EN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59406C29)
    (at 80.6 88.1)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R32 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 10kNTC (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 87 VAA))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C77-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59406798)
    (at 128.15 97.55 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R31 (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C77-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5941615C)
    (at 126.55 97.6 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C77 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(C77-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE59B5)
    (at 129.5 88.75 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R30 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 100R (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 79 servoi))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 74 SERVO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE59B7)
    (at 129.5 87.2 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C76 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 100n (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 74 SERVO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58FC)
    (at 104.75 91)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C73 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5886)
    (at 96.65 87.1)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C72 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58A1)
    (at 96.65 89.05)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C71 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5914)
    (at 100.7 87.1 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C70 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58F0)
    (at 92.6 96.85 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C69 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE587D)
    (at 108.8 89.05 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C68 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A33)
    (at 100.7 92.95)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C67 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A3B)
    (at 104.75 92.95 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C66 (at 0 1.85 180) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A3F)
    (at 104.75 87.1 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C65 (at 0 1.85 180) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5A4A)
    (at 108.8 96.85 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C64 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58D4)
    (at 100.7 89.05 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C59 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59A950B3)
    (at 92.6 91 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C58 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5898)
    (at 96.65 91)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C57 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5869)
    (at 100.7 96.85 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C56 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58CE)
    (at 104.75 92.95)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C55 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58AF)
    (at 96.65 96.85)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C54 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5894)
    (at 100.7 94.9 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C53 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE586D)
    (at 104.75 94.9)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C52 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58CA)
    (at 104.75 87.1)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C51 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58A9)
    (at 100.7 92.95 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C50 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5890)
    (at 104.75 85.15)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C49 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5873)
    (at 104.75 96.85)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C48 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58C7)
    (at 108.8 92.95 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C47 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58A5)
    (at 96.65 92.95)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C46 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE588A)
    (at 96.65 85.15)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C45 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5879)
    (at 100.7 85.15 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C44 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE58E1)
    (at 100.7 89.05)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C43 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE58DD)
    (at 92.6 94.9 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C42 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE585B)
    (at 100.7 96.85)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C41 (at -0.85 7.05) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE585F)
    (at 108.8 91 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C40 (at -0.85 -10.5 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A2F)
    (at 104.75 89.05 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C38 (at 0 1.85 180) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A31)
    (at 104.75 91 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C37 (at 0 1.85 180) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5A3D)
    (at 100.7 91 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C34 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A35)
    (at 100.7 87.1)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C33 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5A48)
    (at 108.8 94.9 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C12 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A4B)
    (at 104.75 85.15 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C5 (at 0 1.85 180) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58EE5A46)
    (at 100.7 94.9)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module mojaKniznica:5x3.2KRISTALL (layer F.Cu) (tedit 58EE5B34)
    (at 121.32331 97.667094 180)
    (fp_text reference X1 (at 0.25908 -1.23952 180) (layer F.SilkS) hide)
    (fp_text value CRYSTAL_SMD (at 0.10922 1.48082 180) (layer F.SilkS) hide)
    (pad 3 smd rect (at -1.99898 -1.19888 180) (size 1.80086 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 1.99898 -1.19888 180) (size 1.80086 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C31-Pad1)"))
    (pad 1 smd rect (at -1.99898 1.19888 180) (size 1.80086 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C30-Pad1)"))
    (pad 3 smd rect (at 1.99898 1.19888 180) (size 1.80086 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model Crystals.3dshapes/Crystal_SMD_5032-4pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE5A5B)
    (at 117.4 97.667094 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 10pF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(C31-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE5A58)
    (at 125.2 97.667094 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C30 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 10pF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(C30-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE5965)
    (at 120 92.2 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R29 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 220R (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59C2)
    (at 122.9 92.2)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R28 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 220R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59C5)
    (at 115.9 90.4 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D4 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 LED_RED))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE596F)
    (at 115.9 91.6 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D3 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 LED_GREEN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE597B)
    (at 129.55 91.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R27 (at 0 1.45 270) (layer B.SilkS) hide)
    (fp_text value 22R (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.45 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 91 "Net-(P10-Pad5)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 62 USB-DP))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5973)
    (at 129.8 94.64 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R25 (at 0 1.45 90) (layer B.SilkS) hide)
    (fp_text value 22R (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 1.45 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 89 "Net-(P10-Pad4)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 61 USB-DM))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58EE59A3)
    (at 118.3 85.05 180)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (solder_paste_ratio -0.1)
    (attr smd)
    (fp_text reference U8 (at 0 -2.9 180) (layer F.SilkS) hide)
    (fp_text value LMR16006 (at 0 2.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C23-Pad2)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(R21-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 78 EN))
    (pad 6 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C23-Pad1)"))
    (pad 5 smd rect (at 1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59A1)
    (at 121.4 84.325)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 8k (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(R21-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59A9)
    (at 123.85 84.325 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 510R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(R21-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58EE5987)
    (at 122.05 87.25 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value D_Schottky (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/0sod-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE5989)
    (at 123.95 87.3 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C25 (at 0 -2.3 270) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 82 +5V))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58EE59BA)
    (at 115.65 84.35 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C24 (at 0 -2.3 90) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 1.45 0 90) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59A6)
    (at 120.6 86.55 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C23 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 220nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C23-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59FA)
    (at 117.2 93.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 100R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 I3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 C3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59F6)
    (at 120 93.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 100R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 I2))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 C2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE59F3)
    (at 122.9 93.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 100R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 I1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 C1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE5945)
    (at 78.5 86.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 2k2 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 SENS_3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE5941)
    (at 78.5 83.825 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 25k5 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 SENS_3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 SH3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE595C)
    (at 78.5 98.35 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 2k2 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 SENS_2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE5959)
    (at 78.5 95.6 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 25k5 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 SENS_2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 SH2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE594A)
    (at 78.5 92.25 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 2k2 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 SENS_1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE594F)
    (at 78.5 89.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 25k5 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 SENS_1))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 SH1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5A10)
    (at 97.7 87.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 7R5 (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(Q6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5A2B)
    (at 91.15 85.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 7R5 (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5A1F)
    (at 97.7 96.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 7R5 (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 84 "Net-(R9-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(Q4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5A73)
    (at 91.15 94.725 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 7R5 (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5A19)
    (at 97.7 92 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 7R5 (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(Q2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58EE5A26)
    (at 91.15 90.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.9 270) (layer B.SilkS) hide)
    (fp_text value 7R5 (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE598C)
    (at 129.1 83.95 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 2k2 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 SENS_SUPPLY))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58EE597D)
    (at 127.55 83.95 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 25k5 (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(Q7-Pad5)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 SENS_SUPPLY))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE5A56)
    (at 124.7 94 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE59AC)
    (at 125.5 97.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 220nF (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(C20-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A7A)
    (at 119 98.64)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 0 1.9) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 87 VAA))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A6C)
    (at 121.9 83.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 0 1.9) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(C18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE5A78)
    (at 115.1 88.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C17-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE5A76)
    (at 117.2 94.8 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 4n7 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 C3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE5A83)
    (at 120 94.8 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 4n7 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 C2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE5A70)
    (at 122.9 94.8 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 4n7 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 C1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE592F)
    (at 75 83.6)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 87 VAA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE593D)
    (at 75 89.4)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 87 VAA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EE593A)
    (at 75.05 95.2)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 87 VAA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A29)
    (at 90.65 87.7 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 1.9 180) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 93 +12V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A22)
    (at 90.7 96.7 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 1.9 180) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 93 +12V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A24)
    (at 90.65 92.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 1.9 180) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 93 +12V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A06)
    (at 89.875 85.6 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 220n (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 36 SH3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A16)
    (at 89.875 94.475 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 220n (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 35 SH2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58EE5A0C)
    (at 89.875 90.15 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.9 90) (layer B.SilkS) hide)
    (fp_text value 220n (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 34 SH1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:MSOP (layer F.Cu) (tedit 58EE5957)
    (at 75 92)
    (descr "MS8E Package; 8-Lead Plastic MSOP, Exposed Die Pad (see Linear Technology 05081662_K_MS8E.pdf)")
    (tags "SSOP 0.65")
    (solder_paste_ratio -0.1)
    (attr smd)
    (fp_text reference U4 (at 0 -2.55) (layer F.SilkS) hide)
    (fp_text value AD8418 (at 0 2.55) (layer F.Fab))
    (pad 8 smd rect (at 2.105 -0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 34 SH1))
    (pad 7 smd rect (at 2.105 -0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 87 VAA))
    (pad 6 smd rect (at 2.105 0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 87 VAA))
    (pad 5 smd rect (at 2.105 0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 50 I1))
    (pad 4 smd rect (at -2.105 0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U4-Pad4)"))
    (pad 3 smd rect (at -2.105 0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -2.105 -0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -2.105 -0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (model Housings_SSOP.3dshapes/MSOP-8-1EP_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:MSOP (layer F.Cu) (tedit 58EE595E)
    (at 75 97.8)
    (descr "MS8E Package; 8-Lead Plastic MSOP, Exposed Die Pad (see Linear Technology 05081662_K_MS8E.pdf)")
    (tags "SSOP 0.65")
    (solder_paste_ratio -0.1)
    (attr smd)
    (fp_text reference U5 (at 0 -2.55) (layer F.SilkS) hide)
    (fp_text value AD8418 (at 0 2.55) (layer F.Fab))
    (pad 8 smd rect (at 2.105 -0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 35 SH2))
    (pad 7 smd rect (at 2.105 -0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 87 VAA))
    (pad 6 smd rect (at 2.105 0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 87 VAA))
    (pad 5 smd rect (at 2.105 0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 51 I2))
    (pad 4 smd rect (at -2.105 0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U5-Pad4)"))
    (pad 3 smd rect (at -2.105 0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -2.105 -0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -2.105 -0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (model Housings_SSOP.3dshapes/MSOP-8-1EP_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:MSOP (layer F.Cu) (tedit 58EE594C)
    (at 75 86.2)
    (descr "MS8E Package; 8-Lead Plastic MSOP, Exposed Die Pad (see Linear Technology 05081662_K_MS8E.pdf)")
    (tags "SSOP 0.65")
    (solder_paste_ratio -0.1)
    (attr smd)
    (fp_text reference U6 (at 0 -2.55) (layer F.SilkS) hide)
    (fp_text value AD8418 (at 0 2.55) (layer F.Fab))
    (pad 8 smd rect (at 2.105 -0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 36 SH3))
    (pad 7 smd rect (at 2.105 -0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 87 VAA))
    (pad 6 smd rect (at 2.105 0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 87 VAA))
    (pad 5 smd rect (at 2.105 0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 52 I3))
    (pad 4 smd rect (at -2.105 0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U6-Pad4)"))
    (pad 3 smd rect (at -2.105 0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -2.105 -0.325) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -2.105 -0.975) (size 0.89 0.42) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (model Housings_SSOP.3dshapes/MSOP-8-1EP_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module crf1:lqfp64_pad_mod (layer B.Cu) (tedit 58EE5A69)
    (at 119.9 91 180)
    (descr LQFP-64)
    (solder_mask_margin -0.015)
    (solder_paste_ratio -0.12)
    (fp_text reference U7 (at 0 -1.143 180) (layer B.SilkS) hide)
    (fp_text value STM32F40X_LQFP64 (at 0 1.143 180) (layer B.SilkS) hide)
    (pad 4 smd rect (at -2.25044 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(U7-Pad4)"))
    (pad 5 smd rect (at -1.75006 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(C30-Pad1)"))
    (pad 6 smd rect (at -1.24968 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(C31-Pad1)"))
    (pad 7 smd rect (at -0.7493 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(C20-Pad2)"))
    (pad 8 smd rect (at -0.24892 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 37 C1))
    (pad 1 smd rect (at -3.74904 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 42 VCC))
    (pad 2 smd rect (at -3.2512 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(U7-Pad2)"))
    (pad 3 smd rect (at -2.75082 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(U7-Pad3)"))
    (pad 17 smd rect (at 5.75056 -3.74904 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(C77-Pad2)"))
    (pad 18 smd rect (at 5.75056 -3.2512 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 19 smd rect (at 5.75056 -2.75082 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 42 VCC))
    (pad 20 smd rect (at 5.75056 -2.25044 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(U7-Pad20)"))
    (pad 21 smd rect (at 5.75056 -1.75006 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 92 ADC_EXT1))
    (pad 22 smd rect (at 5.75056 -1.24968 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 90 ADC_EXT2))
    (pad 23 smd rect (at 5.75056 -0.7493 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(U7-Pad23)"))
    (pad 24 smd rect (at 5.75056 -0.24892 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 75 TEMP_MOTOR))
    (pad 33 smd rect (at 3.74904 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(U7-Pad33)"))
    (pad 34 smd rect (at 3.2512 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 53 LI1))
    (pad 35 smd rect (at 2.75082 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 55 LI2))
    (pad 36 smd rect (at 2.25044 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 57 LI3))
    (pad 37 smd rect (at 1.75006 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 67 HALL_1))
    (pad 38 smd rect (at 1.24968 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 68 HALL_2))
    (pad 39 smd rect (at 0.7493 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 69 HALL_3))
    (pad 40 smd rect (at 0.24892 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(U7-Pad40)"))
    (pad 49 smd rect (at -5.75056 3.74904 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 70 SWCLK))
    (pad 50 smd rect (at -5.75056 3.2512 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(U7-Pad50)"))
    (pad 51 smd rect (at -5.75056 2.75082 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(U7-Pad51)"))
    (pad 52 smd rect (at -5.75056 2.25044 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(U7-Pad52)"))
    (pad 53 smd rect (at -5.75056 1.75006 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(U7-Pad53)"))
    (pad 54 smd rect (at -5.75056 1.24968 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U7-Pad54)"))
    (pad 55 smd rect (at -5.75056 0.7493 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(U7-Pad55)"))
    (pad 56 smd rect (at -5.75056 0.24892 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(U7-Pad56)"))
    (pad 9 smd rect (at 0.24892 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 38 C2))
    (pad 10 smd rect (at 0.7493 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 39 C3))
    (pad 11 smd rect (at 1.24968 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 43 SENS_SUPPLY))
    (pad 25 smd rect (at 5.75056 0.24892 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(U7-Pad25)"))
    (pad 26 smd rect (at 5.75056 0.7493 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 65 LED_GREEN))
    (pad 27 smd rect (at 5.75056 1.24968 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 66 LED_RED))
    (pad 41 smd rect (at -0.24892 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 54 HI1))
    (pad 42 smd rect (at -0.7493 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 56 HI2))
    (pad 43 smd rect (at -1.24968 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 58 HI3))
    (pad 57 smd rect (at -5.75056 -0.24892 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 98 DRIVER))
    (pad 58 smd rect (at -5.75056 -0.7493 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 74 SERVO))
    (pad 59 smd rect (at -5.75056 -1.24968 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(U7-Pad59)"))
    (pad 12 smd rect (at 1.75006 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 13 smd rect (at 2.25044 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 87 VAA))
    (pad 14 smd rect (at 2.75082 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 47 SENS_1))
    (pad 15 smd rect (at 3.2512 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 48 SENS_2))
    (pad 16 smd rect (at 3.74904 -5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 49 SENS_3))
    (pad 28 smd rect (at 5.75056 1.75006 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(U7-Pad28)"))
    (pad 29 smd rect (at 5.75056 2.25044 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 77 TX))
    (pad 30 smd rect (at 5.75056 2.75082 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 76 RX))
    (pad 31 smd rect (at 5.75056 3.2512 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(C17-Pad2)"))
    (pad 32 smd rect (at 5.75056 3.74904 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 42 VCC))
    (pad 44 smd rect (at -1.75006 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 61 USB-DM))
    (pad 45 smd rect (at -2.25044 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 62 USB-DP))
    (pad 46 smd rect (at -2.75082 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 71 SWDIO))
    (pad 47 smd rect (at -3.2512 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(C18-Pad2)"))
    (pad 48 smd rect (at -3.74904 5.75056 180) (size 0.3 1.30048) (layers B.Cu B.Paste B.Mask)
      (net 42 VCC))
    (pad 60 smd rect (at -5.75056 -1.75006 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 61 smd rect (at -5.75056 -2.25044 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 102 RXC))
    (pad 62 smd rect (at -5.75056 -2.75082 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 101 TXC))
    (pad 63 smd rect (at -5.75056 -3.2512 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 64 smd rect (at -5.75056 -3.74904 180) (size 1.30048 0.3) (layers B.Cu B.Paste B.Mask)
      (net 42 VCC))
    (model ../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/bldc-hardware-master/design/Libraries/3D/lqfp-64.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:JST_ZH_1.5_6-Pin (layer F.Cu) (tedit 58EFBE8E)
    (at 112.3 91 90)
    (fp_text reference P9 (at 0 9.5 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -7.5 90) (layer F.Fab) hide)
    (pad 3 thru_hole rect (at 0.75 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 67 HALL_1))
    (pad 4 thru_hole rect (at -0.75 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 68 HALL_2))
    (pad 2 thru_hole rect (at 2.25 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 75 TEMP_MOTOR))
    (pad 1 thru_hole rect (at 3.75 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 82 +5V))
    (pad 5 thru_hole rect (at -2.25 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 69 HALL_3))
    (pad 6 thru_hole rect (at -3.75 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 VSS))
  )
  (module kicad_subory:JST_ZH_1.5_6-Pin (layer F.Cu) (tedit 58EE599E)
    (at 127.575 91 270)
    (fp_text reference P10 (at 0 9.5 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -7.5 270) (layer F.Fab))
    (pad 3 thru_hole rect (at 0.75 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 70 SWCLK))
    (pad 4 thru_hole rect (at -0.75 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 89 "Net-(P10-Pad4)"))
    (pad 2 thru_hole rect (at 2.25 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 71 SWDIO))
    (pad 1 thru_hole rect (at 3.75 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 78 EN))
    (pad 5 thru_hole rect (at -2.25 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 91 "Net-(P10-Pad5)"))
    (pad 6 thru_hole rect (at -3.75 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 VSS))
  )
  (module kicad_subory:JST_ZH_1.5_6-Pin (layer F.Cu) (tedit 58EE59B2)
    (at 131.45 91 270)
    (fp_text reference P11 (at 0 9.5 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -7.5 270) (layer F.Fab))
    (pad 3 thru_hole rect (at 0.75 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 100 CANL))
    (pad 4 thru_hole rect (at -0.75 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 82 +5V))
    (pad 2 thru_hole rect (at 2.25 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 99 CANH))
    (pad 1 thru_hole rect (at 3.75 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 92 ADC_EXT1))
    (pad 5 thru_hole rect (at -2.25 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 79 servoi))
    (pad 6 thru_hole rect (at -3.75 0 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 VSS))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE5937)
    (at 70.4 93.15 90)
    (fp_text reference P1 (at 2 1 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.1 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 1.1 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 1.1 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad1)"))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE5969)
    (at 68.2 94.65 270)
    (fp_text reference P2 (at 2 1 270) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.1 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 1.1 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 1.1 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 32 "Net-(P2-Pad1)"))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE5932)
    (at 70.4 87.35 90)
    (fp_text reference P3 (at 2 1 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.1 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 1.1 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 1.1 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 1.8 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 2.5 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 1 thru_hole rect (at 3.2 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 33 "Net-(P3-Pad1)"))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE5928)
    (at 79.5 88.9 270)
    (fp_text reference P4 (at 2 1 270) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.1 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 SH1))
    (pad 1 thru_hole rect (at 1.1 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 SH1))
    (pad 1 thru_hole rect (at 1.1 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 SH1))
    (pad 1 thru_hole rect (at 1.8 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 SH1))
    (pad 1 thru_hole rect (at 1.8 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 SH1))
    (pad 1 thru_hole rect (at 1.8 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 SH1))
    (pad 1 thru_hole rect (at 2.5 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 SH1))
    (pad 1 thru_hole rect (at 2.5 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 SH1))
    (pad 1 thru_hole rect (at 2.5 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 SH1))
    (pad 1 thru_hole rect (at 3.2 -0.4 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 SH1))
    (pad 1 thru_hole rect (at 3.2 -1.1 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 SH1))
    (pad 1 thru_hole rect (at 3.2 -1.8 270) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 34 SH1))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE592B)
    (at 81.7 98.95 90)
    (fp_text reference P5 (at 2 1 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.1 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 35 SH2))
    (pad 1 thru_hole rect (at 1.1 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 35 SH2))
    (pad 1 thru_hole rect (at 1.1 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 35 SH2))
    (pad 1 thru_hole rect (at 1.8 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 35 SH2))
    (pad 1 thru_hole rect (at 1.8 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 35 SH2))
    (pad 1 thru_hole rect (at 1.8 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 35 SH2))
    (pad 1 thru_hole rect (at 2.5 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 35 SH2))
    (pad 1 thru_hole rect (at 2.5 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 35 SH2))
    (pad 1 thru_hole rect (at 2.5 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 35 SH2))
    (pad 1 thru_hole rect (at 3.2 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 35 SH2))
    (pad 1 thru_hole rect (at 3.2 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 35 SH2))
    (pad 1 thru_hole rect (at 3.2 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 35 SH2))
  )
  (module kicad_subory:prekov (layer F.Cu) (tedit 58EE5924)
    (at 81.7 87.45 90)
    (fp_text reference P6 (at 2 1 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 2 -4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.1 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 SH3))
    (pad 1 thru_hole rect (at 1.1 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 SH3))
    (pad 1 thru_hole rect (at 1.1 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 SH3))
    (pad 1 thru_hole rect (at 1.8 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 SH3))
    (pad 1 thru_hole rect (at 1.8 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 SH3))
    (pad 1 thru_hole rect (at 1.8 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 SH3))
    (pad 1 thru_hole rect (at 2.5 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 SH3))
    (pad 1 thru_hole rect (at 2.5 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 SH3))
    (pad 1 thru_hole rect (at 2.5 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 SH3))
    (pad 1 thru_hole rect (at 3.2 -0.4 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 SH3))
    (pad 1 thru_hole rect (at 3.2 -1.1 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 SH3))
    (pad 1 thru_hole rect (at 3.2 -1.8 90) (size 0.7 0.7) (drill 0.5) (layers *.Cu *.Mask)
      (net 36 SH3))
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59B1B2AE)
    (at 92.6 87.1 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C28 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 59B1B2E0)
    (at 104.75 94.9 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C32 (at 0 1.85 180) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59B1B2BD)
    (at 108.8 85.15 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C35 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59B1B2A3)
    (at 92.6 92.95 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C36 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59B1B2B3)
    (at 92.6 85.15 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C39 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59B1B2B7)
    (at 104.75 89.05)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C60 (at 0 -1.85) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59B1B2C2)
    (at 108.8 87.1 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C61 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 59B1B2A9)
    (at 92.6 89.05 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C62 (at 0 -1.85 180) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 59B1B2FE)
    (at 100.7 85.15)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C63 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 59B1B2E6)
    (at 100.7 91)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C74 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 59B1B306)
    (at 104.75 96.85 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C75 (at 0 1.85 180) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 59B1B302)
    (at 108.8 85.15)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C79 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 59B1B2DB)
    (at 108.8 87.1)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C80 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 59B1B2CD)
    (at 108.8 94.9)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C81 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 59B1B2C9)
    (at 108.8 96.85)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C82 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 59B1B2D8)
    (at 108.8 89.05)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C83 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value C (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 59B1B2D4)
    (at 108.8 91)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C84 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 59B1B2D0)
    (at 108.8 92.95)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C85 (at 0 1.85) (layer B.SilkS) hide)
    (fp_text value 10u (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:DFN5 (layer B.Cu) (tedit 59B3E4F4)
    (at 85.295 91)
    (solder_paste_ratio -0.1)
    (fp_text reference Q1 (at -4.5 0 90) (layer B.SilkS) hide)
    (fp_text value Q_NMOS_GSD (at -0.25 3.5) (layer B.Fab))
    (pad 3 smd rect (at 2.9875 -1.905) (size 0.425 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at -2.795 -1.905) (size 1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -2.795 -0.635) (size 1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 34 SH1))
    (pad 2 smd rect (at -2.795 0.635) (size 1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 34 SH1))
    (pad 2 smd rect (at -2.795 1.905) (size 1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 34 SH1))
    (pad 3 smd rect (at 0.7225 0) (size 4.105 4.56) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 2.9875 1.905) (size 0.425 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at -0.4525 2.5275) (size 0.905 0.495) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at -0.4525 -2.5275) (size 0.905 0.495) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model "../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/1PQFN 5x6.wrl"
      (at (xyz -0.12 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:DFN5 (layer F.Cu) (tedit 59B1B29A)
    (at 85.3 91 180)
    (solder_paste_ratio -0.1)
    (fp_text reference Q2 (at -4.5 0 270) (layer F.SilkS) hide)
    (fp_text value Q_NMOS_GSD (at -0.25 -3.5 180) (layer F.Fab))
    (pad 3 smd rect (at 2.9875 1.905 180) (size 0.425 0.75) (layers F.Cu F.Paste F.Mask)
      (net 34 SH1))
    (pad 1 smd rect (at -2.795 1.905 180) (size 1 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at -2.795 0.635 180) (size 1 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -2.795 -0.635 180) (size 1 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -2.795 -1.905 180) (size 1 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 3 smd rect (at 0.7225 0 180) (size 4.105 4.56) (layers F.Cu F.Paste F.Mask)
      (net 34 SH1))
    (pad 3 smd rect (at 2.9875 -1.905 180) (size 0.425 0.75) (layers F.Cu F.Paste F.Mask)
      (net 34 SH1))
    (pad 3 smd rect (at -0.4525 -2.5275 180) (size 0.905 0.495) (layers F.Cu F.Paste F.Mask)
      (net 34 SH1))
    (pad 3 smd rect (at -0.4525 2.5275 180) (size 0.905 0.495) (layers F.Cu F.Paste F.Mask)
      (net 34 SH1))
    (model "../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/1PQFN 5x6.wrl"
      (at (xyz -0.12 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:DFN5 (layer B.Cu) (tedit 59B3E4F8)
    (at 85.295 96.8)
    (solder_paste_ratio -0.1)
    (fp_text reference Q3 (at -4.5 0 90) (layer B.SilkS) hide)
    (fp_text value Q_NMOS_GSD (at -0.25 3.5) (layer B.Fab))
    (pad 3 smd rect (at 2.9875 -1.905) (size 0.425 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at -2.795 -1.905) (size 1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at -2.795 -0.635) (size 1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 35 SH2))
    (pad 2 smd rect (at -2.795 0.635) (size 1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 35 SH2))
    (pad 2 smd rect (at -2.795 1.905) (size 1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 35 SH2))
    (pad 3 smd rect (at 0.7225 0) (size 4.105 4.56) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 2.9875 1.905) (size 0.425 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at -0.4525 2.5275) (size 0.905 0.495) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at -0.4525 -2.5275) (size 0.905 0.495) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model "../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/1PQFN 5x6.wrl"
      (at (xyz -0.12 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:DFN5 (layer F.Cu) (tedit 59B1B29E)
    (at 85.305 96.8 180)
    (solder_paste_ratio -0.1)
    (fp_text reference Q4 (at -4.5 0 270) (layer F.SilkS) hide)
    (fp_text value Q_NMOS_GSD (at -0.25 -3.5 180) (layer F.Fab))
    (pad 3 smd rect (at 2.9875 1.905 180) (size 0.425 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 SH2))
    (pad 1 smd rect (at -2.795 1.905 180) (size 1 0.75) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at -2.795 0.635 180) (size 1 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -2.795 -0.635 180) (size 1 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -2.795 -1.905 180) (size 1 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 3 smd rect (at 0.7225 0 180) (size 4.105 4.56) (layers F.Cu F.Paste F.Mask)
      (net 35 SH2))
    (pad 3 smd rect (at 2.9875 -1.905 180) (size 0.425 0.75) (layers F.Cu F.Paste F.Mask)
      (net 35 SH2))
    (pad 3 smd rect (at -0.4525 -2.5275 180) (size 0.905 0.495) (layers F.Cu F.Paste F.Mask)
      (net 35 SH2))
    (pad 3 smd rect (at -0.4525 2.5275 180) (size 0.905 0.495) (layers F.Cu F.Paste F.Mask)
      (net 35 SH2))
    (model "../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/1PQFN 5x6.wrl"
      (at (xyz -0.12 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:DFN5 (layer B.Cu) (tedit 59B3E4F0)
    (at 85.295 85.2)
    (solder_paste_ratio -0.1)
    (fp_text reference Q5 (at -4.5 0 90) (layer B.SilkS) hide)
    (fp_text value Q_NMOS_GSD (at -0.25 3.5) (layer B.Fab))
    (pad 3 smd rect (at 2.9875 -1.905) (size 0.425 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 1 smd rect (at -2.795 -1.905) (size 1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at -2.795 -0.635) (size 1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 36 SH3))
    (pad 2 smd rect (at -2.795 0.635) (size 1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 36 SH3))
    (pad 2 smd rect (at -2.795 1.905) (size 1 0.75) (layers B.Cu B.Paste B.Mask)
      (net 36 SH3))
    (pad 3 smd rect (at 0.7225 0) (size 4.105 4.56) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at 2.9875 1.905) (size 0.425 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at -0.4525 2.5275) (size 0.905 0.495) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 3 smd rect (at -0.4525 -2.5275) (size 0.905 0.495) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model "../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/1PQFN 5x6.wrl"
      (at (xyz -0.12 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:DFN5 (layer F.Cu) (tedit 59B1B296)
    (at 85.305 85.2 180)
    (solder_paste_ratio -0.1)
    (fp_text reference Q6 (at -4.5 0 270) (layer F.SilkS) hide)
    (fp_text value Q_NMOS_GSD (at -0.25 -3.5 180) (layer F.Fab))
    (pad 3 smd rect (at 2.9875 1.905 180) (size 0.425 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 SH3))
    (pad 1 smd rect (at -2.795 1.905 180) (size 1 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at -2.795 0.635 180) (size 1 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -2.795 -0.635 180) (size 1 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -2.795 -1.905 180) (size 1 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 3 smd rect (at 0.7225 0 180) (size 4.105 4.56) (layers F.Cu F.Paste F.Mask)
      (net 36 SH3))
    (pad 3 smd rect (at 2.9875 -1.905 180) (size 0.425 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 SH3))
    (pad 3 smd rect (at -0.4525 -2.5275 180) (size 0.905 0.495) (layers F.Cu F.Paste F.Mask)
      (net 36 SH3))
    (pad 3 smd rect (at -0.4525 2.5275 180) (size 0.905 0.495) (layers F.Cu F.Paste F.Mask)
      (net 36 SH3))
    (model "../../../../../../Users/Anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/1PQFN 5x6.wrl"
      (at (xyz -0.12 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mojaKniznica:2512Rv2 (layer B.Cu) (tedit 59B38876)
    (at 75 91)
    (fp_text reference R1 (at 0 -3.6) (layer B.SilkS) hide)
    (fp_text value RSENS (at 0.2 3.4) (layer B.Fab))
    (pad 1 smd rect (at -2.6 0) (size 1.8 3.4) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 2.6 0) (size 1.8 3.4) (layers B.Cu B.Paste B.Mask)
      (net 34 SH1))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mojaKniznica:2512Rv2 (layer B.Cu) (tedit 59B38876)
    (at 75 96.8)
    (fp_text reference R2 (at 0 -3.6) (layer B.SilkS) hide)
    (fp_text value RSENS (at 0.2 3.4) (layer B.Fab))
    (pad 1 smd rect (at -2.6 0) (size 1.8 3.4) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(P2-Pad1)"))
    (pad 2 smd rect (at 2.6 0) (size 1.8 3.4) (layers B.Cu B.Paste B.Mask)
      (net 35 SH2))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mojaKniznica:2512Rv2 (layer B.Cu) (tedit 59B38876)
    (at 75 85.2)
    (fp_text reference R3 (at 0 -3.6) (layer B.SilkS) hide)
    (fp_text value RSENS (at 0.2 3.4) (layer B.Fab))
    (pad 1 smd rect (at -2.6 0) (size 1.8 3.4) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at 2.6 0) (size 1.8 3.4) (layers B.Cu B.Paste B.Mask)
      (net 36 SH3))
    (model Resistors_SMD.3dshapes/R_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59B3E0C0)
    (at 115.1 94.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59B3E41D)
    (at 124.72 83.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 42 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59B3E42B)
    (at 122.85 98.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C27 (at 0 1.5 180) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 42 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59B3E417)
    (at 116.3 88.5 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C29 (at 0 -1.5 270) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mojaKniznica:WE-MAPI (layer F.Cu) (tedit 59B3E413)
    (at 119.25 89.45 270)
    (fp_text reference L1 (at 0.01 2.77 270) (layer F.SilkS) hide)
    (fp_text value 22uH (at -0.03 -2.58 270) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 270) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 1.05 0 270) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask)
      (net 82 +5V))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 2 3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59B3E426)
    (at 116.3 98.63 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C86 (at 0 1.5 180) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 87 VAA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59B3DE17)
    (at 131.7 97.417242 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C87 (at 0 1.5 270) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 82 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59B3DE27)
    (at 126.6 84.4 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C88 (at 0 1.5 90) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 42 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59B3DE23)
    (at 132.79 84.1 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C89 (at 0 1.5 270) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 82 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59B3DE0F)
    (at 127.3 97.417242 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C90 (at 0 1.5 270) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 87 VAA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 59B3DE13)
    (at 129.5 97.6)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U10 (at 0 2.5) (layer B.SilkS) hide)
    (fp_text value MCP1700 (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 87 VAA))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 82 +5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module kicad_subory:WSON10__ (layer B.Cu) (tedit 59B97A00)
    (at 94.62 90.75 270)
    (solder_paste_ratio -0.1)
    (fp_text reference U1 (at 0 -5 270) (layer B.SilkS) hide)
    (fp_text value LM5001 (at 0 3.81 270) (layer B.Fab))
    (pad 7 smd rect (at -0.8 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 54 HI1))
    (pad 9 smd rect (at 0 0 270) (size 3 2.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 6 smd rect (at -1.6 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -1.6 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 0 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 53 LI1))
    (pad 3 smd rect (at 0 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(R6-Pad2)"))
    (pad 2 smd rect (at 0.8 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at 1.6 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 93 +12V))
    (pad 4 smd rect (at -0.8 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 34 SH1))
    (pad 9 smd rect (at 0.8 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 10 smd rect (at 1.6 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(R7-Pad1)"))
    (model ../../../../../../Users/anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/wson.wrl
      (at (xyz -0.07874 0.07874 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad_subory:WSON10__ (layer B.Cu) (tedit 59B97A00)
    (at 94.64 95.25 270)
    (solder_paste_ratio -0.1)
    (fp_text reference U2 (at 0 -5 270) (layer B.SilkS) hide)
    (fp_text value LM5001 (at 0 3.81 270) (layer B.Fab))
    (pad 7 smd rect (at -0.8 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 56 HI2))
    (pad 9 smd rect (at 0 0 270) (size 3 2.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 6 smd rect (at -1.6 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -1.6 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 0 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 55 LI2))
    (pad 3 smd rect (at 0 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R8-Pad2)"))
    (pad 2 smd rect (at 0.8 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at 1.6 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 93 +12V))
    (pad 4 smd rect (at -0.8 1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 35 SH2))
    (pad 9 smd rect (at 0.8 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 10 smd rect (at 1.6 -1.9 270) (size 0.3 0.6) (layers B.Cu B.Paste B.Mask)
      (net 84 "Net-(R9-Pad1)"))
    (model ../../../../../../Users/anton/OneDrive/Work/Work/Kicad/kicad_subory/3dmodels/wson.wrl
      (at (xyz -0.07874 0.07874 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59BC3A9A)
    (at 134.5 85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C91 (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 82 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59BC3A81)
    (at 136.225 93.825)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C92 (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 94 "Net-(C92-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 95 "Net-(C92-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59BC3A8A)
    (at 133.65 93.825 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C93 (at 0 1.5 180) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 96 "Net-(C93-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(C93-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59BC3A9E)
    (at 135.2 83.85)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C94 (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value 2u2 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 106 "Net-(C94-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 59BC3A7B)
    (at 135.1 89.125 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U11 (at 0 3.5 90) (layer B.SilkS) hide)
    (fp_text value MAX662 (at 0 -3.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 94 "Net-(C92-Pad2)"))
    (pad 2 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 95 "Net-(C92-Pad1)"))
    (pad 3 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(C93-Pad1)"))
    (pad 4 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 96 "Net-(C93-Pad2)"))
    (pad 5 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 82 +5V))
    (pad 6 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 106 "Net-(C94-Pad1)"))
    (pad 7 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 8 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 98 DRIVER))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-8-1EP_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 59BC3A6D)
    (at 135.075 95.75 90)
    (descr "8-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.65")
    (attr smd)
    (fp_text reference U12 (at 0 -2.55 90) (layer F.SilkS) hide)
    (fp_text value TJA1051TK/3 (at 0 2.55 90) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -0.975 90) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 101 TXC))
    (pad 2 smd rect (at -1.55 -0.325 90) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 3 smd rect (at -1.55 0.325 90) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 82 +5V))
    (pad 4 smd rect (at -1.55 0.975 90) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 102 RXC))
    (pad 5 smd rect (at 1.55 0.975 90) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (pad 6 smd rect (at 1.55 0.325 90) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 100 CANL))
    (pad 7 smd rect (at 1.55 -0.325 90) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 99 CANH))
    (pad 8 smd rect (at 1.55 -0.975 90) (size 0.65 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 9 smd rect (at 0.3875 0.6 90) (size 0.775 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0.3875 -0.6 90) (size 0.775 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.3875 0.6 90) (size 0.775 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at -0.3875 -0.6 90) (size 0.775 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS) (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59BC3A69)
    (at 135.1 92.9 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C95 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59BC3A71)
    (at 135.1 98.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C96 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 2u2 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 82 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59BC3A4B)
    (at 133.575 83.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value D_Zener (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mojaKniznica:TSMT8 (layer F.Cu) (tedit 59BC3A5C)
    (at 135.175 88.095)
    (fp_text reference Q7 (at 0 4.1) (layer F.SilkS) hide)
    (fp_text value Q8M51TR-E (at 0 -4.1) (layer F.Fab))
    (pad 7 smd rect (at -0.325 -1.205) (size 0.47 0.49) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(Q7-Pad7)"))
    (pad 6 smd rect (at 0.325 -1.205) (size 0.47 0.49) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(Q7-Pad5)"))
    (pad 5 smd rect (at 0.975 -1.205) (size 0.47 0.49) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(Q7-Pad5)"))
    (pad 8 smd rect (at -0.975 -1.205) (size 0.47 0.49) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(Q7-Pad7)"))
    (pad 1 smd rect (at -0.975 1.205) (size 0.47 0.49) (layers F.Cu F.Paste F.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at -0.325 1.205) (size 0.47 0.49) (layers F.Cu F.Paste F.Mask)
      (net 82 +5V))
    (pad 3 smd rect (at 0.325 1.205) (size 0.47 0.49) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 4 smd rect (at 0.975 1.205) (size 0.47 0.49) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/DFN-8-1EP_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 0.75 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59BC3A63)
    (at 133.575 84.9 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value 7R5 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(Q7-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59BC3A54)
    (at 136.025 84.9)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R24 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 7R5 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59BC3A92)
    (at 133.75 95.85 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R26 (at 0 1.45 90) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 78 EN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59BC3A58)
    (at 135.1 91.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R35 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 7R5 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 99 CANH))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 100 CANL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59BC3A50)
    (at 130.65 83.95 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R36 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value 25k5 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 SENS_SUPPLY))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59BC3A47)
    (at 136.025 83.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R37 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value 100R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(C94-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59BCFA01)
    (at 127.83 84.4 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L2 (at 0 1.45 270) (layer B.SilkS) hide)
    (fp_text value 2.2uH (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 107 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 42 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer B.Cu) (tedit 59BCF9FD)
    (at 130.3 84.4 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U9 (at 0 2.9 180) (layer B.SilkS) hide)
    (fp_text value LM3671 (at 0 -2.9 180) (layer B.Fab))
    (fp_text user %R (at 0 0 450) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 82 +5V))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 4 VSS))
    (pad 3 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 82 +5V))
    (pad 4 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 42 VCC))
    (pad 5 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 107 "Net-(L2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text antonchromjak@gmail.com (at 76.38 93.86) (layer B.Mask))
  (gr_text antonchromjak@gmail.com (at 71.79 91.25 90) (layer F.Mask))
  (gr_text antonchromjak@gmail.com (at 76.38 93.86 360) (layer B.Cu))
  (gr_arc (start 136 98) (end 138 98) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_arc (start 136 84) (end 136 82) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 138 84) (end 138 98) (layer Edge.Cuts) (width 0.001))
  (gr_text GND (at 115.6 98 90) (layer F.SilkS))
  (gr_text DP (at 126.2 88.8) (layer F.SilkS))
  (gr_text DM (at 126.2 90.3) (layer F.SilkS))
  (gr_text SWC (at 126.2 91.8) (layer F.SilkS))
  (gr_text SWD (at 126.2 93.3) (layer F.SilkS))
  (gr_text EN (at 126.5 94.8) (layer F.SilkS))
  (gr_text A1 (at 130.3 94.8) (layer F.SilkS))
  (gr_text CH (at 129.9 93.3) (layer F.SilkS))
  (gr_text CL (at 129.9 91.8) (layer F.SilkS))
  (gr_text +5V (at 130 90.3) (layer F.SilkS))
  (gr_text PPM (at 130 88.8) (layer F.SilkS))
  (gr_text GND (at 126.1 87.2) (layer F.SilkS))
  (gr_text GND (at 130 87.3) (layer F.SilkS))
  (gr_text T (at 113.9 88.8) (layer F.SilkS))
  (gr_text GND (at 113.7 95.2) (layer F.SilkS))
  (gr_text H3 (at 113.6 93.3) (layer F.SilkS))
  (gr_text H2 (at 113.6 91.8) (layer F.SilkS))
  (gr_text H1 (at 113.6 90.3) (layer F.SilkS))
  (gr_text +5V (at 113.7 87.2) (layer F.SilkS))
  (gr_arc (start 70 84) (end 68 84) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_arc (start 70 98) (end 70 100) (angle 90) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 68 84) (end 68 98) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 70 100) (end 136 100) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 70 82) (end 136 82) (layer Edge.Cuts) (width 0.001))
  (dimension 70 (width 0.1) (layer Dwgs.User)
    (gr_text "70.000 mm" (at 103 78.705785) (layer Dwgs.User))
    (feature1 (pts (xy 68 82) (xy 68 77.755785)))
    (feature2 (pts (xy 138 82) (xy 138 77.755785)))
    (crossbar (pts (xy 138 79.655785) (xy 68 79.655785)))
    (arrow1a (pts (xy 68 79.655785) (xy 69.126504 79.069364)))
    (arrow1b (pts (xy 68 79.655785) (xy 69.126504 80.242206)))
    (arrow2a (pts (xy 138 79.655785) (xy 136.873496 79.069364)))
    (arrow2b (pts (xy 138 79.655785) (xy 136.873496 80.242206)))
  )
  (dimension 18 (width 0.1) (layer Dwgs.User)
    (gr_text "18.000 mm" (at 64.65 90.956115 90) (layer Dwgs.User))
    (feature1 (pts (xy 68 81.956115) (xy 63.3 81.956115)))
    (feature2 (pts (xy 68 99.956115) (xy 63.3 99.956115)))
    (crossbar (pts (xy 66 99.956115) (xy 66 81.956115)))
    (arrow1a (pts (xy 66 81.956115) (xy 66.586421 83.082619)))
    (arrow1b (pts (xy 66 81.956115) (xy 65.413579 83.082619)))
    (arrow2a (pts (xy 66 99.956115) (xy 66.586421 98.829611)))
    (arrow2b (pts (xy 66 99.956115) (xy 65.413579 98.829611)))
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.6 83.2) (xy 70.6 87.25) (xy 67.65 87.25) (xy 67.65 83.2)
      )
    )
  )
  (zone (net 33) (net_name "Net-(P3-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.03))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 82.4) (xy 71 88) (xy 68 88) (xy 68 82.4)
      )
    )
  )
  (zone (net 33) (net_name "Net-(P3-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.03))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73.3 83.5) (xy 73.3 86.9) (xy 71.5 86.9) (xy 71.137099 87.677223) (xy 70.7 88)
        (xy 68 88) (xy 68 82.4) (xy 70.65 82.4) (xy 71.117815 82.647452) (xy 71.55 83.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67.65 83.2) (xy 67.65 87.25) (xy 70.6 87.25) (xy 70.6 83.2)
      )
    )
  )
  (zone (net 31) (net_name "Net-(P1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.03))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73.3 89.3) (xy 71.55 89.3) (xy 71.115992 88.477243) (xy 70.75 88.2) (xy 68 88.2)
        (xy 68 93.8) (xy 70.75 93.8) (xy 71.086656 93.587579) (xy 71.5 92.7) (xy 73.3 92.7)
      )
    )
  )
  (zone (net 31) (net_name "Net-(P1-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.03))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 88.2) (xy 71 93.8) (xy 68 93.8) (xy 68 88.2)
      )
    )
  )
  (zone (net 32) (net_name "Net-(P2-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.03))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73.3 95.1) (xy 73.3 98.5) (xy 71.5 98.5) (xy 71.129092 99.315998) (xy 70.75 99.6)
        (xy 68 99.6) (xy 68 94) (xy 70.75 94) (xy 71.108778 94.239312) (xy 71.5 95.1)
      )
    )
  )
  (zone (net 32) (net_name "Net-(P2-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.03))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 94) (xy 68 94) (xy 68 99.6) (xy 71 99.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.55 89) (xy 67.65 89) (xy 67.65 93) (xy 70.55 93)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.55 94.8) (xy 67.65 94.8) (xy 67.65 98.8) (xy 70.55 98.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67.65 89) (xy 70.55 89) (xy 70.55 93) (xy 67.65 93)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67.65 94.8) (xy 70.55 94.8) (xy 70.55 98.8) (xy 67.65 98.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.55 83.9) (xy 80.1 83.35) (xy 81.1 83.35) (xy 81.65 83.9) (xy 81.65 86.7)
        (xy 81.1 87.25) (xy 80.1 87.25) (xy 79.55 86.7)
      )
    )
  )
  (zone (net 36) (net_name SH3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.3 82.4) (xy 86.3 87.9) (xy 79.6 87.9) (xy 79.3 87.6) (xy 79.3 82.7)
        (xy 79.6 82.4)
      )
    )
  )
  (zone (net 36) (net_name SH3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.1 82.9) (xy 83.1 87.5) (xy 79.2 87.5) (xy 78.890429 87.367525) (xy 78.5 86.9)
        (xy 76.7 86.9) (xy 76.7 83.5) (xy 78.5 83.5) (xy 78.895375 83.017793) (xy 79.2 82.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.55 83.9) (xy 80.1 83.35) (xy 81.1 83.35) (xy 81.65 83.9) (xy 81.65 86.7)
        (xy 81.1 87.25) (xy 80.1 87.25) (xy 79.55 86.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.65 89.65) (xy 81.1 89.1) (xy 80.1 89.1) (xy 79.55 89.65) (xy 79.55 92.45)
        (xy 80.1 93) (xy 81.1 93) (xy 81.65 92.45)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.65 95.4) (xy 81.1 94.825) (xy 80.1 94.825) (xy 79.55 95.4) (xy 79.55 98.2)
        (xy 80.1 98.8) (xy 81.1 98.8) (xy 81.65 98.2)
      )
    )
  )
  (zone (net 34) (net_name SH1) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.1 88.7) (xy 79.2 88.7) (xy 78.872334 88.855794) (xy 78.5 89.3) (xy 76.7 89.3)
        (xy 76.7 92.7) (xy 78.5 92.7) (xy 78.870472 93.143251) (xy 79.25 93.3) (xy 83.1 93.3)
      )
    )
  )
  (zone (net 35) (net_name SH2) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 83.1 99.1) (xy 83.1 94.5) (xy 79.3 94.5) (xy 78.832472 94.701034) (xy 78.5 95.1)
        (xy 76.7 95.1) (xy 76.7 98.5) (xy 78.5 98.5) (xy 78.822617 98.88714) (xy 79.25 99.1)
      )
    )
  )
  (zone (net 34) (net_name SH1) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.3 88.3) (xy 79.6 88.3) (xy 79.3 88.6) (xy 79.3 93.5) (xy 79.5 93.7)
        (xy 86.3 93.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.1 94.825) (xy 81.1 94.825) (xy 81.65 95.4) (xy 81.65 98.2) (xy 81.1 98.8)
        (xy 80.1 98.8) (xy 79.55 98.2) (xy 79.55 95.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.55 92.45) (xy 80.1 93) (xy 81.1 93) (xy 81.65 92.45) (xy 81.65 89.65)
        (xy 81.1 89.1) (xy 80.1 89.1) (xy 79.55 89.65)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.9 82.4) (xy 86.9 99.6) (xy 114.65 99.6) (xy 114.65 96.35) (xy 110.85 96.35)
        (xy 110.85 97.9) (xy 109.7 97.9) (xy 107.8 84.1) (xy 105.7 84.1) (xy 103.823583 97.9)
        (xy 101.6 97.9) (xy 99.8 84.1) (xy 97.6 84.1) (xy 95.8 97.9) (xy 93.5 97.9)
        (xy 91.6 84.25) (xy 87.749531 84.25) (xy 87.75 82.4)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.6 99.6) (xy 84.15 99.6) (xy 84.1 83.5) (xy 84.1 82.4) (xy 114.65 82.4)
        (xy 114.65 85.65) (xy 110.9 85.6) (xy 110.9 84.1) (xy 109.7 84.1) (xy 107.9 97.7)
        (xy 105.6 97.7) (xy 103.9 84.1) (xy 101.5 84.1) (xy 99.8 97.7) (xy 98.6 97.7)
        (xy 98.6 84.1) (xy 89.6 84.1) (xy 88.85 84.95) (xy 88.85 97.7) (xy 88.6 98.35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.85 84.9) (xy 90.35 84.9) (xy 90.35 97.65) (xy 90.7 98) (xy 110.95 98)
        (xy 110.95 96.45) (xy 114.55 96.45) (xy 114.55 99.5) (xy 90.25 99.5) (xy 88.85 98.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.3 86.46) (xy 97.35 86.32) (xy 97.35 86.18) (xy 97.3 86.04) (xy 97.2 85.94)
        (xy 97.06 85.89) (xy 96.92 85.89) (xy 96.79 85.94) (xy 96.68 86.05) (xy 96.63 86.17)
        (xy 96.63 86.32) (xy 96.68 86.45) (xy 96.79 86.56) (xy 96.92 86.61) (xy 97.06 86.61)
        (xy 97.2 86.56)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71.4 82.4) (xy 71.4 99.6) (xy 79 99.6) (xy 79 82.4)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.8 84.3) (xy 109.8 84.3) (xy 108 97.9) (xy 105.5 97.9) (xy 103.7 84.3)
        (xy 101.7 84.3) (xy 99.8 97.9) (xy 89.05 97.9) (xy 88.9 98.3) (xy 88.85 98.5)
        (xy 88.85 98.9) (xy 88.85 99.6) (xy 114.65 99.6) (xy 114.65 96.35) (xy 110.85 96.35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.5 82.5) (xy 114.5 83.9) (xy 88.85 84) (xy 88.85 82.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.5 99.5) (xy 114.5 98) (xy 89.8 98) (xy 89.8 99.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.55 82.5) (xy 114.55 85.55) (xy 110.95 85.55) (xy 110.95 84) (xy 88.85 84)
        (xy 88.85 82.5)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.65 82.4) (xy 114.65 82.55) (xy 114.95 82.55) (xy 114.95 82.85) (xy 114.65 82.85)
        (xy 114.65 85.65) (xy 110.85 85.65) (xy 110.85 98.15) (xy 88.75 98.15) (xy 88.75 82.4)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.55 88.9) (xy 92.55 91.95) (xy 89.3 91.95) (xy 89.3 93.25) (xy 98.3 93.25)
        (xy 98.3 88.9)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.256)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.55 84.4) (xy 89.54 84.39) (xy 89.25 87.4) (xy 89.25 88.7) (xy 98.3 88.7)
        (xy 98.3 84.4)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.55 93.4) (xy 92.546184 96.45) (xy 89.296184 96.45) (xy 89.3 97.75) (xy 98.3 97.75)
        (xy 98.3 93.4)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.5 84.2) (xy 114.5 84.2) (xy 114.5 82.4) (xy 136 82.4) (xy 136.52 82.47)
        (xy 136.83 82.74) (xy 137.11 82.98) (xy 137.34 83.3) (xy 137.6 84) (xy 137.6 98)
        (xy 137 99) (xy 136 99.6) (xy 90.5 99.6) (xy 90.5 98) (xy 90.492474 99.6)
        (xy 71.4 99.6) (xy 71.4 82.4) (xy 90.506194 82.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.55 86.5) (xy 113.05 86.5) (xy 113.05 95.5) (xy 111.55 95.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.4 95.6) (xy 126.7 95.6) (xy 126.7 86.4) (xy 128.4 86.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.3 95.6) (xy 130.6 95.6) (xy 130.6 86.4) (xy 132.3 86.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.75 82.77) (xy 87.8 82.63) (xy 87.8 82.49) (xy 87.75 82.35) (xy 87.65 82.25)
        (xy 87.51 82.2) (xy 87.37 82.2) (xy 87.24 82.25) (xy 87.13 82.36) (xy 87 82.4)
        (xy 87.08 82.63) (xy 87.13 82.76) (xy 87.24 82.87) (xy 87.37 82.92) (xy 87.51 82.92)
        (xy 87.8 82.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.82 88.58) (xy 87.87 88.44) (xy 87.87 88.3) (xy 87.82 88.16) (xy 87.72 88.06)
        (xy 87.58 88.01) (xy 87.44 88.01) (xy 87.31 88.06) (xy 87 88) (xy 87 88.3)
        (xy 87 88.5) (xy 87.2 88.8) (xy 87.4 88.8) (xy 87.5 88.8) (xy 87.7 88.9)
        (xy 87.8 88.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.92 94.36) (xy 87.75 94.17) (xy 87.75 94.03) (xy 87.87 93.85) (xy 87.62 93.69)
        (xy 87.44 93.67) (xy 87.3 93.69) (xy 87.15 93.76) (xy 87.08 93.9) (xy 87.03 94.02)
        (xy 87.03 94.17) (xy 87.08 94.3) (xy 87.16 94.44) (xy 87.34 94.59) (xy 87.57 94.61)
        (xy 87.8 94.6)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.6 84.2) (xy 96.6 87.3) (xy 104.8 87.3) (xy 107.03 85.13) (xy 107.7 84.25)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97 90) (xy 97 92.45) (xy 108.3 92.4) (xy 110.6 94.7) (xy 110.6 90)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97 92.85) (xy 97 97.1) (xy 111.4 97.1) (xy 111.4 95.6) (xy 108.35 92.65)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71.4 82.4) (xy 71.4 99.6) (xy 90.49 99.6) (xy 90.49 98.01) (xy 96.6 98.009522)
        (xy 96.6 83.99) (xy 90.5 84) (xy 90.5 82.4)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136 82.4) (xy 137 83) (xy 137.6 84) (xy 137.6 98) (xy 137 99)
        (xy 136 99.6) (xy 114.78 99.6) (xy 114.78 97.7) (xy 110.9 97.7) (xy 110.9 89.8)
        (xy 95.55 89.8) (xy 95.55 87.75) (xy 96.7 87.5) (xy 105 87.5) (xy 108.390798 84.041386)
        (xy 114.49 84.01) (xy 114.49 82.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.6 85.4) (xy 88.6 85.8) (xy 89.2 85.8) (xy 89.2 85.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.6 86.6) (xy 89.2 86.6) (xy 89.2 88.3) (xy 88.6 88.3)
      )
    )
  )
  (zone (net 82) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.25 89.4) (xy 125.25 88.2) (xy 123.25 88.2) (xy 123 89.3) (xy 117.2 89.3)
        (xy 117.19583 91.2) (xy 123.39583 91.2)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.5 95.7) (xy 124.1 95.7) (xy 124.1 93) (xy 117.5 93)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137 83) (xy 137.6 84) (xy 137.6 98) (xy 137 99) (xy 136 99.6)
        (xy 133 99.6) (xy 132.996306 97.620103) (xy 126.15 97.65) (xy 126 97.8) (xy 125.993151 99.6)
        (xy 115 99.6) (xy 115 95.9) (xy 124.3 95.9) (xy 124.3 92.8) (xy 117.4 92.8)
        (xy 114.6 95.9) (xy 114.6 96.1) (xy 111.1 96.1) (xy 111.1 85.9) (xy 114.8 85.9)
        (xy 114.8 82.4) (xy 136 82.4)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.5 96.2) (xy 121.5 99.6) (xy 126.3 99.6) (xy 126.3 98.9) (xy 126.3 96)
        (xy 126.461393 95.85) (xy 132.6 95.85) (xy 132.6 95.5) (xy 124 95.5) (xy 124 96.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.62 95.25) (xy 114.9 96.08) (xy 115.87 94.89) (xy 114.86 94.81)
      )
    )
  )
  (zone (net 59) (net_name "Net-(C23-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.2 89.05) (xy 122.9 89.05) (xy 122.9 88.35) (xy 122.55 87.75) (xy 122 87.2)
        (xy 121.25 86.95) (xy 118.55 86.95) (xy 117.8 86.4) (xy 117.8 85.65) (xy 116.6 85.65)
        (xy 116.6 87) (xy 117.2 87.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.9 83.05) (xy 129.05 83.1) (xy 129.25 83.05) (xy 129.4 82.95) (xy 129.45 82.75)
        (xy 129.4 82.6) (xy 129.3 82.45) (xy 129.1 82.4) (xy 128.9 82.45) (xy 128.75 82.65)
        (xy 128.75 82.9)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.8 82.4) (xy 136 82.4) (xy 137 83) (xy 137.6 84) (xy 137.6 98)
        (xy 137 99) (xy 136 99.6) (xy 133 99.6) (xy 133 95.7) (xy 123.8 95.7)
        (xy 123.8 93.2) (xy 121.8 92) (xy 116.5 92) (xy 115.35 93.15) (xy 115.35 94.85)
        (xy 115.35 95.35) (xy 114.9 95.5) (xy 114.6 95.7) (xy 114.6 96.1) (xy 111.1 96.1)
        (xy 111.1 85.9) (xy 114.8 85.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129 83.1) (xy 129.3 83.1) (xy 129.5 82.9) (xy 129.5 82.6) (xy 129.3 82.4)
        (xy 128.9 82.4) (xy 128.7 82.6) (xy 128.7 82.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.3 98.67) (xy 125.45 98.72) (xy 125.65 98.67) (xy 125.8 98.57) (xy 125.85 98.37)
        (xy 125.8 98.22) (xy 125.7 98.07) (xy 125.5 98.02) (xy 125.3 98.07) (xy 125.15 98.27)
        (xy 125.15 98.52)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.5 99.6) (xy 90.5 98) (xy 114.8 98) (xy 114.8 99.6)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.8 82.4) (xy 88.8 83.625) (xy 88.8 83.675) (xy 89.125 84) (xy 92.8 84)
        (xy 114.5 84) (xy 114.5 82.4)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.5 82.4) (xy 114.5 84) (xy 88.8 84) (xy 88.8 82.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.7 88.1) (xy 130.7 86.5) (xy 132.2 86.5) (xy 132.2 88.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.8 88.1) (xy 126.8 86.5) (xy 128.3 86.5) (xy 128.3 88)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.5 83.6) (xy 129.7 83.6) (xy 129.7 82.3) (xy 128.5 82.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.6 86.4) (xy 132.3 86.4) (xy 132.3 88.1) (xy 130.6 88.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.7 88) (xy 132.2 88) (xy 132.2 86.5) (xy 130.7 86.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.55 93.95) (xy 111.55 95.5) (xy 113.05 95.5) (xy 113.05 93.95)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.128))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.55 94) (xy 113.05 94) (xy 113.05 95.5) (xy 111.55 95.5)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.2 99.6) (xy 126.2 97.95) (xy 132.6 98) (xy 132.6 98.05) (xy 132.1 98.9)
        (xy 131.1 99.6)
      )
    )
  )
  (zone (net 33) (net_name "Net-(P3-Pad1)") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.03))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 82.4) (xy 71 88) (xy 68 88) (xy 68 82.4)
      )
    )
  )
  (zone (net 33) (net_name "Net-(P3-Pad1)") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.03))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 82.4) (xy 71 88) (xy 68 88) (xy 68 82.4)
      )
    )
  )
  (zone (net 31) (net_name "Net-(P1-Pad1)") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.03))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 88.2) (xy 71 93.8) (xy 68 93.8) (xy 68 88.2)
      )
    )
  )
  (zone (net 31) (net_name "Net-(P1-Pad1)") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.03))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 88.2) (xy 71 93.8) (xy 68 93.8) (xy 68 88.2)
      )
    )
  )
  (zone (net 32) (net_name "Net-(P2-Pad1)") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.03))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 94) (xy 68 94) (xy 68 99.6) (xy 71 99.6)
      )
    )
  )
  (zone (net 32) (net_name "Net-(P2-Pad1)") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.03))
    (min_thickness 0.03)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 94) (xy 68 94) (xy 68 99.6) (xy 71 99.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.03))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.61 98.67) (xy 126.01 98.47) (xy 126.11 98.17) (xy 125.91 97.87) (xy 125.51 97.77)
        (xy 125.11 97.97) (xy 125.11 98.47) (xy 125.31 98.57)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.75 87.4) (xy 93.175 84.75) (xy 88.75 84.75) (xy 87.125 83.05) (xy 87.125 82)
        (xy 87.925 82) (xy 87.925 82.725) (xy 89.2 83.95) (xy 93.5 83.95) (xy 96.4 86.85)
        (xy 96.45 87.1) (xy 96.425 87.25) (xy 96.125 87.475)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.256)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96 92) (xy 96.325 91.875) (xy 96.5 91.575) (xy 96.375 91.325) (xy 95.375 90.35)
        (xy 89.8 90.35) (xy 87.9 88.525) (xy 87.875 87.95) (xy 86.9 87.9) (xy 87.1 88.925)
        (xy 89.5 91.3) (xy 95 91.275)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.256)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.75 96.025) (xy 96.325 95.75) (xy 93.6 93.15) (xy 87.7 93.15) (xy 87.15 93.675)
        (xy 87.15 94.375) (xy 87.425 94.55) (xy 87.75 94.5) (xy 87.875 94.3) (xy 87.875 94.05)
        (xy 88 93.9) (xy 93.275 93.9) (xy 95.75 96.325) (xy 95.9 96.575) (xy 96.125 96.725)
        (xy 96.45 97.05) (xy 96.75 96.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.729506 83.33) (xy 136.129506 83.33) (xy 136.129506 83.63) (xy 135.704506 83.63) (xy 135.704506 83.33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.811179 95.81184) (xy 136.111179 95.61184) (xy 136.161179 95.23684) (xy 136.061179 94.91184) (xy 135.661179 94.78684)
        (xy 134.386179 94.81184) (xy 134.111179 95.01184) (xy 134.036179 95.36184) (xy 134.211179 95.71184) (xy 134.511179 95.88684)
      )
    )
  )
  (zone (net 35) (net_name SH2) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.3 94.1) (xy 79.5 94.1) (xy 79.3 94.3) (xy 79.3 99.3) (xy 79.5 99.6)
        (xy 86.3 99.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.86 87.45) (xy 96.16 87.5) (xy 96.43 87.36) (xy 96.51 87.14) (xy 96.48 86.87)
        (xy 96.35 86.69) (xy 96.06 86.62) (xy 95.64 86.75) (xy 95.58 86.99) (xy 95.64 87.29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.96 96.46) (xy 96.3 96.42) (xy 96.51 96.24) (xy 96.58 96.02) (xy 96.51 95.81)
        (xy 96.32 95.61) (xy 96.08 95.54)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.68 91.23) (xy 95.59 91.51) (xy 95.7 91.85) (xy 96.03 92.03) (xy 96.4 91.91)
        (xy 96.6 91.65) (xy 96.53 91.37) (xy 96.23 91.16) (xy 95.79 91.18) (xy 95.68 91.22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.8 95.61) (xy 95.61 95.92) (xy 95.69 96.3) (xy 95.92 96.44) (xy 96.31 96.41)
        (xy 96.46 96.28) (xy 96.61 96.02) (xy 96.49 95.72) (xy 96.22 95.55)
      )
    )
  )
  (zone (net 4) (net_name VSS) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.128))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 99.6) (xy 131.1 99.6) (xy 132.1 98.9) (xy 132.6 98) (xy 132.6 96)
        (xy 126.6 96) (xy 126.45 96.15) (xy 126.46 98.95) (xy 126.46 99.59) (xy 121.3 99.6)
        (xy 121.25 96) (xy 123.35 96) (xy 123.35 93.456116) (xy 121.75 92.35) (xy 115.5 92.35)
        (xy 115.5 95.1) (xy 115.5 95.4) (xy 115.25 95.65) (xy 115 95.65)
      )
    )
  )
)
