(kicad_pcb (version 20171130) (host pcbnew 5.1.9-73d0e3b20d~88~ubuntu20.10.1)
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 275)
    (zones 0)
    (modules 27)
    (nets 30)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1.2)
    (user_trace_width 2)
    (user_trace_width 2.54)
    (user_trace_width 3)
    (user_trace_width 4)
    (trace_clearance 0.1524)
    (zone_clearance 0.000001)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.9 0.4)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 40_RSTI)
  (net 4 N$1)
  (net 5 N$2)
  (net 6 N$3)
  (net 7 40_BCLK)
  (net 8 40_IPL2)
  (net 9 40_IPL1)
  (net 10 40_IPL0)
  (net 11 60_IPL2)
  (net 12 60_CLKEN)
  (net 13 60_IPL1)
  (net 14 60_IPL0)
  (net 15 +3V3)
  (net 16 TRA)
  (net 17 SNOOP)
  (net 18 BTT)
  (net 19 IPL2)
  (net 20 IPL1)
  (net 21 IPL0)
  (net 22 CLKEN)
  (net 23 CLA)
  (net 24 40_PCLK)
  (net 25 THERM0)
  (net 26 THERM1)
  (net 27 VCC2)
  (net 28 ND1)
  (net 29 ND2)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net 40_BCLK)
    (add_net 40_IPL0)
    (add_net 40_IPL1)
    (add_net 40_IPL2)
    (add_net 40_PCLK)
    (add_net 40_RSTI)
    (add_net 60_CLKEN)
    (add_net 60_IPL0)
    (add_net 60_IPL1)
    (add_net 60_IPL2)
    (add_net BTT)
    (add_net CLA)
    (add_net CLKEN)
    (add_net GND)
    (add_net IPL0)
    (add_net IPL1)
    (add_net IPL2)
    (add_net N$1)
    (add_net N$2)
    (add_net N$3)
    (add_net ND1)
    (add_net ND2)
    (add_net SNOOP)
    (add_net THERM0)
    (add_net THERM1)
    (add_net TRA)
    (add_net VCC)
    (add_net VCC2)
  )
  (module KiCad/kicad-footprints/Symbol.pretty:OSHW-Logo2_9.8x8mm_Copper (layer Top) (tedit 0)
    (at 136.35 108.375)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_9.8x8mm_Copper (at 0.75 0) (layer F.Fab) hide)
  )
  (module KiCad/kicad-footprints/Resistor_SMD.pretty:R_Array_Concave_4x0603 (layer Top) (tedit 6039A1E4)
    (at 134.875 63.725 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0 -2.6 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 0.85 1.2 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 4 N$1))
    (pad 6 smd rect (at 0.85 0.4 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 6 N$3))
    (pad 7 smd rect (at 0.85 -0.4 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 5 N$2))
    (pad 8 smd rect (at 0.85 -1.2 270) (size 0.9 0.4) (layers Top F.Paste F.Mask))
    (pad 4 smd rect (at -0.85 1.2 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -0.85 -1.2 270) (size 0.9 0.4) (layers Top F.Paste F.Mask))
    (pad 3 smd rect (at -0.85 0.4 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -0.85 -0.4 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/kicad-footprints/Resistor_SMD.pretty:R_Array_Concave_4x0603 (layer Top) (tedit 60399B24)
    (at 138.775 121.475 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN3 (at 0 -2.6 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at -0.85 -0.4 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 15 +3V3))
    (pad 3 smd rect (at -0.85 0.4 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 15 +3V3))
    (pad 1 smd rect (at -0.85 -1.2 270) (size 0.9 0.4) (layers Top F.Paste F.Mask))
    (pad 4 smd rect (at -0.85 1.2 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 15 +3V3))
    (pad 8 smd rect (at 0.85 -1.2 270) (size 0.9 0.4) (layers Top F.Paste F.Mask))
    (pad 7 smd rect (at 0.85 -0.4 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 23 CLA))
    (pad 6 smd rect (at 0.85 0.4 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 17 SNOOP))
    (pad 5 smd rect (at 0.85 1.2 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 18 BTT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/kicad-footprints/Resistor_SMD.pretty:R_Array_Concave_4x0603 (layer Top) (tedit 60399AAC)
    (at 131.6 121.475 270)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 0 -2.6 90) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 0.85 1.2 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 19 IPL2))
    (pad 6 smd rect (at 0.85 0.4 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 20 IPL1))
    (pad 7 smd rect (at 0.85 -0.4 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 16 TRA))
    (pad 8 smd rect (at 0.85 -1.2 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 21 IPL0))
    (pad 4 smd rect (at -0.85 1.2 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 15 +3V3))
    (pad 1 smd rect (at -0.85 -1.2 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 15 +3V3))
    (pad 3 smd rect (at -0.85 0.4 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 15 +3V3))
    (pad 2 smd rect (at -0.85 -0.4 270) (size 0.9 0.4) (layers Top F.Paste F.Mask)
      (net 15 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Bot_68040_mk2a:PGA179_BIG (layer Top) (tedit 60392CDD)
    (at 135.1572 67.056)
    (fp_text reference IC1 (at -22.225 -24.13 180) (layer F.SilkS) hide)
    (fp_text value "" (at -10.795 0.635) (layer F.Fab))
    (pad A01 thru_hole circle (at -21.59 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A02 thru_hole circle (at -19.05 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A03 thru_hole circle (at -16.51 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A04 thru_hole circle (at -13.97 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A05 thru_hole circle (at -11.43 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A06 thru_hole circle (at -8.89 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A07 thru_hole circle (at -6.35 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A08 thru_hole circle (at -3.81 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A09 thru_hole circle (at -1.27 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A10 thru_hole circle (at 1.27 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A11 thru_hole circle (at 3.81 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A12 thru_hole circle (at 6.35 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A13 thru_hole circle (at 8.89 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B13 thru_hole circle (at 8.89 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad M01 thru_hole circle (at -21.59 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad L01 thru_hole circle (at -21.59 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad K01 thru_hole circle (at -21.59 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad J01 thru_hole circle (at -21.59 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad H01 thru_hole circle (at -21.59 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad G01 thru_hole circle (at -21.59 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad F01 thru_hole circle (at -21.59 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad E01 thru_hole circle (at -21.59 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad D01 thru_hole circle (at -21.59 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B01 thru_hole circle (at -21.59 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B02 thru_hole circle (at -19.05 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad B03 thru_hole circle (at -16.51 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B04 thru_hole circle (at -13.97 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad B05 thru_hole circle (at -11.43 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad B06 thru_hole circle (at -8.89 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad B07 thru_hole circle (at -6.35 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B08 thru_hole circle (at -3.81 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad B09 thru_hole circle (at -1.27 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad B10 thru_hole circle (at 1.27 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad B11 thru_hole circle (at 3.81 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B12 thru_hole circle (at 6.35 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R13 thru_hole circle (at 8.89 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad S13 thru_hole circle (at 8.89 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad M02 thru_hole circle (at -19.05 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad L02 thru_hole circle (at -19.05 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad K02 thru_hole circle (at -19.05 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad J02 thru_hole circle (at -19.05 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad H02 thru_hole circle (at -19.05 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad G02 thru_hole circle (at -19.05 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad F02 thru_hole circle (at -19.05 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad E02 thru_hole circle (at -19.05 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad D02 thru_hole circle (at -19.05 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad N02 thru_hole circle (at -19.05 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad T13 thru_hole circle (at 8.89 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T12 thru_hole circle (at 6.35 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T11 thru_hole circle (at 3.81 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T10 thru_hole circle (at 1.27 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T09 thru_hole circle (at -1.27 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T08 thru_hole circle (at -3.81 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 10 40_IPL0) (solder_mask_margin 0.0762))
    (pad T07 thru_hole circle (at -6.35 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 9 40_IPL1) (solder_mask_margin 0.0762))
    (pad T06 thru_hole circle (at -8.89 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 8 40_IPL2) (solder_mask_margin 0.0762))
    (pad T05 thru_hole circle (at -11.43 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T04 thru_hole circle (at -13.97 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad N03 thru_hole circle (at -16.51 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C13 thru_hole circle (at 8.89 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C01 thru_hole circle (at -21.59 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C12 thru_hole circle (at 6.35 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad C11 thru_hole circle (at 3.81 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C10 thru_hole circle (at 1.27 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad C09 thru_hole circle (at -1.27 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C08 thru_hole circle (at -3.81 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad C07 thru_hole circle (at -6.35 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C06 thru_hole circle (at -8.89 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C05 thru_hole circle (at -11.43 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad C04 thru_hole circle (at -13.97 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C03 thru_hole circle (at -16.51 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C02 thru_hole circle (at -19.05 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad N01 thru_hole circle (at -21.59 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad M03 thru_hole circle (at -16.51 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad L03 thru_hole circle (at -16.51 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad K03 thru_hole circle (at -16.51 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad J03 thru_hole circle (at -16.51 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad H03 thru_hole circle (at -16.51 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad G03 thru_hole circle (at -16.51 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad F03 thru_hole circle (at -16.51 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad E03 thru_hole circle (at -16.51 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad D03 thru_hole circle (at -16.51 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S12 thru_hole circle (at 6.35 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R12 thru_hole circle (at 6.35 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad S04 thru_hole circle (at -13.97 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S05 thru_hole circle (at -11.43 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S06 thru_hole circle (at -8.89 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S07 thru_hole circle (at -6.35 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 40_RSTI) (solder_mask_margin 0.0762))
    (pad S08 thru_hole circle (at -3.81 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad S09 thru_hole circle (at -1.27 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad S10 thru_hole circle (at 1.27 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad S11 thru_hole circle (at 3.81 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R11 thru_hole circle (at 3.81 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad R10 thru_hole circle (at 1.27 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad R09 thru_hole circle (at -1.27 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 24 40_PCLK) (solder_mask_margin 0.0762))
    (pad R08 thru_hole circle (at -3.81 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad R07 thru_hole circle (at -6.35 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 40_BCLK) (solder_mask_margin 0.0762))
    (pad R06 thru_hole circle (at -8.89 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad R05 thru_hole circle (at -11.43 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad R04 thru_hole circle (at -13.97 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad P01 thru_hole circle (at -21.59 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q01 thru_hole circle (at -21.59 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R01 thru_hole circle (at -21.59 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S01 thru_hole circle (at -21.59 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A14 thru_hole circle (at 11.43 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A15 thru_hole circle (at 13.97 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A16 thru_hole circle (at 16.51 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A17 thru_hole circle (at 19.05 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad P02 thru_hole circle (at -19.05 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad P03 thru_hole circle (at -16.51 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q02 thru_hole circle (at -19.05 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad Q03 thru_hole circle (at -16.51 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R03 thru_hole circle (at -16.51 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S03 thru_hole circle (at -16.51 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T03 thru_hole circle (at -16.51 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T02 thru_hole circle (at -19.05 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S02 thru_hole circle (at -19.05 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad R02 thru_hole circle (at -19.05 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad B14 thru_hole circle (at 11.43 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad C14 thru_hole circle (at 11.43 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad B15 thru_hole circle (at 13.97 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C15 thru_hole circle (at 13.97 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B16 thru_hole circle (at 16.51 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C16 thru_hole circle (at 16.51 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B17 thru_hole circle (at 19.05 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C17 thru_hole circle (at 19.05 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad B18 thru_hole circle (at 21.59 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C18 thru_hole circle (at 21.59 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad D16 thru_hole circle (at 16.51 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad D17 thru_hole circle (at 19.05 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad D18 thru_hole circle (at 21.59 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad E16 thru_hole circle (at 16.51 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad E17 thru_hole circle (at 19.05 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad E18 thru_hole circle (at 21.59 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad F16 thru_hole circle (at 16.51 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad F17 thru_hole circle (at 19.05 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad F18 thru_hole circle (at 21.59 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad G16 thru_hole circle (at 16.51 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad H16 thru_hole circle (at 16.51 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad J16 thru_hole circle (at 16.51 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad K16 thru_hole circle (at 16.51 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad L16 thru_hole circle (at 16.51 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad M16 thru_hole circle (at 16.51 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad N16 thru_hole circle (at 16.51 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad P16 thru_hole circle (at 16.51 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q16 thru_hole circle (at 16.51 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R16 thru_hole circle (at 16.51 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S16 thru_hole circle (at 16.51 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad T16 thru_hole circle (at 16.51 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T17 thru_hole circle (at 19.05 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S17 thru_hole circle (at 19.05 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad R17 thru_hole circle (at 19.05 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad Q17 thru_hole circle (at 19.05 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad P17 thru_hole circle (at 19.05 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad N17 thru_hole circle (at 19.05 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad M17 thru_hole circle (at 19.05 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad L17 thru_hole circle (at 19.05 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad K17 thru_hole circle (at 19.05 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad J17 thru_hole circle (at 19.05 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad H17 thru_hole circle (at 19.05 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad G17 thru_hole circle (at 19.05 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad G18 thru_hole circle (at 21.59 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad H18 thru_hole circle (at 21.59 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad J18 thru_hole circle (at 21.59 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad K18 thru_hole circle (at 21.59 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad L18 thru_hole circle (at 21.59 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad M18 thru_hole circle (at 21.59 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad N18 thru_hole circle (at 21.59 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad P18 thru_hole circle (at 21.59 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q18 thru_hole circle (at 21.59 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R18 thru_hole circle (at 21.59 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S18 thru_hole circle (at 21.59 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R14 thru_hole circle (at 11.43 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R15 thru_hole circle (at 13.97 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S15 thru_hole circle (at 13.97 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad T15 thru_hole circle (at 13.97 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T14 thru_hole circle (at 11.43 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S14 thru_hole circle (at 11.43 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T18 thru_hole circle (at 21.59 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A18 thru_hole circle (at 21.59 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
  )
  (module Diode_SMD:D_SOD-123F (layer Top) (tedit 5E04C064)
    (at 166.4 98.05 270)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D3 (at -1.325 -1.775 90) (layer F.SilkS))
    (fp_text value 1N4001 (at 0 2.1 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.127 -1.905 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.4 0 270) (size 1.1 1.1) (layers Top F.Paste F.Mask)
      (net 29 ND2))
    (pad 1 smd rect (at -1.4 0 270) (size 1.1 1.1) (layers Top F.Paste F.Mask)
      (net 15 +3V3))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F (layer Top) (tedit 5E04C056)
    (at 166.4 102.55 270)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D2 (at -1.325 -1.775 90) (layer F.SilkS))
    (fp_text value 1N4001 (at 0 2.1 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.127 -1.905 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 270) (size 1.1 1.1) (layers Top F.Paste F.Mask)
      (net 29 ND2))
    (pad 2 smd rect (at 1.4 0 270) (size 1.1 1.1) (layers Top F.Paste F.Mask)
      (net 28 ND1))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F (layer Top) (tedit 5E04C048)
    (at 166.4 107.075 270)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D1 (at -1.375 -1.775 90) (layer F.SilkS))
    (fp_text value 1N4001 (at 0 2.1 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.127 -1.905 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.4 0 270) (size 1.1 1.1) (layers Top F.Paste F.Mask)
      (net 27 VCC2))
    (pad 1 smd rect (at -1.4 0 270) (size 1.1 1.1) (layers Top F.Paste F.Mask)
      (net 28 ND1))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module combined3:6-PIN-1.4HOLES (layer Top) (tedit 5DAE57A6)
    (at 160.328 109.296 270)
    (fp_text reference U6$1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 6POL (at 0 0 90) (layer F.SilkS) hide)
    (pad P6$6 thru_hole circle (at 1.27 0 270) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 27 VCC2) (solder_mask_margin 0.0762))
    (pad P6$5 thru_hole circle (at -1.27 0 270) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 27 VCC2) (solder_mask_margin 0.0762))
    (pad P6$4 thru_hole circle (at -3.81 0 270) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 27 VCC2) (solder_mask_margin 0.0762))
    (pad P6$3 thru_hole circle (at -6.35 0 270) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 27 VCC2) (solder_mask_margin 0.0762))
    (pad P6$2 thru_hole circle (at -8.89 0 270) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 27 VCC2) (solder_mask_margin 0.0762))
    (pad P6$1 thru_hole circle (at -11.43 0 270) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 27 VCC2) (solder_mask_margin 0.0762))
  )
  (module Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown (layer Top) (tedit 5DAE5BB7)
    (at 167.37 113.96 180)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference IC4 (at -1.38 -2.58) (layer F.SilkS))
    (fp_text value LMS1585-3.3 (at 2.54 2) (layer F.Fab))
    (fp_text user %R (at 2.54 -20.58) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 27 VCC2))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole oval (at 2.54 -16.66 180) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer Top) (tedit 5DB0F8B7)
    (at 161.35 136.8 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference H2 (at 0 -2.075 90) (layer F.SilkS))
    (fp_text value Therm (at -2.0574 1.30556) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 THERM0))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 THERM1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer Top) (tedit 5DAE57BB)
    (at 163.35 102.95 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference H1 (at -2.4 -0.825 180) (layer F.SilkS))
    (fp_text value Power (at 3.429 5.6388) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 VCC2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Top_68060_mk2a:PGA206_BIG (layer Top) (tedit 0)
    (at 135.1392 115.646)
    (fp_text reference IC3 (at -22.225 -24.13 180) (layer F.SilkS) hide)
    (fp_text value MC68060RCPGA_BIG (at -10.795 0.635 180) (layer F.Fab) hide)
    (pad P04 thru_hole circle (at -13.97 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad P15 thru_hole circle (at 13.97 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 17 SNOOP) (solder_mask_margin 0.0762))
    (pad N15 thru_hole circle (at 13.97 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad M15 thru_hole circle (at 13.97 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 26 THERM1) (solder_mask_margin 0.0762))
    (pad L15 thru_hole circle (at 13.97 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 25 THERM0) (solder_mask_margin 0.0762))
    (pad K15 thru_hole circle (at 13.97 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 23 CLA) (solder_mask_margin 0.0762))
    (pad J15 thru_hole circle (at 13.97 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad H15 thru_hole circle (at 13.97 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad G15 thru_hole circle (at 13.97 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad F15 thru_hole circle (at 13.97 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad E15 thru_hole circle (at 13.97 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad Q15 thru_hole circle (at 13.97 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 18 BTT) (solder_mask_margin 0.0762))
    (pad Q14 thru_hole circle (at 11.43 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q13 thru_hole circle (at 8.89 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q12 thru_hole circle (at 6.35 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 16 TRA) (solder_mask_margin 0.0762))
    (pad Q11 thru_hole circle (at 3.81 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad Q10 thru_hole circle (at 1.27 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad Q09 thru_hole circle (at -1.27 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad Q08 thru_hole circle (at -3.81 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 22 CLKEN) (solder_mask_margin 0.0762))
    (pad Q07 thru_hole circle (at -6.35 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q06 thru_hole circle (at -8.89 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q05 thru_hole circle (at -11.43 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q04 thru_hole circle (at -13.97 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad L04 thru_hole circle (at -13.97 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad J04 thru_hole circle (at -13.97 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad H04 thru_hole circle (at -13.97 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad G04 thru_hole circle (at -13.97 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad F04 thru_hole circle (at -13.97 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad E04 thru_hole circle (at -13.97 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad D15 thru_hole circle (at 13.97 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad D12 thru_hole circle (at 6.35 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad D10 thru_hole circle (at 1.27 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad D08 thru_hole circle (at -3.81 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad A18 thru_hole circle (at 21.59 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T18 thru_hole circle (at 21.59 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S14 thru_hole circle (at 11.43 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T14 thru_hole circle (at 11.43 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T15 thru_hole circle (at 13.97 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S15 thru_hole circle (at 13.97 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad R15 thru_hole circle (at 13.97 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R14 thru_hole circle (at 11.43 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S18 thru_hole circle (at 21.59 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R18 thru_hole circle (at 21.59 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q18 thru_hole circle (at 21.59 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad P18 thru_hole circle (at 21.59 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad N18 thru_hole circle (at 21.59 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad M18 thru_hole circle (at 21.59 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad L18 thru_hole circle (at 21.59 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad K18 thru_hole circle (at 21.59 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad J18 thru_hole circle (at 21.59 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad H18 thru_hole circle (at 21.59 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad G18 thru_hole circle (at 21.59 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad G17 thru_hole circle (at 19.05 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad H17 thru_hole circle (at 19.05 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad J17 thru_hole circle (at 19.05 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad K17 thru_hole circle (at 19.05 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad L17 thru_hole circle (at 19.05 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad M17 thru_hole circle (at 19.05 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad N17 thru_hole circle (at 19.05 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad P17 thru_hole circle (at 19.05 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q17 thru_hole circle (at 19.05 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad R17 thru_hole circle (at 19.05 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad S17 thru_hole circle (at 19.05 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad T17 thru_hole circle (at 19.05 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T16 thru_hole circle (at 16.51 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S16 thru_hole circle (at 16.51 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad R16 thru_hole circle (at 16.51 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad P16 thru_hole circle (at 16.51 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad N16 thru_hole circle (at 16.51 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad M16 thru_hole circle (at 16.51 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad L16 thru_hole circle (at 16.51 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad K16 thru_hole circle (at 16.51 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad J16 thru_hole circle (at 16.51 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad H16 thru_hole circle (at 16.51 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad G16 thru_hole circle (at 16.51 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad F18 thru_hole circle (at 21.59 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad F17 thru_hole circle (at 19.05 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad F16 thru_hole circle (at 16.51 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad E18 thru_hole circle (at 21.59 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad E17 thru_hole circle (at 19.05 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad E16 thru_hole circle (at 16.51 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad D18 thru_hole circle (at 21.59 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad D17 thru_hole circle (at 19.05 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad D16 thru_hole circle (at 16.51 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C18 thru_hole circle (at 21.59 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B18 thru_hole circle (at 21.59 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C17 thru_hole circle (at 19.05 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad B17 thru_hole circle (at 19.05 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C16 thru_hole circle (at 16.51 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B16 thru_hole circle (at 16.51 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C15 thru_hole circle (at 13.97 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B15 thru_hole circle (at 13.97 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C14 thru_hole circle (at 11.43 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad B14 thru_hole circle (at 11.43 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad R02 thru_hole circle (at -19.05 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad S02 thru_hole circle (at -19.05 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad T02 thru_hole circle (at -19.05 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T03 thru_hole circle (at -16.51 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S03 thru_hole circle (at -16.51 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R03 thru_hole circle (at -16.51 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q03 thru_hole circle (at -16.51 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q02 thru_hole circle (at -19.05 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad P03 thru_hole circle (at -16.51 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad P02 thru_hole circle (at -19.05 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A17 thru_hole circle (at 19.05 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A16 thru_hole circle (at 16.51 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A15 thru_hole circle (at 13.97 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A14 thru_hole circle (at 11.43 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S01 thru_hole circle (at -21.59 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R01 thru_hole circle (at -21.59 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad Q01 thru_hole circle (at -21.59 13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad P01 thru_hole circle (at -21.59 11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R04 thru_hole circle (at -13.97 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad R05 thru_hole circle (at -11.43 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad R06 thru_hole circle (at -8.89 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad R08 thru_hole circle (at -3.81 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad R09 thru_hole circle (at -1.27 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R11 thru_hole circle (at 3.81 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad S11 thru_hole circle (at 3.81 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S10 thru_hole circle (at 1.27 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad S09 thru_hole circle (at -1.27 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad S08 thru_hole circle (at -3.81 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad S07 thru_hole circle (at -6.35 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S06 thru_hole circle (at -8.89 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S05 thru_hole circle (at -11.43 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad S04 thru_hole circle (at -13.97 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R12 thru_hole circle (at 6.35 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad D03 thru_hole circle (at -16.51 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad E03 thru_hole circle (at -16.51 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad F03 thru_hole circle (at -16.51 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad G03 thru_hole circle (at -16.51 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad H03 thru_hole circle (at -16.51 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad J03 thru_hole circle (at -16.51 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad K03 thru_hole circle (at -16.51 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad L03 thru_hole circle (at -16.51 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad M03 thru_hole circle (at -16.51 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad N01 thru_hole circle (at -21.59 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C02 thru_hole circle (at -19.05 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad C03 thru_hole circle (at -16.51 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C04 thru_hole circle (at -13.97 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C05 thru_hole circle (at -11.43 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad C06 thru_hole circle (at -8.89 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C07 thru_hole circle (at -6.35 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C08 thru_hole circle (at -3.81 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad C09 thru_hole circle (at -1.27 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C10 thru_hole circle (at 1.27 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad C11 thru_hole circle (at 3.81 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad C12 thru_hole circle (at 6.35 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad C01 thru_hole circle (at -21.59 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad C13 thru_hole circle (at 8.89 -16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad N03 thru_hole circle (at -16.51 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T04 thru_hole circle (at -13.97 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T05 thru_hole circle (at -11.43 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T06 thru_hole circle (at -8.89 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 19 IPL2) (solder_mask_margin 0.0762))
    (pad T07 thru_hole circle (at -6.35 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 20 IPL1) (solder_mask_margin 0.0762))
    (pad T08 thru_hole circle (at -3.81 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 21 IPL0) (solder_mask_margin 0.0762))
    (pad T10 thru_hole circle (at 1.27 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T11 thru_hole circle (at 3.81 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad T13 thru_hole circle (at 8.89 21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad N02 thru_hole circle (at -19.05 8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad D02 thru_hole circle (at -19.05 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad E02 thru_hole circle (at -19.05 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad F02 thru_hole circle (at -19.05 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad G02 thru_hole circle (at -19.05 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad H02 thru_hole circle (at -19.05 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad J02 thru_hole circle (at -19.05 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad K02 thru_hole circle (at -19.05 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad L02 thru_hole circle (at -19.05 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad M02 thru_hole circle (at -19.05 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad S13 thru_hole circle (at 8.89 19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad R13 thru_hole circle (at 8.89 16.51) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad B12 thru_hole circle (at 6.35 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B11 thru_hole circle (at 3.81 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B10 thru_hole circle (at 1.27 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad B09 thru_hole circle (at -1.27 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad B08 thru_hole circle (at -3.81 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad B07 thru_hole circle (at -6.35 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B06 thru_hole circle (at -8.89 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad B05 thru_hole circle (at -11.43 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad B04 thru_hole circle (at -13.97 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad B03 thru_hole circle (at -16.51 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B02 thru_hole circle (at -19.05 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad B01 thru_hole circle (at -21.59 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad D01 thru_hole circle (at -21.59 -13.97) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad E01 thru_hole circle (at -21.59 -11.43) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad F01 thru_hole circle (at -21.59 -8.89) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad G01 thru_hole circle (at -21.59 -6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad H01 thru_hole circle (at -21.59 -3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad J01 thru_hole circle (at -21.59 -1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad K01 thru_hole circle (at -21.59 1.27) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad L01 thru_hole circle (at -21.59 3.81) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad M01 thru_hole circle (at -21.59 6.35) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad B13 thru_hole circle (at 8.89 -19.05) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad A13 thru_hole circle (at 8.89 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A12 thru_hole circle (at 6.35 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A11 thru_hole circle (at 3.81 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A10 thru_hole circle (at 1.27 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A09 thru_hole circle (at -1.27 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A08 thru_hole circle (at -3.81 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A07 thru_hole circle (at -6.35 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A06 thru_hole circle (at -8.89 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A05 thru_hole circle (at -11.43 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A04 thru_hole circle (at -13.97 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A03 thru_hole circle (at -16.51 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A02 thru_hole circle (at -19.05 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
    (pad A01 thru_hole circle (at -21.59 -21.59) (size 1.7 1.7) (drill 1.4) (layers *.Cu *.Mask)
      (solder_mask_margin 0.0762))
  )
  (module Bot_68040_mk2a:C1206 (layer Top) (tedit 0)
    (at 160.227 66.926 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C3 (at 4.1432 1.1834 180) (layer F.SilkS))
    (fp_text value 100n (at -1.27 2.54 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 270) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad 2 smd rect (at 1.4 0 270) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
  )
  (module combined3:6-PIN-1.4HOLES (layer Top) (tedit 5D98D8A1)
    (at 160.346 60.706 270)
    (fp_text reference U6$1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 6POL (at 0 0 90) (layer F.SilkS) hide)
    (pad P6$1 thru_hole circle (at -11.43 0 270) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad P6$2 thru_hole circle (at -8.89 0 270) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad P6$3 thru_hole circle (at -6.35 0 270) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad P6$4 thru_hole circle (at -3.81 0 270) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad P6$5 thru_hole circle (at -1.27 0 270) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad P6$6 thru_hole circle (at 1.27 0 270) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
  )
  (module Bot_68040_mk2a:C1206 (layer Top) (tedit 0)
    (at 162.14 93.61)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C4 (at -2.49 2.29) (layer F.SilkS))
    (fp_text value 10u (at -1.27 2.54) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.4 0) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad 1 smd rect (at -1.4 0) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
  )
  (module Bot_68040_mk2a:C1206 (layer Top) (tedit 0)
    (at 167.58652 111.35352 180)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C6 (at -2.48848 1.12852 180) (layer F.SilkS))
    (fp_text value 100n (at -1.27 2.54) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 180) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
    (pad 2 smd rect (at 1.4 0 180) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
  )
  (module Bot_68040_mk2a:C1206 (layer Top) (tedit 5DAE57C5)
    (at 162.97088 108.11152 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C5 (at -3.88848 -1.17088 180) (layer F.SilkS))
    (fp_text value 100n (at -1.27 2.54 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.4 0 90) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad 1 smd rect (at -1.4 0 90) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 27 VCC2) (solder_mask_margin 0.0762))
  )
  (module combined3:4-PIN-1.4HOLES (layer Top) (tedit 60392CF3)
    (at 134.1572 77.486 180)
    (fp_text reference U4$1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 4POL (at 0 0) (layer F.SilkS) hide)
    (pad P4$4 thru_hole circle (at -4.81 -1 180) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 11 60_IPL2) (solder_mask_margin 0.0762))
    (pad P4$3 thru_hole circle (at -7.35 -1 180) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 13 60_IPL1) (solder_mask_margin 0.0762))
    (pad P4$2 thru_hole circle (at -9.89 -1 180) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 14 60_IPL0) (solder_mask_margin 0.0762))
    (pad P4$1 thru_hole circle (at -12.43 -1 180) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 12 60_CLKEN) (solder_mask_margin 0.0762))
  )
  (module combined3:4-PIN-1.4HOLES (layer Top) (tedit 60389CD0)
    (at 134.1392 126.076 180)
    (fp_text reference U4$1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 4POL (at 0 0) (layer F.SilkS) hide)
    (pad P4$4 thru_hole circle (at -4.81 -1 180) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 19 IPL2) (solder_mask_margin 0.0762))
    (pad P4$3 thru_hole circle (at -7.35 -1 180) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 20 IPL1) (solder_mask_margin 0.0762))
    (pad P4$2 thru_hole circle (at -9.89 -1 180) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 21 IPL0) (solder_mask_margin 0.0762))
    (pad P4$1 thru_hole circle (at -12.43 -1 180) (size 1.8064 1.8064) (drill 1.4) (layers *.Cu *.Mask)
      (net 22 CLKEN) (solder_mask_margin 0.0762))
  )
  (module Bot_68040_mk2a:SO16 (layer Top) (tedit 0)
    (at 135.1572 70.866)
    (descr "<b>Small Outline package</b> 150 mil")
    (fp_text reference IC2 (at -5.461 1.778) (layer F.SilkS))
    (fp_text value 74F257 (at -4.064 0.635 180) (layer F.Fab) hide)
    (pad 9 smd rect (at 4.445 -3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 13 60_IPL1) (solder_mask_margin 0.0762))
    (pad 8 smd rect (at 4.445 3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad 10 smd rect (at 3.175 -3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 9 40_IPL1) (solder_mask_margin 0.0762))
    (pad 11 smd rect (at 1.905 -3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 5 N$2) (solder_mask_margin 0.0762))
    (pad 7 smd rect (at 3.175 3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 12 60_CLKEN) (solder_mask_margin 0.0762))
    (pad 6 smd rect (at 1.905 3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 7 40_BCLK) (solder_mask_margin 0.0762))
    (pad 12 smd rect (at 0.635 -3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 14 60_IPL0) (solder_mask_margin 0.0762))
    (pad 5 smd rect (at 0.635 3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 7 40_BCLK) (solder_mask_margin 0.0762))
    (pad 13 smd rect (at -0.635 -3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 10 40_IPL0) (solder_mask_margin 0.0762))
    (pad 4 smd rect (at -0.635 3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 11 60_IPL2) (solder_mask_margin 0.0762))
    (pad 14 smd rect (at -1.905 -3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 6 N$3) (solder_mask_margin 0.0762))
    (pad 15 smd rect (at -3.175 -3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad 3 smd rect (at -1.905 3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 8 40_IPL2) (solder_mask_margin 0.0762))
    (pad 2 smd rect (at -3.175 3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 4 N$1) (solder_mask_margin 0.0762))
    (pad 16 smd rect (at -4.445 -3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
    (pad 1 smd rect (at -4.445 3.0734) (size 0.6604 2.032) (layers Top F.Paste F.Mask)
      (net 3 40_RSTI) (solder_mask_margin 0.0762))
  )
  (module Bot_68040_mk2a:C1206 (layer Top) (tedit 0)
    (at 127.51345 66.421 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C2 (at 0.7874 -1.32945 180) (layer F.SilkS))
    (fp_text value 100n (at -1.27 2.54 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.4 0 90) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad 1 smd rect (at -1.4 0 90) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
  )
  (module Bot_68040_mk2a:C1206 (layer Top) (tedit 0)
    (at 137.1502 59.3522)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C1 (at -2.6416 -1.2192) (layer F.SilkS))
    (fp_text value 10u (at -1.27 2.54 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.4 0) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad 1 smd rect (at -1.4 0) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.0762))
  )
  (module Top_68060_mk2a:C1206 (layer Top) (tedit 0)
    (at 126.678 122.1574 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C10 (at 1.4074 -1.128 180) (layer F.SilkS))
    (fp_text value 100n (at -1.27 2.54 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.4 0 90) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad 1 smd rect (at -1.4 0 90) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
  )
  (module Top_68060_mk2a:C1206 (layer Top) (tedit 0)
    (at 143.7568 108.4842 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C8 (at -1.3592 -3.2182 180) (layer F.SilkS))
    (fp_text value 100n (at -1.27 2.54 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.4 0 270) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad 1 smd rect (at -1.4 0 270) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
  )
  (module Top_68060_mk2a:C1206 (layer Top) (tedit 0)
    (at 126.7892 108.856 270)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C7 (at -1.406 1.2142 180) (layer F.SilkS))
    (fp_text value 100n (at -1.27 2.54 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.4 0 270) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad 1 smd rect (at -1.4 0 270) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
  )
  (module Top_68060_mk2a:C1206 (layer Top) (tedit 0)
    (at 143.7604 118.8768 90)
    (descr <b>CAPACITOR</b>)
    (fp_text reference C9 (at 1.2768 1.2896 180) (layer F.SilkS))
    (fp_text value 100n (at -1.27 2.54 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.4 0 90) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0762))
    (pad 1 smd rect (at -1.4 0 90) (size 1.6 1.8) (layers Top F.Paste F.Mask)
      (net 15 +3V3) (solder_mask_margin 0.0762))
  )
  (gr_text "California Dreamin'\namiga.technology" (at 136.175 113.625) (layer F.SilkS))
  (gr_text a1k.org (at 123.725 101.525) (layer F.SilkS))
  (gr_text "040-060 2021-03\n" (at 169.775 92.4 -90) (layer F.SilkS))
  (gr_text "Open\nSource\nenables" (at 168.075 136.975) (layer F.SilkS))
  (gr_text 3V3 (at 166.85 93.025) (layer F.SilkS))
  (gr_text GND (at 166.85 94.125) (layer F.SilkS))
  (gr_text VCC (at 166.85 95.225) (layer F.SilkS))
  (gr_line (start 157.93 92.14) (end 138.81 92.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 138.81 90.55) (end 157.93 90.55) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.93 90.55) (end 157.93 92.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 138.81 90.55) (end 138.81 92.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 111.6442 43.561) (end 111.6442 139.141) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.85 92.14) (end 115.73 92.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 115.73 90.55) (end 134.85 90.55) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.85 90.55) (end 134.85 92.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 161.9288 92.151) (end 161.9288 43.561) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.6992 92.151) (end 161.9288 92.151) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 115.73 90.55) (end 115.73 92.14) (layer Edge.Cuts) (width 0.05))
  (gr_text "Mozart, Lemmy, Matze, richx" (at 128.275 103.475) (layer F.SilkS))
  (gr_text THERM0 (at 166.2 134.525) (layer F.SilkS))
  (gr_text THERM1 (at 161.175 134.525) (layer F.SilkS))
  (gr_text PCLK (at 136.8336 81.0514) (layer F.SilkS))
  (gr_text BCLK (at 129.6454 80.4545) (layer F.SilkS))
  (gr_line (start 161.9288 43.561) (end 111.6442 43.561) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 111.6442 139.141) (end 170.6992 139.141) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.6992 139.141) (end 170.6992 92.151) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.4313 43.434) (xy 162.0916 43.434) (xy 162.0916 90.678) (xy 111.444 90.678)
      )
    )
  )
  (zone (net 2) (net_name VCC) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.4186 43.434) (xy 162.0916 43.434) (xy 162.0916 90.678) (xy 111.444 90.678)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.5172 92.024) (xy 170.8262 92.024) (xy 170.8262 139.268) (xy 111.5172 139.268)
      )
    )
  )
  (zone (net 15) (net_name +3V3) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads yes (clearance 0.000001))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.5172 92.024) (xy 170.8262 92.024) (xy 170.8262 139.268) (xy 111.5172 139.268)
      )
    )
  )
)
