(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 44)
    (no_connects 0)
    (area 114.674999 46.674999 136.825001 80.575001)
    (thickness 1.6)
    (drawings 12)
    (tracks 159)
    (zones 0)
    (modules 9)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.17)
    (zone_clearance 0.05)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.08 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /0.17)
  (net 3 /1.38)
  (net 4 /1.57)
  (net_class Default "This is the default net class."
    (clearance 0.17)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class top-bot ""
    (clearance 3.4)
    (trace_width 3.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /1.57)
  )
  (net_class top-m2 ""
    (clearance 3)
    (trace_width 0.34)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /0.17)
  )
  (net_class top-m3 ""
    (clearance 3.4)
    (trace_width 2.98)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /1.38)
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 5A7A001C)
    (at 134.25 63.5)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module sma:Molex_SMA_Jack_Edge_Mount (layer F.Cu) (tedit 5A7A0032)
    (at 132.5 54.25 180)
    (descr "Molex SMA Jack, Edge Mount, http://www.molex.com/pdm_docs/sd/732511150_sd.pdf")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J2 (at -1.72 7.11 180) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at -1.72 -7.11 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 /0.17))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_SMA_Jack_Edge_Mount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sma:Molex_SMA_Jack_Edge_Mount (layer B.Cu) (tedit 5A7A0042)
    (at 132.5 54.25 180)
    (descr "Molex SMA Jack, Edge Mount, http://www.molex.com/pdm_docs/sd/732511150_sd.pdf")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J4 (at -1.72 -7.11 180) (layer B.SilkS) hide)
    (fp_text value Conn_Coaxial (at -1.72 7.11 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 2.98) (layers B.Cu B.Paste B.Mask)
      (net 3 /1.38))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_SMA_Jack_Edge_Mount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sma:Molex_SMA_Jack_Edge_Mount (layer F.Cu) (tedit 5A7A0027)
    (at 119 54.25)
    (descr "Molex SMA Jack, Edge Mount, http://www.molex.com/pdm_docs/sd/732511150_sd.pdf")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J1 (at -1.72 7.11) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at -1.72 -7.11) (layer F.Fab))
    (pad 1 smd rect (at -1.72 0) (size 5.08 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 /0.17))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_SMA_Jack_Edge_Mount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sma:Molex_SMA_Jack_Edge_Mount (layer B.Cu) (tedit 5A7A0039)
    (at 119 54.25)
    (descr "Molex SMA Jack, Edge Mount, http://www.molex.com/pdm_docs/sd/732511150_sd.pdf")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J3 (at -1.72 -7.11) (layer B.SilkS) hide)
    (fp_text value Conn_Coaxial (at -1.72 7.11) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.72 0) (size 5.08 2.98) (layers B.Cu B.Paste B.Mask)
      (net 3 /1.38))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_SMA_Jack_Edge_Mount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sma:Molex_SMA_Jack_Edge_Mount (layer F.Cu) (tedit 5A7A002E)
    (at 119 73)
    (descr "Molex SMA Jack, Edge Mount, http://www.molex.com/pdm_docs/sd/732511150_sd.pdf")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J5 (at -1.72 7.11) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at -1.72 -7.11) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.72 0) (size 5.08 3.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /1.57))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38) (size 5.08 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38) (size 5.08 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_SMA_Jack_Edge_Mount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sma:Molex_SMA_Jack_Edge_Mount (layer F.Cu) (tedit 5A7A0046)
    (at 132.5 73 180)
    (descr "Molex SMA Jack, Edge Mount, http://www.molex.com/pdm_docs/sd/732511150_sd.pdf")
    (tags "sma edge")
    (attr smd)
    (fp_text reference J6 (at -1.72 7.11 180) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at -1.72 -7.11 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.72 0 180) (size 5.08 3.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /1.57))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 -4.38 180) (size 5.08 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.72 4.38 180) (size 5.08 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_SMA_Jack_Edge_Mount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 5A7A001E)
    (at 117.25 63.5)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module OPENHARDWARE:OSHWLOGO0.3IN (layer B.Cu) (tedit 0)
    (at 129.5 67.75 180)
    (descr "OSHW LOGO")
    (tags "Open Source Hardware Logo")
    (fp_text reference G*** (at 0 -7.27964 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 7.27964 180) (layer B.SilkS) hide)
  )
  (gr_text "DB4UM 2018" (at 125.75 77.75) (layer B.Mask))
  (gr_text "top:m3 2.98 mm" (at 125.75 62.25) (layer B.SilkS))
  (gr_text "top:m1 0.34mm\ntop:m4 3.40mm" (at 125.75 61.5) (layer F.SilkS))
  (gr_text "Microstrip test\nOSH Park 4 Layer" (at 125.75 65) (layer B.SilkS))
  (dimension 33.75 (width 0.3) (layer Dwgs.User)
    (gr_text "33.750 mm" (at 98.4 63.625 90) (layer Dwgs.User))
    (feature1 (pts (xy 114.75 46.75) (xy 97.05 46.75)))
    (feature2 (pts (xy 114.75 80.5) (xy 97.05 80.5)))
    (crossbar (pts (xy 99.75 80.5) (xy 99.75 46.75)))
    (arrow1a (pts (xy 99.75 46.75) (xy 100.336421 47.876504)))
    (arrow1b (pts (xy 99.75 46.75) (xy 99.163579 47.876504)))
    (arrow2a (pts (xy 99.75 80.5) (xy 100.336421 79.373496)))
    (arrow2b (pts (xy 99.75 80.5) (xy 99.163579 79.373496)))
  )
  (dimension 22 (width 0.3) (layer Dwgs.User)
    (gr_text "22.000 mm" (at 125.75 41.9) (layer Dwgs.User))
    (feature1 (pts (xy 136.75 46.75) (xy 136.75 40.55)))
    (feature2 (pts (xy 114.75 46.75) (xy 114.75 40.55)))
    (crossbar (pts (xy 114.75 43.25) (xy 136.75 43.25)))
    (arrow1a (pts (xy 136.75 43.25) (xy 135.623496 43.836421)))
    (arrow1b (pts (xy 136.75 43.25) (xy 135.623496 42.663579)))
    (arrow2a (pts (xy 114.75 43.25) (xy 115.876504 43.836421)))
    (arrow2b (pts (xy 114.75 43.25) (xy 115.876504 42.663579)))
  )
  (dimension 7.5 (width 0.3) (layer Dwgs.User)
    (gr_text "7.500 mm" (at 101.9 50.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 114.75 54.25) (xy 100.55 54.25)))
    (feature2 (pts (xy 114.75 46.75) (xy 100.55 46.75)))
    (crossbar (pts (xy 103.25 46.75) (xy 103.25 54.25)))
    (arrow1a (pts (xy 103.25 54.25) (xy 102.663579 53.123496)))
    (arrow1b (pts (xy 103.25 54.25) (xy 103.836421 53.123496)))
    (arrow2a (pts (xy 103.25 46.75) (xy 102.663579 47.876504)))
    (arrow2b (pts (xy 103.25 46.75) (xy 103.836421 47.876504)))
  )
  (dimension 7.5 (width 0.3) (layer Dwgs.User)
    (gr_text "7.500 mm" (at 101.9 76.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 119 80.5) (xy 100.55 80.5)))
    (feature2 (pts (xy 119 73) (xy 100.55 73)))
    (crossbar (pts (xy 103.25 73) (xy 103.25 80.5)))
    (arrow1a (pts (xy 103.25 80.5) (xy 102.663579 79.373496)))
    (arrow1b (pts (xy 103.25 80.5) (xy 103.836421 79.373496)))
    (arrow2a (pts (xy 103.25 73) (xy 102.663579 74.126504)))
    (arrow2b (pts (xy 103.25 73) (xy 103.836421 74.126504)))
  )
  (gr_line (start 136.75 80.5) (end 114.75 80.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.75 46.75) (end 136.75 80.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.75 46.75) (end 136.75 46.75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.75 80.5) (end 114.75 46.75) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name /0.17) (layer F.Cu) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.325 54.05) (xy 119.825 54.05) (xy 120.15 54.1) (xy 120.15 54.4) (xy 119.825 54.45)
        (xy 119.325 54.45)
      )
    )
  )
  (zone (net 2) (net_name /0.17) (layer F.Cu) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.175 54.45) (xy 131.675 54.45) (xy 131.352824 54.4) (xy 131.352824 54.1) (xy 131.675 54.05)
        (xy 132.175 54.05)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.05)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.75 50.75) (xy 131.75 50.75) (xy 131.75 48) (xy 119.75 48) (xy 119.75 50.75)
        (xy 114.75 50.75) (xy 114.75 46.75) (xy 136.75 46.75)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.05)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.75 67.75) (xy 114.75 59.45) (xy 136.75 59.45) (xy 136.75 67.75) (xy 131.75 67.75)
        (xy 131.75 63.75) (xy 119.75 63.75) (xy 119.75 67.75)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.05)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.75 76.5) (xy 136.75 80.5) (xy 114.75 80.5) (xy 114.75 78.15) (xy 119.75 78.15)
        (xy 119.75 79.75) (xy 131.75 79.75) (xy 131.75 78.1) (xy 136.75 78.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.05)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.75 59.5) (xy 114.75 80.5) (xy 136.75 80.5) (xy 136.75 59.5) (xy 131.75 59.5)
        (xy 131.75 60.75) (xy 119.75 60.75) (xy 119.75 59.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.05)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.75 46.75) (xy 114.75 63.75) (xy 136.75 63.75) (xy 136.75 47) (xy 136.75 46.75)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.05)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.75 50.75) (xy 131.75 50.75) (xy 131.75 48.75) (xy 119.75 48.75) (xy 119.75 50.75)
        (xy 114.75 50.75) (xy 114.75 46.75) (xy 136.75 46.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.05)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.75 46.75) (xy 114.75 59.75) (xy 136.75 59.75) (xy 136.75 46.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.05)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.75 80.5) (xy 114.75 63.25) (xy 136.75 63.25) (xy 136.75 80.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.05)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.75 46.75) (xy 114.75 61.5) (xy 136.75 61.5) (xy 136.75 46.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.05)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.5 63.25) (xy 114.75 63.25) (xy 114.75 59.75) (xy 119.5 59.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch none 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.05))
    (min_thickness 0.05)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.75 63.25) (xy 132 63.25) (xy 132 59.75) (xy 136.75 59.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.05))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.75 61.25) (xy 114.75 80.5) (xy 136.75 80.5) (xy 136.75 61.25) (xy 133 61.25)
        (xy 133 63.5) (xy 131.5 67.5) (xy 131.5 79.5) (xy 120 79.5) (xy 120 67.5)
        (xy 118.75 63.5) (xy 118.75 61.25)
      )
    )
  )
)
