(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 45)
    (no_connects 0)
    (area 186.233999 102.794999 216.229001 152.475001)
    (thickness 1.6)
    (drawings 109)
    (tracks 201)
    (zones 0)
    (modules 32)
    (nets 15)
  )
  (page A4)
  (title_block
    (title "PCB269- Gammon Solar power/ supercap standby/ watchdog")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 1.0414)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "C:/Users/TBoyd/Documents/KiCad-TKB-4-0-4/Project/PCB269-GammonSolarWatchdog/For exports en route elsewhere/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad1)")
  (net 3 +BATT)
  (net 4 "Net-(C3-Pad1)")
  (net 5 ATtiny85_5v)
  (net 6 "Net-(Q2-Pad1)")
  (net 7 "Net-(Q2-Pad5)")
  (net 8 "Net-(P1-Pad1)")
  (net 9 "Net-(Q1-PadGate)")
  (net 10 "Net-(D4-Pad1)")
  (net 11 "Net-(P2-Pad1)")
  (net 12 "Net-(P3-Pad1)")
  (net 13 "Net-(P4-Pad1)")
  (net 14 "Net-(P5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net ATtiny85_5v)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(Q1-PadGate)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q2-Pad5)")
  )
  (module AtbFoot17201:VRegTO92-tb (layer F.Cu) (tedit 5A1DFD92)
    (at 212.2805 138.1125 90)
    (fp_text reference Q3 (at 1.2065 2.8575 90) (layer F.SilkS))
    (fp_text value "Volt Reg- see text" (at -0.0254 -2.5908 90) (layer F.Fab))
    (pad GND thru_hole circle (at 0 1.016 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad VI thru_hole circle (at -1.524 -0.6985 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 ATtiny85_5v))
    (pad VO thru_hole circle (at 1.3335 -0.5715 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (module AtbFoot17201:MountingHole_2.9mm (layer F.Cu) (tedit 5A1DF78E)
    (at 189.6745 149.0345)
    (descr "Mounting Hole 2.9mm, no annular")
    (tags "mounting hole 2.9mm no annular")
    (fp_text reference MH0 (at -8.8265 0.0635) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3.175) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.9 2.9) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module AtbFoot17201:MountingHole_2.9mm (layer F.Cu) (tedit 5A1DF792)
    (at 206.375 106.045)
    (descr "Mounting Hole 2.9mm, no annular")
    (tags "mounting hole 2.9mm no annular")
    (fp_text reference MH1 (at 2.159 -6.223) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3.175) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.9 2.9) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module AtbFoot17201:Cap-Super8x2-tb (layer F.Cu) (tedit 5A03C834)
    (at 199.39 138.938 270)
    (fp_text reference C1 (at 0 5.08 270) (layer F.SilkS))
    (fp_text value "SuperCap-see text" (at -0.508 -4.826 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 7.112 3.048) (drill 1.5494 (offset -1.27 0)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 7.112 3.048) (drill 1.5494 (offset -1.27 0)) (layers *.Cu *.Mask)
      (net 5 ATtiny85_5v))
  )
  (module AtbFoot17201:Cap-Rad-1-tb (layer F.Cu) (tedit 5A1DF8AA)
    (at 211.836 147.574 90)
    (fp_text reference C2 (at -1.778 2.032 90) (layer F.SilkS))
    (fp_text value 1uF (at -0.00254 -1.6764 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.524 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 ATtiny85_5v))
    (pad 2 thru_hole circle (at 1.524 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module AtbFoot17201:Cap-Rad3x1-2-tb (layer F.Cu) (tedit 5A1DF819)
    (at 194.437 107.442 180)
    (fp_text reference C4 (at 3.937 3.556 360) (layer F.SilkS))
    (fp_text value "See text" (at 0 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.524 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 ATtiny85_5v))
    (pad 2 thru_hole circle (at 1.524 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module AtbFoot17201:Cap-Rect-28x12-tb (layer F.Cu) (tedit 5A1DF84F)
    (at 196.6595 123.6345 180)
    (fp_text reference C5 (at -4.7625 -1.3335 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0.07874 -2.32664 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 ATtiny85_5v))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module AtbFoot17201:Diode-Small-4148-tb (layer F.Cu) (tedit 5A1DF849)
    (at 188.849 122.3645 90)
    (fp_text reference D1 (at -0.8255 1.905 90) (layer F.SilkS))
    (fp_text value "See text" (at 0.127 -1.778 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module AtbFoot17201:Diode-Small-4148-tb (layer F.Cu) (tedit 5A050065)
    (at 188.341 129.286 90)
    (fp_text reference D2 (at -0.635 1.905 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.127 -1.778 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 ATtiny85_5v))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module AtbFoot17201:Diode-Small-4148-tb (layer F.Cu) (tedit 5A1DF80F)
    (at 188.341 108.077 270)
    (fp_text reference D3 (at -4.191 0.889 360) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.127 -1.778 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 ATtiny85_5v))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module AtbFoot17201:Skt-DIL-8-tb (layer F.Cu) (tedit 5A1DF829)
    (at 196.85 116.84)
    (fp_text reference Q2 (at 2.286 -5.588) (layer F.SilkS))
    (fp_text value ATtiny85 (at 0.254 -6.096) (layer F.Fab))
    (pad 1 thru_hole circle (at -4.318 -3.81) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(Q2-Pad1)"))
    (pad 2 thru_hole circle (at -4.318 -1.27) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(P3-Pad1)"))
    (pad 3 thru_hole circle (at -4.318 1.27) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(P4-Pad1)"))
    (pad 4 thru_hole circle (at -4.318 3.81) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 4.191 3.81) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(Q2-Pad5)"))
    (pad 6 thru_hole circle (at 4.191 1.27) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad1)"))
    (pad 7 thru_hole circle (at 4.191 -1.27) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad1)"))
    (pad 8 thru_hole circle (at 4.191 -3.81) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 ATtiny85_5v))
  )
  (module AtbFoot17201:Res-Small-0.125-tb (layer F.Cu) (tedit 5A1E0030)
    (at 204.1525 114.6175 90)
    (fp_text reference R3 (at 0 2.667 90) (layer F.SilkS))
    (fp_text value 10k (at 0.127 -1.778 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(Q2-Pad5)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module AtbFoot17201:Res-Small-0.125-tb (layer F.Cu) (tedit 5A1E0297)
    (at 188.849 115.316 270)
    (fp_text reference R4 (at 1.5875 -1.3335 270) (layer F.SilkS))
    (fp_text value 10k (at 0.127 -1.778 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 ATtiny85_5v))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(Q2-Pad1)"))
  )
  (module AtbFoot17201:Cap-Rad-1-tb (layer F.Cu) (tedit 5A1E0463)
    (at 213.995 131.7625 90)
    (fp_text reference C3 (at 0.635 -1.5875 90) (layer F.SilkS))
    (fp_text value "1 uF" (at 0.0127 -1.8288 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.524 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 1.524 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module AtbFoot17201:XistMosFet-TO92-SGB-tb (layer F.Cu) (tedit 5A1DF9F0)
    (at 201.295 108.0135 270)
    (fp_text reference Q1 (at -1.8923 1.7526 270) (layer F.SilkS))
    (fp_text value XistMosfetTO92-SGD2 (at -0.0254 -2.5908 270) (layer F.Fab))
    (pad Gate thru_hole circle (at 0 1.016 270) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-PadGate)"))
    (pad Drai thru_hole circle (at -2.032 -1.016 270) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(P5-Pad1)"))
    (pad Sour thru_hole circle (at 2.032 -1.016 270) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module AtbFoot17201:Res-Small-0.125-tb (layer F.Cu) (tedit 5A1E002B)
    (at 204.1525 121.9835 90)
    (fp_text reference R2 (at 0.0635 2.667 90) (layer F.SilkS))
    (fp_text value 150R (at 0.127 -1.778 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(Q1-PadGate)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(Q2-Pad5)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5A1E03A3)
    (at 213.614 140.9065)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference P90 (at 5.2705 -0.1905) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 ATtiny85_5v))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5A1E03AC)
    (at 211.582 143.0655)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference P91 (at 7.239 -0.8255) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1DF846)
    (at 191.516 126.9365)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 1.016 2.3495) (layer F.SilkS))
    (fp_text value 220R (at 3.81 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +BATT))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5A1DF907)
    (at 204.343 128.0795 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at -1.143 1.8415 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +BATT))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module AtbFoot17201:Res-Small-0.125-tb (layer F.Cu) (tedit 5A1DF8CD)
    (at 208.788 129.794)
    (fp_text reference R5 (at -1.524 1.778) (layer F.SilkS))
    (fp_text value R (at 0.127 -1.778) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5A1E03CF)
    (at 210.8835 133.9215)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference Link1a1 (at 8.8265 -0.3175) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5A1E03CA)
    (at 209.169 132.0165)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference Link1b1 (at 10.541 -0.1905) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5A1DF774)
    (at 209.55 146.304)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference TP1a1 (at -6.096 7.874) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5A1DF770)
    (at 209.55 148.844)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference TP1b1 (at -4.064 7.112) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5A1E039C)
    (at 214.122 144.78)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference Link2a1 (at 5.3975 -0.127) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 ATtiny85_5v))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5A1E0399)
    (at 214.122 147.32)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference Link2b1 (at 5.588 0.0635) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 ATtiny85_5v))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5A1DFB47)
    (at 202.438 114.935)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference P2 (at -6.223 -1.3335) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5A1DFB42)
    (at 190.881 115.1255)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference P3 (at -6.2865 -1.905) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(P3-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 5A1E028F)
    (at 190.881 118.745)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference P4 (at -6.5405 -1.5875) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(P4-Pad1)"))
  )
  (module AtbFoot17201:Sil-5-3-81mm (layer F.Cu) (tedit 5A1DC994)
    (at 209.8675 111.506 270)
    (fp_text reference P5 (at 4.65074 -2.57048 270) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0.58674 2.36728 270) (layer F.SilkS))
    (fp_text user "wires this side" (at 14.351 -2.7305 270) (layer F.SilkS))
    (pad 5 thru_hole circle (at 15.24 0 270) (size 2.5 2.5) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P5-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 2.5 2.5) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 3 +BATT))
    (pad 3 thru_hole circle (at 7.62 0 270) (size 2.5 2.5) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 5 ATtiny85_5v))
    (pad 4 thru_hole circle (at 11.43 0 270) (size 2.5 2.5) (drill 1.0414) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 56C35F63)
    (at 202.438 118.3005 270)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference P1 (at 0 -2 270) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad1)"))
  )
  (gr_text L2 (at 215.392 146.05 90) (layer F.SilkS))
  (gr_text L1 (at 211.074 132.1435 130) (layer B.SilkS))
  (gr_text L1 (at 211.1375 131.826 130) (layer F.SilkS))
  (gr_text L2 (at 215.2015 146.1135 90) (layer B.SilkS))
  (gr_line (start 216.154 152.4) (end 186.3344 152.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.4868 102.87) (end 186.3344 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 216.154 102.87) (end 186.436 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text Q3b (at 208.534 140.716 90) (layer F.SilkS))
  (gr_text a (at 215.138 135.382 90) (layer F.SilkS))
  (gr_line (start 216.154 152.4) (end 216.154 102.87) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Pin 1" (at 204.978 110.744 90) (layer F.SilkS))
  (gr_text Gnd (at 202.8825 144.272 90) (layer B.SilkS))
  (gr_text https://bitly.com/SuperSolarBatt (at 205.486 125.984 90) (layer B.SilkS))
  (gr_text batt (at 202.438 104.5464) (layer F.SilkS))
  (gr_text solar (at 199.8472 104.5464) (layer F.SilkS))
  (gr_text super (at 202.2856 103.5812) (layer F.SilkS))
  (gr_text Bit.ly/ (at 199.136 103.632) (layer F.SilkS))
  (gr_text "Circuit: Nick Gammon" (at 203.708 150.749) (layer F.SilkS))
  (gr_text Ground (at 213.1695 125.095) (layer B.SilkS))
  (gr_text "3V3 out" (at 212.7885 121.0945) (layer B.SilkS))
  (gr_text "Out +ve" (at 212.7885 117.221) (layer B.SilkS))
  (gr_text To/Reset (at 212.344 109.5375) (layer B.SilkS))
  (gr_text R (at 214.503 111.379 90) (layer F.SilkS))
  (gr_text In (at 214.503 115.316 90) (layer F.SilkS))
  (gr_text Out (at 214.4395 118.9355 90) (layer F.SilkS))
  (gr_text 3 (at 214.63 122.936 90) (layer F.SilkS))
  (gr_text Gnd (at 214.503 127.0635 90) (layer F.SilkS))
  (gr_line (start 186.309 102.87) (end 186.309 152.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text SheepdogSoftware.co.uk (at 195.58 124.0155 90) (layer B.SilkS))
  (gr_text v17b28 (at 187.452 136.398 90) (layer F.SilkS))
  (gr_text PCB269 (at 187.452 142.748 90) (layer F.SilkS))
  (gr_text "In +ve" (at 213.233 113.538) (layer B.SilkS))
)
