(kicad_pcb (version 20171130) (host pcbnew 5.1.7-a382d34a8~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 31)
    (tracks 91)
    (zones 0)
    (modules 3)
    (nets 29)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.2032)
    (user_trace_width 0.25)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.4064)
    (via_drill 0.254)
    (via_min_size 0.4064)
    (via_min_drill 0.254)
    (uvia_size 0.4064)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.4064)
    (uvia_min_drill 0.254)
    (edge_width 0.01)
    (segment_width 0.2032)
    (pcb_text_width 0.254)
    (pcb_text_size 1.2192 1.2192)
    (mod_edge_width 0.1)
    (mod_text_size 0.4572 0.4572)
    (mod_text_width 0.0254)
    (pad_size 1.2 1.2)
    (pad_drill 0.75)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 147.2184 99.187)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Teeprom_GERBER"))
  )
  (net 0 "")
  (net 1 /D3)
  (net 2 /A10)
  (net 3 /D4)
  (net 4 /A7)
  (net 5 /D5)
  (net 6 /A6)
  (net 7 /D6)
  (net 8 /A5)
  (net 9 /D7)
  (net 10 /A4)
  (net 11 /A11)
  (net 12 /A3)
  (net 13 /~OE)
  (net 14 /A2)
  (net 15 /A13)
  (net 16 /A1)
  (net 17 /A0)
  (net 18 /A12)
  (net 19 /D0)
  (net 20 /A9)
  (net 21 /D1)
  (net 22 /A8)
  (net 23 /D2)
  (net 24 /~CE)
  (net 25 /A14)
  (net 26 /~WE)
  (net 27 VCC)
  (net 28 GND)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.4064)
    (via_drill 0.254)
    (uvia_dia 0.4064)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /~CE)
    (add_net /~OE)
    (add_net /~WE)
    (add_net GND)
    (add_net VCC)
  )
  (module 000_LOCAL:FlashOpt100_PRG_4x7_male (layer Top) (tedit 5F92FF97)
    (at 147.2184 99.187 270)
    (descr "Through hole straight pin header, 2x07, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x07 2.00mm double row")
    (fp_text reference J2 (at 0 6 270 unlocked) (layer F.SilkS) hide)
    (fp_text value FlashOpt100_PRG_4x7 (at 0 8 90) (layer F.Fab))
    (fp_text user %R (at 0 6 90) (layer F.Fab))
    (pad 21 thru_hole circle (at 9 0 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 /D3))
    (pad 28 thru_hole circle (at 11 -6 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 13 /~OE))
    (pad 25 thru_hole circle (at 9 -4 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 /D7))
    (pad 26 thru_hole circle (at 11 -4 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 24 /~CE))
    (pad 23 thru_hole circle (at 9 -2 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /D5))
    (pad 24 thru_hole circle (at 11 -2 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 /D6))
    (pad 15 thru_hole circle (at 9 6 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 /A1))
    (pad 22 thru_hole circle (at 11 0 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 /D4))
    (pad 16 thru_hole circle (at 11 6 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 17 /A0))
    (pad 27 thru_hole circle (at 9 -6 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 /A10))
    (pad 19 thru_hole circle (at 9 2 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 23 /D2))
    (pad 20 thru_hole circle (at 11 2 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 28 GND))
    (pad 17 thru_hole circle (at 9 4 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 19 /D0))
    (pad 18 thru_hole circle (at 11 4 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 21 /D1))
    (pad 13 thru_hole circle (at -9 6 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 12 /A3))
    (pad 14 thru_hole circle (at -11 6 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 /A2))
    (pad 11 thru_hole circle (at -9 4 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 /A5))
    (pad 12 thru_hole circle (at -11 4 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 /A4))
    (pad 9 thru_hole circle (at -9 2 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /A7))
    (pad 10 thru_hole circle (at -11 2 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 /A6))
    (pad 7 thru_hole circle (at -9 0 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 27 VCC))
    (pad 8 thru_hole circle (at -11 0 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 18 /A12))
    (pad 5 thru_hole circle (at -9 -2 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 25 /A14))
    (pad 6 thru_hole circle (at -11 -2 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 26 /~WE))
    (pad 3 thru_hole circle (at -9 -4 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 22 /A8))
    (pad 4 thru_hole circle (at -11 -4 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 15 /A13))
    (pad 1 thru_hole circle (at -8 -6 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 /A11))
    (pad 2 thru_hole circle (at -10 -6 270) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 20 /A9))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/PinHeader_2x07_P2.00mm_Vertical.step
      (offset (xyz 9 6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/PinHeader_2x06_P2.00mm_Vertical.step
      (offset (xyz -11 4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/PinHeader_2x01_P2.00mm_Vertical.step
      (offset (xyz -10 6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:DIP-28_600 (layer Top) (tedit 5F9E12B7)
    (at 147.2184 99.187)
    (descr "28-lead dip, row spacing 600 mils")
    (tags "DIL DIP PDIP 2.54mm 600 mil")
    (fp_text reference J1 (at -3.81 -16.51) (layer F.SilkS) hide)
    (fp_text value "29F256 / 29C256" (at 0 19.05) (layer F.Fab))
    (fp_text user %R (at -3.81 -16.51) (layer F.Fab))
    (pad 1 thru_hole roundrect (at -7.62 -16.51) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 26 /~WE))
    (pad 2 thru_hole circle (at -7.62 -13.97) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 18 /A12))
    (pad 3 thru_hole circle (at -7.62 -11.43) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 4 /A7))
    (pad 15 thru_hole circle (at 7.62 16.51) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 /D3))
    (pad 4 thru_hole circle (at -7.62 -8.89) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 6 /A6))
    (pad 16 thru_hole circle (at 7.62 13.97) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 3 /D4))
    (pad 5 thru_hole circle (at -7.62 -6.35) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 8 /A5))
    (pad 17 thru_hole circle (at 7.62 11.43) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 5 /D5))
    (pad 6 thru_hole circle (at -7.62 -3.81) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 10 /A4))
    (pad 18 thru_hole circle (at 7.62 8.89) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 7 /D6))
    (pad 7 thru_hole circle (at -7.62 -1.27) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 12 /A3))
    (pad 19 thru_hole circle (at 7.62 6.35) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 9 /D7))
    (pad 8 thru_hole circle (at -7.62 1.27) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 14 /A2))
    (pad 20 thru_hole circle (at 7.62 3.81) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 24 /~CE))
    (pad 9 thru_hole circle (at -7.62 3.81) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 16 /A1))
    (pad 21 thru_hole circle (at 7.62 1.27) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 2 /A10))
    (pad 10 thru_hole circle (at -7.62 6.35) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 17 /A0))
    (pad 22 thru_hole circle (at 7.62 -1.27) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 13 /~OE))
    (pad 11 thru_hole circle (at -7.62 8.89) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 19 /D0))
    (pad 23 thru_hole circle (at 7.62 -3.81) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 11 /A11))
    (pad 12 thru_hole circle (at -7.62 11.43) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 21 /D1))
    (pad 24 thru_hole circle (at 7.62 -6.35) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 20 /A9))
    (pad 13 thru_hole circle (at -7.62 13.97) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 23 /D2))
    (pad 25 thru_hole circle (at 7.62 -8.89) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 22 /A8))
    (pad 14 thru_hole circle (at -7.62 16.51) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 28 GND))
    (pad 26 thru_hole circle (at 7.62 -11.43) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 15 /A13))
    (pad 27 thru_hole circle (at 7.62 -13.97) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 25 /A14))
    (pad 28 thru_hole circle (at 7.62 -16.51) (size 1.524 1.524) (drill 0.9144) (layers *.Cu *.Mask)
      (net 27 VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/PinHeader_1x14_P2.54mm_Vertical.step
      (offset (xyz 7.62 16.51 -1.7272))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/PinHeader_1x14_P2.54mm_Vertical.step
      (offset (xyz -7.62 16.51 -1.7272))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 0))
    )
  )
  (module 000_LOCAL:IC_polarity_notch (layer Top) (tedit 5F934073)
    (at 147.2184 81.407)
    (fp_text reference notch (at 0 2) (layer F.SilkS) hide)
    (fp_text value IC_polarity_notch (at 0 -2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.54 2.54) (drill 2.54) (layers *.Cu *.Mask))
  )
  (gr_text "DIP PINS\nTHIS SIDE" (at 147.2184 84.582) (layer B.SilkS))
  (gr_text "CENTER PINS\nOTHER SIDE" (at 147.2184 92.837) (layer B.SilkS))
  (gr_text "SET PROGRAMMER TO\n29F256 / 29C256" (at 147.2184 115.687) (layer F.SilkS))
  (gr_text tandy.wiki/Teeprom (at 141.5034 99.187 -90) (layer F.SilkS))
  (gr_text "FlashOpt100\nProgramming\nAdapter" (at 147.2184 99.187 -90) (layer F.SilkS))
  (gr_text 28 (at 151.6634 83.312) (layer F.SilkS))
  (gr_text 1 (at 142.1384 83.312) (layer F.SilkS))
  (gr_line (start 156.1084 116.967) (end 138.3284 116.967) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 156.1084 81.407) (end 156.1084 116.967) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 138.3284 81.407) (end 156.1084 81.407) (layer Edge.Cuts) (width 0.01))
  (gr_line (start 138.3284 116.967) (end 138.3284 81.407) (layer Edge.Cuts) (width 0.01))
)
