(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.5748)
    (drawings 19)
    (tracks 96)
    (zones 0)
    (modules 13)
    (nets 13)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.6096)
    (user_trace_width 0.254)
    (user_trace_width 0.6096)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +12V)
  (net 3 /KBD_RDATA)
  (net 4 /KBD_XDATA)
  (net 5 /BLUE-)
  (net 6 /GREEN-)
  (net 7 /RED-)
  (net 8 /MONO-)
  (net 9 /BLUE+)
  (net 10 /GREEN+)
  (net 11 /RED+)
  (net 12 /MONO+)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /KBD_RDATA)
    (add_net /KBD_XDATA)
    (add_net GND)
  )
  (net_class Video75OhmDifferential ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.6096)
    (diff_pair_gap 0.6096)
    (add_net /BLUE+)
    (add_net /BLUE-)
    (add_net /GREEN+)
    (add_net /GREEN-)
    (add_net /MONO+)
    (add_net /MONO-)
    (add_net /RED+)
    (add_net /RED-)
  )
  (module vr2x1breakout:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 94.7674 88.5444)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 0 -1.43) (layer F.SilkS))
    (fp_text value "10 μF" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /BLUE-))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /BLUE-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vr2x1breakout:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 90.1965 89.789)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 -1.43) (layer F.SilkS))
    (fp_text value "10 μF" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /BLUE+))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /BLUE+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vr2x1breakout:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEF)
    (at 86.7664 81.6864)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 1.43 180 unlocked) (layer B.SilkS))
    (fp_text value "10 μF" (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 /GREEN-))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 /GREEN-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vr2x1breakout:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEF)
    (at 92.0242 82.9056)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 1.43 180 unlocked) (layer B.SilkS))
    (fp_text value "10 μF" (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 /GREEN+))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 /GREEN+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vr2x1breakout:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 86.6394 80.2386)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.43) (layer F.SilkS))
    (fp_text value "10 μF" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /RED-))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /RED-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vr2x1breakout:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 92.0242 79.0448)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value "10 μF" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RED+))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /RED+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vr2x1breakout:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEF)
    (at 92.0242 78.613)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 1.43 180 unlocked) (layer B.SilkS))
    (fp_text value "10 μF" (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 /MONO-))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 /MONO-))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vr2x1breakout:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEF)
    (at 97.282 77.3938)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 1.43 180 unlocked) (layer B.SilkS))
    (fp_text value "10 μF" (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 /MONO+))
    (pad 2 smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 /MONO+))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vr2x1breakout:RCJ-32265 (layer F.Cu) (tedit 6085B0D4)
    (at 68.326 72.0598)
    (descr "CUI RCJ-32265 Red/Green/Blue RCA jacks")
    (fp_text reference J5 (at 2.2352 14.986) (layer F.SilkS))
    (fp_text value RCJ-32265 (at 2.2352 14.986) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 15) (size 1.9 3.200001) (drill oval 1.2 2.5) (layers *.Cu *.Mask)
      (net 6 /GREEN-))
    (pad 5 thru_hole oval (at 0 30) (size 1.9 3.200001) (drill oval 1.2 2.5) (layers *.Cu *.Mask)
      (net 5 /BLUE-))
    (pad "" thru_hole oval (at 0 35.3) (size 3.2 2.7) (drill oval 2.5 2) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 0 0) (size 1.9 3.200001) (drill oval 1.2 2.5) (layers *.Cu *.Mask)
      (net 7 /RED-))
    (pad "" thru_hole oval (at 0 -5.3) (size 3.2 2.7) (drill oval 2.5 2) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 4.5 30) (size 3.200001 1.7) (drill oval 2.5 1) (layers *.Cu *.Mask)
      (net 9 /BLUE+))
    (pad 4 thru_hole oval (at 4.5 15) (size 3.200001 1.7) (drill oval 2.5 1) (layers *.Cu *.Mask)
      (net 10 /GREEN+))
    (pad 2 thru_hole oval (at 4.5 0) (size 3.200001 1.7) (drill oval 2.5 1) (layers *.Cu *.Mask)
      (net 11 /RED+))
  )
  (module vr2x1breakout:CUI_RCJ-044 (layer F.Cu) (tedit 6085B0DE)
    (at 81.9404 67.7418 90)
    (descr "CUI RCJ-044 CONN RCA JACK MONO 3.2MM R/A")
    (fp_text reference J4 (at -2.825 -6.635 90) (layer F.SilkS))
    (fp_text value "CUI RCJ-044" (at 0.985 6.635 90) (layer F.Fab))
    (fp_line (start 4 3.35) (end 2.3 3.35) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4 5.15) (end 4 3.35) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.3 5.15) (end 4 5.15) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.3 3.35) (end 2.3 5.15) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4 -5.15) (end 2.3 -5.15) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 4 -3.35) (end 4 -5.15) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.3 -3.35) (end 4 -3.35) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.3 -5.15) (end 2.3 -3.35) (layer Edge.Cuts) (width 0.1))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.95 3.9) (drill oval 1.3 2.5) (layers *.Cu *.Mask)
      (net 8 /MONO-))
    (pad 2 thru_hole oval (at -4.5 0 90) (size 3.400001 1.7) (drill oval 2.5 1) (layers *.Cu *.Mask)
      (net 12 /MONO+))
  )
  (module vr2x1breakout:CUI_PJ-037AH (layer F.Cu) (tedit 6085CE04)
    (at 94.3102 72.1106 90)
    (descr "CUI PJ-037AH barrel jack")
    (fp_text reference J3 (at 2.675 -5.635 90) (layer F.SilkS))
    (fp_text value PJ-037AH (at 7.12 5.635 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.5 5) (drill oval 1 3.500001) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole oval (at 6 0 90) (size 2.25 4.500001) (drill oval 1 2.999999) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/3dmodels/PJ-037AH.step
      (offset (xyz 13.716 0 6.35))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 90))
    )
  )
  (module vr2x1breakout:RJ22_TE_215875 (layer F.Cu) (tedit 603B19B0)
    (at 81.8896 96.1898)
    (descr "RJ22 connector https://www.te.com/usa-en/product-CAT-R52922-C76264.html")
    (tags "RJ22 connector")
    (fp_text reference J2 (at -2.92 -5.32) (layer F.SilkS))
    (fp_text value Keyboard (at 1.905 15.7226) (layer F.Fab))
    (fp_text user %R (at 1.9304 7.8994) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.715 6.35) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 3.81 -2.54) (size 1.52 1.52) (drill 0.889) (layers *.Cu *.Mask)
      (net 3 /KBD_RDATA))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.52 1.52) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 2 thru_hole circle (at 1.27 -2.54) (size 1.52 1.52) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at -1.905 6.35) (size 3.2512 3.2512) (drill 3.2512) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.52 1.52) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 /KBD_XDATA))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ12_Amphenol_54601.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module vr2x1breakout:AMPLIMITE_5788798_DE15 (layer F.Cu) (tedit 603B0DED)
    (at 109.728 77.1652 90)
    (descr "15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm")
    (tags "15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm ")
    (fp_text reference J1 (at -9.695 -2.8 90) (layer F.SilkS))
    (fp_text value DB15_Female (at -9.695 20.81 90) (layer F.Fab))
    (fp_text user %R (at -9.695 16.225 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 5 /BLUE-))
    (pad 2 thru_hole circle (at -2.7432 0 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 6 /GREEN-))
    (pad 3 thru_hole circle (at -5.4864 0 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 7 /RED-))
    (pad 4 thru_hole circle (at -8.2296 0 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 8 /MONO-))
    (pad 5 thru_hole circle (at -10.9728 0 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -13.716 0 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -16.4592 0 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 8 thru_hole circle (at -19.2024 0 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 9 thru_hole circle (at -1.3716 2.8448 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 9 /BLUE+))
    (pad 10 thru_hole circle (at -4.1148 2.8448 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 10 /GREEN+))
    (pad 11 thru_hole circle (at -6.858 2.8448 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 11 /RED+))
    (pad 12 thru_hole circle (at -9.6012 2.8448 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 12 /MONO+))
    (pad 13 thru_hole circle (at -12.3444 2.8448 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole circle (at -15.0876 2.8448 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 3 /KBD_RDATA))
    (pad 15 thru_hole circle (at -17.8308 2.8448 90) (size 1.6 1.6) (drill 1.0414) (layers *.Cu *.Mask)
      (net 4 /KBD_XDATA))
    (pad "" thru_hole circle (at -26.2636 1.4224 90) (size 4 4) (drill 3.175) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 7.0612 1.4224 90) (size 4 4) (drill 3.175) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset9.90mm_Housed_MountingHolesOffset11.32mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 57.15 (width 0.15) (layer Dwgs.User)
    (gr_text "2.2500 in" (at 92.075 116.2096) (layer Dwgs.User))
    (feature1 (pts (xy 120.65 110.49) (xy 120.65 115.496021)))
    (feature2 (pts (xy 63.5 110.49) (xy 63.5 115.496021)))
    (crossbar (pts (xy 63.5 114.9096) (xy 120.65 114.9096)))
    (arrow1a (pts (xy 120.65 114.9096) (xy 119.523496 115.496021)))
    (arrow1b (pts (xy 120.65 114.9096) (xy 119.523496 114.323179)))
    (arrow2a (pts (xy 63.5 114.9096) (xy 64.626504 115.496021)))
    (arrow2b (pts (xy 63.5 114.9096) (xy 64.626504 114.323179)))
  )
  (gr_text KBD_XDATA (at 96.1136 98.425) (layer F.SilkS))
  (gr_text KBD_RDATA (at 96.137409 93.6244) (layer F.SilkS))
  (gr_text MONORET (at 85.915667 78.9178 180) (layer B.SilkS))
  (gr_text MONO (at 87.249 77.089 180) (layer B.SilkS))
  (gr_text GREENRET (at 98.5266 81.3816 180) (layer B.SilkS))
  (gr_text GREEN (at 97.193267 83.2104 180) (layer B.SilkS))
  (gr_text REDRET (at 81.115066 80.5434) (layer F.SilkS))
  (gr_text RED (at 82.4484 78.74) (layer F.SilkS))
  (gr_text BLUERET (at 83.7946 88.1888) (layer F.SilkS))
  (gr_text BLUE (at 85.127933 90.0684) (layer F.SilkS))
  (gr_text SN (at 91.7829 103.0605 180) (layer B.SilkS))
  (dimension 46.99 (width 0.15) (layer Dwgs.User)
    (gr_text "1.85 in" (at 135.0564 86.995 90) (layer Dwgs.User))
    (feature1 (pts (xy 120.65 63.5) (xy 134.342821 63.5)))
    (feature2 (pts (xy 120.65 110.49) (xy 134.342821 110.49)))
    (crossbar (pts (xy 133.7564 110.49) (xy 133.7564 63.5)))
    (arrow1a (pts (xy 133.7564 63.5) (xy 134.342821 64.626504)))
    (arrow1b (pts (xy 133.7564 63.5) (xy 133.169979 64.626504)))
    (arrow2a (pts (xy 133.7564 110.49) (xy 134.342821 109.363496)))
    (arrow2b (pts (xy 133.7564 110.49) (xy 133.169979 109.363496)))
  )
  (gr_text "DEC VR201/VR241 Breakout\n© 2021 Bjoren Davis\nvr2x1breakout\nrev B 2021apr25" (at 88.3285 97.663 180) (layer B.SilkS))
  (gr_line (start 120.65 63.5) (end 63.5 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 120.65 110.49) (end 120.65 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.5 110.49) (end 120.65 110.49) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.5 63.5) (end 63.5 110.49) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.396 110.236) (xy 63.754 110.236) (xy 63.754 63.754) (xy 120.396 63.754)
      )
    )
  )
  (zone (net 2) (net_name +12V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.396 110.236) (xy 63.754 110.236) (xy 63.754 63.754) (xy 120.396 63.754)
      )
    )
  )
)
