(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 82)
    (no_connects 0)
    (area 124.924999 97.924999 173.075001 114.075001)
    (thickness 1.6)
    (drawings 28)
    (tracks 20)
    (zones 0)
    (modules 59)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.0668)
    (trace_clearance 0.2032)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.64 0.64)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 /RF_IN)
  (net 3 /RF_OUT)
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C4-Pad2)")
  (net 7 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 1.0668)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /RF_IN)
    (add_net /RF_OUT)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad2)")
  )
  (module SAWTest:BNC_Molex_73138-5033 (layer B.Cu) (tedit 583E65DF)
    (at 166 106 180)
    (fp_text reference P2 (at -9 0 450) (layer B.SilkS) hide)
    (fp_text value "RF OUT" (at 0 0 270) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 5.08 180) (size 2 2) (drill 2) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at 0 -5.08 180) (size 2 2) (drill 2) (layers *.Cu *.Mask B.SilkS))
    (pad 1 thru_hole circle (at 5.08 0 180) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 3 /RF_OUT))
    (pad 2 thru_hole oval (at 5.08 -2.54 180) (size 2.54 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 GND) (thermal_gap 0.35))
  )
  (module SAWTest:BNC_Molex_73138-5033 (layer B.Cu) (tedit 583E65C4)
    (at 132 106)
    (fp_text reference P1 (at -9 0 270) (layer B.SilkS) hide)
    (fp_text value "RF IN" (at 0 0 90) (layer B.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 5.08) (size 2 2) (drill 2) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at 0 -5.08) (size 2 2) (drill 2) (layers *.Cu *.Mask B.SilkS))
    (pad 1 thru_hole circle (at 5.08 0) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 /RF_IN))
    (pad 2 thru_hole oval (at 5.08 -2.54) (size 2.54 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 GND) (thermal_gap 0.35))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D78)
    (at 165 113)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5C76)
    (at 145 99)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5C72)
    (at 141 99)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D94)
    (at 141 113)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D78)
    (at 157 113)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5C89)
    (at 157 99)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D10)
    (at 151.5 108.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5C7E)
    (at 149 99)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D85)
    (at 149 113)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D89)
    (at 145 113)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D7C)
    (at 153 113)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5C91)
    (at 133 113)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5C84)
    (at 153 99)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CAC)
    (at 159 104.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D99)
    (at 137 113)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D9D)
    (at 144.5 108.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D72)
    (at 155 107.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CC8)
    (at 133 99)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CFE)
    (at 140 110)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CDA)
    (at 140 104.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D1C)
    (at 151.5 110.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CC1)
    (at 137 99)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CA7)
    (at 151.5 103.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D21)
    (at 158 102)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CEB)
    (at 146.5 101.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CF0)
    (at 151.5 101.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CA1)
    (at 161 99)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D38)
    (at 149 110.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D2B)
    (at 163 106)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CFA)
    (at 139 107.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D26)
    (at 155 102)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D34)
    (at 158 107.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5DA1)
    (at 135 106)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D3D)
    (at 144.5 103.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CE6)
    (at 143 104.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5C97)
    (at 165 99)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5C9D)
    (at 161 113)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D03)
    (at 143 110)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D44)
    (at 146.5 110.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CB2)
    (at 149 101.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CF4)
    (at 153.5 103.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D07)
    (at 146.5 108.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D0C)
    (at 149 106)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5D16)
    (at 153.5 108.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (module COMDEV_SAW_5x7 (layer B.Cu) (tedit 583E60A3)
    (at 149 106)
    (fp_text reference F2 (at 0 5) (layer B.SilkS))
    (fp_text value COMDEV-SAW (at 0 4.25) (layer B.Fab))
    (fp_text user COMDEV (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.27 -2.5) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0 -2.5) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 3 smd rect (at 1.27 -2.5) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 4 smd rect (at 3.5 -1.27) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 5 smd rect (at 3.5 1.27) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 6 smd rect (at 1.27 2.5) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 7 smd rect (at 0 2.5) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 8 smd rect (at -1.27 2.5) (size 0.8 2) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 9 smd rect (at -3.5 1.27) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 10 smd rect (at -3.5 -1.27) (size 2 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 583E51B9)
    (at 141.5 106 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 2 180) (layer F.SilkS))
    (fp_text value C (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /RF_IN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 583E61EA)
    (at 156.5 106 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -2 180) (layer F.SilkS))
    (fp_text value C (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /RF_OUT))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 583E5133)
    (at 141.5 106 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.9 180) (layer B.SilkS))
    (fp_text value C (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 /RF_IN))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 583E61F1)
    (at 156.5 106 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -2 180) (layer B.SilkS))
    (fp_text value C (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 /RF_OUT))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SAWTest:TAI-SAW-7x5 (layer F.Cu) (tedit 583E5BDB)
    (at 149 106 270)
    (fp_text reference F1 (at 5 0 360) (layer F.SilkS))
    (fp_text value TAI-SAW (at 0 0 270) (layer F.Fab))
    (fp_text user TA-SAW (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.27 -2.2 270) (size 0.8 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 2 smd rect (at 0 -2.2 270) (size 0.8 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 3 smd rect (at 1.27 -2.2 270) (size 0.8 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 4 smd rect (at 3.2 -1.27 270) (size 1.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 5 smd rect (at 3.2 1.27 270) (size 1.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 6 smd rect (at 1.27 2.2 270) (size 0.8 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 7 smd rect (at 0 2.2 270) (size 0.8 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 8 smd rect (at -1.27 2.2 270) (size 0.8 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 9 smd rect (at -3.2 1.27 270) (size 1.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 10 smd rect (at -3.2 -1.27 270) (size 1.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 583E61E8)
    (at 156.5 104)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L2 (at 0 -2) (layer F.SilkS))
    (fp_text value INDUCTOR (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 583E50EB)
    (at 141.5 108 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L3 (at 0 -2 180) (layer B.SilkS))
    (fp_text value INDUCTOR (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 583E61EE)
    (at 156.5 104)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L4 (at 0 -2) (layer B.SilkS))
    (fp_text value INDUCTOR (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SAWTest:BNC_Molex_73138-5033 (layer F.Cu) (tedit 583E65CE)
    (at 132 106)
    (fp_text reference P1 (at -9 0 90) (layer F.SilkS) hide)
    (fp_text value "RF IN" (at 0 0 90) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 -5.08) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 5.08) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at 5.08 0) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 /RF_IN))
    (pad 2 thru_hole oval (at 5.08 2.54) (size 2.54 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 GND) (thermal_gap 0.35))
  )
  (module SAWTest:BNC_Molex_73138-5033 (layer F.Cu) (tedit 583E65E6)
    (at 166 106 180)
    (fp_text reference P2 (at -9 0 270) (layer F.SilkS) hide)
    (fp_text value "RF OUT" (at 0 0 270) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 -5.08 180) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 5.08 180) (size 2 2) (drill 2) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at 5.08 0 180) (size 1.778 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 3 /RF_OUT))
    (pad 2 thru_hole oval (at 5.08 2.54 180) (size 2.54 1.778) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 GND) (thermal_gap 0.35))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 141.5 108 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L1 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value INDUCTOR (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SAWTest:via_small (layer F.Cu) (tedit 583E5CBB)
    (at 146.5 103.5)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.64 0.64) (drill 0.3) (layers *.Cu)
      (net 7 GND) (zone_connect 2))
  )
  (gr_text "SAW Filter Tester" (at 149 100.25) (layer B.SilkS))
  (gr_text "SAW Filter Tester" (at 149 100.25) (layer F.SilkS))
  (gr_text OUT (at 167 106) (layer F.SilkS))
  (gr_text IN (at 128.5 106) (layer F.SilkS))
  (gr_text COMDEV (at 149 106 180) (layer B.SilkS))
  (gr_text TA-SAW (at 149 106 270) (layer F.SilkS))
  (gr_text OUT (at 166.5 106) (layer B.SilkS))
  (gr_text IN (at 128.5 106) (layer B.SilkS))
  (gr_arc (start 171 112) (end 173 112) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127 112) (end 127 114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127 100) (end 125 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 171 100) (end 171 98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125 112) (end 125 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171 114) (end 127 114) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171 98) (end 127 98) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 100) (end 173 112) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.35) (thermal_bridge_width 0.35))
    (polygon
      (pts
        (xy 125.5 99.5) (xy 126.5 98.5) (xy 171.5 98.5) (xy 172.5 99.5) (xy 172.5 112.5)
        (xy 171.5 113.5) (xy 126.5 113.5) (xy 125.5 112.5)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.35) (thermal_bridge_width 0.35))
    (polygon
      (pts
        (xy 172.5 99.5) (xy 172.5 112.5) (xy 171.5 113.5) (xy 126.5 113.5) (xy 125.5 112.5)
        (xy 125.5 99.5) (xy 126.5 98.5) (xy 171.5 98.5) (xy 172.5 99.5)
      )
    )
  )
)
