<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="60.96" x2="0" y2="2.54" width="0.254" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0.254" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="30.48" y2="0" width="0.254" layer="20"/>
<wire x1="33.02" y1="2.54" x2="33.02" y2="60.96" width="0.254" layer="20"/>
<wire x1="30.48" y1="63.5" x2="2.54" y2="63.5" width="0.254" layer="20"/>
<wire x1="30.48" y1="0" x2="33.02" y2="2.54" width="0.254" layer="20" curve="90"/>
<wire x1="33.02" y1="60.96" x2="30.48" y2="63.5" width="0.254" layer="20" curve="90"/>
<wire x1="2.54" y1="63.5" x2="0" y2="60.96" width="0.254" layer="20" curve="90"/>
<text>KD0GLS 2017</text>
<text>26CV12 36/4E</text>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="SOCKET_PLCC28">
</package>
<package name="CONN_BREAKAWAY_1X14_100_SMT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="kd0gls" package="SOCKET_PLCC28" value="SOCKET_PLCC28"/>
<element name="U$3" library="kd0gls" package="CONN_BREAKAWAY_1X14_100_SMT" value="CONN_BREAKAWAY_1X14_100_SMT"/>
<element name="U$4" library="kd0gls" package="CONN_BREAKAWAY_1X14_100_SMT" value="CONN_BREAKAWAY_1X14_100_SMT"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$2" pad="1"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="3"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="4"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="U$2" pad="5"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="U$3" pad="6"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="7"/>
<contactref element="U$3" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="U$3" pad="8"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="N$10">
<contactref element="U$2" pad="9"/>
<contactref element="U$3" pad="9"/>
</signal>
<signal name="N$11">
<contactref element="U$3" pad="10"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="N$12">
<contactref element="U$2" pad="11"/>
<contactref element="U$3" pad="11"/>
</signal>
<signal name="N$13">
<contactref element="U$3" pad="14"/>
<contactref element="U$2" pad="14"/>
</signal>
<signal name="N$14">
<contactref element="U$3" pad="13"/>
<contactref element="U$2" pad="13"/>
</signal>
<signal name="N$15">
<contactref element="U$3" pad="12"/>
<contactref element="U$2" pad="12"/>
</signal>
<signal name="N$16">
<contactref element="U$2" pad="28"/>
<contactref element="U$4" pad="14"/>
</signal>
<signal name="N$17">
<contactref element="U$2" pad="27"/>
<contactref element="U$4" pad="13"/>
</signal>
<signal name="N$18">
<contactref element="U$2" pad="26"/>
<contactref element="U$4" pad="12"/>
</signal>
<signal name="N$19">
<contactref element="U$2" pad="15"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="U$2" pad="16"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="U$2" pad="17"/>
<contactref element="U$4" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="U$2" pad="18"/>
<contactref element="U$4" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="U$2" pad="19"/>
<contactref element="U$4" pad="5"/>
</signal>
<signal name="N$24">
<contactref element="U$4" pad="6"/>
<contactref element="U$2" pad="20"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="21"/>
<contactref element="U$4" pad="7"/>
</signal>
<signal name="N$26">
<contactref element="U$4" pad="8"/>
<contactref element="U$2" pad="22"/>
</signal>
<signal name="N$27">
<contactref element="U$2" pad="23"/>
<contactref element="U$4" pad="9"/>
</signal>
<signal name="N$28">
<contactref element="U$2" pad="24"/>
<contactref element="U$4" pad="10"/>
</signal>
<signal name="N$29">
<contactref element="U$2" pad="25"/>
<contactref element="U$4" pad="11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
