(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 532)
    (zones 0)
    (modules 103)
    (nets 65)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.635)
    (user_trace_width 2.032)
    (user_trace_width 6.35)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.635)
    (via_min_drill 0.3048)
    (user_via 0.635 0.3048)
    (user_via 0.889 0.508)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 7.000001 1.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 14.986 189.23)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad2)")
  (net 2 "Net-(BT1-Pad1)")
  (net 3 "Net-(BT2-Pad2)")
  (net 4 "Net-(BT2-Pad1)")
  (net 5 "Net-(BT3-Pad2)")
  (net 6 "Net-(BT3-Pad1)")
  (net 7 "Net-(BT6-Pad2)")
  (net 8 "Net-(C1-Pad2)")
  (net 9 "Net-(C1-Pad1)")
  (net 10 "Net-(C2-Pad2)")
  (net 11 "Net-(C2-Pad1)")
  (net 12 GND)
  (net 13 "Net-(C3-Pad1)")
  (net 14 "Net-(C4-Pad1)")
  (net 15 "Net-(C7-Pad1)")
  (net 16 "Net-(C11-Pad1)")
  (net 17 "Net-(C10-Pad2)")
  (net 18 "Net-(C12-Pad2)")
  (net 19 "Net-(C13-Pad1)")
  (net 20 "Net-(C14-Pad2)")
  (net 21 "Net-(C15-Pad1)")
  (net 22 "Net-(C17-Pad1)")
  (net 23 "Net-(C19-Pad1)")
  (net 24 "Net-(D1-Pad2)")
  (net 25 "Net-(D2-Pad2)")
  (net 26 GNDREF)
  (net 27 "Net-(D3-Pad1)")
  (net 28 "Net-(F1-Pad1)")
  (net 29 "Net-(P1-Pad3)")
  (net 30 "Net-(P1-Pad2)")
  (net 31 "Net-(Q1-Pad4)")
  (net 32 "Net-(Q2-Pad5)")
  (net 33 "Net-(Q2-Pad4)")
  (net 34 "Net-(Q3-Pad5)")
  (net 35 "Net-(Q3-Pad4)")
  (net 36 "Net-(Q5-Pad3)")
  (net 37 "Net-(Q6-Pad1)")
  (net 38 "Net-(Q7-Pad1)")
  (net 39 "Net-(R12-Pad1)")
  (net 40 "Net-(R20-Pad1)")
  (net 41 "Net-(TP3-Pad1)")
  (net 42 "Net-(TP4-Pad1)")
  (net 43 "Net-(TP5-Pad1)")
  (net 44 "Net-(TP6-Pad1)")
  (net 45 "Net-(TP7-Pad1)")
  (net 46 "Net-(TP8-Pad1)")
  (net 47 "Net-(TP9-Pad1)")
  (net 48 "Net-(TP10-Pad1)")
  (net 49 "Net-(P1-Pad4)")
  (net 50 "Net-(C20-Pad1)")
  (net 51 "Net-(C21-Pad1)")
  (net 52 "Net-(C22-Pad1)")
  (net 53 "Net-(C23-Pad1)")
  (net 54 "Net-(Q10-Pad4)")
  (net 55 "Net-(Q10-Pad1)")
  (net 56 "Net-(Q11-Pad4)")
  (net 57 "Net-(Q11-Pad1)")
  (net 58 "Net-(R24-Pad1)")
  (net 59 "Net-(R26-Pad1)")
  (net 60 "Net-(Q12-Pad1)")
  (net 61 "Net-(Q12-Pad2)")
  (net 62 "Net-(Q12-Pad3)")
  (net 63 "Net-(TP14-Pad1)")
  (net 64 "Net-(TP15-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net GNDREF)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(BT1-Pad2)")
    (add_net "Net-(BT2-Pad1)")
    (add_net "Net-(BT2-Pad2)")
    (add_net "Net-(BT3-Pad1)")
    (add_net "Net-(BT3-Pad2)")
    (add_net "Net-(BT6-Pad2)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(Q1-Pad4)")
    (add_net "Net-(Q10-Pad1)")
    (add_net "Net-(Q10-Pad4)")
    (add_net "Net-(Q11-Pad1)")
    (add_net "Net-(Q11-Pad4)")
    (add_net "Net-(Q12-Pad1)")
    (add_net "Net-(Q12-Pad2)")
    (add_net "Net-(Q12-Pad3)")
    (add_net "Net-(Q2-Pad4)")
    (add_net "Net-(Q2-Pad5)")
    (add_net "Net-(Q3-Pad4)")
    (add_net "Net-(Q3-Pad5)")
    (add_net "Net-(Q5-Pad3)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(Q7-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R24-Pad1)")
    (add_net "Net-(R26-Pad1)")
    (add_net "Net-(TP10-Pad1)")
    (add_net "Net-(TP14-Pad1)")
    (add_net "Net-(TP15-Pad1)")
    (add_net "Net-(TP3-Pad1)")
    (add_net "Net-(TP4-Pad1)")
    (add_net "Net-(TP5-Pad1)")
    (add_net "Net-(TP6-Pad1)")
    (add_net "Net-(TP7-Pad1)")
    (add_net "Net-(TP8-Pad1)")
    (add_net "Net-(TP9-Pad1)")
  )
  (module t_passive_smd:res2512W (layer F.Cu) (tedit 5FCE8654)
    (at 32.742 84.455 90)
    (fp_text reference R8 (at 0.2 0.1 90) (layer F.SilkS))
    (fp_text value 100 (at 0 -0.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 1.5 90) (size 7.000001 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd rect (at 0 -1.5 90) (size 7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(BT6-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/R2512W.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 38.1 91.836661 180)
    (fp_text reference TP15 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(TP15-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 40.64 91.836661 180)
    (fp_text reference TP14 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(TP14-Pad1)"))
  )
  (module t_MtgHoles:MTG_200_125D (layer F.Cu) (tedit 589FD404)
    (at 120.65 102.489)
    (fp_text reference H6 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 3.175) (layers *.Cu *.Mask)
      (net 12 GND))
  )
  (module t_MtgHoles:MTG_200_125D (layer F.Cu) (tedit 589FD404)
    (at 18.669 102.489)
    (fp_text reference H5 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 3.175) (layers *.Cu *.Mask)
      (net 12 GND))
  )
  (module t_MtgHoles:MTG_200_125D (layer F.Cu) (tedit 589FD404)
    (at 18.796 19.558)
    (fp_text reference H4 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 3.175) (layers *.Cu *.Mask)
      (net 12 GND))
  )
  (module t_MtgHoles:MTG_200_125D (layer F.Cu) (tedit 589FD404)
    (at 18.796 185.42)
    (fp_text reference H3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 3.175) (layers *.Cu *.Mask)
      (net 12 GND))
  )
  (module t_MtgHoles:MTG_200_125D (layer F.Cu) (tedit 589FD404)
    (at 120.65 185.42)
    (fp_text reference H2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 3.175) (layers *.Cu *.Mask)
      (net 12 GND))
  )
  (module t_MtgHoles:MTG_200_125D (layer F.Cu) (tedit 589FD404)
    (at 120.65 19.558)
    (fp_text reference H1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.08 5.08) (drill 3.175) (layers *.Cu *.Mask)
      (net 12 GND))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 22.146 147.314)
    (fp_text reference TP13 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(C23-Pad1)"))
  )
  (module bq40z80:BQ40Z80RSMR (layer F.Cu) (tedit 5FC92FE7)
    (at 29.718 102.362 180)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value BQ40Z80RSMR (at 0 0) (layer F.SilkS))
    (fp_text user Designator9 (at -3.302 -3.9878) (layer F.SilkS))
    (fp_text user .Designator (at 0.049985 -0.216596) (layer Dwgs.User))
    (fp_text user .Designator (at 0.049985 -0.216596) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 32 smd custom (at -1.397 -2.09042 270) (size 0.18 0.18) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C4-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 25 smd custom (at 1.40462 -2.05486 270) (size 0.18 0.18) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C19-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 24 smd custom (at 2.15646 -1.397 270) (size 0.18 0.18) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 17 smd custom (at 2.09296 1.40462 270) (size 0.18 0.18) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(TP7-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 16 smd custom (at 1.397 2.07772 270) (size 0.18 0.18) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(TP4-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 9 smd custom (at -1.40716 2.12598 270) (size 0.18 0.18) (layers F.Cu F.Paste F.Mask)
      (net 12 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 8 smd custom (at -2.13614 1.40208 270) (size 0.18 0.18) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C7-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 1 smd custom (at -2.02692 -1.397 270) (size 0.18 0.18) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C1-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 33 smd rect (at 0 0 180) (size 1.45 1.45) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 31 smd rect (at -1.000001 -1.951246 180) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C14-Pad2)"))
    (pad 30 smd rect (at -0.599999 -1.951246 180) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (pad 29 smd rect (at -0.2 -1.951246 180) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(Q1-Pad4)"))
    (pad 28 smd rect (at 0.2 -1.951246 180) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(Q2-Pad4)"))
    (pad 27 smd rect (at 0.599999 -1.951246 180) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 26 smd rect (at 1.000001 -1.951246 180) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R20-Pad1)"))
    (pad 23 smd rect (at 1.951246 -1.000001 270) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R12-Pad1)"))
    (pad 22 smd rect (at 1.951246 -0.599999 270) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(TP10-Pad1)"))
    (pad 21 smd rect (at 1.951246 -0.2 270) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(TP5-Pad1)"))
    (pad 20 smd rect (at 1.951246 0.2 270) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(TP9-Pad1)"))
    (pad 19 smd rect (at 1.951246 0.599999 270) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P1-Pad2)"))
    (pad 18 smd rect (at 1.951246 1.000001 270) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(P1-Pad3)"))
    (pad 15 smd rect (at 1.000001 1.951246 180) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(TP3-Pad1)"))
    (pad 14 smd rect (at 0.599999 1.951246 180) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 13 smd rect (at 0.2 1.951246 180) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(TP8-Pad1)"))
    (pad 12 smd rect (at -0.2 1.951246 180) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(TP6-Pad1)"))
    (pad 11 smd rect (at -0.599999 1.951246 180) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(TP15-Pad1)"))
    (pad 10 smd rect (at -1.000001 1.951246 180) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(TP14-Pad1)"))
    (pad 7 smd rect (at -1.951246 1.000001 270) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 6 smd rect (at -1.951246 0.599999 270) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (pad 5 smd rect (at -1.951246 0.2 270) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at -1.951246 -0.2 270) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad2)"))
    (pad 3 smd rect (at -1.951246 -0.599999 270) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at -1.951246 -1.000001 270) (size 0.192474 1.009637) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C1-Pad2)"))
    (model ${T_LIBS}/3d/t_qfn/BQ40Z80RSMT.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 19.939 67.31)
    (fp_text reference TP12 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P1-Pad4)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 21.844 159.766 270)
    (fp_text reference TP11 (at -2.032 0.127 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(C21-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 21.844 153.162 270)
    (fp_text reference TP2 (at -2.032 0.127 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(C20-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 25.654 124.968 270)
    (fp_text reference TP1 (at -2.032 0.127 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(Q6-Pad1)"))
  )
  (module t_smd_transistors:sc70 (layer F.Cu) (tedit 5B9F0B6A)
    (at 29.972 167.64)
    (descr SC70)
    (fp_text reference Q13 (at 0 -0.3302) (layer F.SilkS))
    (fp_text value BSS-123 (at 0 0.3302) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.6604 1.016) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q10-Pad4)"))
    (pad 2 smd rect (at 0.6604 1.016) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 3 smd rect (at 0 -1.016) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(Q12-Pad2)"))
    (model ${T_LIBS}/3d/t_smd_transistors/SC-70.stp
      (offset (xyz -0.635 -1.143 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_smd_transistors:sc70 (layer F.Cu) (tedit 5B9F0B6A)
    (at 26.416 167.64)
    (descr SC70)
    (fp_text reference Q12 (at 0 -0.3302) (layer F.SilkS))
    (fp_text value BSS-123 (at 0 0.3302) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.6604 1.016) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(Q12-Pad1)"))
    (pad 2 smd rect (at 0.6604 1.016) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(Q12-Pad2)"))
    (pad 3 smd rect (at 0 -1.016) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(Q12-Pad3)"))
    (model ${T_LIBS}/3d/t_smd_transistors/SC-70.stp
      (offset (xyz -0.635 -1.143 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module tps3700:TPS3700QDDCRQ1 (layer F.Cu) (tedit 0)
    (at 29.718 171.958)
    (fp_text reference U2 (at 0 0) (layer F.SilkS))
    (fp_text value TPS3700QDDCRQ1 (at 0 0) (layer F.SilkS))
    (fp_text user Designator9 (at -1.8288 -2.6162) (layer F.SilkS))
    (fp_text user .Designator (at -0.275001 -0.700001 270) (layer Dwgs.User))
    (fp_text user .Designator (at -0.275001 -0.700001 270) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 6 smd rect (at 1.1684 -0.950001) (size 1.5748 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q10-Pad4)"))
    (pad 5 smd rect (at 1.1684 0) (size 1.5748 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C22-Pad1)"))
    (pad 4 smd rect (at 1.1684 0.950001) (size 1.5748 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R24-Pad1)"))
    (pad 3 smd rect (at -1.1684 0.950001) (size 1.5748 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R26-Pad1)"))
    (pad 2 smd rect (at -1.1684 0) (size 1.5748 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at -1.1684 -0.950001) (size 1.5748 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(Q12-Pad1)"))
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 31.75 163.788 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R31 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(Q12-Pad3)"))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(Q11-Pad4)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 23.368 169.672 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R30 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(Q12-Pad1)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C22-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 34.798 163.83 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R29 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(Q11-Pad4)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C22-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 40.132 157.48 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R28 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q10-Pad4)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C22-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 25.4 174.752 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R27 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R26-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 25.4 172.17 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R26 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(R26-Pad1)"))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C21-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 37.084 174.498 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R25 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R24-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 37.084 171.916 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R24 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(R24-Pad1)"))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C20-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_smd_transistors:PQFN_3x3 (layer F.Cu) (tedit 5BB76E5A)
    (at 35.466 160.004 270)
    (fp_text reference Q11 (at 2.73304 -2.42824 90) (layer F.SilkS))
    (fp_text value P_MOS_8 (at 0.2 0.1 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0 90) (layer F.Fab))
    (pad 9 smd rect (at 0.6 -0.5 270) (size 1 1) (layers F.Paste))
    (pad 9 smd rect (at -0.6 -0.5 270) (size 1 1) (layers F.Paste))
    (pad 8 smd rect (at 0 -0.8 270) (size 2.25 1.7) (layers F.Mask)
      (net 53 "Net-(C23-Pad1)"))
    (pad 8 smd rect (at -1 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C23-Pad1)"))
    (pad 7 smd rect (at -0.333 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C23-Pad1)"))
    (pad 6 smd rect (at 0.333 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C23-Pad1)"))
    (pad 5 smd rect (at 1 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C23-Pad1)"))
    (pad 4 smd rect (at 1 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(Q11-Pad4)"))
    (pad 3 smd rect (at 0.333 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(Q11-Pad1)"))
    (pad 2 smd rect (at -0.333 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(Q11-Pad1)"))
    (pad 1 smd rect (at -1 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(Q11-Pad1)"))
    (model ${T_LIBS}/3d/t_smd_transistors/TDFN-8-EP_3x3mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module t_smd_transistors:PQFN_3x3 (layer F.Cu) (tedit 5BB76E5A)
    (at 35.56 154.94 270)
    (fp_text reference Q10 (at 2.73304 -2.42824 90) (layer F.SilkS))
    (fp_text value P_MOS_8 (at 0.2 0.1 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0 90) (layer F.Fab))
    (pad 9 smd rect (at 0.6 -0.5 270) (size 1 1) (layers F.Paste))
    (pad 9 smd rect (at -0.6 -0.5 270) (size 1 1) (layers F.Paste))
    (pad 8 smd rect (at 0 -0.8 270) (size 2.25 1.7) (layers F.Mask)
      (net 53 "Net-(C23-Pad1)"))
    (pad 8 smd rect (at -1 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C23-Pad1)"))
    (pad 7 smd rect (at -0.333 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C23-Pad1)"))
    (pad 6 smd rect (at 0.333 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C23-Pad1)"))
    (pad 5 smd rect (at 1 -1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C23-Pad1)"))
    (pad 4 smd rect (at 1 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q10-Pad4)"))
    (pad 3 smd rect (at 0.333 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q10-Pad1)"))
    (pad 2 smd rect (at -0.333 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q10-Pad1)"))
    (pad 1 smd rect (at -1 1.43 270) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q10-Pad1)"))
    (model ${T_LIBS}/3d/t_smd_transistors/TDFN-8-EP_3x3mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module t_smd_transistors:PQFN_3x3 (layer F.Cu) (tedit 5BB76E5A)
    (at 29.972 160.02 90)
    (fp_text reference Q9 (at 2.73304 -2.42824 90) (layer F.SilkS))
    (fp_text value P_MOS_8 (at 0.2 0.1 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0 90) (layer F.Fab))
    (pad 9 smd rect (at 0.6 -0.5 90) (size 1 1) (layers F.Paste))
    (pad 9 smd rect (at -0.6 -0.5 90) (size 1 1) (layers F.Paste))
    (pad 8 smd rect (at 0 -0.8 90) (size 2.25 1.7) (layers F.Mask)
      (net 51 "Net-(C21-Pad1)"))
    (pad 8 smd rect (at -1 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C21-Pad1)"))
    (pad 7 smd rect (at -0.333 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C21-Pad1)"))
    (pad 6 smd rect (at 0.333 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C21-Pad1)"))
    (pad 5 smd rect (at 1 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C21-Pad1)"))
    (pad 4 smd rect (at 1 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(Q11-Pad4)"))
    (pad 3 smd rect (at 0.333 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(Q11-Pad1)"))
    (pad 2 smd rect (at -0.333 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(Q11-Pad1)"))
    (pad 1 smd rect (at -1 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(Q11-Pad1)"))
    (model ${T_LIBS}/3d/t_smd_transistors/TDFN-8-EP_3x3mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module t_smd_transistors:PQFN_3x3 (layer F.Cu) (tedit 5BB76E5A)
    (at 29.964 154.848 90)
    (fp_text reference Q8 (at 2.73304 -2.42824 90) (layer F.SilkS))
    (fp_text value P_MOS_8 (at 0.2 0.1 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0 90) (layer F.Fab))
    (pad 9 smd rect (at 0.6 -0.5 90) (size 1 1) (layers F.Paste))
    (pad 9 smd rect (at -0.6 -0.5 90) (size 1 1) (layers F.Paste))
    (pad 8 smd rect (at 0 -0.8 90) (size 2.25 1.7) (layers F.Mask)
      (net 50 "Net-(C20-Pad1)"))
    (pad 8 smd rect (at -1 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C20-Pad1)"))
    (pad 7 smd rect (at -0.333 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C20-Pad1)"))
    (pad 6 smd rect (at 0.333 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C20-Pad1)"))
    (pad 5 smd rect (at 1 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C20-Pad1)"))
    (pad 4 smd rect (at 1 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q10-Pad4)"))
    (pad 3 smd rect (at 0.333 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q10-Pad1)"))
    (pad 2 smd rect (at -0.333 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q10-Pad1)"))
    (pad 1 smd rect (at -1 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q10-Pad1)"))
    (model ${T_LIBS}/3d/t_smd_transistors/TDFN-8-EP_3x3mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module BAS40W-05-7-F:BAS40W-05-7-F (layer F.Cu) (tedit 0)
    (at 33.274 167.386 180)
    (fp_text reference D4 (at 0 0) (layer F.SilkS))
    (fp_text value BAS40W-05-7-F (at 8.89 -46.99) (layer F.SilkS) hide)
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 3 smd rect (at 0 -0.9 180) (size 0.4508 1.1112) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C22-Pad1)"))
    (pad 2 smd rect (at 0.700001 0.900001 180) (size 0.4508 1.1112) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C21-Pad1)"))
    (pad 1 smd rect (at -0.700001 0.900001 180) (size 0.4508 1.1112) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C20-Pad1)"))
  )
  (module t_smd_caps:Tan_Cap_B (layer F.Cu) (tedit 5C1BC686)
    (at 32.258 145.8214 90)
    (descr "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (tags "Tantal Cap. , Size B, EIA-3528, Reflow,")
    (attr smd)
    (fp_text reference C23 (at 1.4986 -2.794 270) (layer F.SilkS))
    (fp_text value CP1 (at 0.2 0.2 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0.2 90) (layer F.Fab))
    (fp_text user + (at -1.4224 -2.921 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.5494 0 90) (size 1.95072 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C23-Pad1)"))
    (pad 2 smd rect (at 1.5494 0 90) (size 1.95072 2.49936) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model ${T_LIBS}/3d/t_smd_caps/CP_EIA-3528-21_Kemet-B.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 34.544 169.672 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C22 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C22-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 25.4 162.052)
    (descr "SMT capacitor, 0402")
    (fp_text reference C21 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C21-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 25.4 155.956)
    (descr "SMT capacitor, 0402")
    (fp_text reference C20 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C20-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 19.431 84.328)
    (fp_text reference TP9 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(TP9-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 25.4 84.582 90)
    (fp_text reference TP17 (at -2.032 0.127 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(BT6-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 19.431 89.408 180)
    (fp_text reference TP10 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(TP10-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 25.4 89.662 90)
    (fp_text reference TP8 (at -2.032 0.127 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(TP8-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 25.4 97.282 90)
    (fp_text reference TP7 (at -2.032 0.127 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -1.524 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(TP7-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 25.4 87.122 90)
    (fp_text reference TP6 (at -2.032 0.127 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(TP6-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 19.431 86.868 180)
    (fp_text reference TP5 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(TP5-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 25.4 94.742 90)
    (fp_text reference TP4 (at -2.032 0 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(TP4-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 25.4 92.202 90)
    (fp_text reference TP3 (at -2.032 0.127 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0.05 -1.375 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(TP3-Pad1)"))
  )
  (module t_connectors:Header4_254 (layer F.Cu) (tedit 5F63AD14)
    (at 19.939 79.756 90)
    (fp_text reference P1 (at 0.635 -4.064 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -0.5 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.62 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 49 "Net-(P1-Pad4)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 GND))
    (model ${T_LIBS}/3d/t_connectors/022112042.stp
      (offset (xyz 3.81 0 1.651))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 32.258 105.918)
    (descr "SMT capacitor, 0402")
    (fp_text reference C14 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C14-Pad2)"))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 34.544 100.33 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C3 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C3-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 38.1 98.806 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C6 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C3-Pad1)"))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_misc:Battery18650_H (layer F.Cu) (tedit 5F6F6FDB)
    (at 69.342 147.574 180)
    (fp_text reference BT1 (at 0 0.5) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 -0.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 9 4 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -9 -4 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 35 180) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)"))
    (pad 1 thru_hole circle (at 0 -35 180) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (model "${T_LIBS}/3d/t_misc/18650 Battery.stp"
      (offset (xyz 0 -32.5 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module t_misc:Battery18650_H (layer F.Cu) (tedit 5F6F6FDB)
    (at 69.342 58.674 180)
    (fp_text reference BT6 (at 0 0.5) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 -0.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 9 4 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -9 -4 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 35 180) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 7 "Net-(BT6-Pad2)"))
    (pad 1 thru_hole circle (at 0 -35 180) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 5 "Net-(BT3-Pad2)"))
    (model "${T_LIBS}/3d/t_misc/18650 Battery.stp"
      (offset (xyz 0 -32.5 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module t_misc:Battery18650_H (layer F.Cu) (tedit 5F6F6FDB)
    (at 90.2335 58.7375 180)
    (fp_text reference BT3 (at 0 0.5) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 -0.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 9 4 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -9 -4 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 35 180) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 5 "Net-(BT3-Pad2)"))
    (pad 1 thru_hole circle (at 0 -35 180) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 6 "Net-(BT3-Pad1)"))
    (model "${T_LIBS}/3d/t_misc/18650 Battery.stp"
      (offset (xyz 0 -32.5 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 29.718 132.546 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R23 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C19-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 44.069 140.928 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R22 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(Q7-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 53.848 135.594 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R21 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D2-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 50.292 132.588 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R20 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R20-Pad1)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D2-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 25.654 128.778 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R19 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.127 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(Q6-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 37.296 128.778 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R18 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 10M (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q3-Pad4)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 37.338 121.158)
    (descr "SMT capacitor, 0402")
    (fp_text reference R17 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 10M (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(Q2-Pad4)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5FC6C17D)
    (at 37.084 112.522 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R16 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D1-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 33.782 90.72 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R15 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 30.988 90.678 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R14 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(BT6-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5FC6AF0B)
    (at 40.386 115.824)
    (descr "SMT capacitor, 0402")
    (fp_text reference R13 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at -0.042 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(Q1-Pad4)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 27.39 107.442)
    (descr "SMT capacitor, 0402")
    (fp_text reference R12 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C13-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 26.162 113.538 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R11 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 1.0k (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q5-Pad3)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 22.352 107.95 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R10 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 20k (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 37.338 137.16 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R9 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(Q3-Pad5)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 44.704 125.18 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R7 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Q2-Pad5)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 40.894 96.774 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R6 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(BT3-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 40.852 99.314 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R5 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(BT3-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 40.852 101.854 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R4 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BT2-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 40.767 104.394 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R3 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(BT2-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 40.767 106.934 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R2 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BT1-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 40.894 109.474 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R1 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value 100 (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_smd_transistors:sc70 (layer F.Cu) (tedit 5B9F0B6A)
    (at 44.958 135.636)
    (descr SC70)
    (fp_text reference Q7 (at 0 -0.3302) (layer F.SilkS))
    (fp_text value BSS-123 (at 0 0.3302 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.6604 1.016) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(Q7-Pad1)"))
    (pad 2 smd rect (at 0.6604 1.016) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C12-Pad2)"))
    (pad 3 smd rect (at 0 -1.016) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D2-Pad2)"))
    (model ${T_LIBS}/3d/t_smd_transistors/SC-70.stp
      (offset (xyz -0.635 -1.143 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_smd_transistors:sc70 (layer F.Cu) (tedit 5B9F0B6A)
    (at 28.702 128.778 270)
    (descr SC70)
    (fp_text reference Q6 (at 0 -0.3302 90) (layer F.SilkS))
    (fp_text value BSS-123 (at 0 0.3302 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.6604 1.016 270) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at 0.6604 1.016 270) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 3 smd rect (at 0 -1.016 270) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q3-Pad4)"))
    (model ${T_LIBS}/3d/t_smd_transistors/SC-70.stp
      (offset (xyz -0.635 -1.143 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_smd_transistors:sc70 (layer F.Cu) (tedit 5B9F0B6A)
    (at 26.162 110.236 180)
    (descr SC70)
    (fp_text reference Q5 (at 0 -0.3302) (layer F.SilkS))
    (fp_text value BSS-123 (at 0 0.3302) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.6604 1.016 180) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.6604 1.016 180) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 3 smd rect (at 0 -1.016 180) (size 0.4572 0.7112) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q5-Pad3)"))
    (model ${T_LIBS}/3d/t_smd_transistors/SC-70.stp
      (offset (xyz -0.635 -1.143 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_smd_transistors:PQFN_3x3 (layer F.Cu) (tedit 5BB76E5A)
    (at 40.378 131.664 90)
    (fp_text reference Q4 (at 0 2.794 270) (layer F.SilkS))
    (fp_text value N_MOS_8 (at 0.2 0.1 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0 90) (layer F.Fab))
    (pad 9 smd rect (at 0.6 -0.5 90) (size 1 1) (layers F.Paste))
    (pad 9 smd rect (at -0.6 -0.5 90) (size 1 1) (layers F.Paste))
    (pad 8 smd rect (at 0 -0.8 90) (size 2.25 1.7) (layers F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 8 smd rect (at -1 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 7 smd rect (at -0.333 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 6 smd rect (at 0.333 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 5 smd rect (at 1 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 4 smd rect (at 1 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D2-Pad2)"))
    (pad 3 smd rect (at 0.333 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C12-Pad2)"))
    (pad 2 smd rect (at -0.333 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C12-Pad2)"))
    (pad 1 smd rect (at -1 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C12-Pad2)"))
    (model ${T_LIBS}/3d/t_smd_transistors/TDFN-8-EP_3x3mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module t_smd_transistors:PQFN_3x3 (layer F.Cu) (tedit 5BB76E5A)
    (at 34.29 131.572 90)
    (fp_text reference Q3 (at 0 -2.794 90) (layer F.SilkS))
    (fp_text value P_MOS_8 (at 0.2 0.1 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0 90) (layer F.Fab))
    (pad 9 smd rect (at 0.6 -0.5 90) (size 1 1) (layers F.Paste))
    (pad 9 smd rect (at -0.6 -0.5 90) (size 1 1) (layers F.Paste))
    (pad 8 smd rect (at 0 -0.8 90) (size 2.25 1.7) (layers F.Mask)
      (net 34 "Net-(Q3-Pad5)"))
    (pad 8 smd rect (at -1 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(Q3-Pad5)"))
    (pad 7 smd rect (at -0.333 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(Q3-Pad5)"))
    (pad 6 smd rect (at 0.333 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(Q3-Pad5)"))
    (pad 5 smd rect (at 1 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(Q3-Pad5)"))
    (pad 4 smd rect (at 1 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q3-Pad4)"))
    (pad 3 smd rect (at 0.333 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at -0.333 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 1 smd rect (at -1 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (model ${T_LIBS}/3d/t_smd_transistors/TDFN-8-EP_3x3mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module t_smd_transistors:PQFN_3x3 (layer F.Cu) (tedit 5BB76E5A)
    (at 34.384 126.254 90)
    (fp_text reference Q2 (at 2.73304 -2.42824 90) (layer F.SilkS))
    (fp_text value P_MOS_8 (at 0.2 0.1 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1 0 90) (layer F.Fab))
    (pad 9 smd rect (at 0.6 -0.5 90) (size 1 1) (layers F.Paste))
    (pad 9 smd rect (at -0.6 -0.5 90) (size 1 1) (layers F.Paste))
    (pad 8 smd rect (at 0 -0.8 90) (size 2.25 1.7) (layers F.Mask)
      (net 32 "Net-(Q2-Pad5)"))
    (pad 8 smd rect (at -1 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Q2-Pad5)"))
    (pad 7 smd rect (at -0.333 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Q2-Pad5)"))
    (pad 6 smd rect (at 0.333 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Q2-Pad5)"))
    (pad 5 smd rect (at 1 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Q2-Pad5)"))
    (pad 4 smd rect (at 1 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(Q2-Pad4)"))
    (pad 3 smd rect (at 0.333 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at -0.333 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 1 smd rect (at -1 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (model ${T_LIBS}/3d/t_smd_transistors/TDFN-8-EP_3x3mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module t_smd_transistors:PQFN_3x3 (layer F.Cu) (tedit 5BB76E5A)
    (at 40.378 126.146 90)
    (fp_text reference Q1 (at 2.73304 -2.42824 90) (layer F.SilkS))
    (fp_text value N_MOS_8 (at 0.2 0.1 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -0.254 90) (layer F.Fab))
    (pad 9 smd rect (at 0.6 -0.5 90) (size 1 1) (layers F.Paste))
    (pad 9 smd rect (at -0.6 -0.5 90) (size 1 1) (layers F.Paste))
    (pad 8 smd rect (at 0 -0.8 90) (size 2.25 1.7) (layers F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 8 smd rect (at -1 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 7 smd rect (at -0.333 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 6 smd rect (at 0.333 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 5 smd rect (at 1 -1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (pad 4 smd rect (at 1 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(Q1-Pad4)"))
    (pad 3 smd rect (at 0.333 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at -0.333 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at -1 1.43 90) (size 0.4 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (model ${T_LIBS}/3d/t_smd_transistors/TDFN-8-EP_3x3mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Fuse:Fuse_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 26.162 116.84 270)
    (descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags fuse)
    (attr smd)
    (fp_text reference F1 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value FUSE (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(F1-Pad1)"))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 44.069 144.145 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value BAV3004 (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 26 GNDREF))
    (pad 1 smd rect (at -1.05 0 270) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 50.292 135.636 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value Diode_TVS_SMA (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323 (layer F.Cu) (tedit 58641739)
    (at 39.844 112.522 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value Diode_TVS_SMA (at 0.1 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.05 0 180) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 27.686 131.572 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C19 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C19-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 32.258 107.696 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C18 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 32.258 109.728 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C17 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C17-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 23.114 104.394 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C16 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 25.146 104.394 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C15 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C15-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 24.384 107.908 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C13 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C13-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 45.466 130.81 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C12 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C12-Pad2)"))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C10-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 34.29 97.028 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C11 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 45.466 128.312 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C10 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 180) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 32.216 94.234 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C9 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C7-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 32.258 92.202 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C8 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 100pF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C11-Pad1)"))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C7-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 30.226 97.028)
    (descr "SMT capacitor, 0402")
    (fp_text reference C7 (at 0 -1.016) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C7-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 38.1 103.886 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C5 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at -0.085 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C1-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 38.1 108.966 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C4 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at -0.042 -0.381 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C4-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 38.1 101.346 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C2 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C2-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5FC65C73)
    (at 38.1 106.426 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C1 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_misc:Battery18650_H (layer F.Cu) (tedit 5F6F6FDB)
    (at 111.1885 58.7375 180)
    (fp_text reference BT5 (at 0 0.5) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 -0.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 9 4 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -9 -4 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 35 180) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 6 "Net-(BT3-Pad1)"))
    (pad 1 thru_hole circle (at 0 -35 180) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 3 "Net-(BT2-Pad2)"))
    (model "${T_LIBS}/3d/t_misc/18650 Battery.stp"
      (offset (xyz 0 -32.5 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module t_misc:Battery18650_H (layer F.Cu) (tedit 5F6F6FDB)
    (at 90.2335 147.6375 180)
    (fp_text reference BT4 (at 0 0.5) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 -0.5 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 9 4 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -9 -4 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 35 180) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 4 "Net-(BT2-Pad1)"))
    (pad 1 thru_hole circle (at 0 -35 180) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)"))
    (model "${T_LIBS}/3d/t_misc/18650 Battery.stp"
      (offset (xyz 0 -32.5 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module t_misc:Battery18650_H (layer F.Cu) (tedit 5F6F6FDB)
    (at 111.1885 147.6375 180)
    (fp_text reference BT2 (at 0 0.5) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 -0.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 9 4 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -9 -4 180) (size 4 4) (drill 4) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 35 180) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 3 "Net-(BT2-Pad2)"))
    (pad 1 thru_hole circle (at 0 -35 180) (size 3.5 3.5) (drill 2) (layers *.Cu *.Mask)
      (net 4 "Net-(BT2-Pad1)"))
    (model "${T_LIBS}/3d/t_misc/18650 Battery.stp"
      (offset (xyz 0 -32.5 9.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (gr_text "bq40z80 Pack Manager Test Board\n12/7/2020" (at 119.507 39.116 90) (layer B.SilkS))
  (gr_line (start 124.968 15.24) (end 124.968 189.738) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 14.478 15.24) (end 124.968 15.24) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 14.478 189.738) (end 14.478 15.24) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.968 189.738) (end 14.478 189.738) (layer Edge.Cuts) (width 0.1))
  (zone (net 12) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.46 189.23) (xy 14.986 189.23) (xy 14.986 189.103) (xy 14.986 15.748) (xy 124.46 15.748)
      )
    )
  )
  (zone (net 12) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.46 189.23) (xy 14.986 189.23) (xy 14.986 15.748) (xy 124.46 15.748)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33.274 88.265) (xy 34.29 88.773) (xy 34.544 91.821) (xy 33.401 93.599) (xy 30.988 93.472)
        (xy 30.353 91.694) (xy 30.226 88.265) (xy 32.258 87.9475) (xy 32.258 84.201) (xy 33.147 84.201)
      )
    )
  )
)
