(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 20)
    (zones 0)
    (modules 6)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad24)")
  (net 2 "Net-(A1-Pad23)")
  (net 3 "Net-(A1-Pad22)")
  (net 4 "Net-(A1-Pad21)")
  (net 5 "Net-(A1-Pad20)")
  (net 6 "Net-(A1-Pad19)")
  (net 7 "Net-(A1-Pad18)")
  (net 8 "Net-(A1-Pad17)")
  (net 9 "Net-(A1-Pad16)")
  (net 10 "Net-(A1-Pad15)")
  (net 11 "Net-(A1-Pad14)")
  (net 12 "Net-(A1-Pad13)")
  (net 13 "Net-(A1-Pad1)")
  (net 14 "Net-(A1-Pad2)")
  (net 15 "Net-(A1-Pad3)")
  (net 16 "Net-(A1-Pad4)")
  (net 17 "Net-(A1-Pad5)")
  (net 18 "Net-(A1-Pad6)")
  (net 19 "Net-(A1-Pad7)")
  (net 20 "Net-(A1-Pad8)")
  (net 21 "Net-(A1-Pad9)")
  (net 22 "Net-(A1-Pad10)")
  (net 23 "Net-(A1-Pad11)")
  (net 24 "Net-(A1-Pad12)")
  (net 25 "Net-(J1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad19)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad22)")
    (add_net "Net-(A1-Pad23)")
    (add_net "Net-(A1-Pad24)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad4)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A1-Pad7)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(J1-Pad2)")
  )
  (module Connectors:PINHEAD1-2 (layer F.Cu) (tedit 0)
    (at 69.85 77.47 270)
    (fp_text reference J2 (at 1.27 -3.9 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.27 3.81 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad4)"))
  )
  (module Converters_DCDC_ACDC:DCDC-Conv_TRACO_TSR-1 (layer F.Cu) (tedit 59FE1FB7)
    (at 77.47 78.74)
    (descr "DCDC-Converter, TRACO, TSR 1-xxxx")
    (tags "DCDC-Converter TRACO TSR-1")
    (fp_text reference U1 (at -1.5 -6.71) (layer F.SilkS))
    (fp_text value TSR_1-2450 (at 2.5 3.25) (layer F.Fab))
    (fp_text user %R (at 3 -3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad1)"))
    (model ${KISYS3DMOD}/Converters_DCDC_ACDC.3dshapes/DCDC-Conv_TRACO_TSR-1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINHEAD1-2 (layer F.Cu) (tedit 0)
    (at 97.79 72.39 90)
    (fp_text reference J3 (at 1.27 -3.9 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.27 3.81 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad2)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 99.06 80.01 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31) (layer F.SilkS))
    (fp_text value 1k (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINHEAD1-2 (layer F.Cu) (tedit 0)
    (at 69.85 72.39 90)
    (fp_text reference J1 (at 1.27 -3.9 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.27 3.81 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad2)"))
  )
  (module digikey-footprints:Particle_Photon (layer F.Cu) (tedit 59CD2E49)
    (at 71.12 83.82 270)
    (fp_text reference A1 (at 8.975 -35.15 90) (layer F.SilkS))
    (fp_text value PHOTONH (at 8.7 5.325 90) (layer F.Fab))
    (fp_text user %R (at 8.35 -13.475 90) (layer F.Fab))
    (pad 24 thru_hole circle (at 17.78 -27.94 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad24)"))
    (pad 23 thru_hole circle (at 17.78 -25.4 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad23)"))
    (pad 22 thru_hole circle (at 17.78 -22.86 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad22)"))
    (pad 21 thru_hole circle (at 17.78 -20.32 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad21)"))
    (pad 20 thru_hole circle (at 17.78 -17.78 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad20)"))
    (pad 19 thru_hole circle (at 17.78 -15.24 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad19)"))
    (pad 18 thru_hole circle (at 17.78 -12.7 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad18)"))
    (pad 17 thru_hole circle (at 17.78 -10.16 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad17)"))
    (pad 16 thru_hole circle (at 17.78 -7.62 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad16)"))
    (pad 15 thru_hole circle (at 17.78 -5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad15)"))
    (pad 14 thru_hole circle (at 17.78 -2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad14)"))
    (pad 13 thru_hole circle (at 17.78 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad13)"))
    (pad 1 thru_hole rect (at 0 -27.94 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -25.4 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad2)"))
    (pad 3 thru_hole circle (at 0 -22.86 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad3)"))
    (pad 4 thru_hole circle (at 0 -20.32 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad4)"))
    (pad 5 thru_hole circle (at 0 -17.78 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad5)"))
    (pad 6 thru_hole circle (at 0 -15.24 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad6)"))
    (pad 7 thru_hole circle (at 0 -12.7 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad7)"))
    (pad 8 thru_hole circle (at 0 -10.16 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad8)"))
    (pad 9 thru_hole circle (at 0 -7.62 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad9)"))
    (pad 10 thru_hole circle (at 0 -5.08 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad10)"))
    (pad 11 thru_hole circle (at 0 -2.54 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad11)"))
    (pad 12 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad12)"))
  )
  (gr_line (start 64.77 104.14) (end 64.77 68.58) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.14 104.14) (end 64.77 104.14) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104.14 68.58) (end 104.14 104.14) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.77 68.58) (end 104.14 68.58) (layer Edge.Cuts) (width 0.1))
)
