(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 31)
    (tracks 480)
    (zones 0)
    (modules 63)
    (nets 70)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4064)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.1524)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.25)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 /A0)
  (net 3 /A1)
  (net 4 /A2)
  (net 5 GND)
  (net 6 "Net-(XA1-PadVIN)")
  (net 7 "Net-(XA1-Pad3V3)")
  (net 8 "Net-(XA1-PadRST1)")
  (net 9 "Net-(XA1-PadIORF)")
  (net 10 "Net-(XA1-PadAREF)")
  (net 11 /A3)
  (net 12 "Net-(D1-Pad2)")
  (net 13 "Net-(D2-Pad2)")
  (net 14 "Net-(D3-Pad2)")
  (net 15 "Net-(D4-Pad2)")
  (net 16 "Net-(D5-Pad2)")
  (net 17 "Net-(D6-Pad2)")
  (net 18 "Net-(D7-Pad2)")
  (net 19 "Net-(D8-Pad2)")
  (net 20 "Net-(D9-Pad2)")
  (net 21 "Net-(D10-Pad2)")
  (net 22 "Net-(D11-Pad2)")
  (net 23 "Net-(D12-Pad2)")
  (net 24 "Net-(D13-Pad2)")
  (net 25 "Net-(D14-Pad2)")
  (net 26 "Net-(D15-Pad2)")
  (net 27 "Net-(D16-Pad2)")
  (net 28 "Net-(D17-Pad2)")
  (net 29 "Net-(D18-Pad2)")
  (net 30 "Net-(D19-Pad2)")
  (net 31 "Net-(D20-Pad2)")
  (net 32 "Net-(J2-Pad1)")
  (net 33 "Net-(J2-Pad3)")
  (net 34 "Net-(J2-Pad5)")
  (net 35 "Net-(J2-Pad7)")
  (net 36 "Net-(J2-Pad9)")
  (net 37 "Net-(J2-Pad11)")
  (net 38 "Net-(J2-Pad13)")
  (net 39 "Net-(J2-Pad15)")
  (net 40 "Net-(J2-Pad17)")
  (net 41 "Net-(J2-Pad19)")
  (net 42 "Net-(J2-Pad2)")
  (net 43 "Net-(J2-Pad4)")
  (net 44 "Net-(J2-Pad6)")
  (net 45 "Net-(J2-Pad8)")
  (net 46 "Net-(J2-Pad10)")
  (net 47 "Net-(J2-Pad12)")
  (net 48 "Net-(J2-Pad14)")
  (net 49 "Net-(J2-Pad16)")
  (net 50 "Net-(J2-Pad18)")
  (net 51 "Net-(J2-Pad20)")
  (net 52 /D0)
  (net 53 /D1)
  (net 54 /D2)
  (net 55 /D3)
  (net 56 /D4)
  (net 57 /D5)
  (net 58 /D6)
  (net 59 /D7)
  (net 60 /D8)
  (net 61 /D9)
  (net 62 /D10)
  (net 63 "Net-(XA1-PadSCL)")
  (net 64 "Net-(XA1-PadSDA)")
  (net 65 /D13)
  (net 66 /D12)
  (net 67 /D11)
  (net 68 /A4)
  (net 69 /A5)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D17-Pad2)")
    (add_net "Net-(D18-Pad2)")
    (add_net "Net-(D19-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D20-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(XA1-Pad3V3)")
    (add_net "Net-(XA1-PadAREF)")
    (add_net "Net-(XA1-PadIORF)")
    (add_net "Net-(XA1-PadRST1)")
    (add_net "Net-(XA1-PadSCL)")
    (add_net "Net-(XA1-PadSDA)")
    (add_net "Net-(XA1-PadVIN)")
  )
  (module footprints:Arduino_Uno_Shield locked (layer F.Cu) (tedit 5FB3F857)
    (at 195.75 66.75 180)
    (descr https://store.arduino.cc/arduino-uno-rev3)
    (fp_text reference XA1 (at 2.54 -54.356) (layer F.SilkS))
    (fp_text value Arduino_Uno_Shield (at 15.494 -54.356) (layer F.Fab))
    (pad A0 thru_hole oval (at 50.8 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /A0))
    (pad VIN thru_hole oval (at 45.72 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(XA1-PadVIN)"))
    (pad GND3 thru_hole oval (at 43.18 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad GND2 thru_hole oval (at 40.64 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 5V1 thru_hole oval (at 38.1 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3V3 thru_hole oval (at 35.56 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(XA1-Pad3V3)"))
    (pad RST1 thru_hole oval (at 33.02 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(XA1-PadRST1)"))
    (pad IORF thru_hole oval (at 30.48 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(XA1-PadIORF)"))
    (pad D0 thru_hole oval (at 63.5 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 /D0))
    (pad D1 thru_hole oval (at 60.96 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 /D1))
    (pad D2 thru_hole oval (at 58.42 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 /D2))
    (pad D3 thru_hole oval (at 55.88 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 /D3))
    (pad D4 thru_hole oval (at 53.34 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 /D4))
    (pad D5 thru_hole oval (at 50.8 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 /D5))
    (pad D6 thru_hole oval (at 48.26 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 /D6))
    (pad D7 thru_hole oval (at 45.72 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 /D7))
    (pad GND1 thru_hole oval (at 26.416 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad D8 thru_hole oval (at 41.656 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 /D8))
    (pad D9 thru_hole oval (at 39.116 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 61 /D9))
    (pad D10 thru_hole oval (at 36.576 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 /D10))
    (pad SCL thru_hole oval (at 18.796 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 "Net-(XA1-PadSCL)"))
    (pad SDA thru_hole oval (at 21.336 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 "Net-(XA1-PadSDA)"))
    (pad AREF thru_hole oval (at 23.876 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(XA1-PadAREF)"))
    (pad D13 thru_hole oval (at 28.956 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 /D13))
    (pad D12 thru_hole oval (at 31.496 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 /D12))
    (pad D11 thru_hole oval (at 34.036 -50.8 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 /D11))
    (pad "" thru_hole oval (at 27.94 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A1 thru_hole oval (at 53.34 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /A1))
    (pad A2 thru_hole oval (at 55.88 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /A2))
    (pad A3 thru_hole oval (at 58.42 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /A3))
    (pad A4 thru_hole oval (at 60.96 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 68 /A4))
    (pad A5 thru_hole oval (at 63.5 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 69 /A5))
  )
  (module footprints:Harwin_Gecko-G125-MVX2005L0X_2x10_P1.25mm_Vertical (layer F.Cu) (tedit 62ED7290)
    (at 147 79)
    (descr "Harwin Gecko Connector, 20 pins, dual row male, vertical entry, no latches, PN:G125-MVX2005L0X")
    (tags "connector harwin gecko")
    (fp_text reference J1 (at -1.5 -0.5) (layer F.SilkS))
    (fp_text value Conn_02x10_Top_Bottom (at 5.625 -4.3) (layer F.Fab))
    (fp_text user %R (at 5.625 0) (layer F.Fab))
    (pad 20 thru_hole circle (at 11.25 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 65 /D13))
    (pad 19 thru_hole circle (at 10 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 66 /D12))
    (pad 18 thru_hole circle (at 8.75 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 67 /D11))
    (pad 17 thru_hole circle (at 7.5 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 62 /D10))
    (pad 16 thru_hole circle (at 6.25 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 2 /A0))
    (pad 15 thru_hole circle (at 5 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 3 /A1))
    (pad 14 thru_hole circle (at 3.75 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 4 /A2))
    (pad 13 thru_hole circle (at 2.5 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 11 /A3))
    (pad 12 thru_hole circle (at 1.25 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 68 /A4))
    (pad 11 thru_hole circle (at 0 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 69 /A5))
    (pad 10 thru_hole circle (at 11.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 61 /D9))
    (pad 9 thru_hole circle (at 10 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 60 /D8))
    (pad 8 thru_hole circle (at 8.75 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 59 /D7))
    (pad 7 thru_hole circle (at 7.5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 58 /D6))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 57 /D5))
    (pad 5 thru_hole circle (at 5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 56 /D4))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 55 /D3))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 54 /D2))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 53 /D1))
    (pad 1 thru_hole rect (at 0 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 52 /D0))
    (model ${KISYS3DMOD}/Connector_Harwin.3dshapes/Harwin_Gecko-G125-MVX2005L0X_2x10_P1.25mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 145 103.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 147 103.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 149 103.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 151 103.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 153 103.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(J2-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 155 103.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D6-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(J2-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 157 103.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(D7-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(J2-Pad7)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 159 103.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(D8-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(J2-Pad8)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 161 103.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(D9-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(J2-Pad9)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 163 103.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(D10-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(J2-Pad10)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 145 89.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(J2-Pad11)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 147 89.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(J2-Pad12)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D12-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 149 89.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(J2-Pad13)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D13-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 151 89.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(J2-Pad14)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D14-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 153 89.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(J2-Pad15)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D15-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 155 89.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(J2-Pad16)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D16-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 157 89.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(J2-Pad17)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(D17-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 159 89.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(J2-Pad18)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(D18-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 161 89.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(J2-Pad19)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(D19-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603_1608Metric (layer F.Cu) (tedit 62D732F1)
    (at 163 89.175 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 330 (at -2.54 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(J2-Pad20)"))
    (pad 1 smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(D20-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 139 113 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 1 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 142.5 113 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D2 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 2 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 146 113 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D3 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 3 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 149.5 113 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D4 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 4 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 153 113 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D5 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 5 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 156.5 113 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D6 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 6 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D6-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 160 113 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D7 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 7 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(D7-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 163.5 113 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D8 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 8 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(D8-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 167 113 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D9 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 9 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(D9-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 170.5 113 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D10 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 10 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(D10-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 139 110.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D11 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 11 (at 0 1.43 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D11-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 142.5 110.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D12 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 12 (at 0 1.43 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(D12-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 146 110.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D13 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 13 (at 0 1.43 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D13-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 149.5 110.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D14 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 14 (at 0 1.43 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(D14-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 153 110.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D15 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 15 (at 0 1.43 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(D15-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 156.5 110.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D16 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 16 (at 0 1.43 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(D16-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 160.0375 110.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D17 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 17 (at 0 1.43 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(D17-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 163.5 110.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D18 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 18 (at 0 1.43 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(D18-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 167 110.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D19 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 19 (at 0 1.43 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(D19-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:LED_0603_1608Metric (layer F.Cu) (tedit 62D730E1)
    (at 170.5 110.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D20 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 20 (at 0 1.43 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(D20-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Harwin_Gecko-G125-MVX2005L0X_2x10_P1.25mm_Vertical (layer F.Cu) (tedit 62D72C93)
    (at 147 97)
    (descr "Harwin Gecko Connector, 20 pins, dual row male, vertical entry, no latches, PN:G125-MVX2005L0X")
    (tags "connector harwin gecko")
    (fp_text reference J2 (at -2 -0.5) (layer F.SilkS))
    (fp_text value Conn_02x10_Top_Bottom (at 5.625 -4.3) (layer F.Fab))
    (fp_text user %R (at 5.625 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 1.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 42 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 2.5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at 3.75 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 43 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at 5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at 6.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 44 "Net-(J2-Pad6)"))
    (pad 7 thru_hole circle (at 7.5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad7)"))
    (pad 8 thru_hole circle (at 8.75 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 45 "Net-(J2-Pad8)"))
    (pad 9 thru_hole circle (at 10 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad9)"))
    (pad 10 thru_hole circle (at 11.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 46 "Net-(J2-Pad10)"))
    (pad 11 thru_hole circle (at 0 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad11)"))
    (pad 12 thru_hole circle (at 1.25 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 47 "Net-(J2-Pad12)"))
    (pad 13 thru_hole circle (at 2.5 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad13)"))
    (pad 14 thru_hole circle (at 3.75 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 48 "Net-(J2-Pad14)"))
    (pad 15 thru_hole circle (at 5 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad15)"))
    (pad 16 thru_hole circle (at 6.25 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 49 "Net-(J2-Pad16)"))
    (pad 17 thru_hole circle (at 7.5 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad17)"))
    (pad 18 thru_hole circle (at 8.75 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 50 "Net-(J2-Pad18)"))
    (pad 19 thru_hole circle (at 10 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad19)"))
    (pad 20 thru_hole circle (at 11.25 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 51 "Net-(J2-Pad20)"))
    (model ${KISYS3DMOD}/Connector_Harwin.3dshapes/Harwin_Gecko-G125-MVX2005L0X_2x10_P1.25mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 146 82.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user 1 (at 0 1) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 52 /D0))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 147.5 82.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP2 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (fp_text user 2 (at 0 1 unlocked) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 53 /D1))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 149 82.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP3 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user 3 (at 0 1 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 54 /D2))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 150.5 82.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP4 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (fp_text user 4 (at 0 1 unlocked) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 55 /D3))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 152 82.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP5 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user 5 (at 0 1 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 56 /D4))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 153.5 82.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP6 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (fp_text user 6 (at 0 1 unlocked) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 57 /D5))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 155 82.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP7 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user 7 (at 0 1 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 58 /D6))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 156.5 82.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP8 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (fp_text user 8 (at 0 1 unlocked) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 59 /D7))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 158 82.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP9 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user 9 (at 0 1 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 60 /D8))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 159.5 82.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP10 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (fp_text user 10 (at 0 1 unlocked) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 61 /D9))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 146 74)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP11 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user 11 (at 0 1) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 69 /A5))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 147.5 74)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP12 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user 12 (at 0 1) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 68 /A4))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 149 74)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP13 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (fp_text user 13 (at 0 1) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 11 /A3))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 150.5 74)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP14 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user 14 (at 0 1) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 4 /A2))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 152 74)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP15 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (fp_text user 15 (at 0 1) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 3 /A1))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 153.5 74)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP16 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user 16 (at 0 1) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 2 /A0))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 155 74)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP17 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (fp_text user 17 (at 0 1 unlocked) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 62 /D10))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 156.5 74)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP18 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user 18 (at 0 1) (layer F.SilkS))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 67 /D11))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 158 74)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP19 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (fp_text user 19 (at 0 1) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 66 /D12))
  )
  (module footprints:TestPoint (layer F.Cu) (tedit 62ED58D5)
    (at 159.5 74)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP20 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (fp_text user 20 (at 0 1) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 65 /D13))
  )
  (gr_text "V 0.0  Aug 2022" (at 169.5 113) (layer B.SilkS))
  (gr_text "Gecko Connector\nTester" (at 170 92 90) (layer F.SilkS))
  (dimension 3 (width 0.15) (layer Dwgs.User)
    (gr_text "3.000 mm" (at 142.7 76.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 147 75) (xy 143.413579 75)))
    (feature2 (pts (xy 147 78) (xy 143.413579 78)))
    (crossbar (pts (xy 144 78) (xy 144 75)))
    (arrow1a (pts (xy 144 75) (xy 144.586421 76.126504)))
    (arrow1b (pts (xy 144 75) (xy 143.413579 76.126504)))
    (arrow2a (pts (xy 144 78) (xy 144.586421 76.873496)))
    (arrow2b (pts (xy 144 78) (xy 143.413579 76.873496)))
  )
  (dimension 3.5 (width 0.15) (layer Dwgs.User)
    (gr_text "3.500 mm" (at 142.7 80.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 147 82.5) (xy 143.413579 82.5)))
    (feature2 (pts (xy 147 79) (xy 143.413579 79)))
    (crossbar (pts (xy 144 79) (xy 144 82.5)))
    (arrow1a (pts (xy 144 82.5) (xy 143.413579 81.373496)))
    (arrow1b (pts (xy 144 82.5) (xy 144.586421 81.373496)))
    (arrow2a (pts (xy 144 79) (xy 143.413579 80.126504)))
    (arrow2b (pts (xy 144 79) (xy 144.586421 80.126504)))
  )
  (gr_line (start 130 108) (end 127 105) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130 118) (end 130 108) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177 120) (end 132 120) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177 67) (end 176 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 177 69) (end 177 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179 118) (end 179 69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130 67) (end 176 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 70) (end 130 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 105) (end 127 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132 118) (end 132 120) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 177 118) (end 179 118) (angle 90) (layer Edge.Cuts) (width 0.15))
)
