(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 68)
    (no_connects 6)
    (area 55.747857 46.795 154.437143 91.735)
    (thickness 1.6)
    (drawings 17)
    (tracks 204)
    (zones 0)
    (modules 26)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 R1)
  (net 2 "Net-(D1-Pad2)")
  (net 3 R2)
  (net 4 "Net-(D2-Pad2)")
  (net 5 R3)
  (net 6 "Net-(D3-Pad2)")
  (net 7 "Net-(D4-Pad2)")
  (net 8 "Net-(D5-Pad2)")
  (net 9 "Net-(D6-Pad2)")
  (net 10 "Net-(IC1-Pad1)")
  (net 11 GND)
  (net 12 "Net-(IC1-Pad5)")
  (net 13 +3V3)
  (net 14 "Net-(IC1-Pad10)")
  (net 15 "Net-(EN1-Pad5)")
  (net 16 "Net-(EN2-Pad5)")
  (net 17 C1)
  (net 18 C2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net C1)
    (add_net C2)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(EN1-Pad5)")
    (add_net "Net-(EN2-Pad5)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad5)")
    (add_net R1)
    (add_net R2)
    (add_net R3)
  )
  (net_class Power ""
    (clearance 0.3)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5ABB105E)
    (at 85.725 59.69 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value 33k (at -2.54 0 450) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 R1))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(EN1-Pad5)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5ABB106C)
    (at 88.265 59.69 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value 15k (at -2.54 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 R1))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(EN2-Pad5)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A138E25)
    (at 86.995 52.07)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.Fab))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A138E2C)
    (at 65.405 86.36)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.Fab))
    (fp_text value MountingHole_3.2mm_M3 (at 0 2.54) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A138E32)
    (at 86.995 86.36)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.Fab))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A138E20)
    (at 65.405 52.07)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.Fab))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A138E46)
    (at 144.78 69.215)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.Fab))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5A138E40)
    (at 119.38 69.215)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.Fab))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Trinket:Trinket_3v3 (layer F.Cu) (tedit 5A120419)
    (at 76.2 48.26)
    (fp_text reference IC1 (at 0 1.27) (layer F.Fab))
    (fp_text value Trinket3v3 (at 0 6.985) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.35 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 3 thru_hole circle (at -6.35 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 R2))
    (pad 4 thru_hole circle (at -6.35 16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 R3))
    (pad 5 thru_hole circle (at -6.35 19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole circle (at 6.35 19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 +3V3))
    (pad 7 thru_hole circle (at 6.35 16.51) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 R1))
    (pad 8 thru_hole circle (at 6.35 13.97) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 C2))
    (pad 9 thru_hole circle (at 6.35 11.43) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 C1))
    (pad 10 thru_hole circle (at 6.35 8.89) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(IC1-Pad10)"))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5ABB107B)
    (at 86.995 71.755 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value 15k (at 3.81 1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 R1))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Misc:Diode_SmallDualSize (layer F.Cu) (tedit 5A2CC86F)
    (at 69.85 76.835 270)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D6 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value D (at 3.81 2.06 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 R3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D6-Pad2)"))
    (pad 2 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Misc:Diode_SmallDualSize (layer F.Cu) (tedit 5A2CC86F)
    (at 72.39 76.835 270)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D5 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value D (at 3.81 2.06 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 R3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D5-Pad2)"))
    (pad 2 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Misc:Diode_SmallDualSize (layer F.Cu) (tedit 5A2CC86F)
    (at 74.93 76.835 270)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D4 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value D (at 3.81 2.06 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 R2))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 2 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Misc:Diode_SmallDualSize (layer F.Cu) (tedit 5A2CC86F)
    (at 77.47 76.835 270)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value D (at 3.81 2.06 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 R2))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 2 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Misc:Diode_SmallDualSize (layer F.Cu) (tedit 5A2CC86F)
    (at 80.01 76.835 270)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value D (at 3.81 2.06 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 R1))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Misc:Diode_SmallDualSize (layer F.Cu) (tedit 5A2CC86F)
    (at 82.55 76.835 270)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value D (at 3.81 2.06 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 R1))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 6.35 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Keyboard:CHERRY_MXML_KAILH_PCB_100H (layer F.Cu) (tedit 5AC01573)
    (at 101.6 59.055 90)
    (fp_text reference SW5 (at 2.921 3.048 90) (layer F.SilkS))
    (fp_text value SPST (at 3.556 3.048 90) (layer F.SilkS) hide)
    (fp_text user 1.00u (at -5.715 8.255 90) (layer Dwgs.User))
    (pad 1 thru_hole circle (at 2.54 -5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 17 C1))
    (pad 2 thru_hole circle (at -3.81 -2.54 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(D5-Pad2)"))
    (pad HOLE thru_hole circle (at 0 0 90) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad HOLE thru_hole circle (at -5.08 0 90) (size 1.7272 1.7272) (drill 1.7272) (layers *.Cu *.Mask))
    (pad HOLE thru_hole circle (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.7272) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -5.08 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(D5-Pad2)"))
    (pad 1 thru_hole circle (at 0 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 17 C1))
    (pad 2 thru_hole circle (at 5.08 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(D5-Pad2)"))
    (pad 2 thru_hole circle (at 0 5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(D5-Pad2)"))
    (pad 1 thru_hole circle (at 0 -5.9 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 17 C1))
    (pad HOLE thru_hole circle (at 5.5 0 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.SilkS *.Mask))
    (pad HOLE thru_hole circle (at -5.5 0 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.SilkS *.Mask))
  )
  (module Keyboard:CHERRY_MXML_KAILH_PCB_100H (layer F.Cu) (tedit 5AC0157D)
    (at 121.92 59.055 90)
    (fp_text reference SW3 (at 2.921 3.048 90) (layer F.SilkS))
    (fp_text value SPST (at 3.556 3.048 90) (layer F.SilkS) hide)
    (fp_text user 1.00u (at -5.715 8.255 90) (layer Dwgs.User))
    (pad 1 thru_hole circle (at 2.54 -5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 17 C1))
    (pad 2 thru_hole circle (at -3.81 -2.54 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad HOLE thru_hole circle (at 0 0 90) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad HOLE thru_hole circle (at -5.08 0 90) (size 1.7272 1.7272) (drill 1.7272) (layers *.Cu *.Mask))
    (pad HOLE thru_hole circle (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.7272) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -5.08 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 thru_hole circle (at 0 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 17 C1))
    (pad 2 thru_hole circle (at 5.08 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 2 thru_hole circle (at 0 5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 thru_hole circle (at 0 -5.9 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 17 C1))
    (pad HOLE thru_hole circle (at 5.5 0 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.SilkS *.Mask))
    (pad HOLE thru_hole circle (at -5.5 0 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.SilkS *.Mask))
  )
  (module Keyboard:CHERRY_MXML_KAILH_PCB_100H (layer F.Cu) (tedit 5AC015A1)
    (at 142.24 59.055 90)
    (fp_text reference SW1 (at 2.921 3.048 90) (layer F.SilkS))
    (fp_text value SPST (at 3.556 3.048 90) (layer F.SilkS) hide)
    (fp_text user 1.00u (at -5.715 8.255 90) (layer Dwgs.User))
    (pad 1 thru_hole circle (at 2.54 -5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 17 C1))
    (pad 2 thru_hole circle (at -3.81 -2.54 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad HOLE thru_hole circle (at 0 0 90) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad HOLE thru_hole circle (at -5.08 0 90) (size 1.7272 1.7272) (drill 1.7272) (layers *.Cu *.Mask))
    (pad HOLE thru_hole circle (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.7272) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -5.08 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at 0 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 17 C1))
    (pad 2 thru_hole circle (at 5.08 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 0 5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at 0 -5.9 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 17 C1))
    (pad HOLE thru_hole circle (at 5.5 0 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.SilkS *.Mask))
    (pad HOLE thru_hole circle (at -5.5 0 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.SilkS *.Mask))
  )
  (module Keyboard:CHERRY_MXML_KAILH_PCB_100H (layer F.Cu) (tedit 5AC01598)
    (at 142.24 79.375 90)
    (fp_text reference SW2 (at -2.794 3.048 90) (layer F.SilkS))
    (fp_text value SPST (at 3.556 3.048 90) (layer F.SilkS) hide)
    (fp_text user 1.00u (at -5.715 8.255 90) (layer Dwgs.User))
    (pad 1 thru_hole circle (at 2.54 -5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 18 C2))
    (pad 2 thru_hole circle (at -3.81 -2.54 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad HOLE thru_hole circle (at 0 0 90) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad HOLE thru_hole circle (at -5.08 0 90) (size 1.7272 1.7272) (drill 1.7272) (layers *.Cu *.Mask))
    (pad HOLE thru_hole circle (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.7272) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -5.08 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at 0 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 18 C2))
    (pad 2 thru_hole circle (at 5.08 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 0 5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at 0 -5.9 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 18 C2))
    (pad HOLE thru_hole circle (at 5.5 0 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.SilkS *.Mask))
    (pad HOLE thru_hole circle (at -5.5 0 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.SilkS *.Mask))
  )
  (module Keyboard:CHERRY_MXML_KAILH_PCB_100H (layer F.Cu) (tedit 5AC01587)
    (at 121.92 79.375 90)
    (fp_text reference SW4 (at -2.794 3.048 90) (layer F.SilkS))
    (fp_text value SPST (at 3.556 3.048 90) (layer F.SilkS) hide)
    (fp_text user 1.00u (at -5.715 8.255 90) (layer Dwgs.User))
    (pad 1 thru_hole circle (at 2.54 -5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 18 C2))
    (pad 2 thru_hole circle (at -3.81 -2.54 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad HOLE thru_hole circle (at 0 0 90) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad HOLE thru_hole circle (at -5.08 0 90) (size 1.7272 1.7272) (drill 1.7272) (layers *.Cu *.Mask))
    (pad HOLE thru_hole circle (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.7272) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -5.08 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 1 thru_hole circle (at 0 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 18 C2))
    (pad 2 thru_hole circle (at 5.08 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 2 thru_hole circle (at 0 5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(D4-Pad2)"))
    (pad 1 thru_hole circle (at 0 -5.9 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 18 C2))
    (pad HOLE thru_hole circle (at 5.5 0 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.SilkS *.Mask))
    (pad HOLE thru_hole circle (at -5.5 0 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.SilkS *.Mask))
  )
  (module Keyboard:CHERRY_MXML_KAILH_PCB_100H (layer F.Cu) (tedit 5AC0155C)
    (at 101.6 79.375 90)
    (fp_text reference SW6 (at -2.794 3.048 90) (layer F.SilkS))
    (fp_text value SPST (at 3.556 3.048 90) (layer F.SilkS) hide)
    (fp_text user 1.00u (at -5.715 8.255 90) (layer Dwgs.User))
    (pad 1 thru_hole circle (at 2.54 -5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 18 C2))
    (pad 2 thru_hole circle (at -3.81 -2.54 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(D6-Pad2)"))
    (pad HOLE thru_hole circle (at 0 0 90) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad HOLE thru_hole circle (at -5.08 0 90) (size 1.7272 1.7272) (drill 1.7272) (layers *.Cu *.Mask))
    (pad HOLE thru_hole circle (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.7272) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -5.08 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(D6-Pad2)"))
    (pad 1 thru_hole circle (at 0 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 18 C2))
    (pad 2 thru_hole circle (at 5.08 -3.81 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(D6-Pad2)"))
    (pad 2 thru_hole circle (at 0 5.08 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(D6-Pad2)"))
    (pad 1 thru_hole circle (at 0 -5.9 90) (size 2.286 2.286) (drill 1.4986) (layers *.Cu *.Mask)
      (net 18 C2))
    (pad HOLE thru_hole circle (at 5.5 0 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.SilkS *.Mask))
    (pad HOLE thru_hole circle (at -5.5 0 90) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.SilkS *.Mask))
  )
  (module Logos:a-015-1200 (layer F.Cu) (tedit 0)
    (at 65.405 58.42 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module "Rotary Encoder:Encoder_Bourns_PEC11_12mm_123" (layer F.Cu) (tedit 5AC0156D)
    (at 103.505 69.215 90)
    (fp_text reference EN1 (at 0 0 90) (layer F.SilkS))
    (fp_text value ROTARY_ENCODER_SWITCH (at 0 9.525 90) (layer F.Fab))
    (pad "" thru_hole rect (at -5.7 0 90) (size 3.4 3.4) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.5 7.5 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 R3))
    (pad 3 thru_hole circle (at 2.5 7.5 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 R2))
    (pad 2 thru_hole circle (at 0 7.5 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad "" thru_hole rect (at 5.7 0 90) (size 3.4 3.4) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 2.5 -7 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(EN1-Pad5)"))
    (pad 4 thru_hole circle (at -2.5 -7 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
  )
  (module "Rotary Encoder:Encoder_Bourns_PEC11_12mm_123" (layer F.Cu) (tedit 5AC01591)
    (at 132.08 69.215 90)
    (fp_text reference EN2 (at 0 0 90) (layer F.SilkS))
    (fp_text value ROTARY_ENCODER_SWITCH (at 0 9.525 90) (layer F.Fab))
    (pad "" thru_hole rect (at -5.7 0 90) (size 3.4 3.4) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.5 7.5 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 C1))
    (pad 3 thru_hole circle (at 2.5 7.5 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 18 C2))
    (pad 2 thru_hole circle (at 0 7.5 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
    (pad "" thru_hole rect (at 5.7 0 90) (size 3.4 3.4) (drill 2.6) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 2.5 -7 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(EN2-Pad5)"))
    (pad 4 thru_hole circle (at -2.5 -7 90) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 GND))
  )
  (module Logos:a-015-1200 (layer B.Cu) (tedit 0)
    (at 76.2 62.23 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text "CC BY-NC-SA 4.0\nRev 3, March 2018" (at 92.075 69.215 270) (layer F.SilkS))
  (gr_line (start 62.865 48.26) (end 64.135 48.26) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 62.865 90.17) (end 64.135 90.17) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 151.765 90.17) (end 64.135 90.17) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 64.135 48.26) (end 151.765 48.26) (layer Edge.Cuts) (width 0.2))
  (gr_text "MiniKbd : Andy Clymer\nwww.andy.ac/minikbd" (at 65.405 60.96 270) (layer F.SilkS))
  (gr_text "Adafruit\nTrinket M0" (at 76.2 55.88) (layer F.SilkS))
  (gr_arc (start 62.865 49.53) (end 61.595 49.53) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 62.865 88.9) (end 62.865 90.17) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 61.595 49.53) (end 61.595 88.9) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 153.035 49.53) (end 153.035 88.9) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 151.765 88.9) (end 153.035 88.9) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 151.765 49.53) (end 151.765 48.26) (angle 90) (layer Edge.Cuts) (width 0.2))
)
