<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="17.78" y1="18.7452" x2="0" y2="18.7452" width="0" layer="20"/>
<wire x1="0" y1="18.7452" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="17.78" y2="0" width="0" layer="20"/>
<wire x1="17.78" y1="0" x2="17.78" y2="18.7452" width="0" layer="20"/>
<hole x="16.2052" y="17.1704" drill="1.6"/>
<text>USB Snoop 
(C) KC Lee
CC-BY
4.0</text>
</plain>
<libraries>
<library name="con-berg">
<description>&lt;b&gt;Berg Connectors&lt;/b&gt;&lt;p&gt;
Based on  the following source:
&lt;ul&gt;
&lt;li&gt;http://catalog.fciconnect.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="PN87520-S">
<description>&lt;b&gt;USB connector&lt;/b&gt; with shield&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="Misc Conn">
<packages>
<package name="CHINESE_USB_M_SMT-2">
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="2X03M_TH">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2</description>
</package>
</packages>
</library>
<library name="ipc-7351-capacitor">
<description>&lt;b&gt;IPC-7351 compliant SMT capacitors&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Symbols copied from CadSoft rcl.lbr&lt;br&gt;
Packages generated using genpkg_chp.ulp, genpkg_cae.ulp and genpkg_mld.ulp&lt;br&gt;
Devices are Vishay chip types, generic AEC types and Kemet T491 series molded body types.&lt;br&gt;
&lt;br&gt;
Weartronics 2006&lt;br&gt;
http://www.weartronics.com/</description>
<packages>
<package name="CAPC1608X92N">
</package>
</packages>
</library>
<library name="Misc Power">
<packages>
<package name="SOT95P280X135-3N">
</package>
</packages>
</library>
<library name="Misc Processor">
<packages>
<package name="TSSOP20">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TC26H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74xx-little-us">
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
SOT753 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML0603">
<description>&lt;b&gt;SML0603-XXX (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;AG3K&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;B1K&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R1K&lt;/td&gt;&lt;td&gt;SUPER RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R3K&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3K&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3KH&lt;/td&gt;&lt;td&gt;SOFT ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3KH&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3K&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;2CW&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0092.pdf</description>
</package>
</packages>
</library>
<library name="ipc-7351-resistor">
<description>&lt;b&gt;IPC-7351 compliant SMT resistors&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Symbols copied from CadSoft rcl.lbr.&lt;br&gt;
Packages generated using genpkg_chp.ulp.&lt;br&gt;
Devices are Panasonic ERJ series types.&lt;br&gt;
&lt;br&gt;
Weartronics 2006&lt;br&gt;
http://www.weartronics.com/</description>
<packages>
<package name="RESC1608X55N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="Misc Processor" package="TSSOP20" value="STM32F030F4P6">
<attribute name="PARTNO" value="*"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="ipc-7351-capacitor" package="CAPC1608X92N" value="0.1uF">
<attribute name="PARTNO" value="*"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="Misc Conn" package="1X04" value="">
<attribute name="VALUE"/>
<attribute name="PARTNO" value="1x04 header 2.54mm"/>
</element>
<element name="X1" library="crystal" package="TC26H" value="16MHz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="PARTNO" value="*"/>
</element>
<element name="C2" library="ipc-7351-capacitor" package="CAPC1608X92N" value="22pF">
<attribute name="PARTNO" value="*"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="ipc-7351-capacitor" package="CAPC1608X92N" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNO" value="*"/>
</element>
<element name="C6" library="ipc-7351-capacitor" package="CAPC1608X92N" value="1uF">
<attribute name="PARTNO" value="STOCK: 1UF/10V 20% TDK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="ipc-7351-capacitor" package="CAPC1608X92N" value="1uF">
<attribute name="PARTNO" value="STOCK: 1UF/10V 20% TDK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Misc Power" package="SOT95P280X135-3N" value="XC6206P332MR">
<attribute name="PARTNO" value="*"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="con-berg" package="PN87520-S" value="PN87520-S">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="Misc Conn" package="CHINESE_USB_M_SMT-2" value="USBA-M-DXSMT2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="ipc-7351-capacitor" package="CAPC1608X92N" value="0.1uF">
<attribute name="PARTNO" value="*"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="74xx-little-us" package="SOT23-5" value="74LVC1G02DBV">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="ipc-7351-capacitor" package="CAPC1608X92N" value="0.1uF">
<attribute name="PARTNO" value="*"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="Misc Conn" package="2X03M_TH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="SML0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="ipc-7351-resistor" package="RESC1608X55N" value="1K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="AGND">
<contactref element="U2" pad="15"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="J3" pad="S1"/>
<contactref element="J3" pad="S2"/>
<contactref element="J2" pad="S1"/>
<contactref element="J2" pad="S2"/>
<contactref element="J2" pad="4"/>
<contactref element="J3" pad="4"/>
<contactref element="U2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="C7" pad="1"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="+3.3V">
<contactref element="U2" pad="16"/>
<contactref element="U2" pad="5"/>
<contactref element="J1" pad="4"/>
<contactref element="U1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U3" pad="5"/>
<contactref element="C7" pad="2"/>
<contactref element="J4" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="!RST">
<contactref element="U2" pad="4"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="SWCLK">
<contactref element="U2" pad="20"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SWDIO">
<contactref element="U2" pad="19"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$41">
<contactref element="X1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="VUSB">
<contactref element="U1" pad="3"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$21">
</signal>
<signal name="D-">
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="D+">
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="3"/>
<contactref element="U3" pad="1"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="N$1">
<contactref element="C2" pad="2"/>
<contactref element="X1" pad="2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="!RXD">
<contactref element="U2" pad="9"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="SE0">
<contactref element="U3" pad="4"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="!RTS">
<contactref element="U2" pad="7"/>
<contactref element="J4" pad="3"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="!CTS">
<contactref element="U2" pad="6"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="!TXD">
<contactref element="U2" pad="8"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="!LED">
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="18"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
