<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="21.1" y2="0" width="0" layer="20"/>
<wire x1="21.1" y1="0" x2="21.1" y2="21.7" width="0" layer="20"/>
<wire x1="21.1" y1="21.7" x2="0" y2="21.7" width="0" layer="20"/>
<wire x1="0" y1="21.7" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="rcl_smd">
<description>&lt;p&gt;&lt;b&gt;Resistors, Capacitors, Inductors in chip/molded packages&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Land patterns as per IPC-SM-782&lt;/p&gt;
&lt;p&gt;Silk screen outlines as per &lt;a href="http://www.pcblibraries.com/forum/smt-library-silkscreen-outlines_topic26.html"&gt;http://www.pcblibraries.com/forum/smt-library-silkscreen-outlines_topic26.html&lt;/a&gt; with 0.3 mm between the body/pad and line center.&lt;/p&gt;</description>
<packages>
<package name="C0805">
<description>Metric: 2012</description>
</package>
<package name="R0805">
<description>Metric: 2012</description>
</package>
</packages>
</library>
<library name="HeaterMeterPI">
<description>Generated from &lt;b&gt;HeaterMeterPI.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="AnalogDevices">
<packages>
<package name="MS_MSOP8">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl_smd" package="C0805" value="1n"/>
<element name="C9" library="rcl_smd" package="C0805" value="1n"/>
<element name="C2" library="rcl_smd" package="C0805" value="10n"/>
<element name="C3" library="rcl_smd" package="C0805" value="1n"/>
<element name="C4" library="rcl_smd" package="C0805" value="1n"/>
<element name="C5" library="rcl_smd" package="C0805" value="10n"/>
<element name="C6" library="rcl_smd" package="C0805" value="1n"/>
<element name="C7" library="rcl_smd" package="C0805" value="1n"/>
<element name="C8" library="rcl_smd" package="C0805" value="10n"/>
<element name="JP1" library="HeaterMeterPI" package="1X05" value=""/>
<element name="R1" library="rcl_smd" package="R0805" value="10k"/>
<element name="R2" library="rcl_smd" package="R0805" value="10k"/>
<element name="R9" library="rcl_smd" package="R0805" value="1k"/>
<element name="R7" library="rcl_smd" package="R0805" value="10k"/>
<element name="R8" library="rcl_smd" package="R0805" value="10k"/>
<element name="R3" library="rcl_smd" package="R0805" value="1k"/>
<element name="R4" library="rcl_smd" package="R0805" value="10k"/>
<element name="R5" library="rcl_smd" package="R0805" value="10k"/>
<element name="R6" library="rcl_smd" package="R0805" value="1k"/>
<element name="U1" library="AnalogDevices" package="MS_MSOP8" value="AD8495RMZ"/>
<element name="U2" library="AnalogDevices" package="MS_MSOP8" value="AD8495RMZ"/>
<element name="U3" library="AnalogDevices" package="MS_MSOP8" value="AD8495RMZ"/>
<element name="JP4" library="SparkFun" package="1X02" value=""/>
<element name="JP2" library="SparkFun" package="1X02" value=""/>
<element name="JP3" library="SparkFun" package="1X02" value=""/>
<element name="C11" library="resistor" package="C0805" value="0.1u"/>
<element name="F1" library="rcl_smd" package="C0805" value="81-BLM21P221SG "/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C7" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="C11" pad="2"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="5"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R7" pad="1"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="5"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R1" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U3" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="U3" pad="8"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="R4" pad="1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="JP1" pad="4"/>
<contactref element="U3" pad="7"/>
<contactref element="U1" pad="7"/>
<contactref element="U2" pad="7"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="5"/>
<contactref element="F1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
