<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="27.94" y2="0" width="0" layer="20"/>
<wire x1="27.94" y1="0" x2="27.94" y2="29.21" width="0" layer="20"/>
<wire x1="27.94" y1="29.21" x2="0" y2="29.21" width="0" layer="20"/>
<wire x1="0" y1="29.21" x2="0" y2="0" width="0" layer="20"/>
<text>SLEEPYROBOT.COM</text>
<text>TVP5151 for OVERO</text>
<text>VID</text>
<text>GND</text>
<text>Rev 1</text>
</plain>
<libraries>
<library name="chris_eagle6_library">
<packages>
<package name="TQFP32">
</package>
<package name="FH26-27S">
</package>
</packages>
</library>
<library name="00SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOT23-3">
</package>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="chris_eagle6_library" package="TQFP32" value="TVP5151">
<attribute name="NAME"/>
</element>
<element name="U2" library="chris_eagle6_library" package="FH26-27S" value="OVERO_IMAGEROVERO_IMAGER"/>
<element name="C1" library="00SparkFun" package="C0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="00SparkFun" package="C0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="00SparkFun" package="C0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="00SparkFun" package="R0805" value="2.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="00SparkFun" package="R0805" value="2.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="00SparkFun" package="R0805" value="2.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="00SparkFun" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="00SparkFun" package="R0805" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="00SparkFun" package="C0805" value="33pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="00SparkFun" package="C0805" value="33pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="00SparkFun" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="00SparkFun" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="00SparkFun" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="00SparkFun" package="SOT23-3" value="MOSFET-NCHANNELSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="00SparkFun" package="R0805" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="00SparkFun" package="R0805" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="00SparkFun" package="C0805" value="2.7uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="00SparkFun" package="C0805" value="180pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="00SparkFun" package="C0805" value="180pF">
<attribute name="VALUE"/>
</element>
<element name="C11" library="00SparkFun" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="00SparkFun" package="R0805" value="37.4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="00SparkFun" package="R0805" value="37.4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="00SparkFun" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y2" library="00SparkFun" package="HC49US" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="JP1" library="00SparkFun" package="1X02" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="P$30"/>
</signal>
<signal name="N$2">
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="P$29"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="P$31"/>
<contactref element="U1" pad="P$19"/>
<contactref element="U1" pad="P$7"/>
<contactref element="U1" pad="P$3"/>
<contactref element="R4" pad="1"/>
<contactref element="U2" pad="P$23"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="U1" pad="P$2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="P$28"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="TVP_SCL">
<contactref element="U1" pad="P$21"/>
<contactref element="R3" pad="1"/>
<contactref element="U2" pad="P$26"/>
</signal>
<signal name="TVP_SDA">
<contactref element="U1" pad="P$22"/>
<contactref element="R2" pad="1"/>
<contactref element="U2" pad="P$27"/>
</signal>
<signal name="1.8V">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="P$32"/>
<contactref element="U1" pad="P$20"/>
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="P$10"/>
<contactref element="U2" pad="P$21"/>
<contactref element="U1" pad="P$4"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="TVP_INTRQ">
<contactref element="U1" pad="P$27"/>
</signal>
<signal name="AVID">
<contactref element="U1" pad="P$26"/>
</signal>
<signal name="OV_HS">
<contactref element="U1" pad="P$25"/>
<contactref element="U2" pad="P$1"/>
</signal>
<signal name="OV_VS">
<contactref element="U1" pad="P$24"/>
<contactref element="U2" pad="P$2"/>
</signal>
<signal name="OV_FID">
<contactref element="U1" pad="P$23"/>
<contactref element="U2" pad="P$5"/>
</signal>
<signal name="OV_D0">
<contactref element="U1" pad="P$18"/>
<contactref element="U2" pad="P$6"/>
</signal>
<signal name="OV_D1">
<contactref element="U1" pad="P$17"/>
<contactref element="U2" pad="P$7"/>
</signal>
<signal name="OV_D2">
<contactref element="U1" pad="P$16"/>
<contactref element="U2" pad="P$8"/>
</signal>
<signal name="OV_D3">
<contactref element="U1" pad="P$15"/>
<contactref element="U2" pad="P$9"/>
</signal>
<signal name="OV_D4">
<contactref element="U1" pad="P$14"/>
<contactref element="U2" pad="P$10"/>
</signal>
<signal name="OV_D5">
<contactref element="U1" pad="P$13"/>
<contactref element="U2" pad="P$11"/>
</signal>
<signal name="OV_D6">
<contactref element="U1" pad="P$12"/>
<contactref element="U2" pad="P$12"/>
</signal>
<signal name="OV_D7">
<contactref element="U1" pad="P$11"/>
<contactref element="R4" pad="2"/>
<contactref element="U2" pad="P$13"/>
</signal>
<signal name="OV_DCLK">
<contactref element="U1" pad="P$9"/>
<contactref element="U2" pad="P$4"/>
</signal>
<signal name="TVP_RESET">
<contactref element="U1" pad="P$8"/>
<contactref element="R7" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="P$6"/>
<contactref element="R5" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="Y2" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="P$24"/>
</signal>
<signal name="OV_RESET">
<contactref element="Q1" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="U2" pad="P$15"/>
</signal>
<signal name="CAM_VID">
<contactref element="L1" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="L1" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="C4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="P$5"/>
<contactref element="Y2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="C11" pad="1"/>
<contactref element="U1" pad="P$1"/>
</signal>
<signal name="N$9">
</signal>
</signals>
</board>
</drawing>
</eagle>
